// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Copyright (c) 2022 Rockchip Electronics Co., Ltd.
 *
 */

/dts-v1/;
#include "rk3368.dtsi"
#include "rk3368-android.dtsi"
#include "rk3368-cif-sensor.dtsi"
#include <dt-bindings/pwm/pwm.h>
#include <dt-bindings/sensor-dev.h>

/ {
	model = "Rockchip PX5 EVB V11";
	compatible = "rockchip,px5-evb", "rockchip,px5", "rockchip,rk3368";

	chosen: chosen {
		bootargs = "earlycon=uart8250,mmio32,0xff1c0000 firmware_class.path=/system/vendor/firmware";
	};

	fiq_debugger: fiq-debugger {
		compatible = "rockchip,fiq-debugger";
			rockchip,serial-id = <4>;
			rockchip,wake-irq = <0>;
			/* If enable uart uses irq instead of fiq */
			rockchip,irq-mode-enable = <0>;
			/* Only 115200 and 1500000 */
			rockchip,baudrate = <115200>;
			pinctrl-names = "default";
			pinctrl-0 = <&uart4_xfer>;
			interrupts = <GIC_SPI 154 IRQ_TYPE_LEVEL_HIGH>;
	};

	firmware {
		android {
			compatible = "android,firmware";
			fstab {
				compatible = "android,fstab";
				system {
					compatible = "android,system";
					dev = "/dev/block/platform/ff0f0000.dwmmc/by-name/system";
					type = "ext4";
					mnt_flags = "ro,barrier=1,inode_readahead_blks=8";
					fsmgr_flags = "wait";
				};
				vendor {
					compatible = "android,vendor";
					dev = "/dev/block/platform/ff0f0000.dwmmc/by-name/vendor";
					type = "ext4";
					mnt_flags = "ro,barrier=1,inode_readahead_blks=8";
					fsmgr_flags = "wait";
				};
			};
		};
	};

	xin32k: xin32k {
		status = "okay";
		compatible = "pwm-clock";
		#clock-cells = <0>;
		clock-frequency = <32768>;
		clock-output-names = "xin32k";
		pwms = <&pwm1 0 30518 0>; /* 1 / 30518 ns = 32.7675 KHz */
	};

	sdio_pwrseq: sdio-pwrseq {
		compatible = "mmc-pwrseq-simple";
		clocks = <&rk808 1>;
		clock-names = "ext_clock";
		pinctrl-names = "default";
		pinctrl-0 = <&wifi_enable_h>;

		/*
		 * On the module itself this is one of these (depending
		 * on the actual card populated):
		 * - SDIO_RESET_L_WL_REG_ON
		 * - PDN (power down when low)
		 */
		reset-gpios = <&gpio3 RK_PA5 GPIO_ACTIVE_LOW>; /* GPIO3_A5 */
	};

	es8396-sound {
		compatible = "simple-audio-card";
		simple-audio-card,format = "i2s";
		simple-audio-card,name = "rockchip,es8396-codec";
		simple-audio-card,mclk-fs = <256>;
		simple-audio-card,widgets =
			"Microphone", "Microphone Jack",
			"Line", "Microphone Headset",
			"Headphone", "Headphone Jack";
		simple-audio-card,routing =
			"MIC", "Microphone Jack",
			"DMIC", "Microphone Headset",
			"Headphone Jack", "LOUTP",
			"Headphone Jack", "ROUTN";
		simple-audio-card,cpu {
			sound-dai = <&i2s_8ch>;
		};
		simple-audio-card,codec {
			sound-dai = <&es8396>;
		};
	};

	backlight: backlight {
		compatible = "pwm-backlight";
		pwms = <&pwm0 0 25000 0>;
		brightness-levels = <
			  0   1   2   3   4   5   6   7
			  8   9  10  11  12  13  14  15
			 16  17  18  19  20  21  22  23
			 24  25  26  27  28  29  30  31
			 32  33  34  35  36  37  38  39
			 40  41  42  43  44  45  46  47
			 48  49  50  51  52  53  54  55
			 56  57  58  59  60  61  62  63
			 64  65  66  67  68  69  70  71
			 72  73  74  75  76  77  78  79
			 80  81  82  83  84  85  86  87
			 88  89  90  91  92  93  94  95
			 96  97  98  99 100 101 102 103
			104 105 106 107 108 109 110 111
			112 113 114 115 116 117 118 119
			120 121 122 123 124 125 126 127
			128 129 130 131 132 133 134 135
			136 137 138 139 140 141 142 143
			144 145 146 147 148 149 150 151
			152 153 154 155 156 157 158 159
			160 161 162 163 164 165 166 167
			168 169 170 171 172 173 174 175
			176 177 178 179 180 181 182 183
			184 185 186 187 188 189 190 191
			192 193 194 195 196 197 198 199
			200 201 202 203 204 205 206 207
			208 209 210 211 212 213 214 215
			216 217 218 219 220 221 222 223
			224 225 226 227 228 229 230 231
			232 233 234 235 236 237 238 239
			240 241 242 243 244 245 246 247
			248 249 250 251 252 253 254 255>;
		default-brightness-level = <200>;
		enable-gpios = <&gpio0 RK_PB6 GPIO_ACTIVE_HIGH>;
	};

	rk_key: rockchip-key {
		compatible = "rockchip,key";
		status = "okay";

		io-channels = <&saradc 1>;

		vol-up-key {
			linux,code = <115>;
			label = "volume up";
			rockchip,adc_value = <1>;
		};

		vol-down-key {
			linux,code = <114>;
			label = "volume down";
			rockchip,adc_value = <170>;
		};

		power-key {
			gpios = <&gpio0 RK_PA2 GPIO_ACTIVE_LOW>;
			linux,code = <116>;
			label = "power";
			gpio-key,wakeup;
		};

		menu-key {
			linux,code = <59>;
			label = "menu";
			rockchip,adc_value = <355>;
		};

		home-key {
			linux,code = <102>;
			label = "home";
			rockchip,adc_value = <746>;
		};

		back-key {
			linux,code = <158>;
			label = "back";
			rockchip,adc_value = <560>;
		};

		camera-key {
			linux,code = <212>;
			label = "camera";
			rockchip,adc_value = <450>;
		};
	};

	wireless-wlan {
		compatible = "wlan-platdata";

		wifi_chip_type = "rtl8723ds";
		sdio_vref = <1800>; /*1800mv or 3300mv*/
		WIFI,host_wake_irq = <&gpio3 RK_PA6 GPIO_ACTIVE_HIGH>;
		WIFI,vbat_gpio  = <&gpio3 RK_PA4 GPIO_ACTIVE_HIGH>;
		status = "okay";
	};

	wireless-bluetooth {
		compatible = "bluetooth-platdata";

		keep_bt_power_on;
		BT,power_gpio = <&gpio3 4 GPIO_ACTIVE_HIGH>; /* GPIO3_A4 */
		BT,reset_gpio = <&gpio3 2 GPIO_ACTIVE_HIGH>; /* GPIO3_A2 */
		BT,wake_gpio = <&gpio3 7 GPIO_ACTIVE_HIGH>; /* GPIO3_A7 */
		BT,wake_host_irq = <&gpio3 3 GPIO_ACTIVE_HIGH>; /* GPIO3_A3 */

		status = "okay";
	};

	gpio_det: gpio-det {
		compatible = "gpio-detection";
		status = "okay";

		pinctrl-0 = <&gpio3_b1 &gpio3_b2>;
		pinctrl-names = "default";

		car-reverse {
			car-reverse-gpios = <&gpio3 10 GPIO_ACTIVE_LOW>;
			linux,debounce-ms = <5>;
			label = "car-reverse";
			gpio,wakeup;
		};

		car-acc {
			car-acc-gpios = <&gpio3 9 GPIO_ACTIVE_LOW>;
			linux,debounce-ms = <5>;
			label = "car-acc";
			gpio,wakeup;
		};
	};

	vcc_sys: vcc-sys-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vcc_sys";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <3800000>;
		regulator-max-microvolt = <3800000>;
	};

	vcc_host: vcc-host {
		compatible = "regulator-fixed";
		enable-active-low;
		gpio = <&gpio0 RK_PA3 GPIO_ACTIVE_LOW>;
		pinctrl-names = "default";
		pinctrl-0 = <&host_vbus_drv>;
		regulator-name = "vcc_host";
		regulator-always-on;
	};

	vcc18_lcd_n: vcc18-lcd-n {
		compatible = "regulator-fixed";
		regulator-name = "vcc18_lcd_n";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <1800000>;
		regulator-max-microvolt = <1800000>;
		gpio = <&gpio2 RK_PD3 GPIO_ACTIVE_HIGH>;
		enable-active-high;
		startup-delay-us = <70000>;
		vin-supply = <&vcc_18>;

		regulator-state-mem {
			regulator-off-in-suspend;
		};
	};

	panel {
		compatible = "samsung,lsl070nl01", "simple-panel";
		power-supply = <&vcc33_lcd>;
		backlight = <&backlight>;
		prepare-delay-ms = <120>;
		unprepare-delay-ms = <120>;
		bus-format = <MEDIA_BUS_FMT_RGB888_1X7X4_SPWG>;

		display-timings {
			native-mode = <&timing0>;

			timing0: timing0 {
				clock-frequency = <48000000>;
				hactive = <1024>;
				vactive = <600>;
				hback-porch = <90>;
				hfront-porch = <90>;
				vback-porch = <10>;
				vfront-porch = <10>;
				hsync-len = <90>;
				vsync-len = <10>;
				hsync-active = <0>;
				vsync-active = <0>;
				de-active = <0>;
				pixelclk-active = <0>;
			};
		};

		port {
			panel_in_lvds: endpoint {
				remote-endpoint = <&lvds_out_panel>;
			};
		};
	};
};

&firmware_android {
	compatible = "android,firmware";
	fstab {
		compatible = "android,fstab";
		system {
			compatible = "android,system";
			dev = "/dev/block/by-name/system";
			type = "ext4";
			mnt_flags = "ro,barrier=1,inode_readahead_blks=8";
			fsmgr_flags = "wait,verify";
		};
		vendor {
			compatible = "android,vendor";
			dev = "/dev/block/by-name/vendor";
			type = "ext4";
			mnt_flags = "ro,barrier=1,inode_readahead_blks=8";
			fsmgr_flags = "wait,verify";
		};
	};
};

&cif_sensor {
	status = "okay";
};

&cluster0_opp {
	rockchip,threshold-freq = <408000>;
	rockchip,freq-limit;
};

&cluster1_opp {
	rockchip,threshold-freq = <1416000>;
};

&cpu_l0 {
	cpu-supply = <&vdd_cpu>;
};

&cpu_l1 {
	cpu-supply = <&vdd_cpu>;
};

&cpu_l2 {
	cpu-supply = <&vdd_cpu>;
};

&cpu_l3 {
	cpu-supply = <&vdd_cpu>;
};

&cpu_b0 {
	cpu-supply = <&vdd_cpu>;
};

&cpu_b1 {
	cpu-supply = <&vdd_cpu>;
};

&cpu_b2 {
	cpu-supply = <&vdd_cpu>;
};

&cpu_b3 {
	cpu-supply = <&vdd_cpu>;
};

&gpu {
	logic-supply = <&vdd_log>;
};

&isp {
	pinctrl-names =
		"isp_mipi_fl_prefl", "isp_flash_as_gpio",
		"isp_flash_as_trigger_out";
	pinctrl-0 = <&isp_prelight>;
	pinctrl-1 = <&isp_flash_trigger_as_gpio>;
	pinctrl-2 = <&isp_flash_trigger>;
};

&rockchip_suspend {
	status = "okay";
	rockchip,sleep-mode-config = <
		(0
		| RKPM_SLP_ARMOFF
		| RKPM_SLP_PMU_PLLS_PWRDN
		| RKPM_SLP_PMU_PMUALIVE_32K
		| RKPM_SLP_SFT_PLLS_DEEP
		| RKPM_SLP_PMU_DIS_OSC
		| RKPM_SLP_SFT_PD_NBSCUS
		)
	>;
	rockchip,wakeup-config = <
		(0
		| RKPM_GPIO_WKUP_EN
		| RKPM_USB_WKUP_EN
		| RKPM_CLUSTER_L_WKUP_EN
		)
	>;
};

&emmc {
	status = "okay";
	bus-width = <8>;
	clock-frequency = <150000000>;
	keep-power-in-suspend;
	cap-mmc-highspeed;
	mmc-hs200-1_8v;
	no-sdio;
	no-sd;
	disable-wp;
	non-removable;
	num-slots = <1>;
	pinctrl-names = "default";
	pinctrl-0 = <&emmc_clk &emmc_cmd &emmc_bus8>;
	vmmc-supply = <&vcc_io>;
	vqmmc-supply = <&vcc18_flash>;
};

&sdmmc {
	status = "okay";
	clock-frequency = <37500000>;
	clock-freq-min-max = <400000 37500000>;
	no-sdio;
	no-mmc;
	cap-mmc-highspeed;
	cap-sd-highspeed;
	card-detect-delay = <200>;
	disable-wp;
	num-slots = <1>;
	pinctrl-names = "default";
	pinctrl-0 = <&sdmmc_clk &sdmmc_cmd &sdmmc_cd &sdmmc_bus4>;
	vmmc-supply = <&vcc_sd>;
	vqmmc-supply = <&vccio_sd>;
};

&sdio0 {
	status = "okay";
	clock-frequency = <50000000>;
	clock-freq-min-max = <200000 50000000>;
	no-sd;
	no-mmc;
	bus-width = <4>;
	disable-wp;
	cap-sd-highspeed;
	cap-sdio-irq;
	keep-power-in-suspend;
	mmc-pwrseq = <&sdio_pwrseq>;
	non-removable;
	num-slots = <1>;
	pinctrl-names = "default";
	pinctrl-0 = <&sdio0_bus4 &sdio0_cmd &sdio0_clk>;
	sd-uhs-sdr104;
};

&i2c0 {
	status = "okay";

	rk808: pmic@1b {
		compatible = "rockchip,rk808";
		reg = <0x1b>;
		interrupt-parent = <&gpio0>;
		interrupts = <5 IRQ_TYPE_LEVEL_LOW>;
		pinctrl-names = "default";
		pinctrl-0 = <&pmic_int>;
		rockchip,system-power-controller;
		wakeup-source;
		#clock-cells = <1>;
		clock-output-names = "rk808-clkout1", "rk808-clkout2";

		vcc1-supply = <&vcc_sys>;
		vcc2-supply = <&vcc_sys>;
		vcc3-supply = <&vcc_sys>;
		vcc4-supply = <&vcc_sys>;
		vcc6-supply = <&vcc_sys>;
		vcc7-supply = <&vcc_sys>;
		vcc8-supply = <&vcc_io>;
		vcc9-supply = <&vcc_sys>;
		vcc10-supply = <&vcc_sys>;
		vcc11-supply = <&vcc_sys>;
		vcc12-supply = <&vcc_io>;

		regulators {
			vdd_cpu: DCDC_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <700000>;
				regulator-max-microvolt = <1500000>;
				regulator-name = "vdd_cpu";
				regulator-ramp-delay = <6000>;
				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <1000000>;
				};
			};

			vdd_log: DCDC_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <700000>;
				regulator-max-microvolt = <1500000>;
				regulator-name = "vdd_log";
				regulator-ramp-delay = <6000>;
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1000000>;
				};
			};

			vcc_ddr: DCDC_REG3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vcc_ddr";
				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};

			vcc_io: DCDC_REG4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vcc_io";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vcc18_flash: LDO_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc18_flash";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vcca_33: LDO_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vcca_33";
				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vdd_10: LDO_REG3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <1000000>;
				regulator-name = "vdd_10";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1000000>;
				};
			};

			avdd_33: LDO_REG4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "avdd_33";
				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vccio_sd: LDO_REG5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vccio_sd";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vdd10_lcd: LDO_REG6 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <1000000>;
				regulator-name = "vdd10_lcd";
				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <1000000>;
				};
			};

			vcc_18: LDO_REG7 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc_18";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vcc18_lcd: LDO_REG8 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc18_lcd";
				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vcc_sd: SWITCH_REG1 {
				regulator-boot-on;
				regulator-name = "vcc_sd";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc33_lcd: SWITCH_REG2 {
				regulator-boot-on;
				regulator-name = "vcc33_lcd";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};
		};
	};
};

&i2c1 {
	status = "okay";

	bma2x2: bma250@18 {
		compatible = "bma2xx_acc";
		status = "okay";
		reg = <0x18>;
		type = <SENSOR_TYPE_ACCEL>;
		pinctrl-names = "default";
		pinctrl-0 = <&gpio2_c1>;
		irq-gpio = <&gpio2 17 IRQ_TYPE_LEVEL_LOW>;
		irq_enable = <1>;
		poll_delay_ms = <200>;
		layout = <6>;
		reprobe_en = <1>;/* this sensor need to be probe again */
	};

	ls_stk3410: light@48 {
		compatible = "ls_stk3410";
		status = "okay";
		reg = <0x48>;
		type = <SENSOR_TYPE_LIGHT>;
		irq_enable = <0>;
		als_threshold_high = <100>;
		als_threshold_low = <10>;
		als_ctrl_gain = <2>; /* 0:x1 1:x4 2:x16 3:x64 */
		poll_delay_ms = <100>;
	};

	ps_stk3410: proximity@48 {
		compatible = "ps_stk3410";
		status = "okay";
		reg = <0x48>;
		type = <SENSOR_TYPE_PROXIMITY>;
		pinctrl-names = "default";
		pinctrl-0 = <&gpio2_c3>;
		irq-gpio = <&gpio2 19 IRQ_TYPE_LEVEL_LOW>;
		irq_enable = <1>;
		ps_threshold_high = <0x200>;
		ps_threshold_low = <0x100>;
		ps_ctrl_gain = <3>; /* 0:x1 1:x4 2:x16 3:x64 */
		ps_led_current = <3>; /* 0:12.5mA 1:25mA 2:50mA 3:100mA */
		poll_delay_ms = <100>;
	};
};

&i2c2 {
	status = "okay";
	clock-frequency = <200000>;

	gsl1680: touchscreen@40 {
		compatible = "silead,gsl1680";
		reg = <0x40>;
		interrupt-parent = <&gpio3>;
		interrupts = <28 IRQ_TYPE_EDGE_FALLING>;
		power-gpios = <&gpio3 RK_PB7 GPIO_ACTIVE_HIGH>;
		touchscreen-size-x = <800>;
		touchscreen-size-y = <1280>;
		silead,max-fingers = <5>;
	};

	gt9xx: gt9xx@14 {
		compatible = "goodix,gt9xx";
		reg = <0x14>;
		touch-gpio = <&gpio3 RK_PD4 IRQ_TYPE_LEVEL_HIGH>;
		reset-gpio = <&gpio3 RK_PB7 GPIO_ACTIVE_LOW>;
		max-x = <1024>;
		max-y = <600>;
		tp-size = <910>;
		tp-supply = <&vcc_io>;
		status = "okay";
	};
};

&i2c3 {
	status = "okay";
	clock-frequency = <200000>;

	fm1288: fm1288@60{
		compatible = "fm1288";
		reg = <0x60>;
		pwd-gpios = <&gpio0 RK_PD1 GPIO_ACTIVE_HIGH>;
		bypass-gpios = <&gpio0 RK_PD4 GPIO_ACTIVE_HIGH>;
		status = "okay";
	};

	es8396: es8396@10 {
		status = "okay";
		#sound-dai-cells = <0>;
		compatible = "es8396";
		reg = <0x10>;
		clocks = <&cru SCLK_I2S_8CH_OUT>;
		clock-names = "mclk";
		spk-con-gpio = <&gpio2 RK_PC7 GPIO_ACTIVE_HIGH>;
		lineout-con-gpio = <&gpio0 RK_PD7 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2s_8ch_mclk>;
	};
};

&i2c4 {
	status = "okay";
};

&i2s_8ch {
	status = "okay";
	rockchip,i2s-broken-burst-len;
	rockchip,playback-channels = <8>;
	rockchip,capture-channels = <2>;
	#sound-dai-cells = <0>;
	pinctrl-names = "default";
	pinctrl-0 = <&i2s_8ch_bus>;
};

&io_domains {
	status = "okay";
	dvp-supply = <&vcc_18>;
	audio-supply = <&vcc_io>;
	gpio30-supply = <&vcc_io>;
	gpio1830-supply = <&vcc_io>;
	sdcard-supply = <&vccio_sd>;
	wifi-supply = <&vcc_io>;
};

&pmu_io_domains {
	status = "okay";
	pmu-supply = <&vcc_io>;
	vop-supply = <&vcca_33>;
};

&pwm0 {
	status = "okay";
};

&pwm1 {
	status = "okay";
};

&u2phy {
	status = "okay";

	u2phy_host: host-port {
		phy-supply = <&vcc_host>;
		status = "okay";
	};
};

&usb_host0_ehci {
	status = "okay";
};

&usb_host0_ohci {
	status = "okay";
};

&dfi {
	status = "okay";
};

&dmc {
	vop-dclk-mode = <1>;
	center-supply = <&vdd_log>;
	system-status-freq = <
		/*system status			freq(KHz)*/
		SYS_STATUS_NORMAL		600000
		SYS_STATUS_REBOOT		600000
		SYS_STATUS_SUSPEND		192000
		SYS_STATUS_VIDEO_1080P	600000
		SYS_STATUS_VIDEO_4K		600000
		SYS_STATUS_PERFORMANCE	600000
		SYS_STATUS_BOOST		600000
		SYS_STATUS_DUALVIEW		600000
		SYS_STATUS_ISP			600000
	>;
	status = "okay";
};

&lvds {
	status = "okay";

	ports {
		port@1 {
			reg = <1>;

			lvds_out_panel: endpoint {
				remote-endpoint = <&panel_in_lvds>;
			};
		};
	};
};

&route_lvds {
	status = "okay";
};

&mailbox {
	status = "okay";
};

&mailbox_scpi {
	status = "okay";
};

&saradc {
	status = "okay";
};

&thermal_zones {
	status = "okay";
};

&tsadc {
	tsadc-supply = <&vdd_cpu>;
	status = "okay";
};

&uart1 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart1_xfer &uart1_cts>;
	status = "okay";
};

&uart2 {
	status = "disabled";
};

&uart4 {
	status = "okay";
};

&pinctrl {
	pmic {
		pmic_int: pmic-int {
			rockchip,pins = <0 RK_PA5 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	dc_det {
		dc_irq_gpio: dc-irq-gpio {
			rockchip,pins = <0 RK_PC1 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	sdio-pwrseq {
		wifi_enable_h: wifi-enable-h {
			rockchip,pins = <3 RK_PA5 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	usb2 {
		host_vbus_drv: host-vbus-drv {
			rockchip,pins = <0 RK_PA3 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	wireless-bluetooth {
		uart0_rts_gpio: uart0-rts-gpio {
			rockchip,pins = <2 RK_PD3 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	gpio0_gpio {
		gpio0_c7: gpio0-c7 {
			rockchip,pins = <0 RK_PC7 RK_FUNC_GPIO  &pcfg_pull_down>;
		};
		gpio0_a3: gpio0-a3 {
			rockchip,pins = <0 RK_PA3 3 &pcfg_pull_none>;
		};
		gpio0_c2: gpio0-c2 {
			rockchip,pins = <0 RK_PC2 RK_FUNC_GPIO &pcfg_pull_down>;
		};
		gpio0_c3: gpio0-c3 {
			rockchip,pins = <0 RK_PC4 RK_FUNC_GPIO &pcfg_pull_up>;
		};
		gpio0_c1: gpio0-c1 {
			rockchip,pins = <0 RK_PC1 RK_FUNC_GPIO &pcfg_pull_up>;
		};
		gpio2_c1: gpio2-c1 {
			rockchip,pins = <2 RK_PC1 RK_FUNC_GPIO &pcfg_pull_up>;
		};
		gpio2_c3: gpio2-c3 {
			rockchip,pins = <2 RK_PC3 RK_FUNC_GPIO &pcfg_pull_up>;
		};

		gpio3_b1: gpio3-b1 {
			rockchip,pins = <3 RK_PB1 RK_FUNC_GPIO &pcfg_pull_up>;
		};

		gpio3_b2: gpio3-b2 {
			rockchip,pins = <3 RK_PB2 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};
	i2s {
		i2s_8ch_bus: i2s-8ch-bus {
			rockchip,pins = <2 RK_PB4 1 &pcfg_pull_none>,
					<2 RK_PB5 1 &pcfg_pull_none>,
					<2 RK_PB6 1 &pcfg_pull_none>,
					<2 RK_PB7 1 &pcfg_pull_none>,
					<2 RK_PC0 1 &pcfg_pull_none>,
					<2 RK_PC2 1 &pcfg_pull_none>;
		};
	};
};
