/* board base */
//#include "../rk3588-evb4-lp4-v10-linux.dts"
#include "rp-rk3588-board.dtsi"

#include "rp-tp-i2c6-gt911.dtsi"
#include "rd-rk3588-lcd-gpio.dtsi"

/* usb */
#include "rp-usb-typec-rk3588.dtsi"
#include "rp-usb-host.dtsi"

/* ethernet */
#include "rp-eth-pcie2gmac-rk3588.dtsi"
#include "rp-eth-gmac1.dtsi"

/* pcie */
#include "rp-pcie-power-rk3588.dtsi"
#include "rp-pcie3.dtsi" //need comment when use board of  make it youself,and remove the pcie function
#include "rp-pcie-5g.dtsi"

/* audio */
#include "rp-audio-rt5640.dtsi"

/* wifi/bt */
#include "rp-wifi-bt-vs2275p-rk3588.dtsi"

/* hdmi rx */
#include "rp-hdmirx.dtsi"

/* mipi camera */
/* use dcphy0 camera , need to disabled rp-hdmirx.dtsi*/
/***********all camera config********/


//#include "rp-camera-dcphy0.dtsi"
#include "rp-camera-dcphy1.dtsi"
#include "rp-camera-dphy0.dtsi"
#include "rp-camera-dphy1.dtsi"

//#include "rp-camera-dcphy0-ov13855.dtsi"
//#include "rp-camera-dcphy1-ov13855.dtsi"
//#include "rp-camera-dphy0-ov13855.dtsi"
//#include "rp-camera-dphy1-ov13855.dtsi"

//#include "rp-camera-dcphy0-gc8034.dtsi"
//#include "rp-camera-dcphy1-gc8034.dtsi"
//#include "rp-camera-dphy0-gc8034.dtsi"
//#include "rp-camera-dphy1-gc8034.dtsi"

//#include "rp-camera-dcphy0-imx415.dtsi"
//#include "rp-camera-dcphy1-imx415.dtsi"
//#include "rp-camera-dphy0-imx415.dtsi"
//#include "rp-camera-dphy1-imx415.dtsi"

/**********4 channel must be disabled hdmi in*********/
//#include "rp-camera-dcphy1-gc8034.dtsi"
//#include "rp-camera-dphy1-gc8034.dtsi"
//#include "rp-camera-dcphy0-imx415.dtsi"
//#include "rp-camera-dphy0-imx415.dtsi"
/******************************************/

//#include "rp-lcd-hdmi0.dtsi"        //batch ignore
//#include "rp-lcd-hdmi1.dtsi"        //batch ignore
//#include "rp-lcd-typec-dp0.dtsi"    //usb edp0,must be enable rp-usb-typec.dtsi, batch ignore
#include "rp-lcd-multi-hdmi0-hdmi1-dp0.dtsi" 

/* lcd */
#include "rp-lcd-mipi0-5-720-1280-v2-boxTP.dtsi"
//#include "rp-lcd-mipi0-7-720-1280.dtsi"
//#include "rp-lcd-mipi0-8-800-1280-v3.dtsi"
//#include "rp-lcd-mipi0-8-1200-1920.dtsi"
//#include "rp-lcd-mipi0-10-800-1280-v3.dtsi"
//#include "rp-lcd-mipi0-10-1200-1920.dtsi"
//#include "rp-lcd-mipi0-10-1920-1200-jc.dtsi"

/ {
    model = "rp-rk3588";
    reserved-memory {
        #address-cells = <2>;
        #size-cells = <2>;
        ranges;
        dma_trans: dma-trans@3c000000 {
            reg = <0x0 0x3c000000 0x0 0x04000000>;
        };
    };

    vcc_1v1_nldo_s3: vcc-1v1-nldo-s3 {
        compatible = "regulator-fixed";
        regulator-name = "vcc_1v1_nldo_s3";
        regulator-always-on;
        regulator-boot-on;
        regulator-min-microvolt = <1100000>;
        regulator-max-microvolt = <1100000>;
        vin-supply = <&vcc5v0_sys>;
    };

	fan_gpio_control {
            compatible = "fan_gpio_control";
            gpio-pin = <&gpio4 RK_PA7 GPIO_ACTIVE_HIGH>;
            thermal-zone = "soc-thermal";
            threshold-temp = <60000>; //60C
            running-time = <10000>; //10s
            status = "okay";
        };

        rp_power{
                status = "okay";
                compatible = "rp_power";
                rp_not_deep_sleep = <1>;

//#define GPIO_FUNCTION_OUTPUT 0
//#define GPIO_FUNCTION_INPUT 1
//#define GPIO_FUNCTION_IRQ 2
//#define GPIO_FUNCTION_FLASH 3
//#define GPIO_FUNCTION_OUTPUT_CTRL 4

                //fan {   
                //        gpio_num = <&gpio4 RK_PA7 GPIO_ACTIVE_HIGH>;
                //        gpio_function = <4>;
                //};

                led {  
                        gpio_num = <&gpio4 RK_PA6 GPIO_ACTIVE_HIGH>;
                        gpio_function = <3>;
                };

                usb-host-power {  
                        gpio_num = <&gpio2 RK_PC1 GPIO_ACTIVE_HIGH>;
                        gpio_function = <4>;
                };

                usb-hub-reset {  
                        gpio_num = <&gpio3 RK_PB2 GPIO_ACTIVE_HIGH>;
                        gpio_function = <4>;
                };
    };

        rp_gpio{
                status = "okay";
                compatible = "rp_gpio";

                gpio1d2 {  
                        gpio_num = <&gpio1 RK_PD2 GPIO_ACTIVE_HIGH>;
                        gpio_function = <0>;
                };

                gpio3c6 {  
                        gpio_num = <&gpio3 RK_PC6 GPIO_ACTIVE_HIGH>;
                        gpio_function = <0>;
                };



        };
};


&uart0 {
    status = "okay";
    pinctrl-names = "default";
    pinctrl-0 = <&uart0m0_xfer>;
};

&uart6 {
    status = "okay";
    pinctrl-names = "default";
    pinctrl-0 = <&uart6m0_xfer>;
};

&uart7 {
    status = "okay";
    pinctrl-names = "default";
    pinctrl-0 = <&uart7m1_xfer>;
};

&uart8 {
    status = "okay";
    pinctrl-names = "default";
    pinctrl-0 = <&uart8m0_xfer>;
};

&can0 {
    assigned-clocks = <&cru CLK_CAN0>;
    assigned-clock-rates = <200000000>;
    status = "okay";
    pinctrl-names = "default";
    pinctrl-0 = <&can0m0_pins>;
};

&can1 {
    assigned-clocks = <&cru CLK_CAN1>;
    assigned-clock-rates = <200000000>;
    status = "okay";
    pinctrl-names = "default";
    pinctrl-0 = <&can1m1_pins>;
};

&i2c4 {
    status = "okay";
    pinctrl-names = "default";
    pinctrl-0 = <&i2c4m1_xfer>;

    hym8563: hym8563@51 {
        compatible = "haoyu,hym8563";
        reg = <0x51>;
        #clock-cells = <0>;
        clock-frequency = <32768>;
        clock-output-names = "hym8563";
        //pinctrl-names = "default";
        //pinctrl-0 = <&hym8563_int>;
        //interrupt-parent = <&gpio0>;
        //interrupts = <RK_PD4 IRQ_TYPE_LEVEL_LOW>;
        //wakeup-source;
    };

};


&sdmmc {
    status = "okay";
    //vmmc-supply = <&vccio_sd_s0>;
};

&fiq_debugger {
    rockchip,baudrate = <115200>;
};

&display_subsystem {
clocks = <&hdptxphy_hdmi_clk0>, <&hdptxphy_hdmi_clk1>;
clock-names = "hdmi0_phy_pll", "hdmi1_phy_pll";
};

&hdptxphy_hdmi_clk0 {
            status = "okay";
};

&hdptxphy_hdmi_clk1 {
            status = "okay";
};

