// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Copyright (c) 2018 Fuzhou Rockchip Electronics Co., Ltd
 */

#include <dt-bindings/clock/px30-cru.h>
#include <dt-bindings/display/media-bus-format.h>
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/interrupt-controller/arm-gic.h>
#include <dt-bindings/interrupt-controller/irq.h>
#include <dt-bindings/pinctrl/rockchip.h>
#include <dt-bindings/power/px30-power.h>
#include <dt-bindings/soc/rockchip,boot-mode.h>
#include <dt-bindings/soc/rockchip-system-status.h>
#include <dt-bindings/suspend/rockchip-px30.h>
#include <dt-bindings/thermal/thermal.h>
#include "px30-dram-default-timing.dtsi"
#include "px30s-dram-default-timing.dtsi"

/ {
	compatible = "rockchip,px30";

	interrupt-parent = <&gic>;
	#address-cells = <2>;
	#size-cells = <2>;

	aliases {
		ethernet0 = &gmac;
		gpio0 = &gpio0;
		gpio1 = &gpio1;
		gpio2 = &gpio2;
		gpio3 = &gpio3;
		i2c0 = &i2c0;
		i2c1 = &i2c1;
		i2c2 = &i2c2;
		i2c3 = &i2c3;
		mmc0 = &sdmmc;
		mmc1 = &sdio;
		mmc2 = &emmc;
		serial0 = &uart0;
		serial1 = &uart1;
		serial2 = &uart2;
		serial3 = &uart3;
		serial4 = &uart4;
		serial5 = &uart5;
		spi0 = &spi0;
		spi1 = &spi1;
		spi2 = &sfc;
	};

	cpus {
		#address-cells = <2>;
		#size-cells = <0>;

		cpu0: cpu@0 {
			device_type = "cpu";
			compatible = "arm,cortex-a35";
			reg = <0x0 0x0>;
			enable-method = "psci";
			clocks = <&cru ARMCLK>;
			#cooling-cells = <2>;
			cpu-idle-states = <&CPU_SLEEP &CLUSTER_SLEEP>;
			dynamic-power-coefficient = <90>;
			operating-points-v2 = <&cpu0_opp_table>;
		};

		cpu1: cpu@1 {
			device_type = "cpu";
			compatible = "arm,cortex-a35";
			reg = <0x0 0x1>;
			enable-method = "psci";
			clocks = <&cru ARMCLK>;
			#cooling-cells = <2>;
			cpu-idle-states = <&CPU_SLEEP &CLUSTER_SLEEP>;
			dynamic-power-coefficient = <90>;
			operating-points-v2 = <&cpu0_opp_table>;
		};

		cpu2: cpu@2 {
			device_type = "cpu";
			compatible = "arm,cortex-a35";
			reg = <0x0 0x2>;
			enable-method = "psci";
			clocks = <&cru ARMCLK>;
			#cooling-cells = <2>;
			cpu-idle-states = <&CPU_SLEEP &CLUSTER_SLEEP>;
			dynamic-power-coefficient = <90>;
			operating-points-v2 = <&cpu0_opp_table>;
		};

		cpu3: cpu@3 {
			device_type = "cpu";
			compatible = "arm,cortex-a35";
			reg = <0x0 0x3>;
			enable-method = "psci";
			clocks = <&cru ARMCLK>;
			#cooling-cells = <2>;
			cpu-idle-states = <&CPU_SLEEP &CLUSTER_SLEEP>;
			dynamic-power-coefficient = <90>;
			operating-points-v2 = <&cpu0_opp_table>;
		};

		idle-states {
			entry-method = "psci";

			CPU_SLEEP: cpu-sleep {
				compatible = "arm,idle-state";
				local-timer-stop;
				arm,psci-suspend-param = <0x0010000>;
				entry-latency-us = <120>;
				exit-latency-us = <250>;
				min-residency-us = <900>;
			};

			CLUSTER_SLEEP: cluster-sleep {
				compatible = "arm,idle-state";
				local-timer-stop;
				arm,psci-suspend-param = <0x1010000>;
				entry-latency-us = <400>;
				exit-latency-us = <500>;
				min-residency-us = <2000>;
			};
		};
	};

	cpu0_opp_table: cpu0-opp-table {
		compatible = "operating-points-v2";
		opp-shared;

		rockchip,temp-hysteresis = <5000>;
		rockchip,low-temp = <0>;
		rockchip,low-temp-min-volt = <1000000>;
		rockchip,low-temp-adjust-volt = <
			/* MHz    MHz    uV */
			0      1512   50000
		>;

		clocks = <&cru PLL_APLL>;
		rockchip,avs-scale = <4>;
		rockchip,max-volt = <1350000>;
		rockchip,evb-irdrop = <25000>;
		nvmem-cells = <&cpu_leakage>, <&performance>;
		nvmem-cell-names = "cpu_leakage", "performance";
		rockchip,bin-scaling-sel = <
			0               13
			1               15
		>;

		rockchip,pvtm-voltage-sel = <
			0        50000   0
			50001    54000   1
			54001    60000   2
			60001    99999   3
		>;
		rockchip,pvtm-freq = <408000>;
		rockchip,pvtm-volt = <1000000>;
		rockchip,pvtm-ch = <0 0>;
		rockchip,pvtm-sample-time = <1000>;
		rockchip,pvtm-number = <10>;
		rockchip,pvtm-error = <1000>;
		rockchip,pvtm-ref-temp = <40>;
		rockchip,pvtm-temp-prop = <(-56) (-56)>;
		rockchip,thermal-zone = "soc-thermal";

		opp-408000000 {
			opp-hz = /bits/ 64 <408000000>;
			opp-microvolt = <950000 950000 1350000>;
			opp-microvolt-L0 = <950000 950000 1350000>;
			opp-microvolt-L1 = <950000 950000 1350000>;
			opp-microvolt-L2 = <950000 950000 1350000>;
			opp-microvolt-L3 = <950000 950000 1350000>;
			clock-latency-ns = <40000>;
			opp-suspend;
		};
		opp-600000000 {
			opp-hz = /bits/ 64 <600000000>;
			opp-microvolt = <950000 950000 1350000>;
			opp-microvolt-L0 = <950000 950000 1350000>;
			opp-microvolt-L1 = <950000 950000 1350000>;
			opp-microvolt-L2 = <950000 950000 1350000>;
			opp-microvolt-L3 = <950000 950000 1350000>;
			clock-latency-ns = <40000>;
		};
		opp-816000000 {
			opp-hz = /bits/ 64 <816000000>;
			opp-microvolt = <1050000 1050000 1350000>;
			opp-microvolt-L0 = <1050000 1050000 1350000>;
			opp-microvolt-L1 = <1000000 1000000 1350000>;
			opp-microvolt-L2 = <1000000 1000000 1350000>;
			opp-microvolt-L3 = <950000  950000  1350000>;
			clock-latency-ns = <40000>;
		};
		opp-1008000000 {
			opp-hz = /bits/ 64 <1008000000>;
			opp-microvolt = <1175000 1175000 1350000>;
			opp-microvolt-L0 = <1175000 1175000 1350000>;
			opp-microvolt-L1 = <1125000 1125000 1350000>;
			opp-microvolt-L2 = <1125000 1125000 1350000>;
			opp-microvolt-L3 = <1050000 1050000 1350000>;
			clock-latency-ns = <40000>;
		};
		opp-1200000000 {
			opp-hz = /bits/ 64 <1200000000>;
			opp-microvolt = <1300000 1300000 1350000>;
			opp-microvolt-L0 = <1300000 1300000 1350000>;
			opp-microvolt-L1 = <1275000 1275000 1350000>;
			opp-microvolt-L2 = <1250000 1250000 1350000>;
			opp-microvolt-L3 = <1200000 1200000 1350000>;
			clock-latency-ns = <40000>;
		};
		opp-1248000000 {
			opp-hz = /bits/ 64 <1248000000>;
			opp-microvolt = <1350000 1350000 1350000>;
			opp-microvolt-L0 = <1350000 1350000 1350000>;
			opp-microvolt-L1 = <1300000 1300000 1350000>;
			opp-microvolt-L2 = <1275000 1275000 1350000>;
			opp-microvolt-L3 = <1225000 1225000 1350000>;
			clock-latency-ns = <40000>;
		};
		opp-1296000000 {
			opp-hz = /bits/ 64 <1296000000>;
			opp-microvolt = <1350000 1350000 1350000>;
			opp-microvolt-L0 = <1350000 1350000 1350000>;
			opp-microvolt-L1 = <1350000 1350000 1350000>;
			opp-microvolt-L2 = <1300000 1300000 1350000>;
			opp-microvolt-L3 = <1250000 1250000 1350000>;
			clock-latency-ns = <40000>;
		};
		opp-1416000000 {
			opp-hz = /bits/ 64 <1416000000>;
			opp-microvolt = <1350000 1350000 1350000>;
			opp-microvolt-L0 = <1350000 1350000 1350000>;
			opp-microvolt-L1 = <1350000 1350000 1350000>;
			opp-microvolt-L2 = <1300000 1300000 1350000>;
			opp-microvolt-L3 = <1250000 1250000 1350000>;
			clock-latency-ns = <40000>;
		};
		opp-1512000000 {
			opp-hz = /bits/ 64 <1512000000>;
			opp-microvolt = <1350000 1350000 1350000>;
			opp-microvolt-L0 = <1350000 1350000 1350000>;
			opp-microvolt-L1 = <1350000 1350000 1350000>;
			opp-microvolt-L2 = <1300000 1300000 1350000>;
			opp-microvolt-L3 = <1250000 1250000 1350000>;
			clock-latency-ns = <40000>;
		};
	};

	px30s_cpu0_opp_table: px30s-cpu0-opp-table {
		compatible = "operating-points-v2";
		opp-shared;

		nvmem-cells = <&cpu_leakage>;
		nvmem-cell-names = "cpu_leakage";

		rockchip,pvtm-voltage-sel = <
			0        69850   0
			69851    73800   1
			73801    77750   2
			77751    81700   3
			81701    99999   4
		>;

		rockchip,pvtm-freq = <408000>;
		rockchip,pvtm-volt = <900000>;
		rockchip,pvtm-ch = <0 0>;
		rockchip,pvtm-sample-time = <1000>;
		rockchip,pvtm-number = <10>;
		rockchip,pvtm-error = <1000>;
		rockchip,pvtm-ref-temp = <0>;
		rockchip,pvtm-temp-prop = <0 0>;
		rockchip,thermal-zone = "soc-thermal";

		opp-408000000 {
			opp-hz = /bits/ 64 <408000000>;
			opp-microvolt = <850000 850000 1150000>;
			clock-latency-ns = <40000>;
			opp-suspend;
		};
		opp-600000000 {
			opp-hz = /bits/ 64 <600000000>;
			opp-microvolt = <850000 850000 1150000>;
			clock-latency-ns = <40000>;
		};
		opp-816000000 {
			opp-hz = /bits/ 64 <816000000>;
			opp-microvolt = <850000 850000 1150000>;
			clock-latency-ns = <40000>;
		};
		opp-1008000000 {
			opp-hz = /bits/ 64 <1008000000>;
			opp-microvolt = <950000 950000 1150000>;
			opp-microvolt-L0 = <950000 950000 1150000>;
			opp-microvolt-L1 = <925000 925000 1150000>;
			opp-microvolt-L2 = <900000 900000 1150000>;
			opp-microvolt-L3 = <875000 875000 1150000>;
			opp-microvolt-L4 = <850000 850000 1150000>;
			clock-latency-ns = <40000>;
		};
		opp-1200000000 {
			opp-hz = /bits/ 64 <1200000000>;
			opp-microvolt = <1050000 1050000 1150000>;
			opp-microvolt-L0 = <1050000 1050000 1150000>;
			opp-microvolt-L1 = <1025000 1025000 1150000>;
			opp-microvolt-L2 = <1000000 1000000 1150000>;
			opp-microvolt-L3 = <975000 975000 1150000>;
			opp-microvolt-L4 = <950000 950000 1150000>;
			clock-latency-ns = <40000>;
		};
		opp-1248000000 {
			opp-hz = /bits/ 64 <1248000000>;
			opp-microvolt = <1075000 1075000 1150000>;
			opp-microvolt-L0 = <1075000 1075000 1150000>;
			opp-microvolt-L1 = <1050000 1050000 1150000>;
			opp-microvolt-L2 = <1025000 1025000 1150000>;
			opp-microvolt-L3 = <1000000 1000000 1150000>;
			opp-microvolt-L4 = <975000 975000 1150000>;
			clock-latency-ns = <40000>;
		};
		opp-1296000000 {
			opp-hz = /bits/ 64 <1296000000>;
			opp-microvolt = <1100000 1100000 1150000>;
			opp-microvolt-L0 = <1100000 1100000 1150000>;
			opp-microvolt-L1 = <1075000 1075000 1150000>;
			opp-microvolt-L2 = <1050000 1050000 1150000>;
			opp-microvolt-L3 = <1025000 1025000 1150000>;
			opp-microvolt-L4 = <1000000 1000000 1150000>;
			clock-latency-ns = <40000>;
		};
		opp-1416000000 {
			opp-hz = /bits/ 64 <1416000000>;
			opp-microvolt = <1150000 1150000 1150000>;
			opp-microvolt-L0 = <1150000 1150000 1150000>;
			opp-microvolt-L1 = <1125000 1125000 1150000>;
			opp-microvolt-L2 = <1100000 1100000 1150000>;
			opp-microvolt-L3 = <1075000 1075000 1150000>;
			opp-microvolt-L4 = <1050000 1050000 1150000>;
			clock-latency-ns = <40000>;
		};
		opp-1512000000 {
			opp-hz = /bits/ 64 <1512000000>;
			opp-microvolt = <1150000 1150000 1150000>;
			opp-microvolt-L0 = <1150000 1150000 1150000>;
			opp-microvolt-L1 = <1125000 1125000 1150000>;
			opp-microvolt-L2 = <1100000 1100000 1150000>;
			opp-microvolt-L3 = <1075000 1075000 1150000>;
			opp-microvolt-L4 = <1050000 1050000 1150000>;
			clock-latency-ns = <40000>;
		};
	};

	arm-pmu {
		compatible = "arm,cortex-a35-pmu";
		interrupts = <GIC_SPI 100 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 101 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 102 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 103 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-affinity = <&cpu0>, <&cpu1>, <&cpu2>, <&cpu3>;
	};

	bus_soc: bus-soc {
		compatible = "rockchip,px30-bus";
		rockchip,busfreq-policy = "autocs";
		soc-bus0 {
			bus-id = <0>;
			timer-us = <20>;
			enable-msk = <0x40f7>;
		};
		soc-bus1 {
			bus-id = <1>;
			timer-us = <200>;
			enable-msk = <0x40bf>;
			status = "disabled";
		};
		soc-bus2 {
			bus-id = <2>;
			timer-us = <200>;
			enable-msk = <0x4007>;
			status = "disabled";
		};
	};

	bus_apll: bus-apll {
		compatible = "rockchip,px30-bus";
		rockchip,busfreq-policy = "clkfreq";
		clocks = <&cru PLL_APLL>;
		clock-names = "bus";
		operating-points-v2 = <&bus_apll_opp_table>;
		status = "disabled";
	};

	bus_apll_opp_table: bus-apll-opp-table {
		compatible = "operating-points-v2";
		opp-shared;

		opp-1512000000 {
			opp-hz = /bits/ 64 <1512000000>;
			opp-microvolt = <1000000>;
		};
		opp-1008000000 {
			opp-hz = /bits/ 64 <1008000000>;
			opp-microvolt = <950000>;
		};
	};

	cpuinfo {
		compatible = "rockchip,cpuinfo";
		nvmem-cells = <&cpu_id>;
		nvmem-cell-names = "id";
	};

	display_subsystem: display-subsystem {
		compatible = "rockchip,display-subsystem";
		ports = <&vopb_out>, <&vopl_out>;
		status = "disabled";
	};

	firmware {
		optee: optee {
			compatible = "linaro,optee-tz";
			method = "smc";
		};

		scmi: scmi {
			compatible = "arm,scmi-smc";
			shmem = <&scmi_shmem>;
			arm,smc-id = <0x82000010>;
			#address-cells = <1>;
			#size-cells = <0>;

			scmi_clk: protocol@14 {
				reg = <0x14>;
				#clock-cells = <1>;
			};
		};

		sdei: sdei {
			compatible = "arm,sdei-1.0";
			method = "smc";
		};
	};

	gmac_clkin: external-gmac-clock {
		compatible = "fixed-clock";
		clock-frequency = <50000000>;
		clock-output-names = "gmac_clkin";
		#clock-cells = <0>;
	};

	psci {
		compatible = "arm,psci-1.0";
		method = "smc";
	};

	rockchip_suspend: rockchip-suspend {
		compatible = "rockchip,pm-px30";
		status = "disabled";
		rockchip,sleep-debug-en = <0>;
		rockchip,sleep-mode-config = <
			(0
			| RKPM_SLP_ARMOFF
			| RKPM_SLP_PMU_HW_PLLS_PD
			| RKPM_SLP_PMU_PMUALIVE_32K
			| RKPM_SLP_PMU_DIS_OSC
			| RKPM_SLP_PMIC_LP
			)
		>;
		rockchip,wakeup-config = <
			(0
			| RKPM_CLUSTER_WKUP_EN
			| RKPM_GPIO_WKUP_EN
			| RKPM_USB_WKUP_EN
			)
		>;
	};

	timer {
		compatible = "arm,armv8-timer";
		interrupts = <GIC_PPI 13 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_HIGH)>,
			     <GIC_PPI 14 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_HIGH)>,
			     <GIC_PPI 11 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_HIGH)>,
			     <GIC_PPI 10 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_HIGH)>;
	};

	thermal_zones: thermal-zones {
		soc_thermal: soc-thermal {
			polling-delay-passive = <20>;
			polling-delay = <1000>;
			sustainable-power = <750>;
			thermal-sensors = <&tsadc 0>;

			trips {
				threshold: trip-point-0 {
					temperature = <70000>;
					hysteresis = <2000>;
					type = "passive";
				};

				target: trip-point-1 {
					temperature = <85000>;
					hysteresis = <2000>;
					type = "passive";
				};

				soc_crit: soc-crit {
					temperature = <115000>;
					hysteresis = <2000>;
					type = "critical";
				};
			};

			cooling-maps {
				map0 {
					trip = <&target>;
					cooling-device = <&cpu0 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
					contribution = <4096>;
				};

				map1 {
					trip = <&target>;
					cooling-device = <&gpu THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
					contribution = <4096>;
				};
			};
		};

		gpu_thermal: gpu-thermal {
			polling-delay-passive = <100>; /* milliseconds */
			polling-delay = <1000>; /* milliseconds */
			thermal-sensors = <&tsadc 1>;
		};
	};

	xin24m: xin24m {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <24000000>;
		clock-output-names = "xin24m";
	};

	xin32k: xin32k {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <32768>;
		clock-output-names = "xin32k";
	};

	scmi_shmem: scmi-shmem@10f000 {
		compatible = "arm,scmi-shmem";
		reg = <0x0 0x0010f000 0x0 0x100>;
	};

	pmu: power-management@ff000000 {
		compatible = "rockchip,px30-pmu", "syscon", "simple-mfd";
		reg = <0x0 0xff000000 0x0 0x1000>;

		power: power-controller {
			compatible = "rockchip,px30-power-controller";
			#power-domain-cells = <1>;
			#address-cells = <1>;
			#size-cells = <0>;

			/* These power domains are grouped by VD_LOGIC */
			power-domain@PX30_PD_USB {
				reg = <PX30_PD_USB>;
				clocks = <&cru HCLK_HOST>,
					 <&cru HCLK_OTG>,
					 <&cru SCLK_OTG_ADP>;
				pm_qos = <&qos_usb_host>, <&qos_usb_otg>;
			};
			power-domain@PX30_PD_SDCARD {
				reg = <PX30_PD_SDCARD>;
				clocks = <&cru HCLK_SDMMC>,
					 <&cru SCLK_SDMMC>;
				pm_qos = <&qos_sdmmc>;
			};
			power-domain@PX30_PD_GMAC {
				reg = <PX30_PD_GMAC>;
				clocks = <&cru ACLK_GMAC>,
					 <&cru PCLK_GMAC>,
					 <&cru SCLK_MAC_REF>,
					 <&cru SCLK_GMAC_RX_TX>;
				pm_qos = <&qos_gmac>;
			};
			power-domain@PX30_PD_MMC_NAND {
				reg = <PX30_PD_MMC_NAND>;
				clocks =  <&cru HCLK_NANDC>,
					  <&cru HCLK_EMMC>,
					  <&cru HCLK_SDIO>,
					  <&cru HCLK_SFC>,
					  <&cru SCLK_EMMC>,
					  <&cru SCLK_NANDC>,
					  <&cru SCLK_SDIO>,
					  <&cru SCLK_SFC>;
				pm_qos = <&qos_emmc>, <&qos_nand>,
					 <&qos_sdio>, <&qos_sfc>;
			};
			power-domain@PX30_PD_VPU {
				reg = <PX30_PD_VPU>;
				clocks = <&cru ACLK_VPU>,
					 <&cru HCLK_VPU>,
					 <&cru SCLK_CORE_VPU>;
				pm_qos = <&qos_vpu>, <&qos_vpu_r128>;
			};
			power-domain@PX30_PD_VO {
				reg = <PX30_PD_VO>;
				clocks = <&cru ACLK_RGA>,
					 <&cru ACLK_VOPB>,
					 <&cru ACLK_VOPL>,
					 <&cru DCLK_VOPB>,
					 <&cru DCLK_VOPL>,
					 <&cru HCLK_RGA>,
					 <&cru HCLK_VOPB>,
					 <&cru HCLK_VOPL>,
					 <&cru PCLK_MIPI_DSI>,
					 <&cru SCLK_RGA_CORE>,
					 <&cru SCLK_VOPB_PWM>;
				pm_qos = <&qos_rga_rd>, <&qos_rga_wr>,
					 <&qos_vop_m0>, <&qos_vop_m1>;
			};
			power-domain@PX30_PD_VI {
				reg = <PX30_PD_VI>;
				clocks = <&cru ACLK_CIF>,
					 <&cru ACLK_ISP>,
					 <&cru HCLK_CIF>,
					 <&cru HCLK_ISP>,
					 <&cru SCLK_ISP>;
				pm_qos = <&qos_isp_128>, <&qos_isp_rd>,
					 <&qos_isp_wr>, <&qos_isp_m1>,
					 <&qos_vip>;
			};
			power-domain@PX30_PD_GPU {
				reg = <PX30_PD_GPU>;
				clocks = <&cru SCLK_GPU>;
				pm_qos = <&qos_gpu>;
			};
		};
	};

	pmugrf: syscon@ff010000 {
		compatible = "rockchip,px30-pmugrf", "syscon", "simple-mfd";
		reg = <0x0 0xff010000 0x0 0x1000>;
		#address-cells = <1>;
		#size-cells = <1>;

		pmu_io_domains: io-domains {
			compatible = "rockchip,px30-pmu-io-voltage-domain";
			status = "disabled";
		};

		reboot_mode: reboot-mode {
			compatible = "syscon-reboot-mode";
			offset = <0x200>;
			mode-bootloader = <BOOT_BL_DOWNLOAD>;
			mode-fastboot = <BOOT_FASTBOOT>;
			mode-loader = <BOOT_BL_DOWNLOAD>;
			mode-normal = <BOOT_NORMAL>;
			mode-recovery = <BOOT_RECOVERY>;
		};

		pmu_pvtm: pmu-pvtm {
			compatible = "rockchip,px30-pmu-pvtm";
			#address-cells = <1>;
			#size-cells = <0>;
			status = "okay";

			pvtm@1 {
				reg = <1>;
				clocks = <&pmucru SCLK_PVTM_PMU>;
				clock-names = "clk";
			};
		};
	};

	uart0: serial@ff030000 {
		compatible = "rockchip,px30-uart", "snps,dw-apb-uart";
		reg = <0x0 0xff030000 0x0 0x100>;
		interrupts = <GIC_SPI 15 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&pmucru SCLK_UART0_PMU>, <&pmucru PCLK_UART0_PMU>;
		clock-names = "baudclk", "apb_pclk";
		dmas = <&dmac 0>, <&dmac 1>;
		/*You can add it to enable dma*/
		/*dma-names = "tx", "rx";*/
		reg-shift = <2>;
		reg-io-width = <4>;
		pinctrl-names = "default";
		pinctrl-0 = <&uart0_xfer &uart0_cts &uart0_rts>;
		status = "disabled";
	};

	i2s0_8ch: i2s@ff060000 {
		compatible = "rockchip,px30-i2s-tdm";
		reg = <0x0 0xff060000 0x0 0x1000>;
		interrupts = <GIC_SPI 12 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_I2S0_TX>, <&cru SCLK_I2S0_RX>, <&cru HCLK_I2S0>;
		clock-names = "mclk_tx", "mclk_rx", "hclk";
		dmas = <&dmac 16>, <&dmac 17>;
		dma-names = "tx", "rx";
		resets = <&cru SRST_I2S0_TX>, <&cru SRST_I2S0_RX>;
		reset-names = "tx-m", "rx-m";
		rockchip,cru = <&cru>;
		rockchip,grf = <&grf>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2s0_8ch_sclktx
			     &i2s0_8ch_sclkrx
			     &i2s0_8ch_lrcktx
			     &i2s0_8ch_lrckrx
			     &i2s0_8ch_sdi0
			     &i2s0_8ch_sdi1
			     &i2s0_8ch_sdi2
			     &i2s0_8ch_sdi3
			     &i2s0_8ch_sdo0
			     &i2s0_8ch_sdo1
			     &i2s0_8ch_sdo2
			     &i2s0_8ch_sdo3>;
		status = "disabled";
	};

	i2s1_2ch: i2s@ff070000 {
		compatible = "rockchip,px30-i2s", "rockchip,rk3066-i2s";
		reg = <0x0 0xff070000 0x0 0x1000>;
		interrupts = <GIC_SPI 13 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_I2S1>, <&cru HCLK_I2S1>;
		clock-names = "i2s_clk", "i2s_hclk";
		dmas = <&dmac 18>, <&dmac 19>;
		dma-names = "tx", "rx";
		pinctrl-names = "default";
		pinctrl-0 = <&i2s1_2ch_sclk &i2s1_2ch_lrck
			     &i2s1_2ch_sdi &i2s1_2ch_sdo>;
		#sound-dai-cells = <0>;
		status = "disabled";
	};

	i2s2_2ch: i2s@ff080000 {
		compatible = "rockchip,px30-i2s", "rockchip,rk3066-i2s";
		reg = <0x0 0xff080000 0x0 0x1000>;
		interrupts = <GIC_SPI 14 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_I2S2>, <&cru HCLK_I2S2>;
		clock-names = "i2s_clk", "i2s_hclk";
		dmas = <&dmac 20>, <&dmac 21>;
		dma-names = "tx", "rx";
		pinctrl-names = "default";
		pinctrl-0 = <&i2s2_2ch_sclk &i2s2_2ch_lrck
			     &i2s2_2ch_sdi &i2s2_2ch_sdo>;
		#sound-dai-cells = <0>;
		status = "disabled";
	};

	crypto: crypto@ff0b0000 {
		compatible = "rockchip,px30-crypto";
		reg = <0x0 0xff0b0000 0x0 0x400>, <0x0 0xff0b0480 0x0 0x3B80>;
		interrupts = <GIC_SPI 82 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru ACLK_CRYPTO >, <&cru HCLK_CRYPTO >,
			 <&cru SCLK_CRYPTO>, <&cru SCLK_CRYPTO_APK>;
		clock-names = "aclk", "hclk", "sclk", "apb_pclk";
		resets = <&cru SRST_CRYPTO>;
		reset-names = "crypto-rst";
		status = "disabled";
	};

	rng: rng@ff0b0000 {
		compatible = "rockchip,cryptov2-rng";
		reg = <0x0 0xff0b0400 0x0 0x80>;
		clocks = <&cru SCLK_CRYPTO>, <&cru SCLK_CRYPTO_APK>,
			 <&cru ACLK_CRYPTO>, <&cru HCLK_CRYPTO>;
		clock-names = "clk_crypto", "clk_crypto_apk",
			      "aclk_crypto", "hclk_crypto";
		assigned-clocks = <&cru SCLK_CRYPTO>, <&cru SCLK_CRYPTO_APK>,
				  <&cru ACLK_CRYPTO>, <&cru HCLK_CRYPTO>;
		assigned-clock-rates = <150000000>, <150000000>,
				       <200000000>, <200000000>;
		resets = <&cru SRST_CRYPTO>;
		reset-names = "reset";
		status = "disabled";
	};

	gic: interrupt-controller@ff131000 {
		compatible = "arm,gic-400";
		#interrupt-cells = <3>;
		#address-cells = <0>;
		interrupt-controller;
		reg = <0x0 0xff131000 0 0x1000>,
		      <0x0 0xff132000 0 0x2000>,
		      <0x0 0xff134000 0 0x2000>,
		      <0x0 0xff136000 0 0x2000>;
		interrupts = <GIC_PPI 9
		      (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_HIGH)>;
	};

	grf: syscon@ff140000 {
		compatible = "rockchip,px30-grf", "syscon", "simple-mfd";
		reg = <0x0 0xff140000 0x0 0x1000>;
		#address-cells = <1>;
		#size-cells = <1>;

		io_domains: io-domains {
			compatible = "rockchip,px30-io-voltage-domain";
			status = "disabled";
		};

		lvds: lvds {
			compatible = "rockchip,px30-lvds";
			phys = <&video_phy>;
			phy-names = "phy";
			status = "disabled";

			ports {
				#address-cells = <1>;
				#size-cells = <0>;

				port@0 {
					reg = <0>;
					#address-cells = <1>;
					#size-cells = <0>;

					lvds_vopb_in: endpoint@0 {
						reg = <0>;
						remote-endpoint = <&vopb_out_lvds>;
					};

					lvds_vopl_in: endpoint@1 {
						reg = <1>;
						remote-endpoint = <&vopl_out_lvds>;
					};
				};
			};
		};

		rgb: rgb {
			compatible = "rockchip,px30-rgb";
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&lcdc_m0_rgb_pins>;
			pinctrl-1 = <&lcdc_m0_sleep_pins>;
			status = "disabled";

			ports {
				#address-cells = <1>;
				#size-cells = <0>;

				port@0 {
					reg = <0>;
					#address-cells = <1>;
					#size-cells = <0>;

					rgb_in_vopb: endpoint@0 {
						reg = <0>;
						remote-endpoint = <&vopb_out_rgb>;
					};

					rgb_in_vopl: endpoint@1 {
						reg = <1>;
						remote-endpoint = <&vopl_out_rgb>;
					};
				};
			};
		};
	};

	core_grf: syscon@ff148000 {
		compatible = "syscon", "simple-mfd";
		reg = <0x0 0xff148000 0x0 0x1000>;
		#address-cells = <1>;
		#size-cells = <1>;

		pvtm: pvtm {
			compatible = "rockchip,px30-pvtm";
			#address-cells = <1>;
			#size-cells = <0>;
			status = "okay";

			pvtm@0 {
				reg = <0>;
				clocks = <&cru SCLK_PVTM>;
				clock-names = "clk";
			};
		};
	};

	uart1: serial@ff158000 {
		compatible = "rockchip,px30-uart", "snps,dw-apb-uart";
		reg = <0x0 0xff158000 0x0 0x100>;
		interrupts = <GIC_SPI 16 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_UART1>, <&cru PCLK_UART1>;
		clock-names = "baudclk", "apb_pclk";
		dmas = <&dmac 2>, <&dmac 3>;
		/*You can add it to enable dma*/
		/*dma-names = "tx", "rx";*/
		reg-shift = <2>;
		reg-io-width = <4>;
		pinctrl-names = "default";
		pinctrl-0 = <&uart1_xfer &uart1_cts &uart1_rts>;
		status = "disabled";
	};

	uart2: serial@ff160000 {
		compatible = "rockchip,px30-uart", "snps,dw-apb-uart";
		reg = <0x0 0xff160000 0x0 0x100>;
		interrupts = <GIC_SPI 17 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_UART2>, <&cru PCLK_UART2>;
		clock-names = "baudclk", "apb_pclk";
		dmas = <&dmac 4>, <&dmac 5>;
		/*You can add it to enable dma*/
		/*dma-names = "tx", "rx";*/
		reg-shift = <2>;
		reg-io-width = <4>;
		pinctrl-names = "default";
		pinctrl-0 = <&uart2m0_xfer>;
		status = "disabled";
	};

	uart3: serial@ff168000 {
		compatible = "rockchip,px30-uart", "snps,dw-apb-uart";
		reg = <0x0 0xff168000 0x0 0x100>;
		interrupts = <GIC_SPI 18 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_UART3>, <&cru PCLK_UART3>;
		clock-names = "baudclk", "apb_pclk";
		dmas = <&dmac 6>, <&dmac 7>;
		/*You can add it to enable dma*/
		/*dma-names = "tx", "rx";*/
		reg-shift = <2>;
		reg-io-width = <4>;
		pinctrl-names = "default";
		pinctrl-0 = <&uart3m1_xfer &uart3m1_cts &uart3m1_rts>;
		status = "disabled";
	};

	uart4: serial@ff170000 {
		compatible = "rockchip,px30-uart", "snps,dw-apb-uart";
		reg = <0x0 0xff170000 0x0 0x100>;
		interrupts = <GIC_SPI 19 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_UART4>, <&cru PCLK_UART4>;
		clock-names = "baudclk", "apb_pclk";
		dmas = <&dmac 8>, <&dmac 9>;
		/*You can add it to enable dma*/
		/*dma-names = "tx", "rx";*/
		reg-shift = <2>;
		reg-io-width = <4>;
		pinctrl-names = "default";
		pinctrl-0 = <&uart4_xfer &uart4_cts &uart4_rts>;
		status = "disabled";
	};

	uart5: serial@ff178000 {
		compatible = "rockchip,px30-uart", "snps,dw-apb-uart";
		reg = <0x0 0xff178000 0x0 0x100>;
		interrupts = <GIC_SPI 20 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_UART5>, <&cru PCLK_UART5>;
		clock-names = "baudclk", "apb_pclk";
		dmas = <&dmac 10>, <&dmac 11>;
		/*You can add it to enable dma*/
		/*dma-names = "tx", "rx";*/
		reg-shift = <2>;
		reg-io-width = <4>;
		pinctrl-names = "default";
		pinctrl-0 = <&uart5_xfer &uart5_cts &uart5_rts>;
		status = "disabled";
	};

	i2c0: i2c@ff180000 {
		compatible = "rockchip,px30-i2c", "rockchip,rk3399-i2c";
		reg = <0x0 0xff180000 0x0 0x1000>;
		clocks =  <&cru SCLK_I2C0>, <&cru PCLK_I2C0>;
		clock-names = "i2c", "pclk";
		interrupts = <GIC_SPI 7 IRQ_TYPE_LEVEL_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2c0_xfer>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	i2c1: i2c@ff190000 {
		compatible = "rockchip,px30-i2c", "rockchip,rk3399-i2c";
		reg = <0x0 0xff190000 0x0 0x1000>;
		clocks = <&cru SCLK_I2C1>, <&cru PCLK_I2C1>;
		clock-names = "i2c", "pclk";
		interrupts = <GIC_SPI 8 IRQ_TYPE_LEVEL_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2c1_xfer>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	i2c2: i2c@ff1a0000 {
		compatible = "rockchip,px30-i2c", "rockchip,rk3399-i2c";
		reg = <0x0 0xff1a0000 0x0 0x1000>;
		clocks = <&cru SCLK_I2C2>, <&cru PCLK_I2C2>;
		clock-names = "i2c", "pclk";
		interrupts = <GIC_SPI 9 IRQ_TYPE_LEVEL_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2c2_xfer>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	i2c3: i2c@ff1b0000 {
		compatible = "rockchip,px30-i2c", "rockchip,rk3399-i2c";
		reg = <0x0 0xff1b0000 0x0 0x1000>;
		clocks = <&cru SCLK_I2C3>, <&cru PCLK_I2C3>;
		clock-names = "i2c", "pclk";
		interrupts = <GIC_SPI 10 IRQ_TYPE_LEVEL_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2c3_xfer>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	spi0: spi@ff1d0000 {
		compatible = "rockchip,px30-spi", "rockchip,rk3066-spi";
		reg = <0x0 0xff1d0000 0x0 0x1000>;
		interrupts = <GIC_SPI 26 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_SPI0>, <&cru PCLK_SPI0>;
		clock-names = "spiclk", "apb_pclk";
		dmas = <&dmac 12>, <&dmac 13>;
		dma-names = "tx", "rx";
		pinctrl-names = "default";
		pinctrl-0 = <&spi0_clk &spi0_csn &spi0_miso &spi0_mosi>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	spi1: spi@ff1d8000 {
		compatible = "rockchip,px30-spi", "rockchip,rk3066-spi";
		reg = <0x0 0xff1d8000 0x0 0x1000>;
		interrupts = <GIC_SPI 27 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_SPI1>, <&cru PCLK_SPI1>;
		clock-names = "spiclk", "apb_pclk";
		dmas = <&dmac 14>, <&dmac 15>;
		dma-names = "tx", "rx";
		pinctrl-names = "default";
		pinctrl-0 = <&spi1_clk &spi1_csn0 &spi1_csn1 &spi1_miso &spi1_mosi>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	wdt: watchdog@ff1e0000 {
		compatible = "snps,dw-wdt";
		reg = <0x0 0xff1e0000 0x0 0x100>;
		clocks = <&cru PCLK_WDT_NS>;
		interrupts = <GIC_SPI 37 IRQ_TYPE_LEVEL_HIGH>;
		status = "disabled";
	};

	pwm0: pwm@ff200000 {
		compatible = "rockchip,px30-pwm", "rockchip,rk3328-pwm";
		reg = <0x0 0xff200000 0x0 0x10>;
		interrupts = <GIC_SPI 24 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_PWM0>, <&cru PCLK_PWM0>;
		clock-names = "pwm", "pclk";
		pinctrl-names = "active";
		pinctrl-0 = <&pwm0_pin>;
		#pwm-cells = <3>;
		status = "disabled";
	};

	pwm1: pwm@ff200010 {
		compatible = "rockchip,px30-pwm", "rockchip,rk3328-pwm";
		reg = <0x0 0xff200010 0x0 0x10>;
		interrupts = <GIC_SPI 24 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_PWM0>, <&cru PCLK_PWM0>;
		clock-names = "pwm", "pclk";
		pinctrl-names = "active";
		pinctrl-0 = <&pwm1_pin>;
		#pwm-cells = <3>;
		status = "disabled";
	};

	pwm2: pwm@ff200020 {
		compatible = "rockchip,px30-pwm", "rockchip,rk3328-pwm";
		reg = <0x0 0xff200020 0x0 0x10>;
		interrupts = <GIC_SPI 24 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_PWM0>, <&cru PCLK_PWM0>;
		clock-names = "pwm", "pclk";
		pinctrl-names = "active";
		pinctrl-0 = <&pwm2_pin>;
		#pwm-cells = <3>;
		status = "disabled";
	};

	pwm3: pwm@ff200030 {
		compatible = "rockchip,px30-pwm", "rockchip,rk3328-pwm";
		reg = <0x0 0xff200030 0x0 0x10>;
		interrupts = <GIC_SPI 24 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 89 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_PWM0>, <&cru PCLK_PWM0>;
		clock-names = "pwm", "pclk";
		pinctrl-names = "active";
		pinctrl-0 = <&pwm3_pin>;
		#pwm-cells = <3>;
		status = "disabled";
	};

	pwm4: pwm@ff208000 {
		compatible = "rockchip,px30-pwm", "rockchip,rk3328-pwm";
		reg = <0x0 0xff208000 0x0 0x10>;
		interrupts = <GIC_SPI 25 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_PWM1>, <&cru PCLK_PWM1>;
		clock-names = "pwm", "pclk";
		pinctrl-names = "active";
		pinctrl-0 = <&pwm4_pin>;
		#pwm-cells = <3>;
		status = "disabled";
	};

	pwm5: pwm@ff208010 {
		compatible = "rockchip,px30-pwm", "rockchip,rk3328-pwm";
		reg = <0x0 0xff208010 0x0 0x10>;
		interrupts = <GIC_SPI 25 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_PWM1>, <&cru PCLK_PWM1>;
		clock-names = "pwm", "pclk";
		pinctrl-names = "active";
		pinctrl-0 = <&pwm5_pin>;
		#pwm-cells = <3>;
		status = "disabled";
	};

	pwm6: pwm@ff208020 {
		compatible = "rockchip,px30-pwm", "rockchip,rk3328-pwm";
		reg = <0x0 0xff208020 0x0 0x10>;
		interrupts = <GIC_SPI 25 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_PWM1>, <&cru PCLK_PWM1>;
		clock-names = "pwm", "pclk";
		pinctrl-names = "active";
		pinctrl-0 = <&pwm6_pin>;
		#pwm-cells = <3>;
		status = "disabled";
	};

	pwm7: pwm@ff208030 {
		compatible = "rockchip,px30-pwm", "rockchip,rk3328-pwm";
		reg = <0x0 0xff208030 0x0 0x10>;
		interrupts = <GIC_SPI 25 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 90 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_PWM1>, <&cru PCLK_PWM1>;
		clock-names = "pwm", "pclk";
		pinctrl-names = "active";
		pinctrl-0 = <&pwm7_pin>;
		#pwm-cells = <3>;
		status = "disabled";
	};

	rktimer: timer@ff210000 {
		compatible = "rockchip,px30-timer", "rockchip,rk3288-timer";
		reg = <0x0 0xff210000 0x0 0x1000>;
		interrupts = <GIC_SPI 30 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru PCLK_TIMER>, <&cru SCLK_TIMER0>;
		clock-names = "pclk", "timer";
	};

	amba: bus {
		compatible = "simple-bus";
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;

		dmac: dmac@ff240000 {
			compatible = "arm,pl330", "arm,primecell";
			reg = <0x0 0xff240000 0x0 0x4000>;
			interrupts = <GIC_SPI 1 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 2 IRQ_TYPE_LEVEL_HIGH>;
			arm,pl330-periph-burst;
			clocks = <&cru ACLK_DMAC>;
			clock-names = "apb_pclk";
			#dma-cells = <1>;
		};
	};

	tsadc: tsadc@ff280000 {
		compatible = "rockchip,px30-tsadc";
		reg = <0x0 0xff280000 0x0 0x100>;
		interrupts = <GIC_SPI 36 IRQ_TYPE_LEVEL_HIGH>;
		assigned-clocks = <&cru SCLK_TSADC>;
		assigned-clock-rates = <50000>;
		clocks = <&cru SCLK_TSADC>, <&cru PCLK_TSADC>;
		clock-names = "tsadc", "apb_pclk";
		resets = <&cru SRST_TSADC>;
		reset-names = "tsadc-apb";
		rockchip,grf = <&grf>;
		rockchip,hw-tshut-temp = <120000>;
		pinctrl-names = "init", "default", "sleep";
		pinctrl-0 = <&tsadc_otp_pin>;
		pinctrl-1 = <&tsadc_otp_out>;
		pinctrl-2 = <&tsadc_otp_pin>;
		#thermal-sensor-cells = <1>;
		status = "disabled";
	};

	saradc: saradc@ff288000 {
		compatible = "rockchip,px30-saradc", "rockchip,rk3399-saradc";
		reg = <0x0 0xff288000 0x0 0x100>;
		interrupts = <GIC_SPI 84 IRQ_TYPE_LEVEL_HIGH>;
		#io-channel-cells = <1>;
		clocks = <&cru SCLK_SARADC>, <&cru PCLK_SARADC>;
		clock-names = "saradc", "apb_pclk";
		resets = <&cru SRST_SARADC_P>;
		reset-names = "saradc-apb";
		status = "disabled";
	};

	otp: nvmem@ff290000 {
		compatible = "rockchip,px30-otp";
		reg = <0x0 0xff290000 0x0 0x4000>;
		clocks = <&cru SCLK_OTP_USR>, <&cru PCLK_OTP_NS>,
			 <&cru PCLK_OTP_PHY>;
		clock-names = "otp", "apb_pclk", "phy";
		resets = <&cru SRST_OTP_PHY>;
		reset-names = "phy";
		#address-cells = <1>;
		#size-cells = <1>;

		/* Data cells */
		cpu_id: id@7 {
			reg = <0x07 0x10>;
		};
		cpu_leakage: cpu-leakage@17 {
			reg = <0x17 0x1>;
		};
		performance: performance@1e {
			reg = <0x1e 0x1>;
			bits = <4 3>;
		};
	};

	cru: clock-controller@ff2b0000 {
		compatible = "rockchip,px30-cru";
		reg = <0x0 0xff2b0000 0x0 0x1000>;
		rockchip,grf = <&grf>;
		#clock-cells = <1>;
		#reset-cells = <1>;

		assigned-clocks = <&cru PLL_NPLL>;
		assigned-clock-rates = <1188000000>;
	};

	pmucru: clock-controller@ff2bc000 {
		compatible = "rockchip,px30-pmucru";
		reg = <0x0 0xff2bc000 0x0 0x1000>;
		rockchip,grf = <&grf>;
		#clock-cells = <1>;
		#reset-cells = <1>;

		assigned-clocks =
			<&pmucru PLL_GPLL>, <&pmucru PCLK_PMU_PRE>,
			<&pmucru SCLK_WIFI_PMU>, <&cru ARMCLK>,
			<&cru ACLK_BUS_PRE>, <&cru ACLK_PERI_PRE>,
			<&cru HCLK_BUS_PRE>, <&cru HCLK_PERI_PRE>,
			<&cru PCLK_BUS_PRE>, <&cru SCLK_GPU>;
		assigned-clock-rates =
			<1200000000>, <100000000>,
			<26000000>, <600000000>,
			<200000000>, <200000000>,
			<150000000>, <150000000>,
			<100000000>, <200000000>;
	};

	usb2phy_grf: syscon@ff2c0000 {
		compatible = "rockchip,px30-usb2phy-grf", "syscon",
			     "simple-mfd";
		reg = <0x0 0xff2c0000 0x0 0x10000>;
		#address-cells = <1>;
		#size-cells = <1>;

		u2phy: usb2-phy@100 {
			compatible = "rockchip,px30-usb2phy";
			reg = <0x100 0x20>;
			clocks = <&pmucru SCLK_USBPHY_REF>;
			clock-names = "phyclk";
			#clock-cells = <0>;
			assigned-clocks = <&cru USB480M>, <&cru SCLK_UART1_SRC>;
			assigned-clock-parents = <&u2phy>, <&cru USB480M>;
			clock-output-names = "usb480m_phy";
			status = "disabled";

			u2phy_host: host-port {
				#phy-cells = <0>;
				interrupts = <GIC_SPI 68 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-names = "linestate";
				status = "disabled";
			};

			u2phy_otg: otg-port {
				#phy-cells = <0>;
				interrupts = <GIC_SPI 66 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 65 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 64 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-names = "otg-bvalid", "otg-id",
						  "linestate";
				status = "disabled";
			};
		};
	};

	video_phy: dsi_dphy: phy@ff2e0000 {
		compatible = "rockchip,px30-dsi-dphy", "rockchip,px30-video-phy";
		reg = <0x0 0xff2e0000 0x0 0x10000>,
		      <0x0 0xff450000 0x0 0x10000>;
		reg-names = "phy", "host";
		clocks = <&pmucru SCLK_MIPIDSIPHY_REF>,
			 <&cru PCLK_MIPIDSIPHY>, <&cru PCLK_MIPI_DSI>;
		clock-names = "ref", "pclk", "pclk_host";
		resets = <&cru SRST_MIPIDSIPHY_P>;
		reset-names = "apb";
		#phy-cells = <0>;
		power-domains = <&power PX30_PD_VO>;
		status = "disabled";
	};

	mipi_dphy_rx0: mipi-dphy-rx0@ff2f0000 {
		compatible = "rockchip,rk3326-mipi-dphy";
		reg = <0x0 0xff2f0000 0x0 0x4000>;
		clocks = <&cru PCLK_MIPICSIPHY>;
		clock-names = "dphy-ref";
		power-domains = <&power PX30_PD_VI>;
		rockchip,grf = <&grf>;
		status = "disabled";
	};

	usb20_otg: usb@ff300000 {
		compatible = "rockchip,px30-usb", "rockchip,rk3066-usb",
			     "snps,dwc2";
		reg = <0x0 0xff300000 0x0 0x40000>;
		interrupts = <GIC_SPI 62 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru HCLK_OTG>;
		clock-names = "otg";
		dr_mode = "otg";
		g-np-tx-fifo-size = <16>;
		g-rx-fifo-size = <280>;
		g-tx-fifo-size = <256 128 128 64 32 16>;
		phys = <&u2phy_otg>;
		phy-names = "usb2-phy";
		power-domains = <&power PX30_PD_USB>;
		status = "disabled";
	};

	usb_host0_ehci: usb@ff340000 {
		compatible = "generic-ehci";
		reg = <0x0 0xff340000 0x0 0x10000>;
		interrupts = <GIC_SPI 60 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru HCLK_HOST>, <&u2phy>;
		clock-names = "usbhost", "utmi";
		phys = <&u2phy_host>;
		phy-names = "usb";
		power-domains = <&power PX30_PD_USB>;
		status = "disabled";
	};

	usb_host0_ohci: usb@ff350000 {
		compatible = "generic-ohci";
		reg = <0x0 0xff350000 0x0 0x10000>;
		interrupts = <GIC_SPI 61 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru HCLK_HOST>, <&u2phy>;
		clock-names = "usbhost", "utmi";
		phys = <&u2phy_host>;
		phy-names = "usb";
		power-domains = <&power PX30_PD_USB>;
		status = "disabled";
	};

	gmac: ethernet@ff360000 {
		compatible = "rockchip,px30-gmac";
		reg = <0x0 0xff360000 0x0 0x10000>;
		interrupts = <GIC_SPI 43 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "macirq";
		clocks = <&cru SCLK_GMAC>, <&cru SCLK_GMAC_RX_TX>,
			 <&cru SCLK_GMAC_RX_TX>, <&cru SCLK_MAC_REF>,
			 <&cru SCLK_MAC_REFOUT>, <&cru ACLK_GMAC>,
			 <&cru PCLK_GMAC>, <&cru SCLK_GMAC_RMII>;
		clock-names = "stmmaceth", "mac_clk_rx",
			      "mac_clk_tx", "clk_mac_ref",
			      "clk_mac_refout", "aclk_mac",
			      "pclk_mac", "clk_mac_speed";
		rockchip,grf = <&grf>;
		phy-mode = "rmii";
		pinctrl-names = "default";
		pinctrl-0 = <&rmii_pins &mac_refclk_12ma>;
		power-domains = <&power PX30_PD_GMAC>;
		resets = <&cru SRST_GMAC_A>;
		reset-names = "stmmaceth";
		status = "disabled";
	};

	sdmmc: dwmmc@ff370000 {
		compatible = "rockchip,px30-dw-mshc", "rockchip,rk3288-dw-mshc";
		reg = <0x0 0xff370000 0x0 0x4000>;
		interrupts = <GIC_SPI 54 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru HCLK_SDMMC>, <&cru SCLK_SDMMC>,
			 <&cru SCLK_SDMMC_DRV>, <&cru SCLK_SDMMC_SAMPLE>;
		clock-names = "biu", "ciu", "ciu-drive", "ciu-sample";
		bus-width = <4>;
		fifo-depth = <0x100>;
		max-frequency = <150000000>;
		pinctrl-names = "default";
		pinctrl-0 = <&sdmmc_clk &sdmmc_cmd &sdmmc_det &sdmmc_bus4>;
		power-domains = <&power PX30_PD_SDCARD>;
		status = "disabled";
	};

	sdio: dwmmc@ff380000 {
		compatible = "rockchip,px30-dw-mshc", "rockchip,rk3288-dw-mshc";
		reg = <0x0 0xff380000 0x0 0x4000>;
		interrupts = <GIC_SPI 55 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru HCLK_SDIO>, <&cru SCLK_SDIO>,
			 <&cru SCLK_SDIO_DRV>, <&cru SCLK_SDIO_SAMPLE>;
		clock-names = "biu", "ciu", "ciu-drive", "ciu-sample";
		bus-width = <4>;
		fifo-depth = <0x100>;
		max-frequency = <150000000>;
		pinctrl-names = "default";
		pinctrl-0 = <&sdio_bus4 &sdio_cmd &sdio_clk>;
		power-domains = <&power PX30_PD_MMC_NAND>;
		status = "disabled";
	};

	emmc: dwmmc@ff390000 {
		compatible = "rockchip,px30-dw-mshc", "rockchip,rk3288-dw-mshc";
		reg = <0x0 0xff390000 0x0 0x4000>;
		interrupts = <GIC_SPI 53 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru HCLK_EMMC>, <&cru SCLK_EMMC>,
			 <&cru SCLK_EMMC_DRV>, <&cru SCLK_EMMC_SAMPLE>;
		clock-names = "biu", "ciu", "ciu-drive", "ciu-sample";
		bus-width = <8>;
		fifo-depth = <0x100>;
		max-frequency = <150000000>;
		pinctrl-names = "default";
		pinctrl-0 = <&emmc_clk &emmc_cmd &emmc_bus8>;
		power-domains = <&power PX30_PD_MMC_NAND>;
		status = "disabled";
	};

	sfc: spi@ff3a0000 {
		compatible = "rockchip,sfc";
		reg = <0x0 0xff3a0000 0x0 0x4000>;
		interrupts = <GIC_SPI 56 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_SFC>, <&cru HCLK_SFC>;
		clock-names = "clk_sfc", "hclk_sfc";
		assigned-clocks = <&cru SCLK_SFC>;
		assigned-clock-rates = <100000000>;
		status = "disabled";
	};

	nandc0: nandc@ff3b0000 {
		compatible = "rockchip,rk-nandc";
		reg = <0x0 0xff3b0000 0x0 0x4000>;
		interrupts = <GIC_SPI 57 IRQ_TYPE_LEVEL_HIGH>;
		nandc_id = <0>;
		clocks = <&cru SCLK_NANDC>, <&cru HCLK_NANDC>;
		clock-names = "clk_nandc", "hclk_nandc";
		assigned-clocks = <&cru SCLK_NANDC>;
		assigned-clock-parents = <&cru SCLK_NANDC_DIV50>;
		power-domains = <&power PX30_PD_MMC_NAND>;
		status = "disabled";
	};

	gpu: gpu@ff400000 {
		compatible = "rockchip,px30-mali", "arm,mali-bifrost";
		reg = <0x0 0xff400000 0x0 0x4000>;
		interrupts = <GIC_SPI 45 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 46 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 47 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "GPU", "MMU", "JOB";
		clocks = <&cru SCLK_GPU>;
		#cooling-cells = <2>;
		power-domains = <&power PX30_PD_GPU>;
		operating-points-v2 = <&gpu_opp_table>;
		upthreshold = <40>;
		downdifferential = <10>;
		status = "disabled";
		power_model {
			compatible = "arm,mali-simple-power-model";
			static-coefficient = <411000>;
			dynamic-coefficient = <733>;
			ts = <32000 4700 (-80) 2>;
			thermal-zone = "gpu-thermal";
		};
	};

	gpu_opp_table: gpu-opp-table {
		compatible = "operating-points-v2";

		rockchip,thermal-zone = "soc-thermal";
		rockchip,temp-hysteresis = <5000>;
		rockchip,low-temp = <0>;
		rockchip,low-temp-min-volt = <1000000>;
		rockchip,low-temp-adjust-volt = <
			/* MHz    MHz    uV */
			0      480     50000
		>;

		rockchip,max-volt = <1175000>;
		rockchip,evb-irdrop = <25000>;

		rockchip,pvtm-voltage-sel = <
			0        50000   0
			50001    54000   1
			54001    60000   2
			60001    99999   3
		>;
		rockchip,pvtm-ch = <0 0>;

		opp-200000000 {
			opp-hz = /bits/ 64 <200000000>;
			opp-microvolt = <950000>;
			opp-microvolt-L0 = <950000>;
			opp-microvolt-L1 = <950000>;
			opp-microvolt-L2 = <950000>;
			opp-microvolt-L3 = <950000>;
		};
		opp-300000000 {
			opp-hz = /bits/ 64 <300000000>;
			opp-microvolt = <975000>;
			opp-microvolt-L0 = <975000>;
			opp-microvolt-L1 = <950000>;
			opp-microvolt-L2 = <950000>;
			opp-microvolt-L3 = <950000>;
		};
		opp-400000000 {
			opp-hz = /bits/ 64 <400000000>;
			opp-microvolt = <1050000>;
			opp-microvolt-L0 = <1050000>;
			opp-microvolt-L1 = <1025000>;
			opp-microvolt-L2 = <975000>;
			opp-microvolt-L3 = <950000>;
		};
		opp-480000000 {
			opp-hz = /bits/ 64 <480000000>;
			opp-microvolt = <1125000>;
			opp-microvolt-L0 = <1125000>;
			opp-microvolt-L1 = <1100000>;
			opp-microvolt-L2 = <1050000>;
			opp-microvolt-L3 = <1000000>;
		};
	};

	px30s_gpu_opp_table: px30s-gpu-opp-table {
		compatible = "operating-points-v2";

		rockchip,pvtm-voltage-sel = <
			0        69850   0
			69851    73800   1
			73801    77750   2
			77751    81700   3
			81701    99999   4
		>;
		rockchip,pvtm-ch = <0 0>;

		opp-200000000 {
			opp-hz = /bits/ 64 <200000000>;
			opp-microvolt = <950000>;
		};
		opp-300000000 {
			opp-hz = /bits/ 64 <300000000>;
			opp-microvolt = <950000>;
		};
		opp-400000000 {
			opp-hz = /bits/ 64 <400000000>;
			opp-microvolt = <950000>;
		};
		opp-520000000 {
			opp-hz = /bits/ 64 <520000000>;
			opp-microvolt = <1000000>;
			opp-microvolt-L0 = <1000000>;
			opp-microvolt-L1 = <975000>;
			opp-microvolt-L2 = <950000>;
			opp-microvolt-L3 = <950000>;
			opp-microvolt-L4 = <950000>;
		};
	};

	mpp_srv: mpp-srv {
		compatible = "rockchip,mpp-service";
		rockchip,taskqueue-count = <1>;
		rockchip,resetgroup-count = <1>;
		rockchip,grf = <&grf>;
		rockchip,grf-offset = <0x0410>;
		rockchip,grf-values = <0x80008000>, <0x80000000>, <0x80000000>;
		rockchip,grf-names = "grf_rkvdec", "grf_vdpu2", "grf_vepu2";
		status = "disabled";
	};

	vdpu: vdpu@ff442400 {
		compatible = "rockchip,vpu-decoder-px30";
		reg = <0x0 0xff442400 0x0 0x400>;
		interrupts = <GIC_SPI 79 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "irq_dec";
		clocks = <&cru ACLK_VPU>, <&cru HCLK_VPU>;
		clock-names = "aclk_vcodec", "hclk_vcodec";
		resets = <&cru SRST_VPU_A>, <&cru SRST_VPU_H>;
		reset-names = "shared_video_a", "shared_video_h";
		iommus = <&vpu_mmu>;
		power-domains = <&power PX30_PD_VPU>;
		rockchip,srv = <&mpp_srv>;
		rockchip,taskqueue-node = <0>;
		rockchip,resetgroup-node = <0>;
		status = "disabled";
	};

	vpu_mmu: iommu@ff442800 {
		compatible = "rockchip,iommu";
		reg = <0x0 0xff442800 0x0 0x100>;
		interrupts = <GIC_SPI 81 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "vpu_mmu";
		clocks = <&cru ACLK_VPU>, <&cru HCLK_VPU>;
		clock-names = "aclk", "iface";
		power-domains = <&power PX30_PD_VPU>;
		rockchip,shootdown-entire;
		#iommu-cells = <0>;
		status = "disabled";
	};

	vepu: vepu@ff442000 {
		compatible = "rockchip,vpu-encoder-px30";
		reg = <0x0 0xff442000 0x0 0x400>;
		interrupts = <GIC_SPI 80 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "irq_enc";
		clocks = <&cru ACLK_VPU>, <&cru HCLK_VPU>;
		clock-names = "aclk_vcodec", "hclk_vcodec";
		resets = <&cru SRST_VPU_A>, <&cru SRST_VPU_H>;
		reset-names = "shared_video_a", "shared_video_h";
		iommus = <&vpu_mmu>;
		power-domains = <&power PX30_PD_VPU>;
		rockchip,srv = <&mpp_srv>;
		rockchip,taskqueue-node = <0>;
		rockchip,resetgroup-node = <0>;
		status = "disabled";
	};

	hevc: hevc@ff440000 {
		compatible = "rockchip,hevc-decoder-px30";
		reg = <0x0 0xff440000 0x0 0x400>;
		interrupts = <GIC_SPI 49 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "irq_dec";
		clocks = <&cru ACLK_VPU>, <&cru HCLK_VPU>, <&cru SCLK_CORE_VPU>;
		clock-names = "aclk_vcodec", "hclk_vcodec", "clk_core";
		resets = <&cru SRST_VPU_A>, <&cru SRST_VPU_H>,
			 <&cru SRST_VPU_NIU_A>, <&cru SRST_VPU_NIU_H>,
			 <&cru SRST_VPU_CORE>;
		reset-names = "shared_video_a", "shared_video_h",
			      "niu_a", "niu_h",
			      "video_core";
		iommus = <&hevc_mmu>;
		rockchip,srv = <&mpp_srv>;
		rockchip,taskqueue-node = <0>;
		rockchip,resetgroup-node = <0>;
		power-domains = <&power PX30_PD_VPU>;
		status = "disabled";
	};

	hevc_mmu: iommu@ff440440 {
		compatible = "rockchip,iommu";
		reg = <0x0 0xff440440 0x0 0x40>, <0x0 0xff440480 0x0 0x40>;
		interrupts = <GIC_SPI 50 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "hevc_mmu";
		clocks = <&cru ACLK_VPU>, <&cru HCLK_VPU>;
		clock-names = "aclk", "iface";
		power-domains = <&power PX30_PD_VPU>;
		rockchip,shootdown-entire;
		#iommu-cells = <0>;
		status = "disabled";
	};

	dsi: dsi@ff450000 {
		compatible = "rockchip,px30-mipi-dsi";
		reg = <0x0 0xff450000 0x0 0x10000>;
		interrupts = <GIC_SPI 75 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru PCLK_MIPI_DSI>;
		clock-names = "pclk";
		phys = <&video_phy>;
		phy-names = "dphy";
		power-domains = <&power PX30_PD_VO>;
		resets = <&cru SRST_MIPIDSI_HOST_P>;
		reset-names = "apb";
		rockchip,grf = <&grf>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				#address-cells = <1>;
				#size-cells = <0>;

				dsi_in_vopb: endpoint@0 {
					reg = <0>;
					remote-endpoint = <&vopb_out_dsi>;
				};

				dsi_in_vopl: endpoint@1 {
					reg = <1>;
					remote-endpoint = <&vopl_out_dsi>;
				};
			};
		};
	};

	vopb: vop@ff460000 {
		compatible = "rockchip,px30-vop-big";
		reg = <0x0 0xff460000 0x0 0x260>, <0x0 0xff460a00 0x0 0x400>;
		rockchip,grf = <&grf>;
		reg-names = "regs", "gamma_lut";
		interrupts = <GIC_SPI 77 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru ACLK_VOPB>, <&cru DCLK_VOPB>,
			 <&cru HCLK_VOPB>;
		clock-names = "aclk_vop", "dclk_vop", "hclk_vop";
		resets = <&cru SRST_VOPB_A>, <&cru SRST_VOPB_H>, <&cru SRST_VOPB>;
		reset-names = "axi", "ahb", "dclk";
		iommus = <&vopb_mmu>;
		power-domains = <&power PX30_PD_VO>;
		status = "disabled";

		vopb_out: port {
			#address-cells = <1>;
			#size-cells = <0>;

			vopb_out_dsi: endpoint@0 {
				reg = <0>;
				remote-endpoint = <&dsi_in_vopb>;
			};

			vopb_out_lvds: endpoint@1 {
				reg = <1>;
				remote-endpoint = <&lvds_vopb_in>;
			};

			vopb_out_rgb: endpoint@2 {
				reg = <2>;
				remote-endpoint = <&rgb_in_vopb>;
			};
		};
	};

	vopb_mmu: iommu@ff460f00 {
		compatible = "rockchip,iommu";
		reg = <0x0 0xff460f00 0x0 0x100>;
		interrupts = <GIC_SPI 77 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "vopb_mmu";
		clocks = <&cru ACLK_VOPB>, <&cru HCLK_VOPB>;
		clock-names = "aclk", "iface";
		power-domains = <&power PX30_PD_VO>;
		#iommu-cells = <0>;
		rockchip,disable-device-link-resume;
		status = "disabled";
	};

	vopl: vop@ff470000 {
		compatible = "rockchip,px30-vop-lit";
		reg = <0x0 0xff470000 0x0 0x1fc>, <0x0 0xff470a00 0x0 0x400>;
		rockchip,grf = <&grf>;
		reg-names = "regs", "gamma_lut";
		interrupts = <GIC_SPI 78 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru ACLK_VOPL>, <&cru DCLK_VOPL>,
			 <&cru HCLK_VOPL>;
		clock-names = "aclk_vop", "dclk_vop", "hclk_vop";
		resets = <&cru SRST_VOPL_A>, <&cru SRST_VOPL_H>, <&cru SRST_VOPL>;
		reset-names = "axi", "ahb", "dclk";
		iommus = <&vopl_mmu>;
		power-domains = <&power PX30_PD_VO>;
		status = "disabled";

		vopl_out: port {
			#address-cells = <1>;
			#size-cells = <0>;

			vopl_out_dsi: endpoint@0 {
				reg = <0>;
				remote-endpoint = <&dsi_in_vopl>;
			};

			vopl_out_lvds: endpoint@1 {
				reg = <1>;
				remote-endpoint = <&lvds_vopl_in>;
			};

			vopl_out_rgb: endpoint@2 {
				reg = <2>;
				remote-endpoint = <&rgb_in_vopl>;
			};
		};
	};

	vopl_mmu: iommu@ff470f00 {
		compatible = "rockchip,iommu";
		reg = <0x0 0xff470f00 0x0 0x100>;
		interrupts = <GIC_SPI 78 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "vopl_mmu";
		clocks = <&cru ACLK_VOPL>, <&cru HCLK_VOPL>;
		clock-names = "aclk", "iface";
		power-domains = <&power PX30_PD_VO>;
		#iommu-cells = <0>;
		rockchip,disable-device-link-resume;
		status = "disabled";
	};

	rk_rga: rk_rga@ff480000 {
		compatible = "rockchip,rga2";
		//dev_mode = <1>;
		reg = <0x0 0xff480000 0x0 0x1000>;
		interrupts = <GIC_SPI 76 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru ACLK_RGA>, <&cru HCLK_RGA>, <&cru SCLK_RGA_CORE>;
		clock-names = "aclk_rga", "hclk_rga", "clk_rga";
		power-domains = <&power PX30_PD_VO>;
		status = "disabled";
	};

	cif: cif@ff490000 {
		compatible = "rockchip,cif";
		reg = <0x0 0xff490000 0x0 0x200>;
		interrupts = <GIC_SPI 69 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru ACLK_CIF>, <&cru HCLK_CIF>, <&cru PCLK_CIF>, <&cru SCLK_CIF_OUT>;
		clock-names = "aclk_cif0", "hclk_cif0", "pclk_cif", "cif0_out";
		resets = <&cru SRST_CIF_A>, <&cru SRST_CIF_H>, <&cru SRST_CIF_PCLKIN>;
		reset-names = "rst_cif_a", "rst_cif_h", "rst_cif_pclkin";
		power-domains = <&power PX30_PD_VI>;
		pinctrl-names = "cif_pin_all";
		pinctrl-0 = <&dvp_d2d9_m0>;
		iommus = <&vip_mmu>;
		status = "disabled";
	};

	cif_new: cif-new@ff490000 {
		compatible = "rockchip,px30-cif";
		reg = <0x0 0xff490000 0x0 0x200>;
		interrupts = <GIC_SPI 69 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru ACLK_CIF>, <&cru HCLK_CIF>, <&cru PCLK_CIF>, <&cru SCLK_CIF_OUT>;
		clock-names = "aclk_cif", "hclk_cif", "pclk_cif", "cif_out";
		resets = <&cru SRST_CIF_A>, <&cru SRST_CIF_H>, <&cru SRST_CIF_PCLKIN>;
		reset-names = "rst_cif_a", "rst_cif_h", "rst_cif_pclkin";
		power-domains = <&power PX30_PD_VI>;
		iommus = <&vip_mmu>;
		status = "disabled";
	};

	vip_mmu: iommu@ff490800{
		compatible = "rockchip,iommu";
		reg = <0x0 0xff490800 0x0 0x100>;
		interrupts = <GIC_SPI 69 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "vip_mmu";
		clocks = <&cru ACLK_CIF>, <&cru HCLK_CIF>;
		clock-names = "aclk", "iface";
		power-domains = <&power PX30_PD_VI>;
		rk_iommu,disable_reset_quirk;
		#iommu-cells = <0>;
		status = "disabled";
	};

	rk_isp: rk_isp@ff4a0000 {
		compatible = "rockchip,px30-isp", "rockchip,isp";
		reg = <0x0 0xff4a0000 0x0 0x8000>;
		interrupts = <GIC_SPI 70 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru ACLK_ISP>, <&cru HCLK_ISP>, <&cru SCLK_ISP>, <&cru SCLK_ISP>,
			 <&cru PCLK_ISP>, <&cru SCLK_CIF_OUT>, <&cru SCLK_CIF_OUT>, <&cru PCLK_MIPICSIPHY>;
		clock-names = "aclk_isp", "hclk_isp", "clk_isp", "clk_isp_jpe",
			      "pclkin_isp", "clk_cif_pll", "clk_cif_out", "pclk_dphyrx";
		resets = <&cru SRST_ISP>, <&cru SRST_MIPICSIPHY_P>;
		reset-names = "rst_isp", "rst_mipicsiphy";
		power-domains = <&power PX30_PD_VI>;
		pinctrl-names = "default", "isp_dvp8bit2", "isp_dvp10bit", "isp_dvp12bit";
		pinctrl-0 = <&cif_clkout_m0>;
		pinctrl-1 = <&dvp_d2d9_m0>;
		pinctrl-2 = <&dvp_d2d9_m0 &dvp_d10d11_m0>;
		pinctrl-3 = <&dvp_d0d1_m0 &dvp_d2d9_m0 &dvp_d10d11_m0>;
		rockchip,isp,mipiphy = <1>;
		rockchip,isp,csiphy,reg = <0xff2f0000 0x4000>;
		rockchip,grf = <&grf>;
		rockchip,cru = <&cru>;
		rockchip,isp,iommu-enable = <1>;
		iommus = <&isp_mmu>;
		status = "disabled";
	};

	rkisp1: rkisp1@ff4a0000 {
		compatible = "rockchip,rk3326-rkisp1";
		reg = <0x0 0xff4a0000 0x0 0x8000>;
		interrupts = <GIC_SPI 70 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 73 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 74 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "isp_irq", "mi_irq", "mipi_irq";
		clocks = <&cru ACLK_ISP>, <&cru HCLK_ISP>,
			 <&cru SCLK_ISP>, <&cru PCLK_ISP>;
		clock-names = "aclk_isp", "hclk_isp",
			      "clk_isp", "pclk_isp";
		devfreq = <&dmc>;
		power-domains = <&power PX30_PD_VI>;
		iommus = <&isp_mmu>;
		rockchip,grf = <&grf>;
		status = "disabled";
	};

	isp_mmu: iommu@ff4a8000 {
		compatible = "rockchip,iommu";
		reg = <0x0 0xff4a8000 0x0 0x100>;
		interrupts = <GIC_SPI 70 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "isp_mmu";
		clocks = <&cru ACLK_ISP>, <&cru HCLK_ISP>;
		clock-names = "aclk", "iface";
		power-domains = <&power PX30_PD_VI>;
		rk_iommu,disable_reset_quirk;
		#iommu-cells = <0>;
		status = "disabled";
	};

	qos_gmac: qos@ff518000 {
		compatible = "syscon";
		reg = <0x0 0xff518000 0x0 0x20>;
	};

	qos_gpu: qos@ff520000 {
		compatible = "syscon";
		reg = <0x0 0xff520000 0x0 0x20>;
	};

	qos_sdmmc: qos@ff52c000 {
		compatible = "syscon";
		reg = <0x0 0xff52c000 0x0 0x20>;
	};

	qos_emmc: qos@ff538000 {
		compatible = "syscon";
		reg = <0x0 0xff538000 0x0 0x20>;
	};

	qos_nand: qos@ff538080 {
		compatible = "syscon";
		reg = <0x0 0xff538080 0x0 0x20>;
	};

	qos_sdio: qos@ff538100 {
		compatible = "syscon";
		reg = <0x0 0xff538100 0x0 0x20>;
	};

	qos_sfc: qos@ff538180 {
		compatible = "syscon";
		reg = <0x0 0xff538180 0x0 0x20>;
	};

	qos_usb_host: qos@ff540000 {
		compatible = "syscon";
		reg = <0x0 0xff540000 0x0 0x20>;
	};

	qos_usb_otg: qos@ff540080 {
		compatible = "syscon";
		reg = <0x0 0xff540080 0x0 0x20>;
	};

	qos_isp_128: qos@ff548000 {
		compatible = "syscon";
		reg = <0x0 0xff548000 0x0 0x20>;
	};

	qos_isp_rd: qos@ff548080 {
		compatible = "syscon";
		reg = <0x0 0xff548080 0x0 0x20>;
	};

	qos_isp_wr: qos@ff548100 {
		compatible = "syscon";
		reg = <0x0 0xff548100 0x0 0x20>;
	};

	qos_isp_m1: qos@ff548180 {
		compatible = "syscon";
		reg = <0x0 0xff548180 0x0 0x20>;
	};

	qos_vip: qos@ff548200 {
		compatible = "syscon";
		reg = <0x0 0xff548200 0x0 0x20>;
	};

	qos_rga_rd: qos@ff550000 {
		compatible = "syscon";
		reg = <0x0 0xff550000 0x0 0x20>;
	};

	qos_rga_wr: qos@ff550080 {
		compatible = "syscon";
		reg = <0x0 0xff550080 0x0 0x20>;
	};

	qos_vop_m0: qos@ff550100 {
		compatible = "syscon";
		reg = <0x0 0xff550100 0x0 0x20>;
	};

	qos_vop_m1: qos@ff550180 {
		compatible = "syscon";
		reg = <0x0 0xff550180 0x0 0x20>;
	};

	qos_vpu: qos@ff558000 {
		compatible = "syscon";
		reg = <0x0 0xff558000 0x0 0x20>;
	};

	qos_vpu_r128: qos@ff558080 {
		compatible = "syscon";
		reg = <0x0 0xff558080 0x0 0x20>;
	};

	dfi: dfi@ff610000 {
		reg = <0x00 0xff610000 0x00 0x400>;
		compatible = "rockchip,px30-dfi";
		rockchip,pmugrf = <&pmugrf>;
		status = "disabled";
	};

	dmc: dmc {
		compatible = "rockchip,px30-dmc";
		interrupts = <GIC_SPI 105 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "complete_irq";
		devfreq-events = <&dfi>;
		clocks = <&cru SCLK_DDRCLK>;
		clock-names = "dmc_clk";
		operating-points-v2 = <&dmc_opp_table>;
		ddr_timing = <&ddr_timing>;
		upthreshold = <40>;
		downdifferential = <20>;
		system-status-freq = <
			/*system status         freq(KHz)*/
			SYS_STATUS_NORMAL       666000
			SYS_STATUS_REBOOT       450000
			SYS_STATUS_SUSPEND      194000
			SYS_STATUS_VIDEO_1080P  450000
			SYS_STATUS_BOOST        666000
			SYS_STATUS_ISP          666000
			SYS_STATUS_PERFORMANCE  1056000
		>;
		auto-min-freq = <328000>;
		auto-freq-en = <1>;
		#cooling-cells = <2>;
		status = "disabled";

		ddr_power_model: ddr_power_model {
			compatible = "ddr_power_model";
			dynamic-power-coefficient = <120>;
			static-power-coefficient = <200>;
			ts = <32000 4700 (-80) 2>;
			thermal-zone = "soc-thermal";
		};
	};

	dmc_fsp: dmc-fsp {
		compatible = "rockchip,px30s-dmc-fsp";

		debug_print_level = <0>;
		phy_de_skew_en = <1>;
		ddr3_params = <&ddr3_params>;
		ddr4_params = <&ddr4_params>;
		lpddr2_params = <&lpddr2_params>;
		lpddr3_params = <&lpddr3_params>;
		lpddr4_params = <&lpddr4_params>;
		ddr_timing = <&ddr_timing>;
		status = "okay";
	};

	dmc_opp_table: dmc-opp-table {
		compatible = "operating-points-v2";

		rockchip,max-volt = <1150000>;
		rockchip,evb-irdrop = <25000>;

		rockchip,pvtm-voltage-sel = <
			0        50000   0
			50001    54000   1
			54001    60000   2
			60001    99999   3
		>;
		rockchip,pvtm-ch = <0 0>;

		opp-194000000 {
			opp-hz = /bits/ 64 <194000000>;
			opp-microvolt = <950000>;
			opp-microvolt-L0 = <950000>;
			opp-microvolt-L1 = <950000>;
			opp-microvolt-L2 = <950000>;
			opp-microvolt-L3 = <950000>;
		};
		opp-328000000 {
			opp-hz = /bits/ 64 <328000000>;
			opp-microvolt = <950000>;
			opp-microvolt-L0 = <950000>;
			opp-microvolt-L1 = <950000>;
			opp-microvolt-L2 = <950000>;
			opp-microvolt-L3 = <950000>;
		};
		opp-450000000 {
			opp-hz = /bits/ 64 <450000000>;
			opp-microvolt = <950000>;
			opp-microvolt-L0 = <950000>;
			opp-microvolt-L1 = <950000>;
			opp-microvolt-L2 = <950000>;
			opp-microvolt-L3 = <950000>;
		};
		opp-666000000 {
			opp-hz = /bits/ 64 <666000000>;
			opp-microvolt = <1050000>;
			opp-microvolt-L0 = <1050000>;
			opp-microvolt-L1 = <1000000>;
			opp-microvolt-L2 = <975000>;
			opp-microvolt-L3 = <950000>;
		};
		opp-786000000 {
			opp-hz = /bits/ 64 <786000000>;
			opp-microvolt = <1100000>;
			opp-microvolt-L0 = <1100000>;
			opp-microvolt-L1 = <1050000>;
			opp-microvolt-L2 = <1025000>;
			opp-microvolt-L3 = <1000000>;
			status = "disabled";
		};
	};

	px30s_dmc_opp_table: px30s-dmc-opp-table {
		compatible = "operating-points-v2";

		opp-194000000 {
			opp-hz = /bits/ 64 <194000000>;
			opp-microvolt = <950000>;
		};
		opp-328000000 {
			opp-hz = /bits/ 64 <328000000>;
			opp-microvolt = <950000>;
		};
		opp-666000000 {
			opp-hz = /bits/ 64 <666000000>;
			opp-microvolt = <950000>;
		};
		opp-786000000 {
			opp-hz = /bits/ 64 <786000000>;
			opp-microvolt = <950000>;
			status = "disabled";
		};
		opp-924000000 {
			opp-hz = /bits/ 64 <924000000>;
			opp-microvolt = <950000>;
			status = "disabled";
		};
		/* 1056M only for LP4 */
		opp-1056000000 {
			opp-hz = /bits/ 64 <1056000000>;
			opp-microvolt = <950000>;
			status = "disabled";
		};
	};

	dmcdbg: dmcdbg {
		compatible = "rockchip,px30-dmcdbg";
		status = "okay";
	};

	rockchip_system_monitor: rockchip-system-monitor {
		compatible = "rockchip,system-monitor";

		rockchip,thermal-zone = "soc-thermal";
		rockchip,polling-delay = <200>; /* milliseconds */
	};

	pinctrl: pinctrl {
		compatible = "rockchip,px30-pinctrl";
		rockchip,grf = <&grf>;
		rockchip,pmu = <&pmugrf>;
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;

		gpio0: gpio0@ff040000 {
			compatible = "rockchip,gpio-bank";
			reg = <0x0 0xff040000 0x0 0x100>;
			interrupts = <GIC_SPI 3 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&pmucru PCLK_GPIO0_PMU>;
			gpio-controller;
			#gpio-cells = <2>;

			interrupt-controller;
			#interrupt-cells = <2>;
		};

		gpio1: gpio1@ff250000 {
			compatible = "rockchip,gpio-bank";
			reg = <0x0 0xff250000 0x0 0x100>;
			interrupts = <GIC_SPI 4 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cru PCLK_GPIO1>;
			gpio-controller;
			#gpio-cells = <2>;

			interrupt-controller;
			#interrupt-cells = <2>;
		};

		gpio2: gpio2@ff260000 {
			compatible = "rockchip,gpio-bank";
			reg = <0x0 0xff260000 0x0 0x100>;
			interrupts = <GIC_SPI 5 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cru PCLK_GPIO2>;
			gpio-controller;
			#gpio-cells = <2>;

			interrupt-controller;
			#interrupt-cells = <2>;
		};

		gpio3: gpio3@ff270000 {
			compatible = "rockchip,gpio-bank";
			reg = <0x0 0xff270000 0x0 0x100>;
			interrupts = <GIC_SPI 6 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cru PCLK_GPIO3>;
			gpio-controller;
			#gpio-cells = <2>;

			interrupt-controller;
			#interrupt-cells = <2>;
		};

		pcfg_pull_up: pcfg-pull-up {
			bias-pull-up;
		};

		pcfg_pull_down: pcfg-pull-down {
			bias-pull-down;
		};

		pcfg_pull_none: pcfg-pull-none {
			bias-disable;
		};

		pcfg_pull_none_2ma: pcfg-pull-none-2ma {
			bias-disable;
			drive-strength = <2>;
		};

		pcfg_pull_up_2ma: pcfg-pull-up-2ma {
			bias-pull-up;
			drive-strength = <2>;
		};

		pcfg_pull_up_4ma: pcfg-pull-up-4ma {
			bias-pull-up;
			drive-strength = <4>;
		};

		pcfg_pull_none_4ma: pcfg-pull-none-4ma {
			bias-disable;
			drive-strength = <4>;
		};

		pcfg_pull_down_4ma: pcfg-pull-down-4ma {
			bias-pull-down;
			drive-strength = <4>;
		};

		pcfg_pull_none_8ma: pcfg-pull-none-8ma {
			bias-disable;
			drive-strength = <8>;
		};

		pcfg_pull_up_8ma: pcfg-pull-up-8ma {
			bias-pull-up;
			drive-strength = <8>;
		};

		pcfg_pull_none_12ma: pcfg-pull-none-12ma {
			bias-disable;
			drive-strength = <12>;
		};

		pcfg_pull_up_12ma: pcfg-pull-up-12ma {
			bias-pull-up;
			drive-strength = <12>;
		};

		pcfg_pull_none_smt: pcfg-pull-none-smt {
			bias-disable;
			input-schmitt-enable;
		};

		pcfg_output_high: pcfg-output-high {
			output-high;
		};

		pcfg_output_low: pcfg-output-low {
			output-low;
		};

		pcfg_input_high: pcfg-input-high {
			bias-pull-up;
			input-enable;
		};

		pcfg_input: pcfg-input {
			input-enable;
		};

		i2c0 {
			i2c0_xfer: i2c0-xfer {
				rockchip,pins =
					<0 RK_PB0 1 &pcfg_pull_none_smt>,
					<0 RK_PB1 1 &pcfg_pull_none_smt>;
			};
		};

		i2c1 {
			i2c1_xfer: i2c1-xfer {
				rockchip,pins =
					<0 RK_PC2 1 &pcfg_pull_none_smt>,
					<0 RK_PC3 1 &pcfg_pull_none_smt>;
			};
		};

		i2c2 {
			i2c2_xfer: i2c2-xfer {
				rockchip,pins =
					<2 RK_PB7 2 &pcfg_pull_none_smt>,
					<2 RK_PC0 2 &pcfg_pull_none_smt>;
			};
		};

		i2c3 {
			i2c3_xfer: i2c3-xfer {
				rockchip,pins =
					<1 RK_PB4 4 &pcfg_pull_none_smt>,
					<1 RK_PB5 4 &pcfg_pull_none_smt>;
			};
		};

		tsadc {
			tsadc_otp_gpio: tsadc_otp_pin: tsadc-otp-pin {
				rockchip,pins =
					<0 RK_PA6 RK_FUNC_GPIO &pcfg_pull_none>;
			};

			tsadc_otp_out: tsadc-otp-out {
				rockchip,pins =
					<0 RK_PA6 1 &pcfg_pull_none>;
			};
		};

		uart0 {
			uart0_xfer: uart0-xfer {
				rockchip,pins =
					<0 RK_PB2 1 &pcfg_pull_up>,
					<0 RK_PB3 1 &pcfg_pull_up>;
			};

			uart0_cts: uart0-cts {
				rockchip,pins =
					<0 RK_PB4 1 &pcfg_pull_none>;
			};

			uart0_rts: uart0-rts {
				rockchip,pins =
					<0 RK_PB5 1 &pcfg_pull_none>;
			};
		};

		uart1 {
			uart1_xfer: uart1-xfer {
				rockchip,pins =
					<1 RK_PC1 1 &pcfg_pull_up>,
					<1 RK_PC0 1 &pcfg_pull_up>;
			};

			uart1_cts: uart1-cts {
				rockchip,pins =
					<1 RK_PC2 1 &pcfg_pull_none>;
			};

			uart1_rts: uart1-rts {
				rockchip,pins =
					<1 RK_PC3 1 &pcfg_pull_none>;
			};

			uart1_rts_gpio: uart1-rts-gpio {
				rockchip,pins =
					<1 RK_PC3 RK_FUNC_GPIO &pcfg_pull_none>;
			};
		};

		uart2-m0 {
			uart2m0_xfer: uart2m0-xfer {
				rockchip,pins =
					<1 RK_PD2 2 &pcfg_pull_up>,
					<1 RK_PD3 2 &pcfg_pull_up>;
			};
		};

		uart2-m1 {
			uart2m1_xfer: uart2m1-xfer {
				rockchip,pins =
					<2 RK_PB4 2 &pcfg_pull_up>,
					<2 RK_PB6 2 &pcfg_pull_up>;
			};
		};

		uart3-m0 {
			uart3m0_xfer: uart3m0-xfer {
				rockchip,pins =
					<0 RK_PC0 2 &pcfg_pull_up>,
					<0 RK_PC1 2 &pcfg_pull_up>;
			};

			uart3m0_cts: uart3m0-cts {
				rockchip,pins =
					<0 RK_PC2 2 &pcfg_pull_none>;
			};

			uart3m0_rts: uart3m0-rts {
				rockchip,pins =
					<0 RK_PC3 2 &pcfg_pull_none>;
			};
		};

		uart3-m1 {
			uart3m1_xfer: uart3m1-xfer {
				rockchip,pins =
					<1 RK_PB6 2 &pcfg_pull_up>,
					<1 RK_PB7 2 &pcfg_pull_up>;
			};

			uart3m1_cts: uart3m1-cts {
				rockchip,pins =
					<1 RK_PB4 2 &pcfg_pull_none>;
			};

			uart3m1_rts: uart3m1-rts {
				rockchip,pins =
					<1 RK_PB5 2 &pcfg_pull_none>;
			};
		};

		uart4 {
			uart4_xfer: uart4-xfer {
				rockchip,pins =
					<1 RK_PD4 2 &pcfg_pull_up>,
					<1 RK_PD5 2 &pcfg_pull_up>;
			};

			uart4_cts: uart4-cts {
				rockchip,pins =
					<1 RK_PD6 2 &pcfg_pull_none>;
			};

			uart4_rts: uart4-rts {
				rockchip,pins =
					<1 RK_PD7 2 &pcfg_pull_none>;
			};
		};

		uart5 {
			uart5_xfer: uart5-xfer {
				rockchip,pins =
					<3 RK_PA2 4 &pcfg_pull_up>,
					<3 RK_PA1 4 &pcfg_pull_up>;
			};

			uart5_cts: uart5-cts {
				rockchip,pins =
					<3 RK_PA3 4 &pcfg_pull_none>;
			};

			uart5_rts: uart5-rts {
				rockchip,pins =
					<3 RK_PA5 4 &pcfg_pull_none>;
			};
		};

		spi0 {
			spi0_clk: spi0-clk {
				rockchip,pins =
					<1 RK_PB7 3 &pcfg_pull_up_4ma>;
			};

			spi0_csn: spi0-csn {
				rockchip,pins =
					<1 RK_PB6 3 &pcfg_pull_up_4ma>;
			};

			spi0_miso: spi0-miso {
				rockchip,pins =
					<1 RK_PB5 3 &pcfg_pull_up_4ma>;
			};

			spi0_mosi: spi0-mosi {
				rockchip,pins =
					<1 RK_PB4 3 &pcfg_pull_up_4ma>;
			};

			spi0_clk_hs: spi0-clk-hs {
				rockchip,pins =
					<1 RK_PB7 3 &pcfg_pull_up_8ma>;
			};

			spi0_miso_hs: spi0-miso-hs {
				rockchip,pins =
					<1 RK_PB5 3 &pcfg_pull_up_8ma>;
			};

			spi0_mosi_hs: spi0-mosi-hs {
				rockchip,pins =
					<1 RK_PB4 3 &pcfg_pull_up_8ma>;
			};
		};

		spi1 {
			spi1_clk: spi1-clk {
				rockchip,pins =
					<3 RK_PB7 4 &pcfg_pull_up_4ma>;
			};

			spi1_csn0: spi1-csn0 {
				rockchip,pins =
					<3 RK_PB1 4 &pcfg_pull_up_4ma>;
			};

			spi1_csn1: spi1-csn1 {
				rockchip,pins =
					<3 RK_PB2 2 &pcfg_pull_up_4ma>;
			};

			spi1_miso: spi1-miso {
				rockchip,pins =
					<3 RK_PB6 4 &pcfg_pull_up_4ma>;
			};

			spi1_mosi: spi1-mosi {
				rockchip,pins =
					<3 RK_PB4 4 &pcfg_pull_up_4ma>;
			};

			spi1_clk_hs: spi1-clk-hs {
				rockchip,pins =
					<3 RK_PB7 4 &pcfg_pull_up_8ma>;
			};

			spi1_miso_hs: spi1-miso-hs {
				rockchip,pins =
					<3 RK_PB6 4 &pcfg_pull_up_8ma>;
			};

			spi1_mosi_hs: spi1-mosi-hs {
				rockchip,pins =
					<3 RK_PB4 4 &pcfg_pull_up_8ma>;
			};
		};

		pdm {
			pdm_clk0m0: pdm-clk0m0 {
				rockchip,pins =
					<3 RK_PC6 2 &pcfg_pull_none>;
			};

			pdm_clk0m1: pdm-clk0m1 {
				rockchip,pins =
					<2 RK_PC6 1 &pcfg_pull_none>;
			};

			pdm_clk1: pdm-clk1 {
				rockchip,pins =
					<3 RK_PC7 2 &pcfg_pull_none>;
			};

			pdm_sdi0m0: pdm-sdi0m0 {
				rockchip,pins =
					<3 RK_PD3 2 &pcfg_pull_none>;
			};

			pdm_sdi0m1: pdm-sdi0m1 {
				rockchip,pins =
					<2 RK_PC5 2 &pcfg_pull_none>;
			};

			pdm_sdi1: pdm-sdi1 {
				rockchip,pins =
					<3 RK_PD0 2 &pcfg_pull_none>;
			};

			pdm_sdi2: pdm-sdi2 {
				rockchip,pins =
					<3 RK_PD1 2 &pcfg_pull_none>;
			};

			pdm_sdi3: pdm-sdi3 {
				rockchip,pins =
					<3 RK_PD2 2 &pcfg_pull_none>;
			};

			pdm_clk0m0_sleep: pdm-clk0m0-sleep {
				rockchip,pins =
					<3 RK_PC6 RK_FUNC_GPIO &pcfg_input_high>;
			};

			pdm_clk0m_sleep1: pdm-clk0m1-sleep {
				rockchip,pins =
					<2 RK_PC6 RK_FUNC_GPIO &pcfg_input_high>;
			};

			pdm_clk1_sleep: pdm-clk1-sleep {
				rockchip,pins =
					<3 RK_PC7 RK_FUNC_GPIO &pcfg_input_high>;
			};

			pdm_sdi0m0_sleep: pdm-sdi0m0-sleep {
				rockchip,pins =
					<3 RK_PD3 RK_FUNC_GPIO &pcfg_input_high>;
			};

			pdm_sdi0m1_sleep: pdm-sdi0m1-sleep {
				rockchip,pins =
					<2 RK_PC5 RK_FUNC_GPIO &pcfg_input_high>;
			};

			pdm_sdi1_sleep: pdm-sdi1-sleep {
				rockchip,pins =
					<3 RK_PD0 RK_FUNC_GPIO &pcfg_input_high>;
			};

			pdm_sdi2_sleep: pdm-sdi2-sleep {
				rockchip,pins =
					<3 RK_PD1 RK_FUNC_GPIO &pcfg_input_high>;
			};

			pdm_sdi3_sleep: pdm-sdi3-sleep {
				rockchip,pins =
					<3 RK_PD2 RK_FUNC_GPIO &pcfg_input_high>;
			};
		};

		i2s0 {
			i2s0_8ch_mclk: i2s0-8ch-mclk {
				rockchip,pins =
					<3 RK_PC1 2 &pcfg_pull_none_smt>;
			};

			i2s0_8ch_sclktx: i2s0-8ch-sclktx {
				rockchip,pins =
					<3 RK_PC3 2 &pcfg_pull_none_smt>;
			};

			i2s0_8ch_sclkrx: i2s0-8ch-sclkrx {
				rockchip,pins =
					<3 RK_PB4 2 &pcfg_pull_none_smt>;
			};

			i2s0_8ch_lrcktx: i2s0-8ch-lrcktx {
				rockchip,pins =
					<3 RK_PC2 2 &pcfg_pull_none_smt>;
			};

			i2s0_8ch_lrckrx: i2s0-8ch-lrckrx {
				rockchip,pins =
					<3 RK_PB5 2 &pcfg_pull_none_smt>;
			};

			i2s0_8ch_sdo0: i2s0-8ch-sdo0 {
				rockchip,pins =
					<3 RK_PC4 2 &pcfg_pull_none>;
			};

			i2s0_8ch_sdo1: i2s0-8ch-sdo1 {
				rockchip,pins =
					<3 RK_PC0 2 &pcfg_pull_none>;
			};

			i2s0_8ch_sdo2: i2s0-8ch-sdo2 {
				rockchip,pins =
					<3 RK_PB7 2 &pcfg_pull_none>;
			};

			i2s0_8ch_sdo3: i2s0-8ch-sdo3 {
				rockchip,pins =
					<3 RK_PB6 2 &pcfg_pull_none>;
			};

			i2s0_8ch_sdi0: i2s0-8ch-sdi0 {
				rockchip,pins =
					<3 RK_PC5 2 &pcfg_pull_none>;
			};

			i2s0_8ch_sdi1: i2s0-8ch-sdi1 {
				rockchip,pins =
					<3 RK_PB3 2 &pcfg_pull_none>;
			};

			i2s0_8ch_sdi2: i2s0-8ch-sdi2 {
				rockchip,pins =
					<3 RK_PB1 2 &pcfg_pull_none>;
			};

			i2s0_8ch_sdi3: i2s0-8ch-sdi3 {
				rockchip,pins =
					<3 RK_PB0 2 &pcfg_pull_none>;
			};
		};

		i2s1 {
			i2s1_2ch_mclk: i2s1-2ch-mclk {
				rockchip,pins =
					<2 RK_PC3 1 &pcfg_pull_none_smt>;
			};

			i2s1_2ch_sclk: i2s1-2ch-sclk {
				rockchip,pins =
					<2 RK_PC2 1 &pcfg_pull_none_smt>;
			};

			i2s1_2ch_lrck: i2s1-2ch-lrck {
				rockchip,pins =
					<2 RK_PC1 1 &pcfg_pull_none_smt>;
			};

			i2s1_2ch_sdi: i2s1-2ch-sdi {
				rockchip,pins =
					<2 RK_PC5 1 &pcfg_pull_none>;
			};

			i2s1_2ch_sdo: i2s1-2ch-sdo {
				rockchip,pins =
					<2 RK_PC4 1 &pcfg_pull_none>;
			};
		};

		i2s2 {
			i2s2_2ch_mclk: i2s2-2ch-mclk {
				rockchip,pins =
					<3 RK_PA1 2 &pcfg_pull_none_smt>;
			};

			i2s2_2ch_sclk: i2s2-2ch-sclk {
				rockchip,pins =
					<3 RK_PA2 2 &pcfg_pull_none_smt>;
			};

			i2s2_2ch_lrck: i2s2-2ch-lrck {
				rockchip,pins =
					<3 RK_PA3 2 &pcfg_pull_none_smt>;
			};

			i2s2_2ch_sdi: i2s2-2ch-sdi {
				rockchip,pins =
					<3 RK_PA5 2 &pcfg_pull_none>;
			};

			i2s2_2ch_sdo: i2s2-2ch-sdo {
				rockchip,pins =
					<3 RK_PA7 2 &pcfg_pull_none>;
			};
		};

		sdmmc {
			sdmmc_clk: sdmmc-clk {
				rockchip,pins =
					<1 RK_PD6 1 &pcfg_pull_none_8ma>;
			};

			sdmmc_cmd: sdmmc-cmd {
				rockchip,pins =
					<1 RK_PD7 1 &pcfg_pull_up_8ma>;
			};

			sdmmc_det: sdmmc-det {
				rockchip,pins =
					<0 RK_PA3 1 &pcfg_pull_up_8ma>;
			};

			sdmmc_bus1: sdmmc-bus1 {
				rockchip,pins =
					<1 RK_PD2 1 &pcfg_pull_up_8ma>;
			};

			sdmmc_bus4: sdmmc-bus4 {
				rockchip,pins =
					<1 RK_PD2 1 &pcfg_pull_up_8ma>,
					<1 RK_PD3 1 &pcfg_pull_up_8ma>,
					<1 RK_PD4 1 &pcfg_pull_up_8ma>,
					<1 RK_PD5 1 &pcfg_pull_up_8ma>;
			};
		};

		sdio {
			sdio_clk: sdio-clk {
				rockchip,pins =
					<1 RK_PC5 1 &pcfg_pull_none>;
			};

			sdio_cmd: sdio-cmd {
				rockchip,pins =
					<1 RK_PC4 1 &pcfg_pull_up>;
			};

			sdio_bus4: sdio-bus4 {
				rockchip,pins =
					<1 RK_PC6 1 &pcfg_pull_up>,
					<1 RK_PC7 1 &pcfg_pull_up>,
					<1 RK_PD0 1 &pcfg_pull_up>,
					<1 RK_PD1 1 &pcfg_pull_up>;
			};
		};

		emmc {
			emmc_clk: emmc-clk {
				rockchip,pins =
					<1 RK_PB1 2 &pcfg_pull_none_8ma>;
			};

			emmc_cmd: emmc-cmd {
				rockchip,pins =
					<1 RK_PB2 2 &pcfg_pull_up_8ma>;
			};

			emmc_rstnout: emmc-rstnout {
				rockchip,pins =
					<1 RK_PB3 2 &pcfg_pull_none>;
			};

			emmc_bus1: emmc-bus1 {
				rockchip,pins =
					<1 RK_PA0 2 &pcfg_pull_up_8ma>;
			};

			emmc_bus4: emmc-bus4 {
				rockchip,pins =
					<1 RK_PA0 2 &pcfg_pull_up_8ma>,
					<1 RK_PA1 2 &pcfg_pull_up_8ma>,
					<1 RK_PA2 2 &pcfg_pull_up_8ma>,
					<1 RK_PA3 2 &pcfg_pull_up_8ma>;
			};

			emmc_bus8: emmc-bus8 {
				rockchip,pins =
					<1 RK_PA0 2 &pcfg_pull_up_8ma>,
					<1 RK_PA1 2 &pcfg_pull_up_8ma>,
					<1 RK_PA2 2 &pcfg_pull_up_8ma>,
					<1 RK_PA3 2 &pcfg_pull_up_8ma>,
					<1 RK_PA4 2 &pcfg_pull_up_8ma>,
					<1 RK_PA5 2 &pcfg_pull_up_8ma>,
					<1 RK_PA6 2 &pcfg_pull_up_8ma>,
					<1 RK_PA7 2 &pcfg_pull_up_8ma>;
			};
		};

		flash {
			flash_cs0: flash-cs0 {
				rockchip,pins =
					<1 RK_PB0 1 &pcfg_pull_none>;
			};

			flash_rdy: flash-rdy {
				rockchip,pins =
					<1 RK_PB1 1 &pcfg_pull_none>;
			};

			flash_dqs: flash-dqs {
				rockchip,pins =
					<1 RK_PB2 1 &pcfg_pull_none>;
			};

			flash_ale: flash-ale {
				rockchip,pins =
					<1 RK_PB3 1 &pcfg_pull_none>;
			};

			flash_cle: flash-cle {
				rockchip,pins =
					<1 RK_PB4 1 &pcfg_pull_none>;
			};

			flash_wrn: flash-wrn {
				rockchip,pins =
					<1 RK_PB5 1 &pcfg_pull_none>;
			};

			flash_csl: flash-csl {
				rockchip,pins =
					<1 RK_PB6 1 &pcfg_pull_none>;
			};

			flash_rdn: flash-rdn {
				rockchip,pins =
					<1 RK_PB7 1 &pcfg_pull_none>;
			};

			flash_bus8: flash-bus8 {
				rockchip,pins =
					<1 RK_PA0 1 &pcfg_pull_up_12ma>,
					<1 RK_PA1 1 &pcfg_pull_up_12ma>,
					<1 RK_PA2 1 &pcfg_pull_up_12ma>,
					<1 RK_PA3 1 &pcfg_pull_up_12ma>,
					<1 RK_PA4 1 &pcfg_pull_up_12ma>,
					<1 RK_PA5 1 &pcfg_pull_up_12ma>,
					<1 RK_PA6 1 &pcfg_pull_up_12ma>,
					<1 RK_PA7 1 &pcfg_pull_up_12ma>;
			};
		};

		lcdc {
			lcdc_m0_rgb_pins: lcdc-m0-rgb-pins {
				rockchip,pins =
					<3 RK_PA0 1 &pcfg_pull_none_8ma>,	/* LCDC_DCLK */
					<3 RK_PA1 1 &pcfg_pull_none_8ma>,	/* LCDC_HSYNC */
					<3 RK_PA2 1 &pcfg_pull_none_8ma>,	/* LCDC_VSYNC */
					<3 RK_PA3 1 &pcfg_pull_none_8ma>,	/* LCDC_DEN */
					<3 RK_PA4 1 &pcfg_pull_none_8ma>,	/* LCDC_D0 */
					<3 RK_PA5 1 &pcfg_pull_none_8ma>,	/* LCDC_D1 */
					<3 RK_PA6 1 &pcfg_pull_none_8ma>,	/* LCDC_D2 */
					<3 RK_PA7 1 &pcfg_pull_none_8ma>,	/* LCDC_D3 */
					<3 RK_PB0 1 &pcfg_pull_none_8ma>,	/* LCDC_D4 */
					<3 RK_PB1 1 &pcfg_pull_none_8ma>,	/* LCDC_D5 */
					<3 RK_PB2 1 &pcfg_pull_none_8ma>,	/* LCDC_D6 */
					<3 RK_PB3 1 &pcfg_pull_none_8ma>,	/* LCDC_D7 */
					<3 RK_PB4 1 &pcfg_pull_none_8ma>,	/* LCDC_D8 */
					<3 RK_PB5 1 &pcfg_pull_none_8ma>,	/* LCDC_D9 */
					<3 RK_PB6 1 &pcfg_pull_none_8ma>,	/* LCDC_D10 */
					<3 RK_PB7 1 &pcfg_pull_none_8ma>,	/* LCDC_D11 */
					<3 RK_PC0 1 &pcfg_pull_none_8ma>,	/* LCDC_D12 */
					<3 RK_PC1 1 &pcfg_pull_none_8ma>,	/* LCDC_D13 */
					<3 RK_PC2 1 &pcfg_pull_none_8ma>,	/* LCDC_D14 */
					<3 RK_PC3 1 &pcfg_pull_none_8ma>,	/* LCDC_D15 */
					<3 RK_PC4 1 &pcfg_pull_none_8ma>,	/* LCDC_D16 */
					<3 RK_PC5 1 &pcfg_pull_none_8ma>,	/* LCDC_D17 */
					<3 RK_PC6 1 &pcfg_pull_none_8ma>,	/* LCDC_D18 */
					<3 RK_PC7 1 &pcfg_pull_none_8ma>,	/* LCDC_D19 */
					<3 RK_PD0 1 &pcfg_pull_none_8ma>,	/* LCDC_D20 */
					<3 RK_PD1 1 &pcfg_pull_none_8ma>,	/* LCDC_D21 */
					<3 RK_PD2 1 &pcfg_pull_none_8ma>,	/* LCDC_D22 */
					<3 RK_PD3 1 &pcfg_pull_none_8ma>;	/* LCDC_D23 */
			};

			lcdc_m0_sleep_pins: lcdc-m0-sleep-pins {
				rockchip,pins =
					<3 RK_PA0 RK_FUNC_GPIO &pcfg_pull_none>,	/* LCDC_DCLK */
					<3 RK_PA1 RK_FUNC_GPIO &pcfg_pull_none>,	/* LCDC_HSYNC */
					<3 RK_PA2 RK_FUNC_GPIO &pcfg_pull_none>,	/* LCDC_VSYNC */
					<3 RK_PA3 RK_FUNC_GPIO &pcfg_pull_none>,	/* LCDC_DEN */
					<3 RK_PA4 RK_FUNC_GPIO &pcfg_pull_none>,	/* LCDC_D0 */
					<3 RK_PA5 RK_FUNC_GPIO &pcfg_pull_none>,	/* LCDC_D1 */
					<3 RK_PA6 RK_FUNC_GPIO &pcfg_pull_none>,	/* LCDC_D2 */
					<3 RK_PA7 RK_FUNC_GPIO &pcfg_pull_none>,	/* LCDC_D3 */
					<3 RK_PB0 RK_FUNC_GPIO &pcfg_pull_none>,	/* LCDC_D4 */
					<3 RK_PB1 RK_FUNC_GPIO &pcfg_pull_none>,	/* LCDC_D5 */
					<3 RK_PB2 RK_FUNC_GPIO &pcfg_pull_none>,	/* LCDC_D6 */
					<3 RK_PB3 RK_FUNC_GPIO &pcfg_pull_none>,	/* LCDC_D7 */
					<3 RK_PB4 RK_FUNC_GPIO &pcfg_pull_none>,	/* LCDC_D8 */
					<3 RK_PB5 RK_FUNC_GPIO &pcfg_pull_none>,	/* LCDC_D9 */
					<3 RK_PB6 RK_FUNC_GPIO &pcfg_pull_none>,	/* LCDC_D10 */
					<3 RK_PB7 RK_FUNC_GPIO &pcfg_pull_none>,	/* LCDC_D11 */
					<3 RK_PC0 RK_FUNC_GPIO &pcfg_pull_none>,	/* LCDC_D12 */
					<3 RK_PC1 RK_FUNC_GPIO &pcfg_pull_none>,	/* LCDC_D13 */
					<3 RK_PC2 RK_FUNC_GPIO &pcfg_pull_none>,	/* LCDC_D14 */
					<3 RK_PC3 RK_FUNC_GPIO &pcfg_pull_none>,	/* LCDC_D15 */
					<3 RK_PC4 RK_FUNC_GPIO &pcfg_pull_none>,	/* LCDC_D16 */
					<3 RK_PC5 RK_FUNC_GPIO &pcfg_pull_none>,	/* LCDC_D17 */
					<3 RK_PC6 RK_FUNC_GPIO &pcfg_pull_none>,	/* LCDC_D18 */
					<3 RK_PC7 RK_FUNC_GPIO &pcfg_pull_none>,	/* LCDC_D19 */
					<3 RK_PD0 RK_FUNC_GPIO &pcfg_pull_none>,	/* LCDC_D20 */
					<3 RK_PD1 RK_FUNC_GPIO &pcfg_pull_none>,	/* LCDC_D21 */
					<3 RK_PD2 RK_FUNC_GPIO &pcfg_pull_none>,	/* LCDC_D22 */
					<3 RK_PD3 RK_FUNC_GPIO &pcfg_pull_none>;	/* LCDC_D23 */
			};
		};

		pwm0 {
			pwm0_pin: pwm0-pin {
				rockchip,pins =
					<0 RK_PB7 1 &pcfg_pull_none>;
			};
		};

		pwm1 {
			pwm1_pin: pwm1-pin {
				rockchip,pins =
					<0 RK_PC0 1 &pcfg_pull_none>;
			};
		};

		pwm2 {
			pwm2_pin: pwm2-pin {
				rockchip,pins =
					<2 RK_PB5 1 &pcfg_pull_none>;
			};
		};

		pwm3 {
			pwm3_pin: pwm3-pin {
				rockchip,pins =
					<0 RK_PC1 1 &pcfg_pull_none>;
			};
		};

		pwm4 {
			pwm4_pin: pwm4-pin {
				rockchip,pins =
					<3 RK_PC2 3 &pcfg_pull_none>;
			};
		};

		pwm5 {
			pwm5_pin: pwm5-pin {
				rockchip,pins =
					<3 RK_PC3 3 &pcfg_pull_none>;
			};
		};

		pwm6 {
			pwm6_pin: pwm6-pin {
				rockchip,pins =
					<3 RK_PC4 3 &pcfg_pull_none>;
			};
		};

		pwm7 {
			pwm7_pin: pwm7-pin {
				rockchip,pins =
					<3 RK_PC5 3 &pcfg_pull_none>;
			};
		};

		gmac {
			rmii_pins: rmii-pins {
				rockchip,pins =
					<2 RK_PA0 2 &pcfg_pull_none_12ma>, /* mac_txen */
					<2 RK_PA1 2 &pcfg_pull_none_12ma>, /* mac_txd1 */
					<2 RK_PA2 2 &pcfg_pull_none_12ma>, /* mac_txd0 */
					<2 RK_PA3 2 &pcfg_pull_none>, /* mac_rxd0 */
					<2 RK_PA4 2 &pcfg_pull_none>, /* mac_rxd1 */
					<2 RK_PA5 2 &pcfg_pull_none>, /* mac_rxer */
					<2 RK_PA6 2 &pcfg_pull_none>, /* mac_rxdv */
					<2 RK_PA7 2 &pcfg_pull_none>, /* mac_mdio */
					<2 RK_PB1 2 &pcfg_pull_none>; /* mac_mdc */
			};

			mac_refclk_12ma: mac-refclk-12ma {
				rockchip,pins =
					<2 RK_PB2 2 &pcfg_pull_none_12ma>;
			};

			mac_refclk: mac-refclk {
				rockchip,pins =
					<2 RK_PB2 2 &pcfg_pull_none>;
			};
		};

		cif-m0 {
			cif_clkout_m0: cif-clkout-m0 {
				rockchip,pins =
					<2 RK_PB3 1 &pcfg_pull_none_12ma>;/* cif_clkout */
			};

			dvp_d2d9_m0: dvp-d2d9-m0 {
				rockchip,pins =
					<2 RK_PA0 1 &pcfg_pull_none>, /* cif_data2 */
					<2 RK_PA1 1 &pcfg_pull_none>, /* cif_data3 */
					<2 RK_PA2 1 &pcfg_pull_none>, /* cif_data4 */
					<2 RK_PA3 1 &pcfg_pull_none>, /* cif_data5 */
					<2 RK_PA4 1 &pcfg_pull_none>, /* cif_data6 */
					<2 RK_PA5 1 &pcfg_pull_none>, /* cif_data7 */
					<2 RK_PA6 1 &pcfg_pull_none>, /* cif_data8 */
					<2 RK_PA7 1 &pcfg_pull_none>, /* cif_data9 */
					<2 RK_PB0 1 &pcfg_pull_none>, /* cif_sync */
					<2 RK_PB1 1 &pcfg_pull_none>, /* cif_href */
					<2 RK_PB2 1 &pcfg_pull_none>, /* cif_clkin */
					<2 RK_PB3 1 &pcfg_pull_none>; /* cif_clkout */
			};

			dvp_d0d1_m0: dvp-d0d1-m0 {
				rockchip,pins =
					<2 RK_PB4 1 &pcfg_pull_none>, /* cif_data0 */
					<2 RK_PB6 1 &pcfg_pull_none>; /* cif_data1 */
			};

			dvp_d10d11_m0:d10-d11-m0 {
				rockchip,pins =
					<2 RK_PB7 1 &pcfg_pull_none>, /* cif_data10 */
					<2 RK_PC0 1 &pcfg_pull_none>; /* cif_data11 */
			};
		};

		cif-m1 {
			cif_clkout_m1: cif-clkout-m1 {
				rockchip,pins =
					<3 RK_PD0 3 &pcfg_pull_none>;
			};

			dvp_d2d9_m1: dvp-d2d9-m1 {
				rockchip,pins =
					<3 RK_PA3 3 &pcfg_pull_none>, /* cif_data2 */
					<3 RK_PA5 3 &pcfg_pull_none>, /* cif_data3 */
					<3 RK_PA7 3 &pcfg_pull_none>, /* cif_data4 */
					<3 RK_PB0 3 &pcfg_pull_none>, /* cif_data5 */
					<3 RK_PB1 3 &pcfg_pull_none>, /* cif_data6 */
					<3 RK_PB4 3 &pcfg_pull_none>, /* cif_data7 */
					<3 RK_PB6 3 &pcfg_pull_none>, /* cif_data8 */
					<3 RK_PB7 3 &pcfg_pull_none>, /* cif_data9 */
					<3 RK_PD1 3 &pcfg_pull_none>, /* cif_sync */
					<3 RK_PD2 3 &pcfg_pull_none>, /* cif_href */
					<3 RK_PD3 3 &pcfg_pull_none>, /* cif_clkin */
					<3 RK_PD0 3 &pcfg_pull_none>; /* cif_clkout */
			};

			dvp_d0d1_m1: dvp-d0d1-m1 {
				rockchip,pins =
					<3 RK_PA1 3 &pcfg_pull_none>, /* cif_data0 */
					<3 RK_PA2 3 &pcfg_pull_none>; /* cif_data1 */
			};

			dvp_d10d11_m1:d10-d11-m1 {
				rockchip,pins =
					<3 RK_PC6 3 &pcfg_pull_none>, /* cif_data10 */
					<3 RK_PC7 3 &pcfg_pull_none>; /* cif_data11 */
			};
		};

		isp {
			isp_prelight: isp-prelight {
				rockchip,pins =
					<3 RK_PD1 4 &pcfg_pull_none>;
			};
		};
	};
};
#include "px30s-pinctrl.dtsi"
