// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Copyright (c) 2022 Rockchip Electronics Co., Ltd.
 *
 */

/dts-v1/;
#include <dt-bindings/pwm/pwm.h>
#include "rk3368.dtsi"
#include "rk3368-android.dtsi"

/ {
	model = "Rockchip Sheep board";
	compatible = "rockchip,sheep", "rockchip,rk3368";

	sound {
		compatible = "simple-audio-card";
		simple-audio-card,format = "i2s";
		simple-audio-card,name = "rockchip,rt5640-codec";
		simple-audio-card,mclk-fs = <256>;
		simple-audio-card,widgets =
			"Microphone", "Mic Jack",
			"Headphone", "Headphone Jack";
		simple-audio-card,routing =
			"Mic Jack", "MICBIAS1",
			"IN1P", "Mic Jack",
			"Headphone Jack", "HPOL",
			"Headphone Jack", "HPOR";
		simple-audio-card,cpu {
			sound-dai = <&i2s_8ch>;
		};
		simple-audio-card,codec {
			sound-dai = <&rt5640>;
		};
	};

	backlight: backlight {
		compatible = "pwm-backlight";
		pwms = <&pwm0 0 25000 PWM_POLARITY_INVERTED>;
		brightness-levels = <
			135 135 136 136 137 137 138 138
			139 139 140 140 141 141 142 142
			143 143 143 144 144 145 145 146
			146 147 147 148 148 149 149 150
			150 151 151 151 152 152 153 153
			154 154 155 155 156 156 157 157
			158 158 159 159 159 160 160 161
			161 162 162 163 163 164 164 165
			165 166 166 167 167 167 168 168
			169 169 170 170 171 171 172 172
			173 173 174 174 175 175 175 176
			176 177 177 178 178 179 179 180
			180 181 181 182 182 183 183 183
			184 184 185 185 186 186 187 187
			188 188 189 189 190 190 191 191
			191 192 192 193 193 194 194 195
			195 196 196 197 197 198 198 199
			199 199 200 200 201 201 202 202
			203 203 204 204 205 205 206 206
			207 207 207 208 208 209 209 210
			210 211 211 212 212 213 213 214
			214 215 215 215 216 216 217 217
			218 218 219 219 220 220 221 221
			222 222 223 223 223 224 224 225
			225 226 226 227 227 228 228 229
			229 230 230 231 231 231 232 232
			233 233 234 234 235 235 236 236
			237 237 238 238 239 239 239 240
			240 241 241 242 242 243 243 244
			244 245 245 246 246 247 247 247
			248 248 249 249 250 250 251 251
			252 252 253 253 254 254 255 255>;
		default-brightness-level = <200>;
		enable-gpios = <&gpio0 20 GPIO_ACTIVE_HIGH>;
	};

	rk_key: rockchip-key {
		compatible = "rockchip,key";
		status = "okay";

		io-channels = <&saradc 1>;

		vol-up-key {
			linux,code = <115>;
			label = "volume up";
			rockchip,adc_value = <1>;
		};

		vol-down-key {
			linux,code = <114>;
			label = "volume down";
			rockchip,adc_value = <170>;
		};

		power-key {
			gpios = <&gpio0 2 GPIO_ACTIVE_LOW>;
			linux,code = <116>;
			label = "power";
			gpio-key,wakeup;
		};

		menu-key {
			linux,code = <59>;
			label = "menu";
			rockchip,adc_value = <355>;
		};

		home-key {
			linux,code = <102>;
			label = "home";
			rockchip,adc_value = <746>;
		};

		back-key {
			linux,code = <158>;
			label = "back";
			rockchip,adc_value = <560>;
		};

		camera-key {
			linux,code = <212>;
			label = "camera";
			rockchip,adc_value = <450>;
		};
	};

	vcc_sys: vcc-sys {
		compatible = "regulator-fixed";
		regulator-name = "vcc_sys";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <3800000>;
		regulator-max-microvolt = <3800000>;
	};

	vcc_host: vcc-host {
		compatible = "regulator-fixed";
		enable-active-high;
		gpio = <&gpio0 4 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&host_vbus_drv>;
		regulator-name = "vcc_host";
		regulator-always-on;
	};

	vcc_otg_vbus: otg-vbus-regulator {
		compatible = "regulator-fixed";
		gpio = <&gpio0 RK_PD1 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&otg_vbus_drv>;
		regulator-name = "vcc_otg_vbus";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		enable-active-high;
	};

	xin32k: xin32k {
		compatible = "fixed-clock";
		clock-frequency = <32768>;
		clock-output-names = "xin32k";
		#clock-cells = <0>;
	};
};

&firmware_android {
	compatible = "android,firmware";
	fstab {
		compatible = "android,fstab";
		system {
			compatible = "android,system";
			dev = "/dev/block/by-name/system";
			type = "ext4";
			mnt_flags = "ro,barrier=1,inode_readahead_blks=8";
			fsmgr_flags = "wait,verify";
		};
		vendor {
			compatible = "android,vendor";
			dev = "/dev/block/by-name/vendor";
			type = "ext4";
			mnt_flags = "ro,barrier=1,inode_readahead_blks=8";
			fsmgr_flags = "wait,verify";
		};
	};
};

&emmc {
	status = "okay";
	bus-width = <8>;
	cap-mmc-highspeed;
	mmc-hs200-1_8v;
	no-sdio;
	no-sd;
	disable-wp;
	non-removable;
	num-slots = <1>;
	pinctrl-names = "default";
	pinctrl-0 = <&emmc_clk &emmc_cmd &emmc_bus8>;
};

&sdmmc {
	status = "okay";
	clock-frequency = <37500000>;
	clock-freq-min-max = <400000 37500000>;
	no-sdio;
	no-mmc;
	cap-mmc-highspeed;
	cap-sd-highspeed;
	card-detect-delay = <200>;
	disable-wp;
	num-slots = <1>;
	pinctrl-names = "default";
	pinctrl-0 = <&sdmmc_clk &sdmmc_cmd &sdmmc_cd &sdmmc_bus4>;
};

&i2c0 {
	status = "okay";

	syr827: syr827@40 {
		compatible = "silergy,syr827";
		reg = <0x40>;
		status = "okay";

		regulator-compatible = "fan53555-reg";
		regulator-name = "vdd_arm";
		regulator-min-microvolt = <712500>;
		regulator-max-microvolt = <1500000>;
		regulator-ramp-delay = <1000>;
		fcs,suspend-voltage-selector = <1>;
		pinctrl-0 = <&vsel_gpio>;
		vsel-gpios = <&gpio0 0 GPIO_ACTIVE_HIGH>;
		regulator-always-on;
		regulator-boot-on;
		regulator-initial-state = <3>;
		regulator-state-mem {
			regulator-off-in-suspend;
			regulator-suspend-microvolt = <900000>;
		};
	};

	rk818: pmic@1c {
		compatible = "rockchip,rk818";
		reg = <0x1c>;
		status = "okay";

		clock-output-names = "rk818-clkout1", "wifibt_32kin";
		interrupt-parent = <&gpio0>;
		interrupts = <1 IRQ_TYPE_LEVEL_LOW>;
		pinctrl-names = "default";
		pinctrl-0 = <&pmic_int_l>;
		rockchip,system-power-controller;
		wakeup-source;
		#clock-cells = <1>;

		vcc1-supply = <&vcc_sys>;
		vcc2-supply = <&vcc_sys>;
		vcc3-supply = <&vcc_sys>;
		vcc4-supply = <&vcc_sys>;
		vcc6-supply = <&vcc_sys>;
		vcc7-supply = <&vcc_sys>;
		vcc8-supply = <&vcc_sys>;
		vcc9-supply = <&vcc_io>;

		regulators {
			vdd_logic: DCDC_REG1 {
				regulator-name = "vdd_logic";
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <750000>;
				regulator-max-microvolt = <1450000>;
				regulator-ramp-delay = <6001>;
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1000000>;
				};
			};

			vdd_gpu: DCDC_REG2 {
				regulator-name = "vdd_gpu";
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <800000>;
				regulator-max-microvolt = <1250000>;
				regulator-ramp-delay = <6001>;
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1000000>;
				};
			};

			vcc_ddr: DCDC_REG3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vcc_ddr";
				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};

			vcc_io: DCDC_REG4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vcc_io";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vcca_codec: LDO_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vcca_codec";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vcc_tp: LDO_REG2 {
				regulator-boot-on;
				regulator-min-microvolt = <3000000>;
				regulator-max-microvolt = <3000000>;
				regulator-name = "vcc_tp";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd_10: LDO_REG3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <1000000>;
				regulator-name = "vdd_10";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1000000>;
				};
			};

			vcc18_lcd: LDO_REG4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc18_lcd";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vccio_pmu: LDO_REG5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vccio_pmu";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vdd10_lcd: LDO_REG6 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <1000000>;
				regulator-name = "vdd10_lcd";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1000000>;
				};
			};

			vcc_18: LDO_REG7 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc_18";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vccio_wl: LDO_REG8 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vccio_wl";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vccio_sd: LDO_REG9 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vccio_sd";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vcc_sd: SWITCH_REG {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vcc_sd";
				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};

			boost_otg: DCDC_BOOST {
				regulator-name = "boost_otg";
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <5000000>;
				regulator-max-microvolt = <5000000>;
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <5000000>;
				};
			};
		};

		battery {
			compatible = "rk818-battery";
			pinctrl-names = "default";
			pinctrl-0 = <&dc_irq_gpio>;
			ocv_table = <
				3400 3650 3693 3707 3731 3749 3760
				3770 3782 3796 3812 3829 3852 3882
				3915 3951 3981 4047 4086 4132 4182>;
			design_capacity = <8650>;
			design_qmax = <8800>;
			bat_res = <85>;
			max_input_current = <2000>;
			max_chrg_current = <1800>;
			max_chrg_voltage = <4200>;
			sleep_enter_current = <600>;
			sleep_exit_current = <600>;
			power_off_thresd = <3400>;
			zero_algorithm_vol = <3850>;
			fb_temperature = <115>;
			sample_res = <10>;
			max_soc_offset = <60>;
			energy_mode = <0>;
			monitor_sec = <5>;
			virtual_power = <0>;
			power_dc2otg = <1>;
			support_usb_adp = <1>;
			support_dc_adp = <1>;
			dc_det_gpio = <&gpio0 17 GPIO_ACTIVE_LOW>;
		};
	};
};

&cpu_l0 {
	cpu-supply = <&syr827>;
};

&cpu_l1 {
	cpu-supply = <&syr827>;
};

&cpu_l2 {
	cpu-supply = <&syr827>;
};

&cpu_l3 {
	cpu-supply = <&syr827>;
};

&cpu_b0 {
	cpu-supply = <&syr827>;
};

&cpu_b1 {
	cpu-supply = <&syr827>;
};

&cpu_b2 {
	cpu-supply = <&syr827>;
};

&cpu_b3 {
	cpu-supply = <&syr827>;
};

&dfi {
	status = "okay";
};

&dmc {
	center-supply = <&vdd_logic>;
	status = "okay";
};

&gpu {
	logic-supply = <&vdd_logic>;
};

&rockchip_suspend {
	status = "okay";
};

&i2c1 {
	status = "okay";

	rt5640: rt5640@1c {
		compatible = "realtek,rt5640";
		reg = <0x1c>;
		#sound-dai-cells = <0>;
		clocks = <&cru SCLK_I2S_8CH_OUT>;
		clock-names = "mclk";
		pinctrl-names = "default";
		pinctrl-0 = <&i2s_8ch_mclk>;
		realtek,in1-differential;
		status = "okay";
	};
};

&i2c2 {
	status = "okay";

	gt9xx: gt9xx@14 {
		compatible = "goodix,gt9xx";
		reg = <0x14>;
		touch-gpio = <&gpio0 12 IRQ_TYPE_LEVEL_LOW>;
		reset-gpio = <&gpio0 11 GPIO_ACTIVE_HIGH>;
		max-x = <1200>;
		max-y = <1900>;
		tp-size = <911>;
		tp-supply = <&vcc_tp>;
		status = "okay";
	};
};

&i2s_8ch {
	status = "okay";
	rockchip,i2s-broken-burst-len;
	rockchip,playback-channels = <8>;
	rockchip,capture-channels = <2>;
	#sound-dai-cells = <0>;
};

&io_domains {
	status = "okay";
	dvp-supply = <&vcc_18>;
	audio-supply = <&vcc_io>;
	gpio30-supply = <&vcc_io>;
	gpio1830-supply = <&vcc_io>;
	sdcard-supply = <&vccio_sd>;
	wifi-supply = <&vccio_wl>;
};

&pmu_io_domains {
	status = "okay";

	pmu-supply = <&vcc_io>;
	vop-supply = <&vcc_io>;
};

&pwm0 {
	status = "okay";
};

&u2phy {
	status = "okay";

	u2phy_host: host-port {
		phy-supply = <&vcc_host>;
		status = "okay";
	};

	u2phy_otg: otg-port {
		vbus-supply = <&vcc_otg_vbus>;
		status = "okay";
	};
};

&usb_host0_ehci {
	status = "okay";
};

&usb_host0_ohci {
	status = "okay";
};

&mailbox {
	status = "okay";
};

&mailbox_scpi {
	status = "okay";
};

&dsi {
	status = "okay";

	panel@0 {
		compatible = "simple-panel-dsi";
		reg = <0>;
		backlight = <&backlight>;
		enable-gpios = <&gpio0 22 GPIO_ACTIVE_HIGH>;
		prepare-delay-ms = <120>;

		dsi,flags = <(MIPI_DSI_MODE_VIDEO | MIPI_DSI_MODE_VIDEO_BURST |
			      MIPI_DSI_MODE_LPM | MIPI_DSI_MODE_EOT_PACKET)>;
		dsi,format = <MIPI_DSI_FMT_RGB888>;
		dsi,lanes = <4>;

		display-timings {
			native-mode = <&timing0>;

			timing0: timing0 {
				clock-frequency = <150000000>;
				hactive = <1200>;
				vactive = <1920>;
				hback-porch = <80>;
				hfront-porch = <81>;
				vback-porch = <21>;
				vfront-porch = <21>;
				hsync-len = <10>;
				vsync-len = <3>;
				hsync-active = <0>;
				vsync-active = <0>;
				de-active = <0>;
				pixelclk-active = <0>;
			};
		};

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				panel_in_dsi: endpoint {
					remote-endpoint = <&dsi_out_panel>;
				};
			};
		};
	};

	ports {
		#address-cells = <1>;
		#size-cells = <0>;

		port@1 {
			reg = <1>;
			dsi_out_panel: endpoint {
				remote-endpoint = <&panel_in_dsi>;
			};
		};
	};
};

&route_dsi {
	status = "okay";
};

&saradc {
	status = "okay";
};

&tsadc {
	tsadc-supply = <&syr827>;
	status = "okay";
};

&pinctrl {
	pmic {
		pmic_int_l: pmic-int-l {
			rockchip,pins = <0 RK_PA1 RK_FUNC_GPIO &pcfg_pull_up>;
		};
		vsel_gpio: vsel-gpio {
			rockchip,pins = <0 RK_PA0 RK_FUNC_GPIO &pcfg_pull_down>;
		};
	};

	dc_det {
		dc_irq_gpio: dc-irq-gpio {
			rockchip,pins = <0 RK_PC1 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	usb2 {
		host_vbus_drv: host-vbus-drv {
			rockchip,pins = <0 RK_PA4 RK_FUNC_GPIO &pcfg_pull_none>;
		};

		otg_vbus_drv: otg-bus-drv {
			rockchip,pins = <0 RK_PD1 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};
};
