#include "rp-lcd-hdmi.dtsi"
#define RP_SINGLE_LCD
#define RP_EDP_USED


&edp_panel {
    status = "okay";
        compatible = "simple-panel";
        prepare-delay-ms = <20>;
        enable-delay-ms = <20>;
        disable-delay-ms = <20>;
        unprepare-delay-ms = <20>;
    
        /**
         * power-supply = <>;
         * reset-gpios = <>;
         *
         * lcd reset pin and power supply
         * please refer to ***-lcd-gpio.dtsi
         * that included in main dts.
         */
         
        display-timings {
                native-mode = <&timing0>;

                timing0: timing0 {//EDP 15.6
                        clock-frequency = <150000000>;
                        hactive = <1920>;
                        vactive = <1080>;
                        hfront-porch = <160>;
                        hsync-len = <32>;
                        hback-porch = <160>;
                        vfront-porch = <3>;
                        vsync-len = <5>;
                        vback-porch = <23>;
                        hsync-active = <0>;
                        vsync-active = <0>;
                        de-active = <0>;
                        pixelclk-active = <0>;
                };

                timing1: timing1 {// EDP 13.3 
                        clock-frequency = <138000000>;
                        hactive = <1920>;
                        vactive = <1080>;
                        hfront-porch = <48>;
                        hsync-len = <32>;
                        hback-porch = <80>;
                        vfront-porch = <3>;
                        vsync-len = <5>;
                        vback-porch = <23>;
                        hsync-active = <0>;
                        vsync-active = <0>;
                        de-active = <0>;
                        pixelclk-active = <0>;
                };
        };

        ports {
                    panel_in_edp: endpoint {
                            remote-endpoint = <&edp_out_panel>;
            };
    };
};



&edp {
    status = "okay";
    force-hpd;
        ports {
                port@1 {
                        reg = <1>;

                        edp_out_panel: endpoint {
                                remote-endpoint = <&panel_in_edp>;
                        };
                };
        };
};

&edp_phy {
    status = "okay";
};

&edp_in_vp0 {
    status = "okay";
};

&edp_in_vp1 {
    status = "disabled";
};

&hdmi_in_vp0 {
    status = "disabled";
};
&hdmi_in_vp1 {
    status = "okay";
};

&route_edp {
    status = "okay";
    connect = <&vp0_out_edp>;
};



&gt9xx {
    status = "okay";
    compatible = "goodix,gt9xx";
    reg = <0x5d>;
    gtp_resolution_x = <1920>;
    gtp_resolution_y = <1080>;
    gtp_int_tarigger = <1>;
    gtp_change_x2y = <0>;
    gtp_overturn_x = <0>;
    gtp_overturn_y = <0>;
    gtp_send_cfg = <1>;
    gtp_touch_wakeup = <1>;

    /**
     * goodix_rst_gpio = <>;
     * goodix_irq_gpio = <>;
     *
     * touch panel interrupt and reset pin
     * please refer to ***-lcd-gpio.dtsi
     * that included in main dts.
     */

    goodix,cfg-group0 = [
        64 80 07 38 04 0A 3D 00 01 C8 28 0F
        55 37 03 05 00 00 00 00 00 00 00 18
        1A 1E 14 90 30 AA 25 27 0F 0A 00 00
        00 5A 03 11 00 00 00 00 00 00 00 00
        00 25 00 19 37 94 D5 02 08 14 00 04
        9B 1B 00 8E 1F 00 80 25 00 76 2B 00
        6E 32 00 6E 00 00 00 00 00 00 00 00
        00 00 00 00 00 00 00 00 00 00 00 00
        00 00 00 00 00 00 00 10 00 00 00 00
        00 00 00 00 19 18 17 16 15 14 11 10
        0F 0E 0D 0C 09 08 07 06 05 04 01 00
        00 00 00 00 00 00 00 00 00 00 00 02
        04 06 07 08 0A 0C 0D 0E 0F 10 11 12
        13 14 19 1B 1C 1E 1F 20 21 22 23 24
        25 26 27 28 29 2A 00 00 00 00 00 00
        00 00 00 00 B7 01
    ];
};
