/* board base */
//#include "../rk3588-evb4-lp4-v10-linux.dts"
#include "rp-rk3588-board.dtsi"

#include "rp-tp-i2c6-gt911.dtsi"
#include "rd-rk3588-lcd-gpio.dtsi"
#include "rpdzkj_config.dtsi"

/* usb */
#include "rp-usb-typea-rk3588.dtsi"
#include "rp-usb-host.dtsi"

/* ethernet */
#include "rp-eth-pcie2gmac-rk3588.dtsi"
#include "rp-eth-gmac1.dtsi"

/* pcie */
#include "rp-pcie-power-rk3588.dtsi"
#include "rp-pcie-m2.dtsi"

/* audio */
#include "rp-audio-es8311.dtsi"

/* wifi/bt */
#include "rp-wifi-bt-ap6275p-rk3588.dtsi"

/* hdmi rx */
#include "rp-hdmirx.dtsi"

/* camera */
//#include "rp-camera-dual-ov13855.dtsi"


//#include "rp-lcd-hdmi0.dtsi"        //batch ignore
//#include "rp-lcd-hdmi1.dtsi"          //batch ignore
#include "rp-lcd-multi-hdmi0-hdmi1-dp0.dtsi"

/* lcd */
//#include "rp-lcd-mipi0-5-720-1280-v2-boxTP.dtsi"
//#include "rp-lcd-mipi0-7-720-1280.dtsi"
//#include "rp-lcd-mipi0-8-800-1280-v3.dtsi"
//#include "rp-lcd-mipi0-8-1200-1920.dtsi"
//#include "rp-lcd-mipi0-10-800-1280-v3.dtsi"
//#include "rp-lcd-mipi0-10-1200-1920.dtsi"
//#include "rp-lcd-mipi0-10-1920-1200-jc.dtsi"
//#include "rp-lcd-mipi1-gm8775-lvds-10.1-1024-600.dtsi"
//#include "rp-lcd-mipi1-gm8775-lvds-21-1920-1080.dtsi"

/* quadplex lcd */
//#include "rp-lcd-quadplex-mipi0-5-720-1280-v2-boxTP-mipi1-gm8775-lvds-10.1-1024-600-hdmi0-hdmi1.dtsi"

/ {
    model = "nano-rk3588";
    compatible = "rpdzkj,nano-rk3588", "rockchip,rk3588";

    reserved-memory {
        #address-cells = <2>;
        #size-cells = <2>;
        ranges;
        dma_trans: dma-trans@3c000000 {
            reg = <0x0 0x3c000000 0x0 0x04000000>;
        };
    };

    vcc_1v1_nldo_s3: vcc-1v1-nldo-s3 {
        compatible = "regulator-fixed";
        regulator-name = "vcc_1v1_nldo_s3";
        regulator-always-on;
        regulator-boot-on;
        regulator-min-microvolt = <1100000>;
        regulator-max-microvolt = <1100000>;
        vin-supply = <&vcc5v0_sys>;
    };


    vdd_3v3_5v_control: vdd_3v3_5v_control {
                compatible = "regulator-fixed";
                regulator-name = "vdd_3v3_5v_control";
        regulator-always-on;
                regulator-boot-on;
                regulator-min-microvolt = <3300000>;
                regulator-max-microvolt = <3300000>;
                enable-active-high;
        gpio = <&gpio4 RK_PA5 GPIO_ACTIVE_HIGH>;    //In the uboot phase fixed.c resolves gpio
                gpios = <&gpio4 RK_PA5 GPIO_ACTIVE_HIGH>;
        pinctrl-names = "default";
        pinctrl-0 = <&vdd_control>;         
        };

	fan_gpio_control {
            compatible = "fan_gpio_control";
            gpio-pin = <&gpio4 RK_PA7 GPIO_ACTIVE_HIGH>;
            thermal-zone = "soc-thermal";
            threshold-temp = <60000>; //60C
            running-time = <10000>; //10s
            status = "okay";
        };
	

        rp_power{
                status = "okay";
                compatible = "rp_power";
                rp_not_deep_sleep = <1>;

//#define GPIO_FUNCTION_OUTPUT 0
//#define GPIO_FUNCTION_INPUT 1
//#define GPIO_FUNCTION_IRQ 2
//#define GPIO_FUNCTION_FLASH 3
//#define GPIO_FUNCTION_OUTPUT_CTRL 4

                //fan {   
                //        gpio_num = <&gpio4 RK_PA7 GPIO_ACTIVE_HIGH>;
                //        gpio_function = <4>;
                //};

                led {  
                        gpio_num = <&gpio4 RK_PA6 GPIO_ACTIVE_HIGH>;
                        gpio_function = <3>;
                };

                usb-host-power {  
                        gpio_num = <&gpio2 RK_PC1 GPIO_ACTIVE_HIGH>;
                        gpio_function = <4>;
                };

                otg-power {
                      gpio_num = <&gpio1 RK_PA2 GPIO_ACTIVE_HIGH>;
                      gpio_function = <4>;
                };
 
                usb-hub-reset {  
                        gpio_num = <&gpio3 RK_PB2 GPIO_ACTIVE_HIGH>;
                        gpio_function = <4>;
                };
        
        vdd-4g {   //4g enable
            gpio_num = <&gpio3 RK_PD4 GPIO_ACTIVE_HIGH>;
            gpio_function = <4>;
        };
        
        VDD_USB2_0 {
            gpio_num = <&gpio1 RK_PB1 GPIO_ACTIVE_HIGH>;
                        gpio_function = <4>;
        };

        VDD_USB2_1 {
                        gpio_num = <&gpio1 RK_PB2 GPIO_ACTIVE_HIGH>;
                        gpio_function = <4>;
                };
        
        spk_en {       //spk enable
                        gpio_num = <&gpio4 RK_PB6 GPIO_ACTIVE_HIGH>;
                        gpio_function = <4>;
                };
                spk_mute {       //spk mute
                        gpio_num = <&gpio4 RK_PB4 GPIO_ACTIVE_LOW>;
                        gpio_function = <4>;
                };     
    };

        rp_gpio{
                status = "okay";
                compatible = "rp_gpio";

                gpio4b2 {
                  gpio_num = <&gpio4 RK_PB2 GPIO_ACTIVE_HIGH>;
                  gpio_function = <0>;
                };

                gpio4b3 {
                  gpio_num = <&gpio4 RK_PB3 GPIO_ACTIVE_HIGH>;
                  gpio_function = <0>;
                };

        vdd5v_uart {    
            gpio_num = <&gpio2 RK_PB6 GPIO_ACTIVE_HIGH>;
                        gpio_function = <0>;        
        };
        
        vdd3v3_uart {
            gpio_num = <&gpio1 RK_PC6 GPIO_ACTIVE_HIGH>;
                        gpio_function = <0>;
        };
        };
    
    stm706 {
                status = "okay";
                compatible = "stm706";
                reset_gpio = <&gpio4 RK_PB5 GPIO_ACTIVE_HIGH>;
                wdt_gpio = <&gpio0 RK_PD3 GPIO_ACTIVE_HIGH>;
        };

};

&pinctrl {
    power_control{
        vdd_control: vdd_control {
            rockchip,pins = <4 RK_PA5 RK_FUNC_GPIO &pcfg_pull_up>;
        };
    };
};

&vcc3v3_pcie30 {
    gpios = <&gpio4 RK_PA4 GPIO_ACTIVE_HIGH>;
};

&uart0 {
    status = "okay";
    pinctrl-names = "default";
    pinctrl-0 = <&uart0m0_xfer>;
};

                         

/*uart6 > RS485*/
&uart6 {
    status = "okay";
    pinctrl-names = "default";
    pinctrl-0 = <&uart6m0_xfer>;
};

&uart7 {
    status = "okay";
    pinctrl-names = "default";
    pinctrl-0 = <&uart7m1_xfer>;
};

&uart8 {
    status = "okay";
    pinctrl-names = "default";
    pinctrl-0 = <&uart8m0_xfer>;
};

&can0 {
    assigned-clocks = <&cru CLK_CAN0>;
    assigned-clock-rates = <200000000>;
    status = "okay";
    pinctrl-names = "default";
    pinctrl-0 = <&can0m0_pins>;
};

&i2c4 {
    status = "okay";
    pinctrl-names = "default";
    pinctrl-0 = <&i2c4m1_xfer>;

    hym8563: hym8563@51 {
        compatible = "haoyu,hym8563";
        reg = <0x51>;
        #clock-cells = <0>;
        clock-frequency = <32768>;
        clock-output-names = "hym8563";
        //pinctrl-names = "default";
        //pinctrl-0 = <&hym8563_int>;
        //interrupt-parent = <&gpio0>;
        //interrupts = <RK_PD4 IRQ_TYPE_LEVEL_LOW>;
        //wakeup-source;
    };

};


&i2c2 {
        status = "okay";
        pinctrl-names = "default";
        pinctrl-0 = <&i2c2m4_xfer>;
};

&i2c3 {
        status = "okay";
        pinctrl-names = "default";
        pinctrl-0 = <&i2c3m0_xfer>;
};

&sdmmc {
    status = "okay";
    //vmmc-supply = <&vccio_sd_s0>;
};

&fiq_debugger {
    rockchip,baudrate = <115200>;
};

&display_subsystem {
clocks = <&hdptxphy_hdmi_clk0>, <&hdptxphy_hdmi_clk1>;
clock-names = "hdmi0_phy_pll", "hdmi1_phy_pll";
};

&hdptxphy_hdmi_clk0 {
            status = "okay";
};

&hdptxphy_hdmi_clk1 {
            status = "okay";
};
