// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Copyright (c) 2022 Rockchip Electronics Co., Ltd.
 *
 */

/dts-v1/;
#include <dt-bindings/pinctrl/rockchip.h>
#include "rk3399.dtsi"
#include "rk3399-android.dtsi"
#include "rk3399-opp.dtsi"
#include <dt-bindings/sensor-dev.h>
#include <dt-bindings/pwm/pwm.h>

/ {
	compatible = "rockchip,rk3399-mid", "rockchip,rk3399";

	edp_panel: edp-panel {
		compatible = "auo,b125han03";
		backlight = <&backlight>;
		power-supply = <&vcc3v3_s0>;
		enable-gpios = <&gpio3 RK_PA0 GPIO_ACTIVE_HIGH>;
		bus-format = <MEDIA_BUS_FMT_RGB666_1X18>;
		bpc = <6>;
		prepare-delay-ms = <50>;
		ports {
			panel_in_edp: endpoint {
				remote-endpoint = <&edp_out_panel>;
			};
		};
	};

	usb_cam_gpio: usb-cam-gpio {
		compatible = "usb-cam-gpio";
		pinctrl-names = "default";
		pinctrl-0 = <&usb_cam_on_gpio>;
		hd-cam-gpios = <&gpio3 RK_PA1 GPIO_ACTIVE_HIGH>;
		ir-cam-gpios = <&gpio3 RK_PA2 GPIO_ACTIVE_HIGH>;
		status = "okay";
	};

	vcc_sys: vcc-sys {
		compatible = "regulator-fixed";
		regulator-name = "vcc_sys";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <3900000>;
		regulator-max-microvolt = <3900000>;
	};

	vcc3v3_sys: vcc3v3-sys {
		compatible = "regulator-fixed";
		regulator-name = "vcc3v3_sys";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
	};

	vcc5v0_host: vcc5v0-host-regulator {
		compatible = "regulator-fixed";
		enable-active-high;
		gpio = <&gpio4 25 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&host_vbus_drv>;
		regulator-name = "vcc5v0_host";
		regulator-always-on;
	};

	vdd_log: vdd-log {
		compatible = "pwm-regulator";
		pwms = <&pwm2 0 25000 1>;
		rockchip,pwm_id= <2>;
		rockchip,pwm_voltage = <900000>;
		regulator-name = "vdd_log";
		regulator-min-microvolt = <750000>;
		regulator-max-microvolt = <1350000>;
		regulator-always-on;
		regulator-boot-on;
	};

	xin32k: xin32k {
		compatible = "fixed-clock";
		clock-frequency = <32768>;
		clock-output-names = "xin32k";
		#clock-cells = <0>;
	};

	backlight: backlight {
		compatible = "pwm-backlight";
		pwms = <&pwm0 0 25000 0>;
		brightness-levels = <
			0   1   51  52  52  53  53  54
			54  55  55  56  56  57  57  58
			58  59  59  60  61  61  62  63
			63  64  65  65  66  67  67  68
			69  69  70  71  71  72  73  73
			74  75  75  76  77  77  78  79
			79  80  80  81  81  82  83  83
			84  85  86  86  87  88  89  89
			90  91  92  92  93  94  95  95
			96  97  98  98  99 100 101  101
			102 103 104 104 105 106 107 107
			108 109 110 110 111 112 113 113
			114 115 116 116 117 118 119 119
			120 121 122 122 123 124 125 125
			126 127 128 128 129 130 131 131
			132 133 134 134 135 136 137 137
			138 139 140 140 141 142 143 143
			144 145 146 146 147 148 149 149
			150 151 152 152 153 154 155 155
			156 157 158 158 159 160 161 161
			162 163 164 164 165 166 167 167
			168 169 170 170 171 172 173 173
			174 175 176 176 177 178 179 179
			180 181 182 182 183 184 185 185
			186 187 188 188 189 190 191 191
			216 217 218 218 219 220 221 221
			222 223 224 224 225 226 227 227
			228 229 230 230 231 232 233 233
			234 235 236 236 237 238 239 239
			240 241 242 242 243 244 245 245
			246 247 248 248 249 250 251 251
			252 253 254 254 255 255 255 255>;
		default-brightness-level = <200>;
		enable-gpios = <&gpio3 RK_PA4 GPIO_ACTIVE_HIGH>;
	};

	vcc_phy: vcc-phy-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vcc_phy";
		regulator-always-on;
		regulator-boot-on;
	};

	cx2072x-sound {
		compatible = "simple-audio-card";
		simple-audio-card,format = "i2s";
		simple-audio-card,name = "rockchip,cx2072x-codec";
		simple-audio-card,mclk-fs = <256>;
		simple-audio-card,widgets =
			"Microphone", "Microphone Jack",
			"Line", "Microphone Headset",
			"Headphone", "Headphone Jack",
			"Speaker", "Speaker External";
		simple-audio-card,routing =
			"PORTC", "Microphone Jack",
			"PortD Mic Bias", "Microphone Headset",
			"Headphone Jack", "PORTA",
			"Speaker External", "PORTG";
		simple-audio-card,cpu {
			sound-dai = <&i2s0>;
		};
		simple-audio-card,codec {
			sound-dai = <&cx2072x>;
		};
	};

	sound {
		compatible = "rockchip,cdndp-sound";
		rockchip,cpu = <&i2s2>;
		rockchip,codec = <&cdn_dp>;
		status = "okay";
	};

	bt-sound {
		compatible = "simple-audio-card";
		simple-audio-card,format = "dsp_b";
		simple-audio-card,bitclock-inversion;
		simple-audio-card,mclk-fs = <256>;
		simple-audio-card,name = "rockchip,bt";
		simple-audio-card,cpu {
			sound-dai = <&i2s1>;
		};
		simple-audio-card,codec {
			sound-dai = <&bt_sco>;
		};
	};

	bt_sco: bt-sco {
		compatible = "delta,dfbmcs320";
		#sound-dai-cells = <0>;
	};

	sdio_pwrseq: sdio-pwrseq {
		compatible = "mmc-pwrseq-simple";
		clocks = <&rk808 1>;
		clock-names = "ext_clock";
		pinctrl-names = "default";
		pinctrl-0 = <&wifi_enable_h>;

		/*
		 * On the module itself this is one of these (depending
		 * on the actual card populated):
		 * - SDIO_RESET_L_WL_REG_ON
		 * - PDN (power down when low)
		 */
		reset-gpios = <&gpio0 10 GPIO_ACTIVE_LOW>; /* GPIO0_B2 */
	};

	leds: gpio-leds {
		compatible = "gpio-leds";
		pinctrl-names = "default";
		pinctrl-0 =<&leds_gpio>;

		led@1 {
			gpios = <&gpio1 RK_PC6 GPIO_ACTIVE_HIGH>;
			label = "battery_led_amber";
			retain-state-suspended;
		};

		led@2 {
			gpios = <&gpio1 RK_PD0 GPIO_ACTIVE_HIGH>;
			label = "battery_led_white";
			retain-state-suspended;
		};

		led@3 {
			gpios = <&gpio3 RK_PA5 GPIO_ACTIVE_HIGH>;
			label = "call_answer_led";
		};

		led@4 {
			gpios = <&gpio3 RK_PB1 GPIO_ACTIVE_HIGH>;
			label = "call_decline_led";
		};

		led@5 {
			gpios = <&gpio2 RK_PD3 GPIO_ACTIVE_HIGH>;
			label = "rec_mute_led";
		};

		led@6 {
			gpios = <&gpio2 RK_PD4 GPIO_ACTIVE_HIGH>;
			label = "play_mute_led";
		};

		led@7 {
			gpios = <&gpio4 RK_PD2 GPIO_ACTIVE_HIGH>;
			label = "wl_led";
		};
	};

	wireless-wlan {
		compatible = "wlan-platdata";
		rockchip,grf = <&grf>;
		wifi_chip_type = "ap6354";
		sdio_vref = <1800>;
		WIFI,host_wake_irq = <&gpio0 3 GPIO_ACTIVE_HIGH>; /* GPIO0_a3 */
		status = "okay";
	};

	wireless-bluetooth {
		compatible = "bluetooth-platdata";
		clocks = <&rk808 1>;
		clock-names = "ext_clock";
		//wifi-bt-power-toggle;
		uart_rts_gpios = <&gpio2 19 GPIO_ACTIVE_LOW>; /* GPIO2_C3 */
		pinctrl-names = "default", "rts_gpio";
		pinctrl-0 = <&uart0_rts>;
		pinctrl-1 = <&uart0_gpios>;
		//BT,power_gpio  = <&gpio3 19 GPIO_ACTIVE_HIGH>; /* GPIOx_xx */
		BT,reset_gpio    = <&gpio0 9 GPIO_ACTIVE_HIGH>; /* GPIO0_B1 */
		BT,wake_gpio     = <&gpio2 26 GPIO_ACTIVE_HIGH>; /* GPIO2_D2 */
		BT,wake_host_irq = <&gpio0 4 GPIO_ACTIVE_HIGH>; /* GPIO0_A4 */
		status = "okay";
	};

	uboot-charge {
		compatible = "rockchip,uboot-charge";
		rockchip,uboot-charge-on = <1>;
		rockchip,android-charge-on = <0>;
		rockchip,uboot-exit-charge-level = <2>;
		rockchip,uboot-low-power-level = <1>;
		rockchip,uboot-charge-brightness = <0>;
		max-input-voltage = <20000>;
		max-input-current = <6000>;
	};

	vibrator {
		compatible = "rk-vibrator-gpio";
		vibrator-gpio = <&gpio4 30 GPIO_ACTIVE_LOW>;
		status = "okay";
	};

	rk_headset: rk-headset {
		compatible = "rockchip_headset";
		headset_gpio = <&gpio4 28 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&hp_det>;
		io-channels = <&saradc 2>;
	};

	hall_sensor: hall-mh248 {
		compatible = "hall-mh248";
		pinctrl-names = "default";
		pinctrl-0 = <&mh248_irq_gpio>;
		irq-gpio = <&gpio0 RK_PA1 IRQ_TYPE_EDGE_BOTH>;
		hall-active = <1>;
		status = "okay";
	};
};

&rk_key {
	compatible = "rockchip,key";
	status = "okay";

	io-channels = <&saradc 1>;

	vol-up-key {
		linux,code = <114>;
		label = "volume up";
		rockchip,adc_value = <1>;
	};

	vol-down-key {
		linux,code = <115>;
		label = "volume down";
		rockchip,adc_value = <170>;
	};

	power-key {
		gpios = <&gpio0 5 GPIO_ACTIVE_LOW>;
		linux,code = <116>;
		label = "power";
		gpio-key,wakeup;
	};

	menu-key {
		linux,code = <59>;
		label = "menu";
		rockchip,adc_value = <746>;
	};

	home-key {
		linux,code = <102>;
		label = "home";
		rockchip,adc_value = <355>;
	};

	back-key {
		linux,code = <158>;
		label = "back";
		rockchip,adc_value = <560>;
	};

	camera-key {
		linux,code = <212>;
		label = "camera";
		rockchip,adc_value = <450>;
	};
};

&cpu_l0 {
	cpu-supply = <&vdd_cpu_l>;
};

&cpu_l1 {
	cpu-supply = <&vdd_cpu_l>;
};

&cpu_l2 {
	cpu-supply = <&vdd_cpu_l>;
};

&cpu_l3 {
	cpu-supply = <&vdd_cpu_l>;
};

&cpu_b0 {
	cpu-supply = <&vdd_cpu_b>;
};

&cpu_b1 {
	cpu-supply = <&vdd_cpu_b>;
};

&edp {
	status = "okay";
	pinctrl-names = "default";
	pinctrl-0 = <&edp_hpd>;

	ports {
		edp_out: port@1 {
			reg = <1>;
			#address-cells = <1>;
			#size-cells = <0>;
			edp_out_panel: endpoint@0 {
				reg = <0>;
				remote-endpoint = <&panel_in_edp>;
			};
		};
	};
};

&edp_in_vopl {
	status = "disabled";
};

&emmc_phy {
	status = "okay";
};

&firmware_android {
	compatible = "android,firmware";
	fstab {
		compatible = "android,fstab";
		system {
			compatible = "android,system";
			dev = "/dev/block/by-name/system";
			type = "ext4";
			mnt_flags = "ro,barrier=1,inode_readahead_blks=8";
			fsmgr_flags = "wait,verify";
		};
		vendor {
			compatible = "android,vendor";
			dev = "/dev/block/by-name/vendor";
			type = "ext4";
			mnt_flags = "ro,barrier=1,inode_readahead_blks=8";
			fsmgr_flags = "wait,verify";
		};
	};
};

&gpu {
	status = "okay";
	mali-supply = <&vdd_gpu>;
};

&hdmi {
	status = "disabled";
};

&cdn_dp {
	status = "okay";
	extcon = <&fusb0>, <&fusb1>;
};

&dp_in_vopb {
	status = "disabled";
};

&i2s0 {
	status = "okay";
	rockchip,i2s-broken-burst-len;
	rockchip,playback-channels = <8>;
	rockchip,capture-channels = <8>;
	rockchip,bclk-fs = <32>;
	#sound-dai-cells = <0>;
};

&i2s1 {
	status = "okay";
	rockchip,i2s-broken-burst-len;
	rockchip,playback-channels = <2>;
	rockchip,capture-channels = <2>;
	#sound-dai-cells = <0>;
};

&i2s2 {
	status = "okay";
	#sound-dai-cells = <0>;
};

&i2c0 {
	status = "okay";
	i2c-scl-rising-time-ns = <180>;
	i2c-scl-falling-time-ns = <30>;
	clock-frequency = <400000>;

	vdd_cpu_b: syr837@40 {
		compatible = "silergy,syr827";
		reg = <0x40>;
		vin-supply = <&vcc_sys>;
		regulator-compatible = "fan53555-reg";
		pinctrl-0 = <&vsel1_gpio>;
		vsel-gpios = <&gpio1 17 GPIO_ACTIVE_HIGH>;
		regulator-name = "vdd_cpu_b";
		regulator-min-microvolt = <712500>;
		regulator-max-microvolt = <1500000>;
		regulator-ramp-delay = <1000>;
		fcs,suspend-voltage-selector = <1>;
		regulator-always-on;
		regulator-initial-state = <3>;
		regulator-state-mem {
			regulator-off-in-suspend;
		};
	};

	vdd_gpu: syr828@41 {
		compatible = "silergy,syr828";
		status = "okay";
		reg = <0x41>;
		vin-supply = <&vcc_sys>;
		regulator-compatible = "fan53555-reg";
		pinctrl-0 = <&vsel2_gpio>;
		vsel-gpios = <&gpio1 14 GPIO_ACTIVE_HIGH>;
		regulator-name = "vdd_gpu";
		regulator-min-microvolt = <735000>;
		regulator-max-microvolt = <1400000>;
		regulator-ramp-delay = <1000>;
		fcs,suspend-voltage-selector = <1>;
		regulator-always-on;
		regulator-boot-on;
		regulator-state-mem {
			regulator-off-in-suspend;
		};
	};

	rk808: pmic@1b {
		compatible = "rockchip,rk808";
		reg = <0x1b>;
		interrupt-parent = <&gpio1>;
		interrupts = <21 IRQ_TYPE_LEVEL_LOW>;
		pinctrl-0 = <&pmic_int_l>;
		rockchip,system-power-controller;
		wakeup-source;
		#clock-cells = <1>;
		clock-output-names = "rk808-clkout1", "rk808-clkout2";

		vcc1-supply = <&vcc3v3_sys>;
		vcc2-supply = <&vcc3v3_sys>;
		vcc3-supply = <&vcc3v3_sys>;
		vcc4-supply = <&vcc3v3_sys>;
		vcc6-supply = <&vcc3v3_sys>;
		vcc7-supply = <&vcc3v3_sys>;
		vcc8-supply = <&vcc3v3_sys>;
		vcc9-supply = <&vcc3v3_sys>;
		vcc10-supply = <&vcc3v3_sys>;
		vcc11-supply = <&vcc3v3_sys>;
		vcc12-supply = <&vcc3v3_sys>;
		vddio-supply = <&vcc1v8_pmu>;

		regulators {
			vdd_center: DCDC_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <750000>;
				regulator-max-microvolt = <1350000>;
				regulator-ramp-delay = <6001>;
				regulator-name = "vdd_center";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd_cpu_l: DCDC_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <750000>;
				regulator-max-microvolt = <1350000>;
				regulator-ramp-delay = <6001>;
				regulator-name = "vdd_cpu_l";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_ddr: DCDC_REG3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vcc_ddr";
				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};

			vcc_1v8: DCDC_REG4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc_1v8";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vcc1v8_dvp: LDO_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc1v8_dvp";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc3v0_tp: LDO_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3000000>;
				regulator-max-microvolt = <3000000>;
				regulator-name = "vcc3v0_tp";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc1v8_pmu: LDO_REG3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc1v8_pmu";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vcc_sd: LDO_REG4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3000000>;
				regulator-name = "vcc_sd";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3000000>;
				};
			};

			vcca3v0_codec: LDO_REG5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3000000>;
				regulator-max-microvolt = <3000000>;
				regulator-name = "vcca3v0_codec";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_1v5: LDO_REG6 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1500000>;
				regulator-max-microvolt = <1500000>;
				regulator-name = "vcc_1v5";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1500000>;
				};
			};

			vcca1v8_codec: LDO_REG7 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcca1v8_codec";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_3v0: LDO_REG8 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3000000>;
				regulator-max-microvolt = <3000000>;
				regulator-name = "vcc_3v0";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3000000>;
				};
			};

			vcc3v3_s3: SWITCH_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vcc3v3_s3";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc3v3_s0: SWITCH_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vcc3v3_s0";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};
		};
	};
};

&i2c1 {
	status = "okay";
	i2c-scl-rising-time-ns = <140>;
	i2c-scl-falling-time-ns = <30>;

	cx2072x:cx2072x@33 {
		status = "okay";
		#sound-dai-cells = <0>;
		compatible = "cnxt,cx20723";
		reg = <0x33>;
		clocks = <&cru SCLK_I2S_8CH_OUT>;
		clock-names = "mclk";
		pinctrl-names = "default";
		pinctrl-0 = <&i2s_8ch_mclk>;
		spk-con-gpio = <&gpio0 11 GPIO_ACTIVE_HIGH>;
	};
};

&i2c3 {
	status="okay";

	hidkey@68 {
		clock-frequency = <100000>;
		compatible = "hid-over-i2c";
		interrupt-parent = <&gpio0>;
		interrupts = <RK_PB0 IRQ_TYPE_LEVEL_LOW>;
		pinctrl-names = "default";
		pinctrl-0 = <&hidkey_irq_gpio>;
		reg = <0x68>;
		hid-descr-addr = <0x0001>;
		hid-support-wakeup;
	};

	ec_battery@76 {
		compatible = "rockchip,ec-battery";
		reg = <0x76>;
		virtual_power = <0>;
		monitor_sec = <5>;
		ec-notify-gpios = <&gpio1 RK_PC4 GPIO_ACTIVE_HIGH>;
	};
};

&i2c2 {
	status = "okay";
	i2c-scl-rising-time-ns = <345>;
	i2c-scl-falling-time-ns = <11>;
	clock-frequency = <400000>;

	touchpad: touchpad@2c {
		compatible = "hid-over-i2c";
		interrupt-parent = <&gpio1>;
		interrupts = <RK_PC2 IRQ_TYPE_LEVEL_LOW>;
		pinctrl-names = "default";
		pinctrl-0 = <&touchpad_irq_gpio>;
		reg = <0x2c>;
		hid-descr-addr = <0x002c>;
	};
};

&i2c4 {
	status = "okay";
	clock-frequency = <100000>;
	bq25700: bq25700@09 {//6a
		compatible = "ti,bq25700";
		reg = <0x09>;
		extcon = <&fusb0>, <&fusb1>;

		interrupt-parent = <&gpio1>;
		interrupts = <23 IRQ_TYPE_LEVEL_LOW>;
		pinctrl-names = "default";
		pinctrl-0 = <&charger_ok>;
		ti,charge-current = <2500000>;
		ti,max-input-voltage = <20000000>;
		ti,max-input-current = <6000000>;
		ti,max-charge-voltage = <8750000>;
		ti,input-current = <500000>;
		ti,input-current-sdp = <500000>;
		ti,input-current-dcp = <2000000>;
		ti,input-current-cdp = <2000000>;
		ti,minimum-sys-voltage = <7400000>;
		ti,otg-voltage = <5000000>;
		ti,otg-current = <500000>;
		pd-charge-only = <1>;
		typec0-enable-gpios = <&gpio1 RK_PA3 GPIO_ACTIVE_HIGH>;
		typec1-enable-gpios = <&gpio1 RK_PA4 GPIO_ACTIVE_HIGH>;
	};
};

&i2c6 {
	status = "okay";
	i2c-scl-rising-time-ns = <345>;
	i2c-scl-falling-time-ns = <11>;
	clock-frequency = <400000>;

	fusb1: fusb30x@22 {
		compatible = "fairchild,fusb302";
		reg = <0x22>;
		pinctrl-names = "default";
		pinctrl-0 = <&fusb1_int>;
		vbus-5v-gpios = <&gpio4 RK_PD6 GPIO_ACTIVE_HIGH>;
		int-n-gpios = <&gpio1 RK_PB5 GPIO_ACTIVE_HIGH>;
		discharge-gpios = <&gpio0 RK_PB5 GPIO_ACTIVE_HIGH>;
		charge-dev = <&bq25700>;
		support-uboot-charge = <1>;
		port-num = <1>;
		status = "okay";
	};
};

&i2c7 {
	status = "okay";
	i2c-scl-rising-time-ns = <345>;
	i2c-scl-falling-time-ns = <11>;
	clock-frequency = <400000>;

	fusb0: fusb30x@22 {
		compatible = "fairchild,fusb302";
		reg = <0x22>;
		pinctrl-names = "default";
		pinctrl-0 = <&fusb0_int>;
		vbus-5v-gpios = <&gpio4 RK_PD5 GPIO_ACTIVE_HIGH>;
		int-n-gpios = <&gpio1 RK_PA2 GPIO_ACTIVE_HIGH>;
		discharge-gpios = <&gpio0 RK_PB4 GPIO_ACTIVE_HIGH>;
		charge-dev = <&bq25700>;
		support-uboot-charge = <1>;
		port-num = <0>;
		status = "okay";
	};
};

&io_domains {
	status = "okay";
	bt656-supply = <&vcc_3v0>;
	audio-supply = <&vcca1v8_codec>;
	sdmmc-supply = <&vcc_sd>;
	gpio1830-supply = <&vcc_3v0>;
};

&dsi {
	status = "disabled";
};

&pcie_phy {
	status = "okay";
};

&pcie0 {
	ep-gpios = <&gpio3 7 GPIO_ACTIVE_HIGH>;
	num-lanes = <4>;
	pinctrl-names = "default";
	pinctrl-0 = <&pcie_clkreqn_cpm>;
	status = "okay";
};

&pmu_io_domains {
	status = "okay";
	pmu1830-supply = <&vcc_1v8>;
};

&pwm0 {
	status = "okay";
};

&pwm2 {
	status = "okay";
	pinctrl-names = "active";
	pinctrl-0 = <&pwm2_pin_pull_down>;
};

&route_edp {
	status = "okay";
	logo,mode = "center";
};

&saradc {
	status = "okay";
};

&sdmmc {
	clock-frequency = <50000000>;
	clock-freq-min-max = <400000 150000000>;
	no-sdio;
	no-mmc;
	bus-width = <4>;
	cap-mmc-highspeed;
	cap-sd-highspeed;
	disable-wp;
	num-slots = <1>;
	//sd-uhs-sdr104;
	vqmmc-supply = <&vcc_sd>;
	pinctrl-names = "default";
	pinctrl-0 = <&sdmmc_clk &sdmmc_cmd &sdmmc_cd &sdmmc_bus4>;
	status = "okay";
};

&sdio0 {
	clock-frequency = <150000000>;
	clock-freq-min-max = <200000 150000000>;
	no-sd;
	no-mmc;
	bus-width = <4>;
	disable-wp;
	cap-sd-highspeed;
	cap-sdio-irq;
	keep-power-in-suspend;
	mmc-pwrseq = <&sdio_pwrseq>;
	non-removable;
	num-slots = <1>;
	pinctrl-names = "default";
	pinctrl-0 = <&sdio0_bus4 &sdio0_cmd &sdio0_clk>;
	sd-uhs-sdr104;
	status = "okay";
};

&sdhci {
	bus-width = <8>;
	mmc-hs400-1_8v;
	no-sdio;
	no-sd;
	non-removable;
	keep-power-in-suspend;
	mmc-hs400-enhanced-strobe;
	status = "okay";
};

&spdif {
	status = "okay";
	#sound-dai-cells = <0>;
};

&spi1 {
	status = "disabled";
};

&tcphy0 {
	extcon = <&fusb0>;
	status = "okay";
};

&tcphy1 {
	extcon = <&fusb1>;
	status = "okay";
};

&tsadc {
	rockchip,hw-tshut-mode = <1>; /* tshut mode 0:CRU 1:GPIO */
	rockchip,hw-tshut-polarity = <1>; /* tshut polarity 0:LOW 1:HIGH */
	status = "okay";
};

&u2phy0 {
	status = "okay";
	extcon = <&fusb0>;

	u2phy0_otg: otg-port {
		status = "okay";
	};

	u2phy0_host: host-port {
		phy-supply = <&vcc5v0_host>;
		status = "okay";
	};
};

&u2phy1 {
	status = "okay";
	extcon = <&fusb1>;

	u2phy1_otg: otg-port {
		status = "okay";
	};

	u2phy1_host: host-port {
		phy-supply = <&vcc5v0_host>;
		status = "okay";
	};
};

&uart0 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart0_xfer &uart0_cts>;
	status = "okay";
};

&uart2 {
	status = "okay";
};

&usb_host0_ehci {
	status = "okay";
};

&usb_host0_ohci {
	status = "okay";
};

&usbdrd3_0 {
	status = "okay";
};

&usbdrd_dwc3_0 {
	status = "okay";
	extcon = <&fusb0>;
};

&usb_host1_ehci {
	status = "okay";
};

&usb_host1_ohci {
	status = "okay";
};

&usbdrd3_1 {
	status = "okay";
};

&usbdrd_dwc3_1 {
	status = "okay";
	extcon = <&fusb1>;
};

&rockchip_suspend {
	status = "okay";
	rockchip,sleep-debug-en = <1>;
	rockchip,sleep-mode-config = <
		(0
		| RKPM_SLP_ARMPD
		| RKPM_SLP_PERILPPD
		| RKPM_SLP_DDR_RET
		| RKPM_SLP_PLLPD
		| RKPM_SLP_CENTER_PD
		| RKPM_SLP_AP_PWROFF
		)
		>;
		rockchip,wakeup-config = <
		(0
		| RKPM_GPIO_WKUP_EN
		| RKPM_PWM_WKUP_EN
		)
		>;
		rockchip,pwm-regulator-config = <
		(0
		| PWM2_REGULATOR_EN
		)
		>;
		rockchip,power-ctrl =
		<&gpio1 17 GPIO_ACTIVE_HIGH>,
		<&gpio1 14 GPIO_ACTIVE_HIGH>;
};

&pinctrl {
	sdio-pwrseq {
		wifi_enable_h: wifi-enable-h {
			rockchip,pins = <0 RK_PB2 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	wireless-bluetooth {
		uart0_gpios: uart0-gpios {
			rockchip,pins = <2 RK_PC3 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	pmic {
		pmic_int_l: pmic-int-l {
			rockchip,pins =
				<1 RK_PC5 RK_FUNC_GPIO &pcfg_pull_up>;
		};
		vsel1_gpio: vsel1-gpio {
			rockchip,pins =
				<1 RK_PC1 RK_FUNC_GPIO &pcfg_pull_down>;
		};
		vsel2_gpio: vsel2-gpio {
			rockchip,pins =
				<1 RK_PB6 RK_FUNC_GPIO &pcfg_pull_down>;
		};
	};

	headphone {
		hp_det: hp-det {
			rockchip,pins = <4 RK_PD4 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	hallsensor {
		mh248_irq_gpio: mh248-irq-gpio {
			rockchip,pins = <0 RK_PA1 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	hidkey {
		hidkey_irq_gpio: hidkey-irq-gpio {
			rockchip,pins = <0 RK_PB0 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	touchpad {
		touchpad_irq_gpio: touchpad-irq-gpio {
			rockchip,pins = <1 RK_PC2 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	charger {
		charger_ok: charge-ok {
			rockchip,pins =
				<1 RK_PC7 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	gpio-leds {
		leds_gpio: leds-gpio {
			rockchip,pins =
				<1 RK_PC6 RK_FUNC_GPIO &pcfg_pull_up>,
				<1 RK_PD0 RK_FUNC_GPIO &pcfg_pull_up>,
				<3 RK_PA5 RK_FUNC_GPIO &pcfg_pull_up>,
				<3 RK_PB1 RK_FUNC_GPIO &pcfg_pull_up>,
				<2 RK_PD3 RK_FUNC_GPIO &pcfg_pull_up>,
				<2 RK_PD4 RK_FUNC_GPIO &pcfg_pull_up>,
				<4 RK_PD2 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	usb2 {
		host_vbus_drv: host-vbus-drv {
			rockchip,pins =
				<4 RK_PD1 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	usb_camera {
		usb_cam_on_gpio: usb-cam-on-gpio {
			rockchip,pins =
				<3 RK_PA1 RK_FUNC_GPIO &pcfg_pull_up>,
				<3 RK_PA2 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	fusb30x {
		fusb0_int: fusb0-int {
			rockchip,pins =
				<1 RK_PA2 RK_FUNC_GPIO &pcfg_pull_up>,
				<0 RK_PB4 RK_FUNC_GPIO &pcfg_pull_up>;
		};
		fusb1_int: fusb1-int {
			rockchip,pins =
				<1 RK_PB5 RK_FUNC_GPIO &pcfg_pull_up>,
				<0 RK_PB5 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};
};
