/*
 * Copyright (c) 2018 Fuzhou Rockchip Electronics Co., Ltd
 *
 * SPDX-License-Identifier: (GPL-2.0+ OR MIT)
 */

/dts-v1/;

#include "rk3399-sapphire.dtsi"
#include "rk3399-linux.dtsi"
#include <dt-bindings/input/input.h>

/ {
	model = "Rockchip RK3399 Videostrong Board (Linux Opensource)";
	compatible = "rockchip,rk3399-videostrong-linux", "rockchip,rk3399";

	fiq_debugger: fiq-debugger {
		compatible = "rockchip,fiq-debugger";
		rockchip,serial-id = <2>;
		rockchip,signal-irq = <182>;
		rockchip,wake-irq = <0>;
		rockchip,irq-mode-enable = <1>;  /* If enable uart uses irq instead of fiq */
		rockchip,baudrate = <1500000>;  /* Only 115200 and 1500000 */
		pinctrl-names = "default";
		pinctrl-0 = <&uart2c_xfer>;
	};

	gpio-keys {
		compatible = "gpio-keys";
		#address-cells = <1>;
		#size-cells = <0>;
		autorepeat;

		pinctrl-names = "default";
		pinctrl-0 = <&pwrbtn>;

		button@0 {
			gpios = <&gpio0 5 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_POWER>;
			label = "GPIO Key Power";
			linux,input-type = <1>;
			gpio-key,wakeup = <1>;
			debounce-interval = <100>;
		};
	};

	hdmi_sound: hdmi-sound {
		status = "okay";
	};

	rt5640-sound {
		compatible = "simple-audio-card";
		simple-audio-card,format = "i2s";
		simple-audio-card,name = "rockchip,rt5640-codec";
		simple-audio-card,mclk-fs = <256>;
		simple-audio-card,widgets =
			"Microphone", "Mic Jack",
			"Headphone", "Headphone Jack";
		simple-audio-card,routing =
			"Mic Jack", "MICBIAS1",
			"IN1P", "Mic Jack",
			"Headphone Jack", "HPOL",
			"Headphone Jack", "HPOR";
		simple-audio-card,cpu {
			sound-dai = <&i2s1>;
		};
		simple-audio-card,codec {
			sound-dai = <&rt5640>;
		};
	};

	sdio_pwrseq: sdio-pwrseq {
		compatible = "mmc-pwrseq-simple";
		clocks = <&rk808 1>;
		clock-names = "ext_clock";
		pinctrl-names = "default";
		pinctrl-0 = <&wifi_enable_h>;

		/*
		 * On the module itself this is one of these (depending
		 * on the actual card populated):
		 * - SDIO_RESET_L_WL_REG_ON
		 * - PDN (power down when low)
		 */
		reset-gpios = <&gpio0 10 GPIO_ACTIVE_LOW>; /* GPIO0_B2 */
	};

	spdif-sound {
		status = "okay";
		compatible = "simple-audio-card";
		simple-audio-card,name = "ROCKCHIP,SPDIF";
		simple-audio-card,mclk-fs = <128>;
		simple-audio-card,cpu {
			sound-dai = <&spdif>;
		};
		simple-audio-card,codec {
			sound-dai = <&spdif_out>;
		};
	};

	spdif_out: spdif-out {
		status = "okay";
		compatible = "linux,spdif-dit";
		#sound-dai-cells = <0>;
	};

	vccadc_ref: vccadc-ref {
		compatible = "regulator-fixed";
		regulator-name = "vcc1v8_sys";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <1800000>;
		regulator-max-microvolt = <1800000>;
	};

	wireless-bluetooth {
		compatible = "bluetooth-platdata";
		clocks = <&rk808 1>;
		clock-names = "ext_clock";
		uart_rts_gpios = <&gpio2 19 GPIO_ACTIVE_LOW>; /* GPIO2_C3 */
		pinctrl-names = "default", "rts_gpio";
		pinctrl-0 = <&uart0_rts>;
		pinctrl-1 = <&uart0_gpios>;
		BT,reset_gpio    = <&gpio0 9 GPIO_ACTIVE_HIGH>; /* GPIO0_B1 */
		BT,wake_gpio     = <&gpio2 26 GPIO_ACTIVE_HIGH>; /* GPIO2_D2 */
		BT,wake_host_irq = <&gpio0 4 GPIO_ACTIVE_HIGH>; /* GPIO0_A4 */
		status = "okay";
	};

	wireless-wlan {
		compatible = "wlan-platdata";
		rockchip,grf = <&grf>;
		wifi_chip_type = "ap6354";
		sdio_vref = <1800>;
		WIFI,host_wake_irq = <&gpio0 3 GPIO_ACTIVE_HIGH>; /* GPIO0_a3 */
		status = "okay";
	};
};

&dfi {
	status = "okay";
};

&display_subsystem {
	status = "okay";
};

&dmc {
	status = "okay";
	center-supply = <&vdd_center>;
	upthreshold = <40>;
	downdifferential = <20>;
	system-status-freq = <
		/* system status	freq(KHz) */
		SYS_STATUS_NORMAL       800000
		SYS_STATUS_REBOOT       528000
		SYS_STATUS_SUSPEND      200000
		SYS_STATUS_VIDEO_1080P  200000
		SYS_STATUS_VIDEO_4K     600000
		SYS_STATUS_VIDEO_4K_10B 800000
		SYS_STATUS_PERFORMANCE  800000
		SYS_STATUS_BOOST        400000
		SYS_STATUS_DUALVIEW     600000
		SYS_STATUS_ISP          600000
	>;
	vop-bw-dmc-freq = <
	/* min_bw(MB/s) max_bw(MB/s) freq(KHz) */
		0       577      200000
		578     1701     300000
		1702    99999    400000
	>;
	auto-min-freq = <200000>;
};

&hdmi {
	/* remove the hdmi_cec, reused by edp_hpd */
	pinctrl-0 = <&hdmi_i2c_xfer>;
	#address-cells = <1>;
	#size-cells = <0>;
	#sound-dai-cells = <0>;
	status = "okay";
};

&i2c1 {
	status = "okay";
	i2c-scl-rising-time-ns = <300>;
	i2c-scl-falling-time-ns = <15>;

	rt5640: rt5640@1c {
		#sound-dai-cells = <0>;
		compatible = "realtek,rt5640";
		reg = <0x1c>;
		clocks = <&cru SCLK_I2S_8CH_OUT>;
		clock-names = "mclk";
		realtek,in1-differential;
		pinctrl-names = "default";
		pinctrl-0 = <&i2s_8ch_mclk>;
	};
};

&i2s1 {
	status = "okay";
	rockchip,i2s-broken-burst-len;
	rockchip,playback-channels = <2>;
	rockchip,capture-channels = <2>;
	#sound-dai-cells = <0>;
};

&rkvdec {
	status = "okay";
	/* 0 means ion, 1 means drm */
	//allocator = <0>;
};

&rockchip_suspend {
	status = "okay";
	rockchip,sleep-debug-en = <1>;
	rockchip,sleep-mode-config = <
		(0
		| RKPM_SLP_ARMPD
		| RKPM_SLP_PERILPPD
		| RKPM_SLP_DDR_RET
		| RKPM_SLP_PLLPD
		| RKPM_SLP_CENTER_PD
		| RKPM_SLP_AP_PWROFF
		)
		>;
	rockchip,wakeup-config = <
		(0
		| RKPM_GPIO_WKUP_EN
		| RKPM_PWM_WKUP_EN
		)
		>;
		rockchip,pwm-regulator-config = <
		(0
		| PWM2_REGULATOR_EN
		)
		>;
		rockchip,power-ctrl =
		<&gpio1 17 GPIO_ACTIVE_HIGH>,
		<&gpio1 14 GPIO_ACTIVE_HIGH>;
};

&spdif {
	status = "okay";
	pinctrl-0 = <&spdif_bus>;
	i2c-scl-rising-time-ns = <450>;
	i2c-scl-falling-time-ns = <15>;
	#sound-dai-cells = <0>;
};

&uart0 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart0_xfer &uart0_cts>;
	status = "okay";
};

&vopb {
	status = "okay";
};

&vopb_mmu {
	status = "okay";
};

&vopl {
	status = "okay";
};

&vopl_mmu {
	status = "okay";
};

&pinctrl {
	buttons {
		pwrbtn: pwrbtn {
			rockchip,pins = <0 RK_PA5 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	sdio-pwrseq {
		wifi_enable_h: wifi-enable-h {
			rockchip,pins =
				<0 RK_PB2 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	wireless-bluetooth {
		uart0_gpios: uart0-gpios {
			rockchip,pins =
				<2 RK_PC3 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};
};
