/**
 * multiple lcd config compatible
 */

// MIPI DSI0
&dsi0_panel {
    /** delete property that conflict with other panel, they are common */
    /delete-property/ power-supply;
    /delete-property/ reset-gpios;
    /delete-property/ pinctrl-names;
    /delete-property/ pinctrl-0;
    backlight = <&backlight4>;
};

// MIPI DSI1
&dsi1_panel {
    power-supply = <&vcc3v3_lcd0_n>;
    reset-gpios = <&gpio4 RK_PD2 GPIO_ACTIVE_LOW>;
    pinctrl-names = "default";
    pinctrl-0 = <&lcd_rst_gpio>;
    backlight = <&backlight5>;
};

// LVDS
&lvds_panel {
    backlight = <&backlight4>;
    
    /** delete property that conflict with other panel, they are common */
    /delete-property/ power-supply;
    /delete-property/ reset-gpios;
    /delete-property/ pinctrl-names;
    /delete-property/ pinctrl-0;
};

// EDP
&edp_panel {
    backlight = <&backlight5>;
    
    /** delete property that conflict with other panel, it is common */
    /delete-property/ power-supply;
};


