/*
 * Copyright (c) 2018 Fuzhou Rockchip Electronics Co., Ltd
 *
 * SPDX-License-Identifier: (GPL-2.0+ OR MIT)
 */

/dts-v1/;
#include <dt-bindings/display/drm_mipi_dsi.h>
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/pinctrl/rockchip.h>
#include <dt-bindings/sensor-dev.h>
#include "rk3326.dtsi"
#include "rk3326-863-cif-sensor.dtsi"
#include "px30-android.dtsi"

/ {
	model = "Rockchip rk3326 ai voice assistant evb v11 i2s-dmic board";
	compatible = "rockchip,rk3326-evb-ai-va-v11-i2s-dmic", "rockchip,rk3326";

	adc-keys {
		compatible = "adc-keys";
		io-channels = <&saradc 2>;
		io-channel-names = "buttons";
		poll-interval = <100>;
		keyup-threshold-microvolt = <1800000>;

		mute-key {
			linux,code = <KEY_MUTE>;
			label = "mute";
			press-threshold-microvolt = <1119000>;
		};

		mode-key {
			linux,code = <KEY_MODE>;
			label = "mode";
			press-threshold-microvolt = <892000>;
		};

		media-key {
			linux,code = <KEY_MEDIA>;
			label = "media";
			press-threshold-microvolt = <616000>;
		};

		vol-down-key {
			linux,code = <KEY_VOLUMEDOWN>;
			label = "volume down";
			press-threshold-microvolt = <300000>;
		};

		vol-up-key {
			linux,code = <KEY_VOLUMEUP>;
			label = "volume up";
			press-threshold-microvolt = <15000>;
		};
	};

	backlight: backlight {
		compatible = "pwm-backlight";
		pwms = <&pwm1 0 25000 0>;
		brightness-levels = <
			  0   1   2   3   4   5   6   7
			  8   9  10  11  12  13  14  15
			 16  17  18  19  20  21  22  23
			 24  25  26  27  28  29  30  31
			 32  33  34  35  36  37  38  39
			 40  41  42  43  44  45  46  47
			 48  49  50  51  52  53  54  55
			 56  57  58  59  60  61  62  63
			 64  65  66  67  68  69  70  71
			 72  73  74  75  76  77  78  79
			 80  81  82  83  84  85  86  87
			 88  89  90  91  92  93  94  95
			 96  97  98  99 100 101 102 103
			104 105 106 107 108 109 110 111
			112 113 114 115 116 117 118 119
			120 121 122 123 124 125 126 127
			128 129 130 131 132 133 134 135
			136 137 138 139 140 141 142 143
			144 145 146 147 148 149 150 151
			152 153 154 155 156 157 158 159
			160 161 162 163 164 165 166 167
			168 169 170 171 172 173 174 175
			176 177 178 179 180 181 182 183
			184 185 186 187 188 189 190 191
			192 193 194 195 196 197 198 199
			200 201 202 203 204 205 206 207
			208 209 210 211 212 213 214 215
			216 217 218 219 220 221 222 223
			224 225 226 227 228 229 230 231
			232 233 234 235 236 237 238 239
			240 241 242 243 244 245 246 247
			248 249 250 251 252 253 254 255>;
		default-brightness-level = <200>;
	};

	multi_dais: multi-dais {
			status = "okay";
			compatible = "rockchip,multi-dais";
			dais = <&pdm>, <&i2s0_8ch>;
			capture,channel-mapping = <2 6>;
			playback,channel-mapping = <0 0>;
			#sound-dai-cells = <0>;
	};

	rk809-sound {
		compatible = "simple-audio-card";
		simple-audio-card,name = "rockchip,rk809-codec";
		simple-audio-card,mclk-fs = <256>;
		simple-audio-card,widgets =
			"Microphone", "Mic Jack",
			"Headphone", "Headphone Jack";
		simple-audio-card,routing =
			"Mic Jack", "MICBIAS1",
			"IN1P", "Mic Jack",
			"Headphone Jack", "HPOL",
			"Headphone Jack", "HPOR";
		simple-audio-card,dai-link@0 {
			format = "i2s";
			cpu {
				sound-dai = <&i2s1_2ch>;
			};
			codec {
				sound-dai = <&rk809_codec 0>;
			};
		};
		simple-audio-card,dai-link@1 {
			format = "i2s";
			cpu {
				sound-dai = <&multi_dais>;
			};
			codec {
				sound-dai = <&rk809_codec 1>;
			};
		};
	};

	bt-sound {
		compatible = "simple-audio-card";
		status = "disabled";
		simple-audio-card,format = "dsp_a";
		simple-audio-card,bitclock-inversion;
		simple-audio-card,mclk-fs = <256>;
		simple-audio-card,name = "rockchip,bt";
		simple-audio-card,cpu {
			sound-dai = <&i2s2_2ch>;
		};
		simple-audio-card,codec {
			sound-dai = <&bt_sco>;
		};
	};

	bt_sco: bt-sco {
		compatible = "delta,dfbmcs320";
		#sound-dai-cells = <0>;
		status = "okay";
	};

	rk_headset: rk-headset {
		compatible = "rockchip_headset";
		headset_gpio = <&gpio3 RK_PA4 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&hp_det>;
		io-channels = <&saradc 1>;
	};

	sdio_pwrseq: sdio-pwrseq {
		compatible = "mmc-pwrseq-simple";
		clocks = <&rk809 1>;
		clock-names = "ext_clock";
		pinctrl-names = "default";
		pinctrl-0 = <&wifi_enable_h>;

		/*
		 * On the module itself this is one of these (depending
		 * on the actual card populated):
		 * - SDIO_RESET_L_WL_REG_ON
		 * - PDN (power down when low)
		 */
		reset-gpios = <&gpio0 RK_PA2 GPIO_ACTIVE_LOW>; /* GPIO3_A4 */
	};

	test-power {
		status = "okay";
	};

	vcc5v0_sys: vccsys {
		compatible = "regulator-fixed";
		regulator-name = "vcc5v0_sys";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
	};

	wireless-wlan {
		compatible = "wlan-platdata";
		wifi_chip_type = "AP6255";
		WIFI,host_wake_irq = <&gpio0 RK_PA5 GPIO_ACTIVE_HIGH>;
		status = "okay";
	};

	wireless-bluetooth {
		compatible = "bluetooth-platdata";
		clocks = <&rk809 1>;
		clock-names = "ext_clock";
		uart_rts_gpios = <&gpio1 RK_PC3 GPIO_ACTIVE_LOW>;
		pinctrl-names = "default","rts_gpio";
		pinctrl-0 = <&uart1_rts>;
		pinctrl-1 = <&uart1_rts_gpio>;
		BT,reset_gpio = <&gpio0 RK_PC1 GPIO_ACTIVE_HIGH>;
		BT,wake_gpio = <&gpio0 RK_PA1 GPIO_ACTIVE_HIGH>;
		BT,wake_host_irq = <&gpio0 RK_PA7 GPIO_ACTIVE_HIGH>;
		status = "okay";
	};
};

&bus_apll {
	bus-supply = <&vdd_logic>;
	status = "okay";
};

&cpu0 {
	cpu-supply = <&vdd_arm>;
};

&dfi {
	status = "okay";
};

&display_subsystem {
	status = "okay";
};

&dmc {
	center-supply = <&vdd_logic>;
	status = "okay";
};

&dsi {
	status = "okay";

	panel@0 {
		compatible = "sitronix,st7703", "simple-panel-dsi";
		reg = <0>;
		backlight = <&backlight>;
		enable-gpios = <&gpio0 RK_PB5 GPIO_ACTIVE_HIGH>;
		prepare-delay-ms = <2>;
		reset-delay-ms = <1>;
		init-delay-ms = <20>;
		enable-delay-ms = <120>;
		disable-delay-ms = <50>;
		unprepare-delay-ms = <40>;

		width-mm = <68>;
		height-mm = <121>;

		dsi,flags = <(MIPI_DSI_MODE_VIDEO | MIPI_DSI_MODE_VIDEO_BURST |
			      MIPI_DSI_MODE_LPM | MIPI_DSI_MODE_EOT_PACKET)>;
		dsi,format = <MIPI_DSI_FMT_RGB888>;
		dsi,lanes = <4>;

		panel-init-sequence = [
			05 fa 01 11
			39 00 04 b9 f1 12 83
			39 00 1c ba 33 81 05 f9 0e 0e 00 00 00
				 00 00 00 00 00 44 25 00 91 0a
				 00 00 02 4f 01 00 00 37
			15 00 02 b8 25
			39 00 04 bf 02 11 00
			39 00 0b b3 0c 10 0a 50 03 ff 00 00 00
				 00
			39 00 0a c0 73 73 50 50 00 00 08 70 00
			15 00 02 bc 46
			15 00 02 cc 0b
			15 00 02 b4 80
			39 00 04 b2 c8 12 30
			39 00 0f e3 07 07 0b 0b 03 0b 00 00 00
				 00 ff 00 c0 10
			39 00 0d c1 53 00 1e 1e 77 e1 cc dd 67
				 77 33 33
			39 00 07 c6 00 00 ff ff 01 ff
			39 00 03 b5 09 09
			39 00 03 b6 87 95
			39 00 40 e9 c2 10 05 05 10 05 a0 12 31
				 23 3f 81 0a a0 37 18 00 80 01
				 00 00 00 00 80 01 00 00 00 48
				 f8 86 42 08 88 88 80 88 88 88
				 58 f8 87 53 18 88 88 81 88 88
				 88 00 00 00 01 00 00 00 00 00
				 00 00 00 00
			39 00 3e ea 00 1a 00 00 00 00 02 00 00
				 00 00 00 1f 88 81 35 78 88 88
				 85 88 88 88 0f 88 80 24 68 88
				 88 84 88 88 88 23 10 00 00 1c
				 00 00 00 00 00 00 00 00 00 00
				 00 00 00 00 00 30 05 a0 00 00
				 00 00
			39 00 23 e0 00 06 08 2a 31 3f 38 36 07
				 0c 0d 11 13 12 13 11 18 00 06
				 08 2a 31 3f 38 36 07 0c 0d 11
				 13 12 13 11 18
			05 32 01 29
		];

		panel-exit-sequence = [
			05 00 01 28
			05 00 01 10
		];

		display-timings {
			native-mode = <&timing0>;

			timing0: timing0 {
				clock-frequency = <66000000>;
				hactive = <720>;
				vactive = <1280>;
				hfront-porch = <40>;
				hsync-len = <10>;
				hback-porch = <40>;
				vfront-porch = <22>;
				vsync-len = <4>;
				vback-porch = <11>;
				hsync-active = <0>;
				vsync-active = <0>;
				de-active = <0>;
				pixelclk-active = <0>;
			};
		};

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				panel_in_dsi: endpoint {
					remote-endpoint = <&dsi_out_panel>;
				};
			};
		};
	};

	ports {
		#address-cells = <1>;
		#size-cells = <0>;

		port@1 {
			reg = <1>;
			dsi_out_panel: endpoint {
				remote-endpoint = <&panel_in_dsi>;
			};
		};
	};
};

&dsi_in_vopb {
	status = "okay";
};

&dsi_in_vopl {
	status = "disabled";
};

&route_dsi {
	connect = <&vopb_out_dsi>;
	status = "okay";
};

&emmc {
	bus-width = <8>;
	cap-mmc-highspeed;
	mmc-hs200-1_8v;
	no-sdio;
	no-sd;
	disable-wp;
	non-removable;
	num-slots = <1>;
	status = "okay";
};

&gpu {
	mali-supply = <&vdd_logic>;
	status = "okay";
};

&i2c0 {
	status = "okay";
	clock-frequency = <400000>;
	i2c-scl-rising-time-ns = <280>;
	i2c-scl-falling-time-ns = <16>;

	rk809: pmic@20 {
		compatible = "rockchip,rk809";
		reg = <0x20>;
		interrupt-parent = <&gpio0>;
		interrupts = <10 IRQ_TYPE_LEVEL_LOW>;
		pinctrl-names = "default", "pmic-sleep",
				"pmic-power-off", "pmic-reset";
		pinctrl-0 = <&pmic_int>;
		pinctrl-1 = <&soc_slppin_slp>, <&rk817_slppin_slp>;
		pinctrl-2 = <&soc_slppin_gpio>, <&rk817_slppin_pwrdn>;
		pinctrl-3 = <&soc_slppin_rst>, <&rk817_slppin_rst>;
		rockchip,system-power-controller;
		wakeup-source;
		#clock-cells = <1>;
		clock-output-names = "rk808-clkout1", "rk808-clkout2";
		//fb-inner-reg-idxs = <2>;
		/* 1: rst regs (default in codes), 0: rst the pmic */
		pmic-reset-func = <1>;

		vcc1-supply = <&vcc5v0_sys>;
		vcc2-supply = <&vcc5v0_sys>;
		vcc3-supply = <&vcc5v0_sys>;
		vcc4-supply = <&vcc5v0_sys>;
		vcc5-supply = <&vcc3v3_sys>;
		vcc6-supply = <&vcc3v3_sys>;
		vcc7-supply = <&vcc3v3_sys>;
		vcc8-supply = <&vcc3v3_sys>;
		vcc9-supply = <&vcc5v0_sys>;

		pwrkey {
			status = "okay";
		};

		pinctrl_rk8xx: pinctrl_rk8xx {
			gpio-controller;
			#gpio-cells = <2>;

			rk817_slppin_null: rk817_slppin_null {
				pins = "gpio_slp";
				function = "pin_fun0";
			};

			rk817_slppin_slp: rk817_slppin_slp {
				pins = "gpio_slp";
				function = "pin_fun1";
			};

			rk817_slppin_pwrdn: rk817_slppin_pwrdn {
				pins = "gpio_slp";
				function = "pin_fun2";
			};

			rk817_slppin_rst: rk817_slppin_rst {
				pins = "gpio_slp";
				function = "pin_fun3";
			};
		};

		regulators {
			vdd_logic: DCDC_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <850000>;
				regulator-max-microvolt = <1350000>;
				regulator-ramp-delay = <6001>;
				regulator-initial-mode = <0x2>;
				regulator-name = "vdd_logic";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <950000>;
				};
			};

			vdd_arm: DCDC_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <850000>;
				regulator-max-microvolt = <1350000>;
				regulator-ramp-delay = <6001>;
				regulator-initial-mode = <0x2>;
				regulator-name = "vdd_arm";
				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <950000>;
				};
			};

			vcc_ddr: DCDC_REG3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-initial-mode = <0x2>;
				regulator-name = "vcc_ddr";
				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};

			vcc_3v0: DCDC_REG4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3000000>;
				regulator-max-microvolt = <3000000>;
				regulator-initial-mode = <0x2>;
				regulator-name = "vcc_3v0";
				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <3000000>;
				};
			};

			vcc_1v0: LDO_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <1000000>;
				regulator-name = "vcc_1v0";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1000000>;
				};
			};

			vcc1v8_soc: LDO_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;

				regulator-name = "vcc1v8_soc";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vdd1v0_soc: LDO_REG3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <1000000>;

				regulator-name = "vcc1v0_soc";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1000000>;
				};
			};

			vcc3v0_pmu: LDO_REG4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3000000>;
				regulator-max-microvolt = <3000000>;

				regulator-name = "vcc3v0_pmu";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3000000>;

				};
			};

			vccio_sd: LDO_REG5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;

				regulator-name = "vccio_sd";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vcc_sd: LDO_REG6 {
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;

				regulator-name = "vcc_sd";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;

				};
			};

			vcc2v8_dvp: LDO_REG7 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <2800000>;
				regulator-max-microvolt = <2800000>;

				regulator-name = "vcc2v8_dvp";
				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <2800000>;
				};
			};

			vcc1v8_dvp: LDO_REG8 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;

				regulator-name = "vcc1v8_dvp";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vdd1v5_dvp: LDO_REG9 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1500000>;
				regulator-max-microvolt = <1500000>;

				regulator-name = "vdd1v5_dvp";
				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <1500000>;
				};
			};

			vcc3v3_sys: DCDC_REG5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vcc3v3_sys";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vcc5v0_host: SWITCH_REG1 {
				regulator-name = "vcc5v0_host";
			};

			vcc3v3_lcd: SWITCH_REG2 {
				regulator-boot-on;
				regulator-name = "vcc3v3_lcd";
			};
		};

		rk809_codec: codec {
			#sound-dai-cells = <1>;
			compatible = "rockchip,rk809-codec", "rockchip,rk817-codec";
			clocks = <&cru SCLK_I2S1_OUT>;
			clock-names = "mclk";
			pinctrl-names = "default";
			pinctrl-0 = <&i2s1_2ch_mclk>;
			pdmdata-out-enable;
			use-ext-amplifier;
			adc-for-loopback;
			spk-ctl-gpios = <&gpio3 RK_PB2 GPIO_ACTIVE_HIGH>;
			hp-volume = <20>;
			spk-volume = <20>;
		};
	};
};

&i2c1 {
	status = "okay";
	clock-frequency = <400000>;
	i2c-scl-rising-time-ns = <275>;
	i2c-scl-falling-time-ns = <16>;

	gt1x: gt1x@14 {
	      compatible = "goodix,gt1x";
	      reg = <0x14>;
	      goodix,rst-gpio = <&gpio0 RK_PB4 GPIO_ACTIVE_HIGH>;
	      goodix,irq-gpio = <&gpio0 RK_PB3 IRQ_TYPE_LEVEL_LOW>;
	};

	is31fl3236: led-controller@3c {
		compatible = "issi,is31fl3236";
		reg = <0x3c>;
		#address-cells = <1>;
		#size-cells = <0>;
		reset-gpios = <&gpio3 RK_PA6 GPIO_ACTIVE_HIGH>;
		status = "okay";

		led1: led@1 {
			label = "led1";
			reg = <1>;
			led-max-microamp = <10000>;
			linux,default-trigger = "timer";
			linux,default-trigger-delay-ms = <0>;
			linux,blink-delay-on-ms = <100>;
			linux,blink-delay-off-ms = <1200>;
		};

		led2: led@2 {
			label = "led2";
			reg = <2>;
			led-max-microamp = <10000>;
			linux,default-trigger = "timer";
			linux,default-trigger-delay-ms = <0>;
			linux,blink-delay-on-ms = <100>;
			linux,blink-delay-off-ms = <1200>;
		};

		led3: led@3 {
			label = "led3";
			reg = <3>;
			led-max-microamp = <10000>;
			linux,default-trigger = "default-on";
		};

		led4: led@4 {
			label = "led4";
			reg = <4>;
			led-max-microamp = <10000>;
			linux,default-trigger = "timer";
			linux,default-trigger-delay-ms = <100>;
			linux,blink-delay-on-ms = <100>;
			linux,blink-delay-off-ms = <1200>;
		};

		led5: led@5 {
			label = "led5";
			reg = <5>;
			led-max-microamp = <10000>;
			linux,default-trigger = "timer";
			linux,default-trigger-delay-ms = <100>;
			linux,blink-delay-on-ms = <100>;
			linux,blink-delay-off-ms = <1200>;
		};

		led6: led@6 {
			label = "led6";
			reg = <6>;
			led-max-microamp = <10000>;
			linux,default-trigger = "default-on";
		};

		led7: led@7 {
			label = "led7";
			reg = <7>;
			led-max-microamp = <10000>;
			linux,default-trigger = "timer";
			linux,default-trigger-delay-ms = <200>;
			linux,blink-delay-on-ms = <100>;
			linux,blink-delay-off-ms = <1200>;
		};

		led8: led@8 {
			label = "led8";
			reg = <8>;
			led-max-microamp = <10000>;
			linux,default-trigger = "timer";
			linux,default-trigger-delay-ms = <200>;
			linux,blink-delay-on-ms = <100>;
			linux,blink-delay-off-ms = <1200>;
		};

		led9: led@9 {
			label = "led9";
			reg = <9>;
			led-max-microamp = <10000>;
			linux,default-trigger = "default-on";
		};

		led10: led@10 {
			label = "led10";
			reg = <10>;
			led-max-microamp = <10000>;
			linux,default-trigger = "timer";
			linux,default-trigger-delay-ms = <300>;
			linux,blink-delay-on-ms = <100>;
			linux,blink-delay-off-ms = <1200>;
		};

		led11: led@11 {
			label = "led11";
			reg = <11>;
			led-max-microamp = <10000>;
			linux,default-trigger = "timer";
			linux,default-trigger-delay-ms = <300>;
			linux,blink-delay-on-ms = <100>;
			linux,blink-delay-off-ms = <1200>;
		};

		led12: led@12 {
			label = "led12";
			reg = <12>;
			led-max-microamp = <10000>;
			linux,default-trigger = "default-on";
		};

		led13: led@13 {
			label = "led13";
			reg = <13>;
			led-max-microamp = <10000>;
			linux,default-trigger = "timer";
			linux,default-trigger-delay-ms = <400>;
			linux,blink-delay-on-ms = <100>;
			linux,blink-delay-off-ms = <1200>;
		};

		led14: led@14 {
			label = "led14";
			reg = <14>;
			led-max-microamp = <10000>;
			linux,default-trigger = "timer";
			linux,default-trigger-delay-ms = <400>;
			linux,blink-delay-on-ms = <100>;
			linux,blink-delay-off-ms = <1200>;
		};

		led15: led@15 {
			label = "led15";
			reg = <15>;
			led-max-microamp = <10000>;
			linux,default-trigger = "default-on";
		};

		led16: led@16 {
			label = "led16";
			reg = <16>;
			led-max-microamp = <10000>;
			linux,default-trigger = "timer";
			linux,default-trigger-delay-ms = <500>;
			linux,blink-delay-on-ms = <100>;
			linux,blink-delay-off-ms = <1200>;
		};

		led17: led@17 {
			label = "led17";
			reg = <17>;
			led-max-microamp = <10000>;
			linux,default-trigger = "timer";
			linux,default-trigger-delay-ms = <500>;
			linux,blink-delay-on-ms = <100>;
			linux,blink-delay-off-ms = <1200>;
		};

		led18: led@18 {
			label = "led18";
			reg = <18>;
			led-max-microamp = <10000>;
			linux,default-trigger = "default-on";
		};

		led19: led@19 {
			label = "led19";
			reg = <19>;
			led-max-microamp = <10000>;
			linux,default-trigger = "timer";
			linux,default-trigger-delay-ms = <600>;
			linux,blink-delay-on-ms = <100>;
			linux,blink-delay-off-ms = <1200>;
		};

		led20: led@20 {
			label = "led20";
			reg = <20>;
			led-max-microamp = <10000>;
			linux,default-trigger = "timer";
			linux,default-trigger-delay-ms = <600>;
			linux,blink-delay-on-ms = <100>;
			linux,blink-delay-off-ms = <1200>;
		};

		led21: led@21 {
			label = "led21";
			reg = <21>;
			led-max-microamp = <10000>;
			linux,default-trigger = "default-on";
		};

		led22: led@22 {
			label = "led22";
			reg = <22>;
			led-max-microamp = <10000>;
			linux,default-trigger = "timer";
			linux,default-trigger-delay-ms = <700>;
			linux,blink-delay-on-ms = <100>;
			linux,blink-delay-off-ms = <1200>;
		};

		led23: led@23 {
			label = "led23";
			reg = <23>;
			led-max-microamp = <10000>;
			linux,default-trigger = "timer";
			linux,default-trigger-delay-ms = <700>;
			linux,blink-delay-on-ms = <100>;
			linux,blink-delay-off-ms = <1200>;
		};

		led124: led@24 {
			label = "led24";
			reg = <24>;
			led-max-microamp = <10000>;
			linux,default-trigger = "default-on";
		};

		led25: led@25 {
			label = "led25";
			reg = <25>;
			led-max-microamp = <10000>;
			linux,default-trigger = "timer";
			linux,default-trigger-delay-ms = <800>;
			linux,blink-delay-on-ms = <100>;
			linux,blink-delay-off-ms = <1200>;
		};

		led26: led@26 {
			label = "led26";
			reg = <26>;
			led-max-microamp = <10000>;
			linux,default-trigger = "timer";
			linux,default-trigger-delay-ms = <800>;
			linux,blink-delay-on-ms = <100>;
			linux,blink-delay-off-ms = <1200>;
		};

		led27: led@27 {
			label = "led27";
			reg = <27>;
			led-max-microamp = <10000>;
			linux,default-trigger = "default-on";
		};

		led28: led@28 {
			label = "led28";
			reg = <28>;
			led-max-microamp = <10000>;
			linux,default-trigger = "timer";
			linux,default-trigger-delay-ms = <900>;
			linux,blink-delay-on-ms = <100>;
			linux,blink-delay-off-ms = <1200>;
		};

		led29: led@29 {
			label = "led29";
			reg = <29>;
			led-max-microamp = <10000>;
			linux,default-trigger = "timer";
			linux,default-trigger-delay-ms = <900>;
			linux,blink-delay-on-ms = <100>;
			linux,blink-delay-off-ms = <1200>;
		};

		led30: led@30 {
			label = "led30";
			reg = <30>;
			led-max-microamp = <10000>;
			linux,default-trigger = "default-on";
		};

		led31: led@31 {
			label = "led31";
			reg = <31>;
			led-max-microamp = <10000>;
			linux,default-trigger = "timer";
			linux,default-trigger-delay-ms = <1000>;
			linux,blink-delay-on-ms = <100>;
			linux,blink-delay-off-ms = <1200>;
		};

		led32: led@32 {
			label = "led32";
			reg = <32>;
			led-max-microamp = <10000>;
			linux,default-trigger = "timer";
			linux,default-trigger-delay-ms = <1000>;
			linux,blink-delay-on-ms = <100>;
			linux,blink-delay-off-ms = <1200>;
		};

		led33: led@33 {
			label = "led33";
			reg = <33>;
			led-max-microamp = <10000>;
			linux,default-trigger = "default-on";
		};

		led34: led@34 {
			label = "led34";
			reg = <34>;
			led-max-microamp = <10000>;
			linux,default-trigger = "timer";
			linux,default-trigger-delay-ms = <1100>;
			linux,blink-delay-on-ms = <100>;
			linux,blink-delay-off-ms = <1200>;
		};

		led35: led@35 {
			label = "led35";
			reg = <35>;
			led-max-microamp = <10000>;
			linux,default-trigger = "timer";
			linux,default-trigger-delay-ms = <1100>;
			linux,blink-delay-on-ms = <100>;
			linux,blink-delay-off-ms = <1200>;
		};

		led36: led@36 {
			label = "led36";
			reg = <36>;
			led-max-microamp = <10000>;
			linux,default-trigger = "default-on";
		};
	};

	ls_stk3410: light@48 {
		compatible = "ls_stk3410";
		status = "okay";
		reg = <0x48>;
		type = <SENSOR_TYPE_LIGHT>;
		irq_enable = <0>;
		als_threshold_high = <100>;
		als_threshold_low = <10>;
		als_ctrl_gain = <2>; /* 0:x1 1:x4 2:x16 3:x64 */
		poll_delay_ms = <100>;
	};

	ps_stk3410: proximity@48 {
		compatible = "ps_stk3410";
		status = "okay";
		reg = <0x48>;
		type = <SENSOR_TYPE_PROXIMITY>;
		//pinctrl-names = "default";
		//pinctrl-0 = <&gpio2_c3>;
		//irq-gpio = <&gpio0 RK_PB7 IRQ_TYPE_LEVEL_LOW>;
		//irq_enable = <1>;
		ps_threshold_high = <0x200>;
		ps_threshold_low = <0x100>;
		ps_ctrl_gain = <3>; /* 0:x1 1:x4 2:x16 3:x64 */
		ps_led_current = <3>; /* 0:12.5mA 1:25mA 2:50mA 3:100mA */
		poll_delay_ms = <100>;
	};

};

&i2c2 {
	status = "okay";

	clock-frequency = <100000>;

	/* These are relatively safe rise/fall times; TODO: measure */
	i2c-scl-falling-time-ns = <50>;
	i2c-scl-rising-time-ns = <300>;

	ov5695: ov5695@36 {
		compatible = "ovti,ov5695";
		reg = <0x36>;
		clocks = <&cru SCLK_CIF_OUT>;
		clock-names = "xvclk";
		/*reset-gpios = <&gpio2 14 GPIO_ACTIVE_HIGH>;*/
		pwdn-gpios = <&gpio2 14 GPIO_ACTIVE_HIGH>;
		//pinctrl-names = "default";
		//pinctrl-0 = <&cif_clkout_m0>;
		rockchip,camera-module-index = <0>;
		rockchip,camera-module-facing = "back";
		rockchip,camera-module-name = "TongJu";
		rockchip,camera-module-lens-name = "CHT842-MD";
		port {
			ov5695_out: endpoint {
				remote-endpoint = <&mipi_in>;
				data-lanes = <1 2>;
			};
		};
	};
};

&i2s0_8ch {
	status = "okay";
	#sound-dai-cells = <0>;
	rockchip,no-dmaengine;
};

&i2s1_2ch {
	status = "okay";
	#sound-dai-cells = <0>;
	pinctrl-0 = <&i2s1_2ch_sclk
		     &i2s1_2ch_lrck
		     &i2s1_2ch_sdo>;
};

&i2s2_2ch {
	status = "okay";
	rockchip,bclk-fs = <64>;
	#sound-dai-cells = <0>;
};

&io_domains {
	status = "okay";

	vccio1-supply = <&vcc1v8_soc>;
	vccio2-supply = <&vccio_sd>;
	vccio3-supply = <&vcc1v8_dvp>;
	vccio4-supply = <&vcc1v8_soc>;
	vccio5-supply = <&vcc_3v0>;
};

&isp_mmu {
	status = "okay";
};

&nandc0 {
	status = "okay";
};

&pdm {
	status = "okay";
	#sound-dai-cells = <0>;
	rockchip,no-dmaengine;
	pinctrl-names = "default";
	pinctrl-0 = <&pdm_clk0m1
		&pdm_sdi0m1>;
};

&pinctrl {
	pinctrl-names = "default";
	pinctrl-0 = <&tp_int>;

	headphone {
		hp_det: hp-det {
			rockchip,pins = <3 RK_PA4 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	pmic {
		pmic_int: pmic_int {
			rockchip,pins =
				<0 RK_PB2 RK_FUNC_GPIO &pcfg_pull_up>;
		};

		soc_slppin_gpio: soc_slppin_gpio {
			rockchip,pins =
				<0 RK_PA4 RK_FUNC_GPIO &pcfg_output_low>;
		};

		soc_slppin_slp: soc_slppin_slp {
			rockchip,pins =
				<0 RK_PA4 1 &pcfg_pull_none>;
		};

		soc_slppin_rst: soc_slppin_rst {
			rockchip,pins =
				<0 RK_PA4 2 &pcfg_pull_none>;
		};
	};

	sdio-pwrseq {
		wifi_enable_h: wifi-enable-h {
			rockchip,pins = <0 RK_PA2 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	touchscreen-int {
		tp_int: tp-int {
			rockchip,pins = <0 RK_PB3 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};
};

&pmu_io_domains {
	status = "okay";

	pmuio1-supply = <&vcc3v0_pmu>;
	pmuio2-supply = <&vcc3v0_pmu>;
};

&pwm1 {
	status = "okay";
};

&rk_rga {
	status = "okay";
};

&rockchip_suspend {
	status = "okay";
	rockchip,sleep-debug-en = <1>;
};

&saradc {
	status = "okay";
	vref-supply = <&vcc1v8_soc>;
};

&sdmmc {
	bus-width = <4>;
	cap-mmc-highspeed;
	cap-sd-highspeed;
	no-sdio;
	no-mmc;
	card-detect-delay = <800>;
	ignore-pm-notify;
	/*cd-gpios = <&gpio2 4 GPIO_ACTIVE_HIGH>; [> CD GPIO <]*/
	sd-uhs-sdr12;
	sd-uhs-sdr25;
	sd-uhs-sdr50;
	sd-uhs-sdr104;
	vqmmc-supply = <&vccio_sd>;
	vmmc-supply = <&vcc_sd>;
	status = "okay";
};

&sdio {
	bus-width = <4>;
	cap-sd-highspeed;
	no-sd;
	no-mmc;
	ignore-pm-notify;
	keep-power-in-suspend;
	non-removable;
	mmc-pwrseq = <&sdio_pwrseq>;
	sd-uhs-sdr104;
	status = "okay";
};

&tsadc {
	pinctrl-names = "gpio", "otpout";
	pinctrl-0 = <&tsadc_otp_gpio>;
	pinctrl-1 = <&tsadc_otp_out>;
	status = "okay";
};

&u2phy {
	status = "okay";

	u2phy_host: host-port {
		status = "okay";
	};

	u2phy_otg: otg-port {
		vbus-supply = <&vcc5v0_host>;
		status = "okay";
	};
};

&usb20_otg {
	status = "okay";
};

&uart1 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart1_xfer &uart1_cts>;
	status = "okay";
};

&vopb {
	status = "okay";
};

&vopb_mmu {
	status = "okay";
};

&vopl {
	status = "okay";
};

&vopl_mmu {
	status = "okay";
};

&mpp_srv {
	status = "okay";
};

&vdpu {
	status = "okay";
};

&vepu {
	status = "okay";
};

&vpu_mmu {
	status = "okay";
};

&hevc {
	status = "okay";
};

&hevc_mmu {
	status = "okay";
};

&mipi_dphy_rx0 {
	status = "okay";

	ports {
		#address-cells = <1>;
		#size-cells = <0>;

		port@0 {
			reg = <0>;
			#address-cells = <1>;
			#size-cells = <0>;

			mipi_in: endpoint@1 {
				reg = <1>;
				remote-endpoint = <&ov5695_out>;
				data-lanes = <1 2>;
			};
		};

		port@1 {
			reg = <1>;
			#address-cells = <1>;
			#size-cells = <0>;

			dphy_rx_out: endpoint@0 {
				reg = <0>;
				remote-endpoint = <&isp_mipi_in>;
			};
		};
	};
};

&rkisp1 {
	status = "okay";
	pinctrl-names = "default";
	pinctrl-0 = <&cif_clkout_m0 &dvp_d0d1_m0 &dvp_d2d9_m0>;
	port {
		#address-cells = <1>;
		#size-cells = <0>;

		isp_mipi_in: endpoint@0 {
			reg = <0>;
			remote-endpoint = <&dphy_rx_out>;
		};

	};
};
