// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Copyright (c) 2020 Rockchip Electronics Co., Ltd.
 */

/dts-v1/;
#include <dt-bindings/input/input.h>
#include <dt-bindings/pwm/pwm.h>
#include <dt-bindings/sensor-dev.h>
#include "rk3368.dtsi"
#include "rk3368-android.dtsi"
/ {
	model = "Rockchip rk3368a tablet rk817 board";
	compatible = "rockchip,tablet", "rockchip,rk3368a", "rockchip,rk3368";

	adc_keys: adc-keys {
		compatible = "adc-keys";
		io-channels = <&saradc 1>;
		io-channel-names = "buttons";
		keyup-threshold-microvolt = <1024000>;
		poll-interval = <100>;

		vol-up-key {
			label = "volume up";
			linux,code = <KEY_VOLUMEUP>;
			press-threshold-microvolt = <1000>;
		};

		vol-down-key {
			label = "volume down";
			linux,code = <KEY_VOLUMEDOWN>;
			press-threshold-microvolt = <170000>;
		};
	};

	backlight: backlight {
		compatible = "pwm-backlight";
		pwms = <&pwm0 0 25000 1>;
		brightness-levels = <
			 30  30  30  31  31  31  32  32
			 32  33  33  33  34  34  34  35
			 35  35  36  36  36  37  37  37
			 38  38  38  39  39  39  40  40
			 40  41  41  41  42  42  42  43
			 43  43  44  44  44  45  46  47
			 48  49  50  51  52  53  54  55
			 56  57  58  59  60  61  62  63
			 64  65  66  67  68  69  70  71
			 72  73  74  75  76  77  78  79
			 80  81  82  83  84  85  86  87
			 88  89  90  91  92  93  94  95
			 96  97  98  99 100 101 102 103
			104 105 106 107 108 109 110 111
			112 113 114 115 116 117 118 119
			120 121 122 123 124 125 126 127
			128 129 130 131 132 133 134 135
			136 137 138 139 140 141 142 143
			144 145 146 147 148 149 150 151
			152 153 154 155 156 157 158 159
			160 161 162 163 164 165 166 167
			168 169 170 171 172 173 174 175
			176 177 178 179 180 181 182 183
			184 185 186 187 188 189 190 191
			192 193 194 195 196 197 198 199
			200 201 202 203 204 205 206 207
			208 209 210 211 212 213 214 215
			216 217 218 219 220 221 222 223
			224 225 226 227 228 229 230 231
			232 232 232 233 233 233 234 234
			234 235 235 235 236 236 236 237
			237 238 238 239 239 240 240 240>;
		default-brightness-level = <200>;
		enable-gpios = <&gpio3 28 GPIO_ACTIVE_HIGH>;
	};

	charge-animation {
		compatible = "rockchip,uboot-charge";
		rockchip,uboot-charge-on = <1>;
		rockchip,android-charge-on = <0>;
		rockchip,uboot-low-power-voltage = <3400>;
		rockchip,screen-on-voltage = <3400>;
		status = "okay";
	};

	chosen: chosen {
		bootargs = "earlycon=uart8250,mmio32,0xff690000 console=ttyFIQ0 androidboot.baseband=N/A androidboot.veritymode=enforcing androidboot.hardware=rk30board androidboot.console=ttyFIQ0 init=/init kpti=0";
	};

	rk817-sound {
		compatible = "simple-audio-card";
		simple-audio-card,format = "i2s";
		simple-audio-card,name = "rockchip-rk817-codec";
		simple-audio-card,mclk-fs = <256>;
		simple-audio-card,widgets =
			"Microphone", "Mic Jack",
			"Headphone", "Headphone Jack";
		simple-audio-card,routing =
			"Mic Jack", "MICBIAS1",
			"IN1P", "Mic Jack",
			"Headphone Jack", "HPOL",
			"Headphone Jack", "HPOR";
		simple-audio-card,cpu {
			sound-dai = <&i2s_8ch>;
		};
		simple-audio-card,codec {
			sound-dai = <&rk817_codec>;
		};
	};

	rk_headset: rk-headset {
		compatible = "rockchip_headset";
		headset_gpio = <&gpio0 RK_PC7 GPIO_ACTIVE_LOW>;
		pinctrl-names = "default";
		pinctrl-0 = <&hp_det>;
		io-channels = <&saradc 2>;
	};

	sdio_pwrseq: sdio-pwrseq {
		compatible = "mmc-pwrseq-simple";
		pinctrl-names = "default";
		pinctrl-0 = <&wifi_enable_h>;

		/*
		 * On the module itself this is one of these (depending
		 * on the actual card populated):
		 * - SDIO_RESET_L_WL_REG_ON
		 * - PDN (power down when low)
		 */
		reset-gpios = <&gpio3 4 GPIO_ACTIVE_LOW>; /* GPIO3_A4 */
	};

	vccsys: vccsys {
		compatible = "regulator-fixed";
		regulator-name = "vcc3v8_sys";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <3800000>;
		regulator-max-microvolt = <3800000>;
	};

	wireless-wlan {
		compatible = "wlan-platdata";
		/* wifi_chip_type - wifi chip define
		* ap6210, ap6330, ap6335
		* rtl8188eu, rtl8723bs, rtl8723bu
		* esp8089
		*/
		wifi_chip_type = "rtl8723bs";
		WIFI,vbat_gpio = <&gpio0 2 GPIO_ACTIVE_HIGH>;
		WIFI,host_wake_irq = <&gpio3 6 GPIO_ACTIVE_HIGH>;
		status = "okay";
	};

	wireless-bluetooth {
		compatible = "bluetooth-platdata";
		uart_rts_gpios = <&gpio2 27 GPIO_ACTIVE_LOW>;
		pinctrl-names = "default","rts_gpio";
		pinctrl-0 = <&uart0_rts>;
		pinctrl-1 = <&uart0_rts_gpio>;

		//BT,power_gpio = <&gpio3 3 GPIO_ACTIVE_HIGH>;
		BT,reset_gpio = <&gpio3 13 GPIO_ACTIVE_HIGH>;
		BT,wake_gpio = <&gpio3 2 GPIO_ACTIVE_HIGH>;
		BT,wake_host_irq = <&gpio3 7 GPIO_ACTIVE_HIGH>;

		status = "okay";
	};

	vcc_sys: vcc-sys {
		compatible = "regulator-fixed";
		regulator-name = "vcc_sys";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <3800000>;
		regulator-max-microvolt = <3800000>;
	};

	vcc_host: vcc-host {
		compatible = "regulator-fixed";
		enable-active-high;
		gpio = <&gpio0 4 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&host_vbus_drv>;
		regulator-name = "vcc_host";
		regulator-always-on;
	};

	xin32k: xin32k {
		compatible = "fixed-clock";
		clock-frequency = <32768>;
		clock-output-names = "xin32k";
		#clock-cells = <0>;
	};

};

&cif_clkout {
	/* cif_clkout */
	rockchip,pins = <1 RK_PB3 1 &pcfg_pull_none_4ma>;
};

&cpu_l0 {
	cpu-supply = <&vdd_cpu>;
};

&cpu_l1 {
	cpu-supply = <&vdd_cpu>;
};

&cpu_l2 {
	cpu-supply = <&vdd_cpu>;
};

&cpu_l3 {
	cpu-supply = <&vdd_cpu>;
};

&cpu_b0 {
	cpu-supply = <&vdd_cpu>;
};

&cpu_b1 {
	cpu-supply = <&vdd_cpu>;
};

&cpu_b2 {
	cpu-supply = <&vdd_cpu>;
};

&cpu_b3 {
	cpu-supply = <&vdd_cpu>;
};

&gpu {
	logic-supply = <&vdd_logic>;
};

&dsi {
	status = "okay";
	//rockchip,lane-rate = <500>;

	panel:panel@0 {
		compatible = "simple-panel-dsi";
		reg = <0>;
		backlight = <&backlight>;
		enable-gpios = <&gpio0 RK_PC6 GPIO_ACTIVE_HIGH>;
		prepare-delay-ms = <20>;
		reset-delay-ms = <20>;
		init-delay-ms = <20>;
		enable-delay-ms = <120>;
		disable-delay-ms = <20>;
		unprepare-delay-ms = <20>;

		width-mm = <135>;
		height-mm = <216>;

		dsi,flags = <(MIPI_DSI_MODE_VIDEO | MIPI_DSI_MODE_VIDEO_BURST |
			      MIPI_DSI_MODE_LPM | MIPI_DSI_MODE_EOT_PACKET)>;
		dsi,format = <MIPI_DSI_FMT_RGB888>;
		dsi,lanes = <4>;

		panel-init-sequence = [
			39 00 04 FF 98 81 03
			15 00 02 01 00
			15 00 02 02 00
			15 00 02 03 53
			15 00 02 04 00
			15 00 02 05 00
			15 00 02 06 08
			15 00 02 07 00
			15 00 02 08 00
			15 00 02 09 00
			15 00 02 0A 00
			15 00 02 0B 00
			15 00 02 0C 00
			15 00 02 0D 00
			15 00 02 0E 00
			15 00 02 0F 26
			15 00 02 10 26
			15 00 02 11 00
			15 00 02 12 00
			15 00 02 13 00
			15 00 02 14 00
			15 00 02 15 00
			15 00 02 16 00
			15 00 02 17 00
			15 00 02 18 00
			15 00 02 19 00
			15 00 02 1A 00
			15 00 02 1B 00
			15 00 02 1C 00
			15 00 02 1D 00
			15 00 02 1E 40
			15 00 02 1F C0
			15 00 02 20 06
			15 00 02 21 01
			15 00 02 22 07
			15 00 02 23 00
			15 00 02 24 8A
			15 00 02 25 8A
			15 00 02 26 00
			15 00 02 27 00
			15 00 02 28 33
			15 00 02 29 33
			15 00 02 2A 00
			15 00 02 2B 00
			15 00 02 2C 08
			15 00 02 2D 08
			15 00 02 2E 0B
			15 00 02 2F 0B
			15 00 02 30 00
			15 00 02 31 00
			15 00 02 32 42
			15 00 02 33 00
			15 00 02 34 00
			15 00 02 35 0A
			15 00 02 36 00
			15 00 02 37 08
			15 00 02 38 3C
			15 00 02 39 00
			15 00 02 3A 00
			15 00 02 3B 00
			15 00 02 3C 00
			15 00 02 3D 00
			15 00 02 3E 00
			15 00 02 3F 00
			15 00 02 40 00
			15 00 02 41 00
			15 00 02 42 00
			15 00 02 43 08
			15 00 02 44 00
			15 00 02 50 01
			15 00 02 51 23
			15 00 02 52 45
			15 00 02 53 67
			15 00 02 54 89
			15 00 02 55 AB
			15 00 02 56 01
			15 00 02 57 23
			15 00 02 58 45
			15 00 02 59 67
			15 00 02 5A 89
			15 00 02 5B AB
			15 00 02 5C CD
			15 00 02 5D EF
			15 00 02 5E 00
			15 00 02 5F 01
			15 00 02 60 01
			15 00 02 61 06
			15 00 02 62 06
			15 00 02 63 06
			15 00 02 64 06
			15 00 02 65 00
			15 00 02 66 00
			15 00 02 67 17
			15 00 02 68 02
			15 00 02 69 16
			15 00 02 6A 16
			15 00 02 6B 02
			15 00 02 6C 0D
			15 00 02 6D 0D
			15 00 02 6E 0C
			15 00 02 6F 0C
			15 00 02 70 0F
			15 00 02 71 0F
			15 00 02 72 0E
			15 00 02 73 0E
			15 00 02 74 02
			15 00 02 75 01
			15 00 02 76 01
			15 00 02 77 06
			15 00 02 78 06
			15 00 02 79 06
			15 00 02 7A 06
			15 00 02 7B 00
			15 00 02 7C 00
			15 00 02 7D 17
			15 00 02 7E 02
			15 00 02 7F 16
			15 00 02 80 16
			15 00 02 81 02
			15 00 02 82 0D
			15 00 02 83 0D
			15 00 02 84 0C
			15 00 02 85 0C
			15 00 02 86 0F
			15 00 02 87 0F
			15 00 02 88 0E
			15 00 02 89 0E
			15 00 02 8A 02
			39 00 04 FF 98 81 04
			15 00 02 6E 2B
			15 00 02 6F 35
			15 00 02 3A A4
			15 00 02 8D 1A
			15 00 02 87 BA
			15 00 02 B2 D1
			15 00 02 88 0B
			15 00 02 38 01
			15 00 02 39 00
			15 00 02 B5 07
			15 00 02 31 75
			15 00 02 3B 98
			39 00 04 FF 98 81 01
			15 00 02 22 0A
			15 00 02 31 00
			15 00 02 53 40
			15 00 02 55 40
			15 00 02 50 95
			15 00 02 51 90
			15 00 02 60 22
			15 00 02 62 20
			15 00 02 A0 00
			15 00 02 A1 1B
			15 00 02 A2 2A
			15 00 02 A3 14
			15 00 02 A4 17
			15 00 02 A5 2B
			15 00 02 A6 1F
			15 00 02 A7 20
			15 00 02 A8 93
			15 00 02 A9 1E
			15 00 02 AA 2A
			15 00 02 AB 7E
			15 00 02 AC 1B
			15 00 02 AD 19
			15 00 02 AE 4C
			15 00 02 AF 22
			15 00 02 B0 28
			15 00 02 B1 4B
			15 00 02 B2 59
			15 00 02 B3 23
			15 00 02 C0 00
			15 00 02 C1 1B
			15 00 02 C2 2A
			15 00 02 C3 14
			15 00 02 C4 17
			15 00 02 C5 2B
			15 00 02 C6 1F
			15 00 02 C7 20
			15 00 02 C8 93
			15 00 02 C9 1E
			15 00 02 CA 2A
			15 00 02 CB 7E
			15 00 02 CC 1B
			15 00 02 CD 19
			15 00 02 CE 4C
			15 00 02 CF 22
			15 00 02 D0 28
			15 00 02 D1 4B
			15 00 02 D2 59
			15 00 02 D3 23
			//39 00 04 FF 98 81 04
			//05 00 02 2D 80
			//05 00 02 2F 31
			39 00 04 FF 98 81 00
			05 78 01 11
			05 14 01 29
			15 00 02 35 00
		];

		panel-exit-sequence = [
			05 00 01 28
			05 00 01 10
		];

		display-timings {
			native-mode = <&timing0>;

			timing0: timing0 {
				clock-frequency = <78000000>;
				hactive = <800>;
				vactive = <1280>;
				hfront-porch = <60>;//70 //16
				hsync-len = <30>; //20 //5
				hback-porch = <60>; //59
				vfront-porch = <20>; //16 //8
				vsync-len = <8>; //5
				vback-porch = <16>; //22 //3
				hsync-active = <0>;
				vsync-active = <0>;
				de-active = <0>;
				pixelclk-active = <0>;
			};
		};
	};
};

&dfi {
	status = "okay";
};

&dmc {
	status = "okay";
	center-supply = <&vdd_logic>;
	devfreq-events = <&dfi>;
	upthreshold = <60>;
	downdifferential = <20>;
	system-status-freq = <
		/*system status		freq(KHz)*/
		SYS_STATUS_NORMAL	600000
		SYS_STATUS_REBOOT	600000
		SYS_STATUS_SUSPEND	240000
		SYS_STATUS_VIDEO_1080P	396000
		SYS_STATUS_VIDEO_4K	600000
		SYS_STATUS_PERFORMANCE	600000
		SYS_STATUS_BOOST	396000
		SYS_STATUS_DUALVIEW	600000
		SYS_STATUS_ISP		528000
	>;
	vop-bw-dmc-freq = <
	/* min_bw(MB/s) max_bw(MB/s) freq(KHz) */
		0       582      240000
		583     99999    396000
	>;
	vop-dclk-mode = <1>;
	auto-min-freq = <240000>;
	auto-freq-en = <0>;
};

&emmc {
	bus-width = <8>;
	cap-mmc-highspeed;
	mmc-hs200-1_8v;
	no-sdio;
	no-sd;
	disable-wp;
	non-removable;
	num-slots = <1>;
	status = "okay";
};

&i2c0 {
	status = "okay";

	vdd_cpu: syr827@40 {
		compatible = "silergy,syr827";
		status = "okay";
		reg = <0x40>;

		regulator-compatible = "fan53555-reg";
		regulator-name = "vdd_cpu";
		regulator-min-microvolt = <712500>;
		regulator-max-microvolt = <1500000>;
		regulator-ramp-delay = <1000>;
		fcs,suspend-voltage-selector = <1>;
		pinctrl-0 = <&vsel_gpio>;
		vsel-gpios = <&gpio0 0 GPIO_ACTIVE_HIGH>;
		regulator-always-on;
		regulator-boot-on;
		regulator-initial-state = <3>;
		regulator-state-mem {
			regulator-off-in-suspend;
		};
	};

	rk817: pmic@20 {
		compatible = "rockchip,rk817";
		reg = <0x20>;
		interrupt-parent = <&gpio0>;
		interrupts = <1 IRQ_TYPE_LEVEL_LOW>;
		pinctrl-names = "default", "pmic-sleep",
				"pmic-power-off", "pmic-reset";
		pinctrl-0 = <&pmic_int>;
		pinctrl-1 = <&soc_slppin_slp>, <&rk817_slppin_slp>;
		pinctrl-2 = <&soc_slppin_gpio>, <&rk817_slppin_pwrdn>;
		pinctrl-3 = <&soc_slppin_slp>, <&rk817_slppin_slp>;
		rockchip,system-power-controller;
		wakeup-source;
		#clock-cells = <1>;
		clock-output-names = "rk808-clkout1", "rk808-clkout2";
		//fb-inner-reg-idxs = <2>;
		/* 1: rst regs (default in codes), 0: rst the pmic */
		pmic-reset-func = <1>;

		vcc1-supply = <&vccsys>;
		vcc2-supply = <&vccsys>;
		vcc3-supply = <&vccsys>;
		vcc4-supply = <&vccsys>;
		vcc5-supply = <&vccsys>;
		vcc6-supply = <&vccsys>;
		vcc7-supply = <&vcc_io>;
		vcc8-supply = <&vccsys>;
		vcc9-supply = <&dcdc_boost>;

		pwrkey {
			status = "okay";
		};

		pinctrl_rk8xx: pinctrl_rk8xx {
			gpio-controller;
			#gpio-cells = <2>;

			rk817_ts_gpio1: rk817_ts_gpio1 {
				pins = "gpio_ts";
				function = "pin_fun1";
				/* output-low; */
				/* input-enable; */
			};

			rk817_gt_gpio2: rk817_gt_gpio2 {
				pins = "gpio_gt";
				function = "pin_fun1";
			};

			rk817_pin_ts: rk817_pin_ts {
				pins = "gpio_ts";
				function = "pin_fun0";
			};

			rk817_pin_gt: rk817_pin_gt {
				pins = "gpio_gt";
				function = "pin_fun0";
			};

			rk817_slppin_null: rk817_slppin_null {
				pins = "gpio_slp";
				function = "pin_fun0";
			};

			rk817_slppin_slp: rk817_slppin_slp {
				pins = "gpio_slp";
				function = "pin_fun1";
			};

			rk817_slppin_pwrdn: rk817_slppin_pwrdn {
				pins = "gpio_slp";
				function = "pin_fun2";
			};

			rk817_slppin_rst: rk817_slppin_rst {
				pins = "gpio_slp";
				function = "pin_fun3";
			};
		};

		regulators {
			vdd_logic: DCDC_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <950000>;
				regulator-max-microvolt = <1350000>;
				regulator-ramp-delay = <6001>;
				regulator-initial-mode = <0x2>;
				regulator-name = "vdd_logic";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <950000>;
				};
			};

			vcc_3v3: DCDC_REG2 {
				regulator-name = "vcc_3v3";
				regulator-always-on;
				regulator-boot-on;
				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};

			vcc_ddr: DCDC_REG3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-initial-mode = <0x2>;
				regulator-name = "vcc_ddr";
				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};

			vcc_io: DCDC_REG4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vcc_io";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vcc_1v0: LDO_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <1000000>;
				regulator-name = "vcc_1v0";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1000000>;
				};
			};

			vcc1v8_soc: LDO_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;

				regulator-name = "vcc1v8_soc";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vdd1v0_soc: LDO_REG3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <1000000>;

				regulator-name = "vcc1v0_soc";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1000000>;
				};
			};

			vcc3v3_pmu: LDO_REG4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;

				regulator-name = "vcc3v3_pmu";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;

				};
			};

			vccio_sd: LDO_REG5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;

				regulator-name = "vccio_sd";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vcc_sd: LDO_REG6 {
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;

				regulator-name = "vcc_sd";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;

				};
			};

			vcc2v8_dvp: LDO_REG7 {
				regulator-boot-on;
				regulator-min-microvolt = <2800000>;
				regulator-max-microvolt = <2800000>;

				regulator-name = "vcc2v8_dvp";
				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <2800000>;
				};
			};

			vcc1v8_dvp: LDO_REG8 {
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;

				regulator-name = "vcc1v8_dvp";
				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vdd1v5_dvp: LDO_REG9 {
				regulator-boot-on;
				regulator-min-microvolt = <1500000>;
				regulator-max-microvolt = <1500000>;

				regulator-name = "vdd1v5_dvp";
				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <1500000>;
				};
			};

			dcdc_boost: BOOST {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <5000000>;
				regulator-max-microvolt = <5000000>;
				regulator-name = "boost";
			};

			otg_switch: OTG_SWITCH {
				regulator-name = "otg_switch";
			};
		};

		battery {
			compatible = "rk817,battery";
			ocv_table = <3500 3548 3592 3636 3687 3740 3780
				3806 3827 3846 3864 3889 3929 3964
				3993 4015 4030 4041 4056 4076 4148>;
			design_capacity = <5000>;
			design_qmax = <5500>;
			bat_res = <100>;
			sleep_enter_current = <150>;
			sleep_exit_current = <180>;
			sleep_filter_current = <100>;
			power_off_thresd = <3400>;
			zero_algorithm_vol = <3850>;
			max_soc_offset = <60>;
			monitor_sec = <5>;
			sample_res = <10>;
			virtual_power = <0>;
		};

		charger {
			compatible = "rk817,charger";
			min_input_voltage = <4500>;
			max_input_current = <1500>;
			max_chrg_current = <2000>;
			max_chrg_voltage = <4200>;
			chrg_term_mode = <0>;
			chrg_finish_cur = <300>;
			virtual_power = <0>;
			dc_det_adc = <0>;
			extcon = <&u2phy>;
		};

		rk817_codec: codec {
			#sound-dai-cells = <0>;
			compatible = "rockchip,rk817-codec";
			clocks = <&cru SCLK_I2S_8CH_OUT>;
			clock-names = "mclk";
			pinctrl-names = "default";
			pinctrl-0 = <&i2s_8ch_mclk>;
			hp-volume = <20>;
			spk-volume = <3>;
			mic-in-differential;
			out-l2spk-r2hp;
			spk-ctl-gpios = <&gpio0 RK_PD3 GPIO_ACTIVE_HIGH>;
			status = "okay";
		};
	};
};

&i2c2 {
	status = "okay";

	ts@40 {
		status = "okay";
		compatible = "GSL,GSL_THZY";
		reg = <0x40>;
		irq_gpio_number = <&gpio0 RK_PB4 IRQ_TYPE_LEVEL_HIGH>;
		rst_gpio_number = <&gpio0 RK_PB3 GPIO_ACTIVE_HIGH>;
	};
};

&i2c3 {
	status = "okay";

	gc032a: gc032a@21 {
		status = "okay";
		compatible = "galaxycore,gc032a";
		reg = <0x21>;
		clocks = <&cru SCLK_VIP_OUT>;
		clock-names = "xvclk";

		avdd-supply = <&vcc2v8_dvp>;
		dovdd-supply = <&vcc1v8_dvp>;
		dvdd-supply = <&vdd1v5_dvp>;

		pwdn-gpios = <&gpio1 RK_PB4 GPIO_ACTIVE_HIGH>;
		rockchip,camera-module-index = <1>;
		rockchip,camera-module-facing = "front";
		rockchip,camera-module-name = "CameraKing";
		rockchip,camera-module-lens-name = "Largan";
		port {
			gc0312_out: endpoint {
				remote-endpoint = <&dvp_in_fcam>;
			};
		};
	};

	gc2145: gc2145@3c {
		status = "okay";
		compatible = "galaxycore,gc2145";
		reg = <0x3c>;
		clocks = <&cru SCLK_VIP_OUT>;
		clock-names = "xvclk";

		avdd-supply = <&vcc2v8_dvp>;
		dovdd-supply = <&vcc1v8_dvp>;
		dvdd-supply = <&vdd1v5_dvp>;

		pwdn-gpios = <&gpio1 RK_PB5 GPIO_ACTIVE_HIGH>;
		reset-gpios = <&gpio3 RK_PC4 GPIO_ACTIVE_LOW>;
		rockchip,camera-module-index = <0>;
		rockchip,camera-module-facing = "back";
		rockchip,camera-module-name = "CameraKing";
		rockchip,camera-module-lens-name = "Largan";
		port {
			gc2145_mipi_out: endpoint {
				remote-endpoint = <&mipi_in_bcam>;
				data-lanes = <1>;
			};
		};
	};

	ov8858: ov8858@36 {
		status = "disabled";
		compatible = "ovti,ov8858";
		reg = <0x36>;
		clocks = <&cru SCLK_VIP_OUT>;
		clock-names = "xvclk";

		avdd-supply = <&vcc2v8_dvp>;
		dovdd-supply = <&vcc1v8_dvp>;
		dvdd-supply = <&vdd1v5_dvp>;

		pwdn-gpios = <&gpio1 RK_PB4 GPIO_ACTIVE_HIGH>;
		reset-gpios = <&gpio0 RK_PB6 GPIO_ACTIVE_HIGH>;
		rockchip,camera-module-index = <0>;
		rockchip,camera-module-facing = "back";
		rockchip,camera-module-name = "CameraKing";
		rockchip,camera-module-lens-name = "Largan-9569A2";
		port {
			ov8858_out: endpoint {
				remote-endpoint = <&mipi_in>;
				data-lanes = <1 2>;
			};
		};
	};
};

&i2c4 {
	status = "okay";

	sensor@26 {
		compatible = "gs_da223";
		reg = <0x26>;
		type = <SENSOR_TYPE_ACCEL>;
		irq_enable = <0>;
		poll_delay_ms = <10>;
		layout = <3>;
	};

	sensor@19 {
		compatible = "gs_sc7a20";
		reg = <0x19>;
		type = <SENSOR_TYPE_ACCEL>;
		irq_enable = <0>;
		poll_delay_ms = <10>;
		layout = <1>;
	};

	mpu6500@68 {
		status = "disabled";
		compatible = "invensense,mpu6500";
		pinctrl-names = "default";
		pinctrl-0 = <&mpu6500_irq_gpio>;
		reg = <0x68>;
		irq-gpio = <&gpio3 14 IRQ_TYPE_EDGE_RISING>;
		mpu-int_config = <0x10>;
		mpu-level_shifter = <0>;
		mpu-orientation = <1 0 0 0 1 0 0 0 1>;
		orientation-x= <1>;
		orientation-y= <0>;
		orientation-z= <1>;
		support-hw-poweroff = <1>;
		mpu-debug = <1>;
	};

	sensor@4c {
		status = "disabled";
		compatible = "gs_mc3230";
		reg = <0x4c>;
		type = <SENSOR_TYPE_ACCEL>;
		irq_enable = <0>;
		poll_delay_ms = <30>;
		layout = <9>;
		reprobe_en = <1>;
		irq-gpio = <&gpio3 RK_PB6 IRQ_TYPE_LEVEL_LOW>;
	};

	sensor@18 {
		status = "gs_mc3230";
		compatible = "gs_sc7a30";
		reg = <0x18>;
		type = <SENSOR_TYPE_ACCEL>;
		irq-gpio = <&gpio3 RK_PB6 IRQ_TYPE_LEVEL_LOW>;
		irq_enable = <0>;
		poll_delay_ms = <30>;
		layout = <6>;
		reprobe_en = <1>;
	};

	sensor@10 {
		status = "gs_mc3230";
		compatible = "light_cm3218";
		pinctrl-names = "default";
		pinctrl-0 = <&cm3218_irq_gpio>;
		reg = <0x10>;
		type = <SENSOR_TYPE_LIGHT>;
		irq-gpio = <&gpio3 15 IRQ_TYPE_EDGE_FALLING>;
		irq_enable = <1>;
		poll_delay_ms = <30>;
	};
};

&i2s_8ch {
	status = "okay";
	rockchip,i2s-broken-burst-len;
	rockchip,playback-channels = <8>;
	rockchip,capture-channels = <2>;
	#sound-dai-cells = <0>;
};

&io_domains {
	status = "okay";

	dvp-supply = <&vcc1v8_dvp>;
	audio-supply = <&vcc_io>;
	gpio30-supply = <&vcc_io>;
	gpio1830-supply = <&vcc_io>;
	sdcard-supply = <&vccio_sd>;
	wifi-supply = <&vcc_3v3>;
};

&isp_dvp_d2d9 {
	rockchip,pins =
			/* cif_data4 ... cif_data9 */
			<1 RK_PA2 1 &pcfg_pull_down>,
			<1 RK_PA3 1 &pcfg_pull_down>,
			<1 RK_PA4 1 &pcfg_pull_down>,
			<1 RK_PA5 1 &pcfg_pull_down>,
			<1 RK_PA6 1 &pcfg_pull_down>,
			<1 RK_PA7 1 &pcfg_pull_down>,
			/* cif_sync, cif_href */
			<1 RK_PB0 1 &pcfg_pull_down>,
			<1 RK_PB1 1 &pcfg_pull_down>,
			/* cif_clkin */
			<1 RK_PB2 1 &pcfg_pull_down>;
};

&isp_dvp_d10d11 {
	rockchip,pins =
			/* cif_data10, cif_data11 */
			<1 RK_PB6 1 &pcfg_pull_down>,
			<1 RK_PB7 1 &pcfg_pull_down>;
};

&isp_mmu {
	status = "okay";
};

&mipi_dphy_rx0 {
	status = "okay";

	ports {
		#address-cells = <1>;
		#size-cells = <0>;

		port@0 {
			reg = <0>;
			#address-cells = <1>;
			#size-cells = <0>;
			mipi_in_bcam: endpoint@0 {
				reg = <0>;
				remote-endpoint = <&gc2145_mipi_out>;
				data-lanes = <1>;
			};

			mipi_in: endpoint@1 {
				reg = <1>;
				remote-endpoint = <&ov8858_out>;
				data-lanes = <1 2>;
			};
		};

		port@1 {
			reg = <1>;
			#address-cells = <1>;
			#size-cells = <0>;

			dphy_rx_out: endpoint@0 {
				reg = <0>;
				remote-endpoint = <&isp_mipi_in>;
			};
		};
	};
};

&nandc0 {
	status = "okay";
};

&pmu_io_domains {
	status = "okay";

	pmu-supply = <&vcc3v3_pmu>;
	vop-supply = <&vcc3v3_pmu>;
};

&pwm0 {
	status = "okay";
};

&pinctrl {

	headphone {
		hp_det: hp-det {
			rockchip,pins = <0 RK_PC7 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	pmic {
		pmic_int: pmic_int {
			rockchip,pins =
				<0 RK_PA1 RK_FUNC_GPIO &pcfg_pull_up>;
		};

		soc_slppin_gpio: soc_slppin_gpio {
			rockchip,pins =
				<0 RK_PA0 RK_FUNC_GPIO &pcfg_output_low>;
		};

		soc_slppin_slp: soc_slppin_slp {
			rockchip,pins =
				<0 RK_PA0 1 &pcfg_pull_none>;
		};

		soc_slppin_rst: soc_slppin_rst {
			rockchip,pins =
				<0 RK_PA0 2 &pcfg_pull_none>;
		};

		vsel_gpio: vsel-gpio {
			rockchip,pins = <0 RK_PA0 RK_FUNC_GPIO &pcfg_pull_down>;
		};
	};

	mpu6500 {
		mpu6500_irq_gpio: mpu6500-irq-gpio {
			rockchip,pins = <3 RK_PB6 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	cm3218 {
		cm3218_irq_gpio: cm3218-irq-gpio {
			rockchip,pins = <3 RK_PB7 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	dc_det {
		dc_irq_gpio: dc-irq-gpio {
			rockchip,pins = <0 RK_PC1 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	pcfg_pull_none_4ma: pcfg-pull-none-4ma {
		bias-disable;
		drive-strength = <4>;
	};

	pcfg_pull_none_smt: pcfg-pull-none-smt {
		bias-disable;
		input-schmitt-enable;
	};

	pcfg_output_high: pcfg-output-high {
		output-high;
	};

	pcfg_output_low: pcfg-output-low {
		output-low;
	};

	pcfg_input_high: pcfg-input-high {
		bias-pull-up;
		input-enable;
	};

	pcfg_input: pcfg-input {
		input-enable;
	};

	sdio-pwrseq {
		wifi_enable_h: wifi-enable-h {
			rockchip,pins = <3 RK_PA4 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	usb2 {
		host_vbus_drv: host-vbus-drv {
			rockchip,pins = <0 RK_PA4 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	wireless-bluetooth {
		uart0_rts_gpio: uart0-rts-gpio {
			rockchip,pins = <2 RK_PD3 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};
};

&rkisp1 {
	status = "okay";
	pinctrl-names = "default";
	pinctrl-0 = <&isp_dvp_d2d9 &isp_dvp_d10d11 &cif_clkout>;
	port {
		#address-cells = <1>;
		#size-cells = <0>;

		dvp_in_fcam: endpoint@0 {
			reg = <0>;
			remote-endpoint = <&gc0312_out>;
		};

		isp_mipi_in: endpoint@1 {
			reg = <1>;
			remote-endpoint = <&dphy_rx_out>;
		};
	};
};

&route_dsi {
	status = "okay";
};

&rockchip_suspend {
	status = "okay";
	Rockchip,sleep-debug-en = <1>;
	rockchip,sleep-mode-config = <
		(0
		| RKPM_SLP_ARMOFF
		| RKPM_SLP_PMU_PLLS_PWRDN
		| RKPM_SLP_PMU_PMUALIVE_32K
		| RKPM_SLP_SFT_PLLS_DEEP
		| RKPM_SLP_PMU_DIS_OSC
		| RKPM_SLP_SFT_PD_NBSCUS
		)
	>;
	rockchip,wakeup-config = <
		(0
		| RKPM_GPIO_WKUP_EN
		| RKPM_USB_WKUP_EN
		| RKPM_CLUSTER_L_WKUP_EN
		)
	>;
};

&saradc {
	status = "okay";
};

&sdmmc {
	clock-frequency = <37500000>;
	clock-freq-min-max = <400000 37500000>;
	no-sdio;
	no-mmc;
	cap-mmc-highspeed;
	cap-sd-highspeed;
	card-detect-delay = <200>;
	disable-wp;
	num-slots = <1>;
	vmmc-supply = <&vcc_sd>;
	pinctrl-names = "default";
	pinctrl-0 = <&sdmmc_clk &sdmmc_cmd &sdmmc_cd &sdmmc_bus4>;
	status = "disabled";
};

&sdio0 {
	max-frequency = <50000000>;
	no-sd;
	no-mmc;
	bus-width = <4>;
	disable-wp;
	cap-sd-highspeed;
	cap-sdio-irq;
	keep-power-in-suspend;
	mmc-pwrseq = <&sdio_pwrseq>;
	non-removable;
	num-slots = <1>;
	pinctrl-names = "default";
	pinctrl-0 = <&sdio0_bus4 &sdio0_cmd &sdio0_clk>;
	rockchip,default-sample-phase = <90>;
	status = "okay";
};

&tsadc {
	tsadc-supply = <&vdd_cpu>;
	status = "okay";
};

&uart0 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart0_xfer &uart0_cts>;
	status = "okay";
};

&u2phy {
	status = "okay";

	u2phy_otg: otg-port {
		status = "okay";
	};

	u2phy_host: host-port {
		phy-supply = <&vcc_host>;
		status = "okay";
	};
};

&usb_host0_ehci {
	status = "okay";
};

&usb_host0_ohci {
	status = "okay";
};

