// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Copyright (c) 2022 Rockchip Electronics Co., Ltd.
 *
 */

/dts-v1/;
#include <dt-bindings/pwm/pwm.h>
#include <dt-bindings/sensor-dev.h>
#include "rk3368.dtsi"
#include "rk3368-android.dtsi"

/ {
	es8316-sound {
		compatible = "simple-audio-card";
		simple-audio-card,format = "i2s";
		simple-audio-card,name = "rockchip,rk-es8316-codec";
		simple-audio-card,mclk-fs = <256>;
		simple-audio-card,widgets =
			"Microphone", "Mic Jack",
			"Headphone", "Headphone Jack";
		simple-audio-card,routing =
			"Mic Jack", "MICBIAS1",
			"IN1P", "Mic Jack",
			"Headphone Jack", "HPOL",
			"Headphone Jack", "HPOR";
		simple-audio-card,cpu {
			sound-dai = <&i2s_8ch>;
		};
		simple-audio-card,codec {
			sound-dai = <&es8316>;
		};
	};

	sdio_pwrseq: sdio-pwrseq {
		compatible = "mmc-pwrseq-simple";
		clocks = <&rk818 1>;
		clock-names = "ext_clock";
		pinctrl-names = "default";
		pinctrl-0 = <&wifi_enable_h>;

		/*
		 * On the module itself this is one of these (depending
		 * on the actual card populated):
		 * - SDIO_RESET_L_WL_REG_ON
		 * - PDN (power down when low)
		 */
		reset-gpios = <&gpio3 4 GPIO_ACTIVE_LOW>; /* GPIO3_A4 */
	};

	backlight: backlight {
		compatible = "pwm-backlight";
		pwms = <&pwm0 0 25000 0>;
		brightness-levels = <
			  0   1   2   3   4   5   6   7
			  8   9  10  11  12  13  14  15
			 16  17  18  19  20  21  22  23
			 24  25  26  27  28  29  30  31
			 32  33  34  35  36  37  38  39
			 40  41  42  43  44  45  46  47
			 48  49  50  51  52  53  54  55
			 56  57  58  59  60  61  62  63
			 64  65  66  67  68  69  70  71
			 72  73  74  75  76  77  78  79
			 80  81  82  83  84  85  86  87
			 88  89  90  91  92  93  94  95
			 96  97  98  99 100 101 102 103
			104 105 106 107 108 109 110 111
			112 113 114 115 116 117 118 119
			120 121 122 123 124 125 126 127
			128 129 130 131 132 133 134 135
			136 137 138 139 140 141 142 143
			144 145 146 147 148 149 150 151
			152 153 154 155 156 157 158 159
			160 161 162 163 164 165 166 167
			168 169 170 171 172 173 174 175
			176 177 178 179 180 181 182 183
			184 185 186 187 188 189 190 191
			192 193 194 195 196 197 198 199
			200 201 202 203 204 205 206 207
			208 209 210 211 212 213 214 215
			216 217 218 219 220 221 222 223
			224 225 226 227 228 229 230 231
			232 233 234 235 236 237 238 239
			240 241 242 243 244 245 246 247
			248 249 250 251 252 253 254 255>;
		default-brightness-level = <200>;
		enable-gpios = <&gpio0 20 GPIO_ACTIVE_HIGH>;
	};

	charge-animation {
		compatible = "rockchip,uboot-charge";
		rockchip,uboot-charge-on = <1>;
		rockchip,android-charge-on = <0>;
		rockchip,uboot-low-power-voltage = <3500>;
		rockchip,screen-on-voltage = <3600>;
		status = "okay";
	};

	rk_key: rockchip-key {
		compatible = "rockchip,key";
		status = "okay";

		io-channels = <&saradc 1>;

		vol-up-key {
			linux,code = <115>;
			label = "volume up";
			rockchip,adc_value = <1>;
		};

		vol-down-key {
			linux,code = <114>;
			label = "volume down";
			rockchip,adc_value = <170>;
		};

		power-key {
			gpios = <&gpio0 2 GPIO_ACTIVE_LOW>;
			linux,code = <116>;
			label = "power";
			gpio-key,wakeup;
		};
	};

	wireless-wlan {
		compatible = "wlan-platdata";
		rockchip,grf = <&grf>;
		/* wifi_chip_type - wifi chip define
		* ap6210, ap6330, ap6335
		* rtl8188eu, rtl8723bs, rtl8723bu
		* esp8089
		*/
		wifi_chip_type = "ap6210";
		sdio_vref = <1800>; //1800mv or 3300mv
		WIFI,host_wake_irq = <&gpio3 6 GPIO_ACTIVE_HIGH>;
		status = "okay";
	};

	wireless-bluetooth {
		compatible = "bluetooth-platdata";
		clocks = <&rk818 1>;
		clock-names = "ext_clock";
		uart_rts_gpios = <&gpio2 27 GPIO_ACTIVE_LOW>;
		pinctrl-names = "default","rts_gpio";
		pinctrl-0 = <&uart0_rts>;
		pinctrl-1 = <&uart0_rts_gpio>;

		//BT,power_gpio = <&gpio3 3 GPIO_ACTIVE_HIGH>;
		BT,reset_gpio = <&gpio3 5 GPIO_ACTIVE_HIGH>;
		BT,wake_gpio = <&gpio3 2 GPIO_ACTIVE_HIGH>;
		BT,wake_host_irq = <&gpio3 7 GPIO_ACTIVE_HIGH>;

		status = "okay";
	};

	vcc_sys: vcc-sys {
		compatible = "regulator-fixed";
		regulator-name = "vcc_sys";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <3800000>;
		regulator-max-microvolt = <3800000>;
	};

	vcc_host: vcc-host {
		compatible = "regulator-fixed";
		enable-active-high;
		gpio = <&gpio0 4 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&host_vbus_drv>;
		regulator-name = "vcc_host";
		regulator-always-on;
	};

	xin32k: xin32k {
		compatible = "fixed-clock";
		clock-frequency = <32768>;
		clock-output-names = "xin32k";
		#clock-cells = <0>;
	};
};

&cpu_l0 {
	cpu-supply = <&syr827>;
};

&cpu_l1 {
	cpu-supply = <&syr827>;
};

&cpu_l2 {
	cpu-supply = <&syr827>;
};

&cpu_l3 {
	cpu-supply = <&syr827>;
};

&cpu_b0 {
	cpu-supply = <&syr827>;
};

&cpu_b1 {
	cpu-supply = <&syr827>;
};

&cpu_b2 {
	cpu-supply = <&syr827>;
};

&cpu_b3 {
	cpu-supply = <&syr827>;
};

&gpu {
	logic-supply = <&vdd_logic>;
};

&rockchip_suspend {
	status = "okay";
	rockchip,sleep-mode-config = <
		(0
		| RKPM_SLP_ARMOFF
		| RKPM_SLP_PMU_PLLS_PWRDN
		| RKPM_SLP_PMU_PMUALIVE_32K
		| RKPM_SLP_SFT_PLLS_DEEP
		| RKPM_SLP_PMU_DIS_OSC
		| RKPM_SLP_SFT_PD_NBSCUS
		)
	>;
	rockchip,wakeup-config = <
		(0
		| RKPM_GPIO_WKUP_EN
		| RKPM_USB_WKUP_EN
		| RKPM_CLUSTER_L_WKUP_EN
		)
	>;
};

&emmc {
	bus-width = <8>;
	cap-mmc-highspeed;
	mmc-hs200-1_8v;
	no-sdio;
	no-sd;
	disable-wp;
	non-removable;
	num-slots = <1>;
	pinctrl-names = "default";
	pinctrl-0 = <&emmc_clk &emmc_cmd &emmc_bus8>;
	status = "okay";
};

&nandc0 {
	status = "disabled";
};

&sdmmc {
	clock-frequency = <37500000>;
	clock-freq-min-max = <400000 37500000>;
	no-sdio;
	no-mmc;
	cap-mmc-highspeed;
	cap-sd-highspeed;
	card-detect-delay = <200>;
	disable-wp;
	num-slots = <1>;
	pinctrl-names = "default";
	pinctrl-0 = <&sdmmc_clk &sdmmc_cmd &sdmmc_cd &sdmmc_bus4>;
	status = "disabled";
};

&sdio0 {
	clock-frequency = <50000000>;
	clock-freq-min-max = <200000 50000000>;
	no-sd;
	no-mmc;
	bus-width = <4>;
	disable-wp;
	cap-sd-highspeed;
	cap-sdio-irq;
	keep-power-in-suspend;
	mmc-pwrseq = <&sdio_pwrseq>;
	non-removable;
	num-slots = <1>;
	pinctrl-names = "default";
	pinctrl-0 = <&sdio0_bus4 &sdio0_cmd &sdio0_clk>;
	sd-uhs-sdr104;
	status = "okay";
};

&i2c0 {
	status = "okay";

	syr827: syr827@40 {
		compatible = "silergy,syr827";
		status = "okay";
		reg = <0x40>;
		regulator-compatible = "fan53555-reg";
		regulator-name = "vdd_arm";
		regulator-min-microvolt = <712500>;
		regulator-max-microvolt = <1500000>;
		regulator-ramp-delay = <1000>;
		fcs,suspend-voltage-selector = <1>;
		pinctrl-0 = <&vsel_gpio>;
		vsel-gpios = <&gpio0 0 GPIO_ACTIVE_HIGH>;
		regulator-always-on;
		regulator-boot-on;
		regulator-initial-state = <3>;
		regulator-state-mem {
			regulator-off-in-suspend;
			regulator-suspend-microvolt = <900000>;
		};
	};

	rk818: pmic@1c {
		compatible = "rockchip,rk818";
		status = "okay";
		reg = <0x1c>;
		clock-output-names = "rk818-clkout1", "wifibt_32kin";
		interrupt-parent = <&gpio0>;
		interrupts = <1 IRQ_TYPE_LEVEL_LOW>;
		pinctrl-names = "default";
		pinctrl-0 = <&pmic_int_l>;
		rockchip,system-power-controller;
		wakeup-source;
		#clock-cells = <1>;

		vcc1-supply = <&vcc_sys>;
		vcc2-supply = <&vcc_sys>;
		vcc3-supply = <&vcc_sys>;
		vcc4-supply = <&vcc_sys>;
		vcc6-supply = <&vcc_sys>;
		vcc7-supply = <&vcc_sys>;
		vcc8-supply = <&vcc_sys>;
		vcc9-supply = <&vcc_io>;

		regulators {
			vdd_logic: DCDC_REG1 {
				regulator-name = "vdd_logic";
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <750000>;
				regulator-max-microvolt = <1450000>;
				regulator-ramp-delay = <6001>;
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1000000>;
				};
			};

			vdd_gpu: DCDC_REG2 {
				regulator-name = "vdd_gpu";
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <800000>;
				regulator-max-microvolt = <1250000>;
				regulator-ramp-delay = <6001>;
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1000000>;
				};
			};

			vcc_ddr: DCDC_REG3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vcc_ddr";
				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};

			vcc_io: DCDC_REG4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vcc_io";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vcca_codec: LDO_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vcca_codec";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vcc_tp: LDO_REG2 {
				regulator-boot-on;
				regulator-min-microvolt = <3000000>;
				regulator-max-microvolt = <3000000>;
				regulator-name = "vcc_tp";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd_10: LDO_REG3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <1000000>;
				regulator-name = "vdd_10";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1000000>;
				};
			};

			vcc18_lcd: LDO_REG4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc18_lcd";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vccio_pmu: LDO_REG5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vccio_pmu";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vdd10_lcd: LDO_REG6 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <1000000>;
				regulator-name = "vdd10_lcd";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1000000>;
				};
			};

			vcc_18: LDO_REG7 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc_18";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vccio_wl: LDO_REG8 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vccio_wl";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vccio_sd: LDO_REG9 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vccio_sd";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vcc_sd: SWITCH_REG {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vcc_sd";
				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};

			boost_otg: DCDC_BOOST {
				regulator-name = "boost_otg";
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <5000000>;
				regulator-max-microvolt = <5000000>;
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <5000000>;
				};
			};

			otg_switch: OTG_SWITCH {
				regulator-name = "otg_switch";
			};

			hdmi_switch: HDMI_SWITCH {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "hdmi_switch";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};
		};

		battery {
			compatible = "rk818-battery";
			pinctrl-names = "default";
			pinctrl-0 = <&dc_irq_gpio>;
			ocv_table = <
				3400 3650 3693 3707 3731 3749 3760
				3770 3782 3796 3812 3829 3852 3882
				3915 3951 3981 4047 4086 4132 4182>;
			design_capacity = <8650>;
			design_qmax = <8800>;
			bat_res = <85>;
			max_input_current = <2000>;
			max_chrg_current = <1800>;
			max_chrg_voltage = <4200>;
			sleep_enter_current = <600>;
			sleep_exit_current = <600>;
			power_off_thresd = <3400>;
			zero_algorithm_vol = <3850>;
			fb_temperature = <115>;
			sample_res = <20>;
			max_soc_offset = <60>;
			energy_mode = <0>;
			monitor_sec = <5>;
			virtual_power = <0>;
			power_dc2otg = <1>;
			support_usb_adp = <1>;
			support_dc_adp = <1>;
			dc_det_gpio = <&gpio0 17 GPIO_ACTIVE_LOW>;
		};
	};
};

&i2c1 {
	status = "okay";

	es8316: es8316@10 {
		status = "okay";
		#sound-dai-cells = <0>;
		compatible = "everest,es8316";
		reg = <0x10>;
		clocks = <&cru SCLK_I2S_8CH_OUT>;
		clock-names = "mclk";
		spk-con-gpio = <&gpio0 27 GPIO_ACTIVE_HIGH>;
		hp-det-gpio = <&gpio0 23 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2s_8ch_mclk>;
	};
};

&i2c2 {
	status = "okay";

	gt9xx: gt9xx@14 {
		compatible = "goodix,gt9xx";
		reg = <0x14>;
		touch-gpio = <&gpio0 12 IRQ_TYPE_LEVEL_LOW>;
		reset-gpio = <&gpio0 11 GPIO_ACTIVE_HIGH>;
		max-x = <1920>;
		max-y = <1200>;
		tp-size = <89>;
		status = "okay";
		tp-supply = <&vcc_tp>;
	};
};

&i2c3 {
	status = "okay";
};

&i2c4 {
	status = "okay";

	mpu6500_acc: mpu_acc@68 {
		compatible = "mpu6500_acc";
		reg = <0x68>;
		irq-gpio = <&gpio3 14 IRQ_TYPE_LEVEL_LOW>;
		irq_enable = <0>;
		poll_delay_ms = <30>;
		type = <SENSOR_TYPE_ACCEL>;
		layout = <7>;
	};

	mpu6500_gyro: mpu_gyro@68 {
		compatible = "mpu6500_gyro";
		reg = <0x68>;
		irq_enable = <0>;
		poll_delay_ms = <30>;
		type = <SENSOR_TYPE_GYROSCOPE>;
		layout = <7>;
	};

	mpu6500@68 {
		status = "disabled";
		compatible = "invensense,mpu6500";
		pinctrl-names = "default";
		pinctrl-0 = <&mpu6500_irq_gpio>;
		reg = <0x68>;
		irq-gpio = <&gpio3 14 IRQ_TYPE_EDGE_RISING>;
		mpu-int_config = <0x10>;
		mpu-level_shifter = <0>;
		mpu-orientation = <1 0 0 0 1 0 0 0 1>;
		orientation-x= <1>;
		orientation-y= <0>;
		orientation-z= <1>;
		support-hw-poweroff = <1>;
		mpu-debug = <1>;
	};
};

&i2s_8ch {
	status = "okay";
	rockchip,i2s-broken-burst-len;
	rockchip,playback-channels = <8>;
	rockchip,capture-channels = <2>;
	#sound-dai-cells = <0>;
};

&io_domains {
	status = "okay";

	dvp-supply = <&vcc_18>;
	audio-supply = <&vcc_io>;
	gpio30-supply = <&vcc_io>;
	gpio1830-supply = <&vcc_io>;
	sdcard-supply = <&vccio_sd>;
	wifi-supply = <&vccio_wl>;
};

&pmu_io_domains {
	status = "okay";

	pmu-supply = <&vccio_pmu>;
	vop-supply = <&vccio_pmu>;
};

&pwm0 {
	status = "okay";
};

&uart0 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart0_xfer &uart0_cts>;
	status = "okay";
};

&saradc {
	status = "okay";
};

&u2phy {
	status = "okay";

	u2phy_host: host-port {
		phy-supply = <&vcc_host>;
		status = "okay";
	};
};

&usb_host0_ehci {
	status = "okay";
};

&usb_host0_ohci {
	status = "okay";
};

&dsi {
	status = "okay";

	panel@0 {
		compatible = "simple-panel-dsi";
		reg = <0>;
		backlight = <&backlight>;
		enable-gpios = <&gpio0 22 GPIO_ACTIVE_HIGH>;
		prepare-delay-ms = <120>;
		enable-delay-ms = <200>;

		dsi,flags = <(MIPI_DSI_MODE_VIDEO | MIPI_DSI_MODE_VIDEO_BURST |
			      MIPI_DSI_MODE_LPM | MIPI_DSI_MODE_EOT_PACKET)>;
		dsi,format = <MIPI_DSI_FMT_RGB888>;
		dsi,lanes = <4>;

		display-timings {
			native-mode = <&timing0>;

			timing0: timing0 {
				clock-frequency = <145000000>;
				hactive = <1920>;
				vactive = <1200>;
				hback-porch = <16>;
				hfront-porch = <24>;
				vback-porch = <10>;
				vfront-porch = <16>;
				hsync-len = <10>;
				vsync-len = <3>;
				hsync-active = <0>;
				vsync-active = <0>;
				de-active = <0>;
				pixelclk-active = <0>;
			};
		};

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				panel_in_dsi: endpoint {
					remote-endpoint = <&dsi_out_panel>;
				};
			};
		};
	};

	ports {
		#address-cells = <1>;
		#size-cells = <0>;

		port@1 {
			reg = <1>;
			dsi_out_panel: endpoint {
				remote-endpoint = <&panel_in_dsi>;
			};
		};
	};
};

&route_dsi {
	status = "okay";
};

&tsadc {
	tsadc-supply = <&syr827>;
	status = "okay";
};

&pinctrl {
	pmic {
		pmic_int_l: pmic-int-l {
			rockchip,pins = <0 RK_PA1 RK_FUNC_GPIO &pcfg_pull_up>;
		};
		vsel_gpio: vsel-gpio {
			rockchip,pins = <0 RK_PA0 RK_FUNC_GPIO &pcfg_pull_down>;
		};
	};

	mpu6500 {
		mpu6500_irq_gpio: mpu6500-irq-gpio {
			rockchip,pins = <3 RK_PB6 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	dc_det {
		dc_irq_gpio: dc-irq-gpio {
			rockchip,pins = <0 RK_PC1 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	sdio-pwrseq {
		wifi_enable_h: wifi-enable-h {
			rockchip,pins = <3 RK_PA4 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	usb2 {
		host_vbus_drv: host-vbus-drv {
			rockchip,pins = <0 RK_PA4 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	wireless-bluetooth {
		uart0_rts_gpio: uart0-rts-gpio {
			rockchip,pins = <2 RK_PD3 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};
};

