// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Copyright (c) 2022 Rockchip Electronics Co., Ltd.
 *
 */

/dts-v1/;

#include "dt-bindings/pwm/pwm.h"
#include "rk3399.dtsi"
#include "rk3399-opp.dtsi"
#include <dt-bindings/display/drm_mipi_dsi.h>
#include <dt-bindings/input/input.h>
#include "rk3399-vop-clk-set.dtsi"

/ {
	model = "Rockchip RK3399 Firefly Board (Android)";
	compatible = "rockchip,rk3399-firefly-android", "rockchip,rk3399";

	chosen: chosen {
		bootargs = "earlycon=uart8250,mmio32,0xff1a0000 coherent_pool=1m";
	};

	cpuinfo {
		compatible = "rockchip,cpuinfo";
		nvmem-cells = <&cpu_id>;
		nvmem-cell-names = "id";
	};

	backlight: backlight {
		compatible = "pwm-backlight";
		pwms = <&pwm0 0 25000 0>;
		brightness-levels = <
			  0   1   2   3   4   5   6   7
			  8   9  10  11  12  13  14  15
			 16  17  18  19  20  21  22  23
			 24  25  26  27  28  29  30  31
			 32  33  34  35  36  37  38  39
			 40  41  42  43  44  45  46  47
			 48  49  50  51  52  53  54  55
			 56  57  58  59  60  61  62  63
			 64  65  66  67  68  69  70  71
			 72  73  74  75  76  77  78  79
			 80  81  82  83  84  85  86  87
			 88  89  90  91  92  93  94  95
			 96  97  98  99 100 101 102 103
			104 105 106 107 108 109 110 111
			112 113 114 115 116 117 118 119
			120 121 122 123 124 125 126 127
			128 129 130 131 132 133 134 135
			136 137 138 139 140 141 142 143
			144 145 146 147 148 149 150 151
			152 153 154 155 156 157 158 159
			160 161 162 163 164 165 166 167
			168 169 170 171 172 173 174 175
			176 177 178 179 180 181 182 183
			184 185 186 187 188 189 190 191
			192 193 194 195 196 197 198 199
			200 201 202 203 204 205 206 207
			208 209 210 211 212 213 214 215
			216 217 218 219 220 221 222 223
			224 225 226 227 228 229 230 231
			232 233 234 235 236 237 238 239
			240 241 242 243 244 245 246 247
			248 249 250 251 252 253 254 255>;
		default-brightness-level = <200>;
	};

	clkin_gmac: external-gmac-clock {
		compatible = "fixed-clock";
		clock-frequency = <125000000>;
		clock-output-names = "clkin_gmac";
		#clock-cells = <0>;
	};

	dw_hdmi_audio: dw-hdmi-audio {
		status = "okay";
		compatible = "rockchip,dw-hdmi-audio";
		#sound-dai-cells = <0>;
	};

	edp_panel: edp-panel {
		compatible = "sharp,lcd-f402", "panel-simple";
		status = "okay";

		backlight = <&backlight>;
		power-supply = <&vcc_lcd>;
		enable-gpios = <&gpio4 29 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&lcd_panel_reset>;

		ports {
			panel_in_edp: endpoint {
				remote-endpoint = <&edp_out_panel>;
			};
		};
	};

	fiq_debugger: fiq-debugger {
		compatible = "rockchip,fiq-debugger";
		rockchip,serial-id = <2>;
		rockchip,wake-irq = <0>;
		/* If enable uart uses irq instead of fiq */
		rockchip,irq-mode-enable = <0>;
		/* Only 115200 and 1500000 */
		rockchip,baudrate = <1500000>;
		pinctrl-names = "default";
		pinctrl-0 = <&uart2c_xfer>;
		interrupts = <GIC_SPI 150 IRQ_TYPE_LEVEL_HIGH 0>;
	};

	reserved-memory {
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;

		drm_logo: drm-logo@00000000 {
			compatible = "rockchip,drm-logo";
			reg = <0x0 0x0 0x0 0x0>;
		};

		stb_devinfo: stb-devinfo@00000000 {
			compatible = "rockchip,stb-devinfo";
			reg = <0x0 0x0 0x0 0x0>;
		};

		ramoops: ramoops@110000 {
			compatible = "ramoops";
			reg = <0x0 0x110000 0x0 0xf0000>;
			record-size = <0x20000>;
			console-size = <0x80000>;
			ftrace-size = <0x00000>;
			pmsg-size = <0x50000>;
		};
	};

	rockchip-key {
		compatible = "rockchip,key";
		status = "okay";

		io-channels = <&saradc 1>;
		power-key {
			gpios = <&gpio0 5 GPIO_ACTIVE_LOW>;
			linux,code = <116>;
			label = "power";
			gpio-key,wakeup;
		};
	};

	rt5640-sound {
		compatible = "simple-audio-card";
		simple-audio-card,format = "i2s";
		simple-audio-card,name = "rockchip,rt5640-codec";
		simple-audio-card,mclk-fs = <256>;
		simple-audio-card,widgets =
			"Microphone", "Mic Jack",
			"Headphone", "Headphone Jack";
		simple-audio-card,routing =
			"Mic Jack", "MICBIAS1",
			"IN1P", "Mic Jack",
			"Headphone Jack", "HPOL",
			"Headphone Jack", "HPOR";
		simple-audio-card,cpu {
			sound-dai = <&i2s1>;
		};
		simple-audio-card,codec {
			sound-dai = <&rt5640>;
		};
	};

	hdmi_sound: hdmi-sound {
		status = "disabled";
		compatible = "simple-audio-card";
		simple-audio-card,format = "i2s";
		simple-audio-card,mclk-fs = <256>;
		simple-audio-card,name = "rockchip,hdmi";

		simple-audio-card,cpu {
			sound-dai = <&i2s2>;
		};
		simple-audio-card,codec {
			sound-dai = <&dw_hdmi_audio>;
		};
	};

	hdmi_codec: hdmi-codec {
		compatible = "simple-audio-card";
		simple-audio-card,format = "i2s";
		simple-audio-card,mclk-fs = <256>;
		simple-audio-card,name = "HDMI-CODEC";

		simple-audio-card,cpu {
			sound-dai = <&i2s2>;
		};

		simple-audio-card,codec {
			sound-dai = <&hdmi>;
		};
	};

	rga: rga@ff680000 {
		compatible = "rockchip,rga2";
		dev_mode = <1>;
		reg = <0x0 0xff680000 0x0 0x1000>;
		interrupts = <GIC_SPI 55 IRQ_TYPE_LEVEL_HIGH 0>;
		clocks = <&cru ACLK_RGA>, <&cru HCLK_RGA>, <&cru SCLK_RGA_CORE>;
		clock-names = "aclk_rga", "hclk_rga", "clk_rga";
		power-domains = <&power RK3399_PD_RGA>;
		dma-coherent;
		status = "okay";
	};

	spdif-sound {
		compatible = "simple-audio-card";
		status = "okay";

		simple-audio-card,name = "ROCKCHIP,SPDIF";
		simple-audio-card,mclk-fs = <128>;
		simple-audio-card,cpu {
			sound-dai = <&spdif>;
		};
		simple-audio-card,codec {
			sound-dai = <&spdif_out>;
		};
	};

	spdif_out: spdif-out {
		compatible = "linux,spdif-dit";
		status = "okay";

		#sound-dai-cells = <0>;
	};

	sdio_pwrseq: sdio-pwrseq {
		compatible = "mmc-pwrseq-simple";
		clocks = <&rk808 1>;
		clock-names = "ext_clock";
		pinctrl-names = "default";
		pinctrl-0 = <&wifi_enable_h>;

		/*
		 * On the module itself this is one of these (depending
		 * on the actual card populated):
		 * - SDIO_RESET_L_WL_REG_ON
		 * - PDN (power down when low)
		 */
		reset-gpios = <&gpio0 10 GPIO_ACTIVE_LOW>; /* GPIO0_B2 */
	};

	vcc3v3_pcie: vcc3v3-pcie-regulator {
		compatible = "regulator-fixed";
		enable-active-high;
		regulator-always-on;
		regulator-boot-on;
		gpio = <&gpio1 17 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&pcie_drv>;
		regulator-name = "vcc3v3_pcie";
	};

	vcc3v3_sys: vcc3v3-sys {
		compatible = "regulator-fixed";
		regulator-name = "vcc3v3_sys";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
	};

	vcc5v0_host: vcc5v0-host-regulator {
		compatible = "regulator-fixed";
		enable-active-high;
		gpio = <&gpio1 0 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&host_vbus_drv>;
		regulator-name = "vcc5v0_host";
		regulator-always-on;
	};

	vcc5v0_sys: vcc5v0-sys {
		compatible = "regulator-fixed";
		regulator-name = "vcc5v0_sys";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
	};

	vcc_phy: vcc-phy-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vcc_phy";
		regulator-always-on;
		regulator-boot-on;
	};

	vdd_log: vdd-log {
		compatible = "pwm-regulator";
		pwms = <&pwm2 0 25000 1>;
		regulator-name = "vdd_log";
		regulator-min-microvolt = <800000>;
		/*
		 * the firefly hardware using 3.0 v as APIO2_VDD
		 * voltage, but the pwm divider resistance is designed
		 * based on hardware which the APIO2_VDD is 1.8v, so we
		 * need to change the regulator-max-microvolt from 1.4v
		 * to 1.0v, so the pwm can output 0.9v voltage.
		 */
		regulator-max-microvolt = <1000000>;
		regulator-always-on;
		regulator-boot-on;

		/* for rockchip boot on */
		rockchip,pwm_id= <2>;
		rockchip,pwm_voltage = <900000>;
	};

	vccadc_ref: vccadc-ref {
		compatible = "regulator-fixed";
		regulator-name = "vcc1v8_sys";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <1800000>;
		regulator-max-microvolt = <1800000>;
	};

	vcc_lcd: vcc-lcd-regulator {
		compatible = "regulator-fixed";
		regulator-always-on;
		regulator-boot-on;
		enable-active-high;
		gpio = <&gpio1 1 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&lcd_en>;
		regulator-name = "vcc_lcd";
	};

	xin32k: xin32k {
		compatible = "fixed-clock";
		clock-frequency = <32768>;
		clock-output-names = "xin32k";
		#clock-cells = <0>;
	};

	wireless-wlan {
		compatible = "wlan-platdata";
		rockchip,grf = <&grf>;
		wifi_chip_type = "ap6354";
		sdio_vref = <1800>;
		WIFI,host_wake_irq = <&gpio0 3 GPIO_ACTIVE_HIGH>; /* GPIO0_a3 */
		status = "okay";
	};

	wireless-bluetooth {
		compatible = "bluetooth-platdata";
		//wifi-bt-power-toggle;
		uart_rts_gpios = <&gpio2 19 GPIO_ACTIVE_LOW>; /* GPIO2_C3 */
		pinctrl-names = "default", "rts_gpio";
		pinctrl-0 = <&uart0_rts>;
		pinctrl-1 = <&uart0_gpios>;
		//BT,power_gpio  = <&gpio3 19 GPIO_ACTIVE_HIGH>; /* GPIOx_xx */
		BT,reset_gpio    = <&gpio0 9 GPIO_ACTIVE_HIGH>; /* GPIO0_B1 */
		BT,wake_gpio     = <&gpio2 26 GPIO_ACTIVE_HIGH>; /* GPIO2_D2 */
		BT,wake_host_irq = <&gpio0 4 GPIO_ACTIVE_HIGH>; /* GPIO0_A4 */
		status = "okay";
	};
};

&cpu_l0 {
	cpu-supply = <&vdd_cpu_l>;
};

&cpu_l1 {
	cpu-supply = <&vdd_cpu_l>;
};

&cpu_l2 {
	cpu-supply = <&vdd_cpu_l>;
};

&cpu_l3 {
	cpu-supply = <&vdd_cpu_l>;
};

&cpu_b0 {
	cpu-supply = <&vdd_cpu_b>;
};

&cpu_b1 {
	cpu-supply = <&vdd_cpu_b>;
};

&display_subsystem {
	status = "okay";

	ports = <&vopb_out>, <&vopl_out>;
	logo-memory-region = <&drm_logo>;

	route {
		route_hdmi: route-hdmi {
			status = "okay";
			logo,uboot = "logo.bmp";
			logo,kernel = "logo_kernel.bmp";
			logo,mode = "fullscreen";
			charge_logo,mode = "center";
			connect = <&vopl_out_hdmi>;
		};

		route_edp: route-edp {
			status = "okay";
			logo,uboot = "logo.bmp";
			logo,kernel = "logo_kernel.bmp";
			logo,mode = "fullscreen";
			charge_logo,mode = "center";
			connect = <&vopb_out_edp>;
		};
	};
};

&edp {
	status = "okay";
	pinctrl-names = "default";
	pinctrl-0 = <&edp_hpd>;

	ports {
		edp_out: port@1 {
			reg = <1>;
			#address-cells = <1>;
			#size-cells = <0>;

			edp_out_panel: endpoint@0 {
				reg = <0>;
				remote-endpoint = <&panel_in_edp>;
			};
		};
	};
};

&emmc_phy {
	status = "okay";
};

&gmac {
	phy-supply = <&vcc_phy>;
	phy-mode = "rgmii";
	clock_in_out = "input";
	snps,reset-gpio = <&gpio3 15 GPIO_ACTIVE_LOW>;
	snps,reset-active-low;
	snps,reset-delays-us = <0 10000 50000>;
	assigned-clocks = <&cru SCLK_RMII_SRC>;
	assigned-clock-parents = <&clkin_gmac>;
	pinctrl-names = "default";
	pinctrl-0 = <&rgmii_pins>;
	tx_delay = <0x28>;
	rx_delay = <0x11>;
	status = "okay";
};

&gpu {
	status = "okay";
	mali-supply = <&vdd_gpu>;
};

&hdmi {
	#address-cells = <1>;
	#size-cells = <0>;
	#sound-dai-cells = <0>;
	status = "okay";
};

&i2c0 {
	status = "okay";
	i2c-scl-rising-time-ns = <168>;
	i2c-scl-falling-time-ns = <4>;
	clock-frequency = <400000>;

	vdd_cpu_b: syr827@40 {
		compatible = "silergy,syr827";
		reg = <0x40>;
		vin-supply = <&vcc5v0_sys>;
		regulator-compatible = "fan53555-reg";
		regulator-name = "vdd_cpu_b";
		regulator-min-microvolt = <712500>;
		regulator-max-microvolt = <1500000>;
		regulator-ramp-delay = <1000>;
		vsel-gpios = <&gpio1 18 GPIO_ACTIVE_HIGH>;
		fcs,suspend-voltage-selector = <1>;
		regulator-always-on;
		regulator-boot-on;
		regulator-initial-state = <3>;
			regulator-state-mem {
			regulator-off-in-suspend;
		};
	};

	vdd_gpu: syr828@41 {
		compatible = "silergy,syr828";
		reg = <0x41>;
		vin-supply = <&vcc5v0_sys>;
		regulator-compatible = "fan53555-reg";
		regulator-name = "vdd_gpu";
		regulator-min-microvolt = <712500>;
		regulator-max-microvolt = <1500000>;
		regulator-ramp-delay = <1000>;
		fcs,suspend-voltage-selector = <1>;
		regulator-always-on;
		regulator-boot-on;
		regulator-initial-state = <3>;
			regulator-state-mem {
			regulator-off-in-suspend;
		};
	};

	rk808: pmic@1b {
		compatible = "rockchip,rk808";
		reg = <0x1b>;
		interrupt-parent = <&gpio1>;
		interrupts = <21 IRQ_TYPE_LEVEL_LOW>;
		pinctrl-names = "default";
		pinctrl-0 = <&pmic_int_l &pmic_dvs2>;
		rockchip,system-power-controller;
		wakeup-source;
		#clock-cells = <1>;
		clock-output-names = "rk808-clkout1", "rk808-clkout2";

		vcc1-supply = <&vcc3v3_sys>;
		vcc2-supply = <&vcc3v3_sys>;
		vcc3-supply = <&vcc3v3_sys>;
		vcc4-supply = <&vcc3v3_sys>;
		vcc6-supply = <&vcc3v3_sys>;
		vcc7-supply = <&vcc3v3_sys>;
		vcc8-supply = <&vcc3v3_sys>;
		vcc9-supply = <&vcc3v3_sys>;
		vcc10-supply = <&vcc3v3_sys>;
		vcc11-supply = <&vcc3v3_sys>;
		vcc12-supply = <&vcc3v3_sys>;
		vddio-supply = <&vcc1v8_pmu>;

		regulators {
			vdd_center: DCDC_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <750000>;
				regulator-max-microvolt = <1350000>;
				regulator-ramp-delay = <6001>;
				regulator-name = "vdd_center";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd_cpu_l: DCDC_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <750000>;
				regulator-max-microvolt = <1350000>;
				regulator-ramp-delay = <6001>;
				regulator-name = "vdd_cpu_l";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_ddr: DCDC_REG3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vcc_ddr";
				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};

			vcc_1v8: DCDC_REG4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc_1v8";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vcc1v8_dvp: LDO_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc1v8_dvp";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc3v0_tp: LDO_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3000000>;
				regulator-max-microvolt = <3000000>;
				regulator-name = "vcc3v0_tp";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc1v8_pmu: LDO_REG3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc1v8_pmu";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vcc_sd: LDO_REG4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3000000>;
				regulator-name = "vcc_sd";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3000000>;
				};
			};

			vcca3v0_codec: LDO_REG5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3000000>;
				regulator-max-microvolt = <3000000>;
				regulator-name = "vcca3v0_codec";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_1v5: LDO_REG6 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1500000>;
				regulator-max-microvolt = <1500000>;
				regulator-name = "vcc_1v5";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1500000>;
				};
			};

			vcca1v8_codec: LDO_REG7 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcca1v8_codec";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_3v0: LDO_REG8 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3000000>;
				regulator-max-microvolt = <3000000>;
				regulator-name = "vcc_3v0";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3000000>;
				};
			};

			vcc3v3_s3: SWITCH_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vcc3v3_s3";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc3v3_s0: SWITCH_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vcc3v3_s0";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};
		};
	};
};

&i2c1 {
	status = "okay";
	i2c-scl-rising-time-ns = <300>;
	i2c-scl-falling-time-ns = <15>;

	rt5640: rt5640@1c {
		#sound-dai-cells = <0>;
		compatible = "realtek,rt5640";
		reg = <0x1c>;
		clocks = <&cru SCLK_I2S_8CH_OUT>;
		clock-names = "mclk";
		realtek,in1-differential;
		pinctrl-names = "default";
		pinctrl-0 = <&rt5640_hpcon &i2s_8ch_mclk>;
		hp-con-gpio = <&gpio4 21 GPIO_ACTIVE_HIGH>;
		//hp-det-gpio = <&gpio4 28 GPIO_ACTIVE_LOW>;
		io-channels = <&saradc 4>;
		hp-det-adc-value = <500>;
		status = "okay";
	};
};

&i2c3 {
	status = "okay";
	i2c-scl-rising-time-ns = <450>;
	i2c-scl-falling-time-ns = <15>;
};

&i2c4 {
	status = "okay";
	i2c-scl-rising-time-ns = <600>;
	i2c-scl-falling-time-ns = <20>;

	fusb0: fusb30x@22 {
		compatible = "fairchild,fusb302";
		reg = <0x22>;
		pinctrl-names = "default";
		pinctrl-0 = <&fusb0_int>;
		int-n-gpios = <&gpio1 2 GPIO_ACTIVE_HIGH>;
		vbus-5v-gpios = <&gpio2 0 GPIO_ACTIVE_HIGH>;
		status = "okay";
	};

	gsl3680: gsl3680@41 {
		compatible = "gslX680-pad";
		reg = <0x41>;
		screen_max_x = <1536>;
		screen_max_y = <2048>;
		touch-gpio = <&gpio1 20 IRQ_TYPE_LEVEL_LOW>;
		reset-gpio = <&gpio0 12 GPIO_ACTIVE_HIGH>;
		status = "okay";
	};

	mpu6050: mpu@68 {
		compatible = "invensense,mpu6050";
		reg = <0x68>;
		mpu-int_config = <0x10>;
		mpu-level_shifter = <0>;
		mpu-orientation = <0 1 0 1 0 0 0 0 1>;
		orientation-x= <1>;
		orientation-y= <1>;
		orientation-z= <1>;
		irq-gpio = <&gpio1 4 IRQ_TYPE_LEVEL_LOW>;
		mpu-debug = <1>;
		status = "okay";
	};
};

&i2s0 {
	status = "okay";
	rockchip,i2s-broken-burst-len;
	rockchip,playback-channels = <8>;
	rockchip,capture-channels = <8>;
	#sound-dai-cells = <0>;
};

&i2s1 {
	status = "okay";
	rockchip,i2s-broken-burst-len;
	rockchip,playback-channels = <2>;
	rockchip,capture-channels = <2>;
	#sound-dai-cells = <0>;
};

&i2s2 {
	#sound-dai-cells = <0>;
	status = "okay";
};

&io_domains {
	status = "okay";

	bt656-supply = <&vcc1v8_dvp>;		/* bt656_gpio2ab_ms */
	audio-supply = <&vcca1v8_codec>;	/* audio_gpio3d4a_ms */
	sdmmc-supply = <&vcc_sd>;		/* sdmmc_gpio4b_ms */
	gpio1830-supply = <&vcc_3v0>;		/* gpio1833_gpio4cd_ms */
};

&pcie_phy {
	status = "okay";
};

&pcie0 {
	ep-gpios = <&gpio4 25 GPIO_ACTIVE_HIGH>;
	num-lanes = <4>;
	pinctrl-names = "default";
	pinctrl-0 = <&pcie_clkreqn_cpm>;
	status = "okay";
};

&pmu_io_domains {
	status = "okay";
	pmu1830-supply = <&vcc_3v0>;
};

&pinctrl {

	lcd-panel {
		lcd_panel_reset: lcd-panel-reset {
			rockchip,pins = <4 RK_PD5 RK_FUNC_GPIO &pcfg_pull_up>;
		};

		lcd_en: lcd-en {
			rockchip,pins = <1 RK_PA1 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	pcie {
		pcie_drv: pcie-drv {
			rockchip,pins =
				<1 RK_PC1 RK_FUNC_GPIO &pcfg_pull_none>;
			};
			pcie_3g_drv: pcie-3g-drv {
			rockchip,pins =
				<0 RK_PA2 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	pmic {
		vsel1_gpio: vsel1-gpio {
			rockchip,pins =
				<1 RK_PC2 RK_FUNC_GPIO &pcfg_pull_down>;
		};

		vsel2_gpio: vsel2-gpio {
			rockchip,pins =
			<1 RK_PB6 RK_FUNC_GPIO &pcfg_pull_down>;
		};
	};

	sdio-pwrseq {
		wifi_enable_h: wifi-enable-h {
			rockchip,pins =
				<0 RK_PB2 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	wireless-bluetooth {
		uart0_gpios: uart0-gpios {
			rockchip,pins =
				<2 RK_PC3 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	rt5640 {
		rt5640_hpcon: rt5640-hpcon {
			rockchip,pins = <4 RK_PC5 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	pmic {
		pmic_int_l: pmic-int-l {
			rockchip,pins =
				<1 RK_PC5 RK_FUNC_GPIO &pcfg_pull_up>;
		};

		pmic_dvs2: pmic-dvs2 {
			rockchip,pins =
				<1 RK_PC2 RK_FUNC_GPIO &pcfg_pull_down>;
		};
	};

	usb2 {
		host_vbus_drv: host-vbus-drv {
			rockchip,pins =
				<4 RK_PD1 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	fusb30x {
		fusb0_int: fusb0-int {
			rockchip,pins = <1 RK_PA2 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};
};

&pwm0 {
	status = "okay";
};

&pwm2 {
	status = "okay";
	pinctrl-names = "active";
	pinctrl-0 = <&pwm2_pin_pull_down>;
};

&rockchip_suspend {
	rockchip,power-ctrl =
		<&gpio1 18 GPIO_ACTIVE_LOW>,
		<&gpio1 14 GPIO_ACTIVE_HIGH>;
};

&saradc {
	status = "okay";
	vref-supply = <&vccadc_ref>;
};

&sdhci {
	bus-width = <8>;
	keep-power-in-suspend;
	mmc-hs400-1_8v;
	mmc-hs400-enhanced-strobe;
	non-removable;
	status = "okay";
	no-sdio;
	no-sd;
};

&sdmmc {
	max-frequency = <150000000>;
	no-sdio;
	no-mmc;
	bus-width = <4>;
	cap-mmc-highspeed;
	cap-sd-highspeed;
	disable-wp;
	num-slots = <1>;
	vqmmc-supply = <&vcc_sd>;
	pinctrl-names = "default";
	pinctrl-0 = <&sdmmc_clk &sdmmc_cmd &sdmmc_cd &sdmmc_bus4>;
	status = "okay";
};

&sdio0 {
	max-frequency = <50000000>;
	no-sd;
	no-mmc;
	bus-width = <4>;
	disable-wp;
	cap-sd-highspeed;
	keep-power-in-suspend;
	mmc-pwrseq = <&sdio_pwrseq>;
	non-removable;
	num-slots = <1>;
	pinctrl-names = "default";
	pinctrl-0 = <&sdio0_bus4 &sdio0_cmd &sdio0_clk>;
	sd-uhs-sdr104;
	status = "okay";
};

&spdif {
	status = "okay";
	pinctrl-0 = <&spdif_bus_1>;
	i2c-scl-rising-time-ns = <450>;
	i2c-scl-falling-time-ns = <15>;
	#sound-dai-cells = <0>;
};

&tcphy0 {
	extcon = <&fusb0>;
	status = "okay";
};

&tcphy1 {
	status = "okay";
};

&tsadc {
	/* tshut mode 0:CRU 1:GPIO */
	rockchip,hw-tshut-mode = <1>;
	/* tshut polarity 0:LOW 1:HIGH */
	rockchip,hw-tshut-polarity = <1>;
	status = "okay";
};

&u2phy0 {
	status = "okay";
	extcon = <&fusb0>;

	u2phy0_otg: otg-port {
		status = "okay";
	};

	u2phy0_host: host-port {
		phy-supply = <&vcc5v0_host>;
		status = "okay";
	};
};

&u2phy1 {
	status = "okay";

	u2phy1_otg: otg-port {
		status = "okay";
	};

	u2phy1_host: host-port {
		phy-supply = <&vcc5v0_host>;
		status = "okay";
	};
};

&uart0 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart0_xfer &uart0_cts>;
	status = "okay";
};

&uart2 {
	status = "okay";
};

&usbdrd3_0 {
	status = "okay";
};

&usbdrd3_1 {
	status = "okay";
};

&usbdrd_dwc3_0 {
	status = "okay";
	extcon = <&fusb0>;
};

&usbdrd_dwc3_1 {
	status = "okay";
	dr_mode = "host";
};

&usb_host0_ehci {
	status = "okay";
};

&usb_host0_ohci {
	status = "okay";
};

&usb_host1_ehci {
	status = "okay";
};

&usb_host1_ohci {
	status = "okay";
};

&vopb {
	status = "okay";
};

&vopb_mmu {
	status = "okay";
};

&vopl {
	status = "okay";
};

&vopl_mmu {
	status = "okay";
};
