/**
 * enable pcie2x1 relavent config for rk3568
 */
 
/ {
    vcc3v3_pcie: gpio-regulator {
        compatible = "regulator-fixed";
        regulator-name = "vcc3v3_pcie";
        regulator-min-microvolt = <3300000>;
        regulator-max-microvolt = <3300000>;
        enable-active-high;
        /**
         * gpio config please refer to main dts if have
         * gpio = <&gpio* ** ***>;
         */
        startup-delay-us = <5000>;
        vin-supply = <&dc_12v>;
    };

};


&combphy2_psq {
    status = "okay";
};

&sata2 {
    status = "disabled";
};

&pcie2x1 {
    /**
     * gpio please refer to main dts:
     * reset-gpios = <&gpio* ** ***>;
     */
    vpcie3v3-supply = <&vcc3v3_pcie>;
    status = "okay";
};
