// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Copyright (c) 2017 Fuzhou Rockchip Electronics Co., Ltd
 *
 */

#include "rk3328.dtsi"
#include "rk3328-android.dtsi"
#include <dt-bindings/input/input.h>

/ {
	gmac_clkin: external-gmac-clock {
		compatible = "fixed-clock";
		clock-frequency = <125000000>;
		clock-output-names = "gmac_clkin";
		#clock-cells = <0>;
	};

	vcc_sd: sdmmc-regulator {
		compatible = "regulator-fixed";
		gpio = <&gpio0 30 GPIO_ACTIVE_LOW>;
		pinctrl-names = "default";
		pinctrl-0 = <&sdmmc0m1_gpio>;
		regulator-name = "vcc_sd";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		vin-supply = <&vcc_io>;
	};

	vcc_host_5v: vcc-host-5v-regulator {
		compatible = "regulator-fixed";
		enable-active-high;
		gpio = <&gpio0 0 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&usb30_host_drv>;
		regulator-name = "vcc_host_5v";
		regulator-always-on;
		vin-supply = <&vcc_sys>;
	};

	vcc_host1_5v: vcc_otg_5v: vcc-host1-5v-regulator {
		compatible = "regulator-fixed";
		enable-active-high;
		gpio = <&gpio0 27 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&usb20_host_drv>;
		regulator-name = "vcc_host1_5v";
		regulator-always-on;
		vin-supply = <&vcc_sys>;
	};

	vcc_sys: vcc-sys {
		compatible = "regulator-fixed";
		regulator-name = "vcc_sys";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
	};

	sound {
		compatible = "simple-audio-card";
		simple-audio-card,format = "i2s";
		simple-audio-card,mclk-fs = <256>;
		simple-audio-card,name = "rockchip-rk3328";
		simple-audio-card,cpu {
			sound-dai = <&i2s1>;
		};
		simple-audio-card,codec {
			sound-dai = <&codec>;
		};
	};

	hdmi-sound {
		compatible = "simple-audio-card";
		simple-audio-card,format = "i2s";
		simple-audio-card,mclk-fs = <128>;
		simple-audio-card,name = "rockchip-hdmi";
		simple-audio-card,cpu {
			sound-dai = <&i2s0>;
		};
		simple-audio-card,codec {
			sound-dai = <&hdmi>;
		};
	};

	vcc_phy: vcc-phy-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vcc_phy";
		regulator-always-on;
		regulator-boot-on;
	};

	xin32k: xin32k {
		compatible = "fixed-clock";
		clock-frequency = <32768>;
		clock-output-names = "xin32k";
		#clock-cells = <0>;
	};
};

&avsd {
	status = "okay";
};

&codec {
	#sound-dai-cells = <0>;
	status = "okay";
};

&cpu0 {
	cpu-supply = <&vdd_arm>;
};

&dfi {
	status = "okay";
};

&dmc {
	center-supply = <&vdd_logic>;
	status = "okay";
};

&emmc {
	bus-width = <8>;
	cap-mmc-highspeed;
	mmc-hs200-1_8v;
	no-sdio;
	no-sd;
	disable-wp;
	non-removable;
	num-slots = <1>;
	pinctrl-names = "default";
	pinctrl-0 = <&emmc_clk &emmc_cmd &emmc_bus8>;
	status = "okay";
};

&gmac2io {
	phy-supply = <&vcc_phy>;
	phy-mode = "rgmii";
	clock_in_out = "input";
	snps,reset-gpio = <&gpio1 RK_PC2 GPIO_ACTIVE_LOW>;
	snps,reset-active-low;
	snps,reset-delays-us = <0 10000 50000>;
	assigned-clocks = <&cru SCLK_MAC2IO>, <&cru SCLK_MAC2IO_EXT>;
	assigned-clock-parents = <&gmac_clkin>, <&gmac_clkin>;
	pinctrl-names = "default";
	pinctrl-0 = <&rgmiim1_pins>;
	tx_delay = <0x26>;
	rx_delay = <0x11>;
	status = "okay";
};

&gmac2phy {
	phy-supply = <&vcc_phy>;
	clock_in_out = "output";
	assigned-clocks = <&cru SCLK_MAC2PHY_SRC>;
	assigned-clock-rate = <50000000>;
	assigned-clocks = <&cru SCLK_MAC2PHY>;
	assigned-clock-parents = <&cru SCLK_MAC2PHY_SRC>;
	status = "disabled";
};

&gpu {
	status = "okay";
	mali-supply = <&vdd_logic>;
};

&hdmi {
	#sound-dai-cells = <0>;
	status = "okay";
};

&hdmiphy {
	status = "okay";
};

&i2c1 {
	status = "okay";

	rk805: rk805@18 {
		compatible = "rockchip,rk805";
		status = "okay";
		reg = <0x18>;
		interrupt-parent = <&gpio2>;
		interrupts = <6 IRQ_TYPE_LEVEL_LOW>;
		pinctrl-names = "default";
		pinctrl-0 = <&pmic_int_l>;
		wakeup-source;
		gpio-controller;
		#gpio-cells = <2>;
		#clock-cells = <1>;
		clock-output-names = "rk805-clkout1", "rk805-clkout2";

		vcc1-supply = <&vcc_sys>;
		vcc2-supply = <&vcc_sys>;
		vcc3-supply = <&vcc_sys>;
		vcc4-supply = <&vcc_sys>;
		vcc5-supply = <&vcc_io>;
		vcc6-supply = <&vcc_io>;

		rtc {
			status = "okay";
		};

		pwrkey {
			status = "disabled";
		};

		gpio {
			status = "okay";
		};

		regulators {
			vdd_logic: DCDC_REG1 {
				regulator-name = "vdd_logic";
				regulator-min-microvolt = <712500>;
				regulator-max-microvolt = <1450000>;
				regulator-initial-mode = <0x1>;
				regulator-ramp-delay = <12500>;
				regulator-boot-on;
				regulator-always-on;
				regulator-state-mem {
					regulator-mode = <0x2>;
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1000000>;
				};
			};

			vdd_arm: DCDC_REG2 {
				regulator-name = "vdd_arm";
				regulator-init-microvolt = <1225000>;
				regulator-min-microvolt = <712500>;
				regulator-max-microvolt = <1450000>;
				regulator-initial-mode = <0x1>;
				regulator-ramp-delay = <12500>;
				regulator-boot-on;
				regulator-always-on;
				regulator-state-mem {
					regulator-mode = <0x2>;
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <950000>;
				};
			};

			vcc_ddr: DCDC_REG3 {
				regulator-name = "vcc_ddr";
				regulator-initial-mode = <0x1>;
				regulator-boot-on;
				regulator-always-on;
				regulator-state-mem {
					regulator-mode = <0x2>;
					regulator-on-in-suspend;
				};
			};

			vcc_io: DCDC_REG4 {
				regulator-name = "vcc_io";
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-initial-mode = <0x1>;
				regulator-boot-on;
				regulator-always-on;
				regulator-state-mem {
					regulator-mode = <0x2>;
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vdd_18: LDO_REG1 {
				regulator-name = "vdd_18";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-boot-on;
				regulator-always-on;
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vcc_18emmc: LDO_REG2 {
				regulator-name = "vcc_18emmc";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-boot-on;
				regulator-always-on;
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vdd_11: LDO_REG3 {
				regulator-name = "vdd_11";
				regulator-min-microvolt = <1100000>;
				regulator-max-microvolt = <1100000>;
				regulator-boot-on;
				regulator-always-on;
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1100000>;
				};
			};
		};
	};
};

&i2s0 {
	#sound-dai-cells = <0>;
	rockchip,bclk-fs = <128>;
	status = "okay";
};

&i2s1 {
	#sound-dai-cells = <0>;
	status = "okay";
};

&iep {
	status = "okay";
};

&iep_mmu {
	status = "okay";
};

&io_domains {
	status = "okay";

	vccio1-supply = <&vcc_io>;
	vccio2-supply = <&vcc_18emmc>;
	vccio3-supply = <&vcc_io>;
	vccio4-supply = <&vdd_18>;
	vccio5-supply = <&vcc_io>;
	vccio6-supply = <&vcc_io>;
	pmuio-supply = <&vcc_io>;
};

&mpp_srv {
	status = "okay";
};

&pinctrl {
	pmic {
		pmic_int_l: pmic-int-l {
			rockchip,pins = <2 RK_PA6 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	usb2 {
		usb20_host_drv: usb20-host-drv {
			rockchip,pins = <0 RK_PD3 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	usb3 {
		usb30_host_drv: usb30-host-drv {
			rockchip,pins = <0 RK_PA0 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};
};

&pwm3 {
	status = "okay";
	pinctrl-names = "default";
	pinctrl-0 = <&pwmir_pin>;
	compatible = "rockchip,remotectl-pwm";
	remote_pwm_id = <3>;
	handle_cpu_id = <1>;
	remote_support_psci = <1>;

	ir_key1 {
		rockchip,usercode = <0x4040>;
		rockchip,key_table =
			<0xf2	KEY_REPLY>,
			<0xba	KEY_BACK>,
			<0xf4	KEY_UP>,
			<0xf1	KEY_DOWN>,
			<0xef	KEY_LEFT>,
			<0xee	KEY_RIGHT>,
			<0xbd	KEY_HOME>,
			<0xea	KEY_VOLUMEUP>,
			<0xe3	KEY_VOLUMEDOWN>,
			<0xe2	KEY_SEARCH>,
			<0xb2	KEY_POWER>,
			<0xbc	KEY_MUTE>,
			<0xec	KEY_MENU>,
			<0xbf	0x190>,
			<0xe0	0x191>,
			<0xe1	0x192>,
			<0xe9	183>,
			<0xe6	248>,
			<0xe8	185>,
			<0xe7	186>,
			<0xf0	388>,
			<0xbe	0x175>;
	};

	ir_key2 {
		rockchip,usercode = <0xff00>;
		rockchip,key_table =
			<0xf9	KEY_HOME>,
			<0xbf	KEY_BACK>,
			<0xfb	KEY_MENU>,
			<0xaa	KEY_REPLY>,
			<0xb9	KEY_UP>,
			<0xe9	KEY_DOWN>,
			<0xb8	KEY_LEFT>,
			<0xea	KEY_RIGHT>,
			<0xeb	KEY_VOLUMEDOWN>,
			<0xef	KEY_VOLUMEUP>,
			<0xf7	KEY_MUTE>,
			<0xe7	KEY_POWER>,
			<0xfc	KEY_POWER>,
			<0xa9	KEY_VOLUMEDOWN>,
			<0xa8	KEY_PLAYPAUSE>,
			<0xe0	KEY_VOLUMEDOWN>,
			<0xa5	KEY_VOLUMEDOWN>,
			<0xab	183>,
			<0xb7	388>,
			<0xe8	388>,
			<0xf8	184>,
			<0xaf	185>,
			<0xed	KEY_VOLUMEDOWN>,
			<0xee	186>,
			<0xb3	KEY_VOLUMEDOWN>,
			<0xf1	KEY_VOLUMEDOWN>,
			<0xf2	KEY_VOLUMEDOWN>,
			<0xf3	KEY_SEARCH>,
			<0xb4	KEY_VOLUMEDOWN>,
			<0xa4	KEY_SETUP>,
			<0xbe	KEY_SEARCH>;
	};

	ir_key3 {
		rockchip,usercode = <0x1dcc>;
		rockchip,key_table =
			<0xee	KEY_REPLY>,
			<0xf0	KEY_BACK>,
			<0xf8	KEY_UP>,
			<0xbb	KEY_DOWN>,
			<0xef	KEY_LEFT>,
			<0xed	KEY_RIGHT>,
			<0xfc	KEY_HOME>,
			<0xf1	KEY_VOLUMEUP>,
			<0xfd	KEY_VOLUMEDOWN>,
			<0xb7	KEY_SEARCH>,
			<0xff	KEY_POWER>,
			<0xf3	KEY_MUTE>,
			<0xbf	KEY_MENU>,
			<0xf9	0x191>,
			<0xf5	0x192>,
			<0xb3	388>,
			<0xbe	KEY_1>,
			<0xba	KEY_2>,
			<0xb2	KEY_3>,
			<0xbd	KEY_4>,
			<0xf9	KEY_5>,
			<0xb1	KEY_6>,
			<0xfc	KEY_7>,
			<0xf8	KEY_8>,
			<0xb0	KEY_9>,
			<0xb6	KEY_0>,
			<0xb5	KEY_BACKSPACE>;
	};
};

&rga {
	status = "okay";
};

&rkvdec {
	status = "okay";
	vcodec-supply = <&vdd_logic>;
};

&rkvdec_mmu {
	status = "okay";
};

&rockchip_suspend {
	status = "okay";
	rockchip,virtual-poweroff = <1>;
};

&sdmmc {
	bus-width = <4>;
	cap-mmc-highspeed;
	cap-sd-highspeed;
	disable-wp;
	max-frequency = <150000000>;
	num-slots = <1>;
	pinctrl-names = "default";
	pinctrl-0 = <&sdmmc0_clk &sdmmc0_cmd &sdmmc0_dectn &sdmmc0_bus4>;
	no-sdio;
	no-mmc;
	status = "okay";
	vmmc-supply = <&vcc_sd>;
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "gigadevice,gd25q128", "jedec,spi-nor";
		#address-cells = <1>;
		#size-cells = <1>;
		reg = <0>;
		m25p,fast-read;
		/* The max SCLK of the flash 104/80 MHZ  */
		spi-max-frequency = <50000000>;
	};
};

&threshold {
	temperature = <90000>; /* millicelsius */
};

&target {
	temperature = <105000>; /* millicelsius */
};

&soc_crit {
	temperature = <115000>; /* millicelsius */
};

&tsadc {
	rockchip,hw-tshut-temp = <120000>;
	status = "okay";
};

&u2phy {
	status = "okay";

};

&u2phy_host {
	phy-supply = <&vcc_host1_5v>;
	status = "okay";
};

&u2phy_otg {
	phy-supply = <&vcc_otg_5v>;
	status = "okay";
};

&u3phy {
	phy-supply = <&vcc_host_5v>;
	status = "okay";
};

&u3phy_utmi {
	status = "okay";
};

&u3phy_pipe {
	status = "okay";
};

&usb20_otg {
	status = "okay";
};

&usb_host0_ehci {
	status = "okay";
};

&usb_host0_ohci {
	status = "okay";
};

&usbdrd3 {
	status = "okay";
};

&usbdrd_dwc3 {
	status = "okay";
};

&vdpu {
	status = "okay";
};

&vpu_mmu {
	status = "okay";
};

&vepu {
	status = "okay";
};

&vepu_mmu {
	status = "okay";
};

&vepu22 {
	status = "okay";
};

&vepu22_mmu {
	status = "okay";
};

&vop {
	status = "okay";
};

&vop_mmu {
	status = "okay";
};
