/* board base */
//#include "../rk3588-evb4-lp4-v10-linux.dts"
#include "rp-rk3588-board.dtsi"

#include "rp-tp-i2c6-gt911.dtsi"
#include "rd-rk3588-lcd-gpio.dtsi"
#include "rpdzkj_config.dtsi"

/* usb */
#include "rp-usb-typea-rk3588.dtsi"
#include "rp-usb-host.dtsi"

/* ethernet */
#include "rp-eth-pcie2gmac-rk3588.dtsi"
#include "rp-eth-gmac1.dtsi"

/* pcie */
#include "rp-pcie-power-rk3588.dtsi"
#include "rp-pcie-5g.dtsi"

/* audio */
#include "rp-audio-rt5640.dtsi"

/* wifi/bt */
#include "rp-wifi-bt-ap6275p-rk3588.dtsi"


/* camera */
//#include "rp-camera-dual-ov13855.dtsi"


#include "rp-lcd-hdmi0.dtsi"

/* lcd */
#include "rp-lcd-mipi0-5-720-1280-v2-boxTP.dtsi"
//#include "rp-lcd-mipi0-7-720-1280.dtsi"
//#include "rp-lcd-mipi0-8-800-1280-v3.dtsi"
//#include "rp-lcd-mipi0-8-1200-1920.dtsi"
//#include "rp-lcd-mipi0-10-800-1280-v3.dtsi"
//#include "rp-lcd-mipi0-10-1200-1920.dtsi"
//#include "rp-lcd-box-edp1-13.3-15.6-1920-1080.dtsi"
//#include "rp-lcd-mipi1-gm8775-lvds-21-1920-1080.dtsi"
//#include "rp-lcd-mipi1-gm8775-lvds-10.1-1024-600.dtsi"


/* quadplex lcd */
//#include "rp-lcd-quadplex-mipi0-5-720-1280-v2-boxTP-mipi1-gm8775-lvds-10.1-1024-600-hdmi0-edp1.dtsi"


/ {
    model = "rd-box-rk3588";
    reserved-memory {
        #address-cells = <2>;
        #size-cells = <2>;
        ranges;
        dma_trans: dma-trans@3c000000 {
            reg = <0x0 0x3c000000 0x0 0x04000000>;
        };
    };

    vcc_1v1_nldo_s3: vcc-1v1-nldo-s3 {
        compatible = "regulator-fixed";
        regulator-name = "vcc_1v1_nldo_s3";
        regulator-always-on;
        regulator-boot-on;
        regulator-min-microvolt = <1100000>;
        regulator-max-microvolt = <1100000>;
        vin-supply = <&vcc5v0_sys>;
    };

	fan_gpio_control {
            compatible = "fan_gpio_control";
            gpio-pin = <&gpio4 RK_PA7 GPIO_ACTIVE_HIGH>;
            thermal-zone = "soc-thermal";
    	    threshold-temp = <60000>; //60C
	        running-time = <10000>; //10s

            status = "okay";
        };

        rp_power{
                status = "okay";
                compatible = "rp_power";
                rp_not_deep_sleep = <1>;

//#define GPIO_FUNCTION_OUTPUT 0
//#define GPIO_FUNCTION_INPUT 1
//#define GPIO_FUNCTION_IRQ 2
//#define GPIO_FUNCTION_FLASH 3
//#define GPIO_FUNCTION_OUTPUT_CTRL 4

                //fan {   
                //        gpio_num = <&gpio4 RK_PA7 GPIO_ACTIVE_HIGH>;
                //        gpio_function = <4>;
                //};

                led {  
                        gpio_num = <&gpio4 RK_PA6 GPIO_ACTIVE_HIGH>;
                        gpio_function = <3>;
                };

                usb-host-power {  
                        gpio_num = <&gpio2 RK_PC1 GPIO_ACTIVE_HIGH>;
                        gpio_function = <4>;
                };

                otg-power {
                      gpio_num = <&gpio1 RK_PA2 GPIO_ACTIVE_HIGH>;
                      gpio_function = <4>;
                };
 
                usb-hub-reset {  
                        gpio_num = <&gpio3 RK_PB2 GPIO_ACTIVE_HIGH>;
                        gpio_function = <4>;
                };
    };

        rp_gpio{
                status = "okay";
                compatible = "rp_gpio";

                gpio3c7 {  
                        gpio_num = <&gpio3 RK_PC7 GPIO_ACTIVE_HIGH>;
                        gpio_function = <0>;
                };
                gpio0d3 {
                  gpio_num = <&gpio0 RK_PD3 GPIO_ACTIVE_HIGH>;
                  gpio_function = <0>;
                };
      
                gpio3c4 {
                  gpio_num = <&gpio3 RK_PC4 GPIO_ACTIVE_HIGH>;
                  gpio_function = <0>;
                };

                gpio3c5 {
                  gpio_num = <&gpio3 RK_PC5 GPIO_ACTIVE_HIGH>;
                  gpio_function = <0>;
                };

                gpio3d5 {
                  gpio_num = <&gpio3 RK_PD5 GPIO_ACTIVE_HIGH>;
                  gpio_function = <0>;
                };

                gpio4b2 {
                  gpio_num = <&gpio4 RK_PB2 GPIO_ACTIVE_HIGH>;
                  gpio_function = <0>;
                };

                gpio4b3 {
                  gpio_num = <&gpio4 RK_PB3 GPIO_ACTIVE_HIGH>;
                  gpio_function = <0>;
                };
/*** already use for spi0
                gpio3d1 {
                  gpio_num = <&gpio3 RK_PD1 GPIO_ACTIVE_HIGH>;
                  gpio_function = <0>;
                };

                gpio3d3 {
                  gpio_num = <&gpio3 RK_PD3 GPIO_ACTIVE_HIGH>;
                  gpio_function = <0>;
                };

                gpio3d2 {
                  gpio_num = <&gpio3 RK_PD2 GPIO_ACTIVE_HIGH>;
                  gpio_function = <0>;
                };

                gpio3d4 {
                  gpio_num = <&gpio3 RK_PD4 GPIO_ACTIVE_HIGH>;
                  gpio_function = <0>;
              };
***/
        };

	rp-keys {
		compatible = "rp-keys";
		status = "disabled";
		label = "rp_gpiokeys";

		gpio4b3 {
			gpios = <&gpio4 RK_PB3 GPIO_ACTIVE_LOW>;
		};
        gpio0d3 {
		    label = "gpio0d3_key";
		    gpios = <&gpio0 RK_PD3 GPIO_ACTIVE_LOW>;
		    wakeup;
		    debounce_interval = <10>;
		    press_type = <0>;
		    code = <KEY_ENTER>;
		};
	};

    stm706 {
                status = "okay";
                compatible = "stm706";
                reset_gpio = <&gpio1 RK_PB1 GPIO_ACTIVE_HIGH>;
                wdt_gpio = <&gpio1 RK_PB2 GPIO_ACTIVE_HIGH>;
        };
};


&uart0 {
    status = "okay";
    pinctrl-names = "default";
    pinctrl-0 = <&uart0m0_xfer>;
};

&uart6 {
    status = "okay";
    pinctrl-names = "default";
    pinctrl-0 = <&uart6m0_xfer>;
};

&uart7 {
    status = "okay";
    pinctrl-names = "default";
    pinctrl-0 = <&uart7m1_xfer>;
};

&uart8 {
    status = "okay";
    pinctrl-names = "default";
    pinctrl-0 = <&uart8m0_xfer>;
};

&can0 {
    assigned-clocks = <&cru CLK_CAN0>;
    assigned-clock-rates = <200000000>;
    status = "okay";
    pinctrl-names = "default";
    pinctrl-0 = <&can0m0_pins>;
};


&i2c3{
    status="okay";
};

&i2c4 {
    status = "okay";
    pinctrl-names = "default";
    pinctrl-0 = <&i2c4m1_xfer>;

    hym8563: hym8563@51 {
        compatible = "haoyu,hym8563";
        reg = <0x51>;
        #clock-cells = <0>;
        clock-frequency = <32768>;
        clock-output-names = "hym8563";
        //pinctrl-names = "default";
        //pinctrl-0 = <&hym8563_int>;
        //interrupt-parent = <&gpio0>;
        //interrupts = <RK_PD4 IRQ_TYPE_LEVEL_LOW>;
        //wakeup-source;
    };

};

&spi0 {
    status = "okay";
    pinctrl-0 = <&spi0m3_cs0 &spi0m3_pins>;
    num-cs = <1>;
    spidev@0 {
        status = "okay";
        compatible = "rockchip,spidev";
        reg = <0>;
        spi-max-frequency = <12000000>;
        spi-lsb-first;
    };
};

&sdmmc {
    status = "okay";
   // vmmc-supply = <&vccio_sd_s0>;
};

&fiq_debugger {
    rockchip,baudrate = <115200>;
};

&display_subsystem {
clocks = <&hdptxphy_hdmi_clk0>, <&hdptxphy_hdmi_clk1>;
clock-names = "hdmi0_phy_pll", "hdmi1_phy_pll";
};

&hdptxphy_hdmi_clk0 {
            status = "okay";
};

&hdptxphy_hdmi_clk1 {
            status = "okay";
};
