// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Copyright (c) 2017 Fuzhou Rockchip Electronics Co., Ltd.
 */

#include "dt-bindings/usb/pd.h"
#include "dt-bindings/pwm/pwm.h"
#include "dt-bindings/input/input.h"
#include "rk3399.dtsi"
#include "rk3399-opp.dtsi"

/ {
	compatible = "rockchip,rk3399-sapphire", "rockchip,rk3399";

	chosen {
		stdout-path = "serial2:1500000n8";
	};

	adc_keys: adc-keys {
		compatible = "adc-keys";
		io-channels = <&saradc 1>;
		io-channel-names = "buttons";
		keyup-threshold-microvolt = <1800000>;
		poll-interval = <100>;

		vol-up-key {
			label = "volume up";
			linux,code = <KEY_VOLUMEUP>;
			press-threshold-microvolt = <1750>;
		};

		vol-down-key {
			label = "volume down";
			linux,code = <KEY_VOLUMEDOWN>;
			press-threshold-microvolt = <297500>;
		};

		menu-key {
			label = "menu";
			linux,code = <KEY_MENU>;
			press-threshold-microvolt = <1305500>;
		};

		home-key {
			label = "home";
			linux,code = <KEY_HOME>;
			press-threshold-microvolt = <621250>;
		};

		back-key {
			label = "back";
			linux,code = <KEY_BACK>;
			press-threshold-microvolt = <980000>;
		};

		camera-key {
			label = "camera";
			linux,code = <KEY_CAMERA>;
			press-threshold-microvolt = <787500>;
		};
	};

	clkin_gmac: external-gmac-clock {
		compatible = "fixed-clock";
		clock-frequency = <125000000>;
		clock-output-names = "clkin_gmac";
		#clock-cells = <0>;
	};

	dc_12v: dc-12v {
		compatible = "regulator-fixed";
		regulator-name = "dc_12v";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <12000000>;
		regulator-max-microvolt = <12000000>;
	};

	/*
	 * The fan power supply comes from the baseboard.
	 * For the standalone Sapphire one option is to connect a wire
	 * from  R90030 DNP R0805 pin2  to  C90002 10uF C0805 pin1 (vcc_sys).
	 */
	fan0: gpio-fan {
		#cooling-cells = <2>;
		compatible = "gpio-fan";
		gpio-fan,speed-map = <0 0 3000 1>;
		gpios = <&gpio1 RK_PC2 GPIO_ACTIVE_HIGH>;
		status = "okay";
	};

	keys: gpio-keys {
		compatible = "gpio-keys";
		autorepeat;

		power {
			debounce-interval = <100>;
			gpios = <&gpio0 RK_PA5 GPIO_ACTIVE_LOW>;
			label = "GPIO Power";
			linux,code = <KEY_POWER>;
			linux,input-type = <1>;
			pinctrl-names = "default";
			pinctrl-0 = <&pwr_btn>;
			wakeup-source;
		};
	};

	/* switched by pmic_sleep */
	vcc1v8_s3: vcca1v8_s3: vcc1v8-s3 {
		compatible = "regulator-fixed";
		regulator-name = "vcc1v8_s3";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <1800000>;
		regulator-max-microvolt = <1800000>;
		vin-supply = <&vcc_1v8>;
	};

	vcc3v0_sd: vcc3v0-sd {
		compatible = "regulator-fixed";
		enable-active-high;
		gpio = <&gpio0 RK_PA1 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&sdmmc0_pwr_h>;
		regulator-always-on;
		regulator-max-microvolt = <3000000>;
		regulator-min-microvolt = <3000000>;
		regulator-name = "vcc3v0_sd";
		vin-supply = <&vcc3v3_sys>;
	};

	vcc3v3_sys: vcc3v3-sys {
		compatible = "regulator-fixed";
		regulator-name = "vcc3v3_sys";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		vin-supply = <&vcc_sys>;
	};

	vcc5v0_host: vcc5v0-host-regulator {
		compatible = "regulator-fixed";
		enable-active-high;
		gpio = <&gpio4 RK_PD1 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&vcc5v0_host_en>;
		regulator-name = "vcc5v0_host";
		regulator-always-on;
		vin-supply = <&vcc_sys>;
	};

	vcc5v0_typec0: vcc5v0-typec0-regulator {
		compatible = "regulator-fixed";
		enable-active-high;
		gpio = <&gpio2 RK_PA0 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&vcc5v0_typec0_en>;
		regulator-name = "vcc5v0_typec0";
		vin-supply = <&vcc_sys>;
	};

	vcc_sys: vcc-sys {
		compatible = "regulator-fixed";
		regulator-name = "vcc_sys";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		vin-supply = <&dc_12v>;
	};

	vdd_log: vdd-log {
		compatible = "pwm-regulator";
		pwms = <&pwm2 0 25000 1>;
		regulator-name = "vdd_log";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <800000>;
		regulator-max-microvolt = <1400000>;
		vin-supply = <&vcc_sys>;
	};
};

&cdn_dp {
	status = "okay";
	phys = <&tcphy0_dp>;
};

&cpu_l0 {
	cpu-supply = <&vdd_cpu_l>;
};

&cpu_l1 {
	cpu-supply = <&vdd_cpu_l>;
};

&cpu_l2 {
	cpu-supply = <&vdd_cpu_l>;
};

&cpu_l3 {
	cpu-supply = <&vdd_cpu_l>;
};

&cpu_b0 {
	cpu-supply = <&vdd_cpu_b>;
};

&cpu_b1 {
	cpu-supply = <&vdd_cpu_b>;
};

&cpu_thermal {
	trips {
		cpu_hot: cpu_hot {
			hysteresis = <10000>;
			temperature = <55000>;
			type = "active";
		};
	};

	cooling-maps {
		map2 {
			cooling-device =
				<&fan0 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
			trip = <&cpu_hot>;
		};
	};
};

&emmc_phy {
	status = "okay";
};

&gmac {
	assigned-clocks = <&cru SCLK_RMII_SRC>;
	assigned-clock-parents = <&clkin_gmac>;
	clock_in_out = "input";
	phy-supply = <&vcc_lan>;
	phy-mode = "rgmii";
	pinctrl-names = "default";
	pinctrl-0 = <&rgmii_pins>;
	snps,reset-gpio = <&gpio3 RK_PB7 GPIO_ACTIVE_LOW>;
	snps,reset-active-low;
	snps,reset-delays-us = <0 10000 50000>;
	tx_delay = <0x28>;
	rx_delay = <0x11>;
	status = "okay";
};

&gpu {
	mali-supply = <&vdd_gpu>;
	status = "okay";
};

&hdmi {
	status = "okay";
};

&hdmi_sound {
	status = "okay";
};

&i2c0 {
	clock-frequency = <400000>;
	i2c-scl-rising-time-ns = <168>;
	i2c-scl-falling-time-ns = <4>;
	status = "okay";

	rk808: pmic@1b {
		compatible = "rockchip,rk808";
		reg = <0x1b>;
		interrupt-parent = <&gpio1>;
		interrupts = <21 IRQ_TYPE_LEVEL_LOW>;
		#clock-cells = <1>;
		clock-output-names = "xin32k", "rk808-clkout2";
		pinctrl-names = "default";
		pinctrl-0 = <&pmic_int_l>;
		rockchip,system-power-controller;
		wakeup-source;

		vcc1-supply = <&vcc_sys>;
		vcc2-supply = <&vcc_sys>;
		vcc3-supply = <&vcc_sys>;
		vcc4-supply = <&vcc_sys>;
		vcc6-supply = <&vcc_sys>;
		vcc7-supply = <&vcc_sys>;
		vcc8-supply = <&vcc3v3_sys>;
		vcc9-supply = <&vcc_sys>;
		vcc10-supply = <&vcc_sys>;
		vcc11-supply = <&vcc_sys>;
		vcc12-supply = <&vcc3v3_sys>;
		vddio-supply = <&vcc1v8_pmu>;

		regulators {
			vdd_center: DCDC_REG1 {
				regulator-name = "vdd_center";
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <750000>;
				regulator-max-microvolt = <1350000>;
				regulator-ramp-delay = <6001>;
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd_cpu_l: DCDC_REG2 {
				regulator-name = "vdd_cpu_l";
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <750000>;
				regulator-max-microvolt = <1350000>;
				regulator-ramp-delay = <6001>;
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_ddr: DCDC_REG3 {
				regulator-name = "vcc_ddr";
				regulator-always-on;
				regulator-boot-on;
				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};

			vcc_1v8: DCDC_REG4 {
				regulator-name = "vcc_1v8";
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vcc1v8_dvp: LDO_REG1 {
				regulator-name = "vcc1v8_dvp";
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc3v0_tp: LDO_REG2 {
				regulator-name = "vcc3v0_tp";
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3000000>;
				regulator-max-microvolt = <3000000>;
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc1v8_pmu: LDO_REG3 {
				regulator-name = "vcc1v8_pmu";
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vcc_sdio: LDO_REG4 {
				regulator-name = "vcc_sdio";
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3000000>;
				};
			};

			vcca3v0_codec: LDO_REG5 {
				regulator-name = "vcca3v0_codec";
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3000000>;
				regulator-max-microvolt = <3000000>;
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_1v5: LDO_REG6 {
				regulator-name = "vcc_1v5";
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1500000>;
				regulator-max-microvolt = <1500000>;
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1500000>;
				};
			};

			vcca1v8_codec: LDO_REG7 {
				regulator-name = "vcca1v8_codec";
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_3v0: LDO_REG8 {
				regulator-name = "vcc_3v0";
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3000000>;
				regulator-max-microvolt = <3000000>;
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3000000>;
				};
			};

			vcc3v3_s3: vcc_lan: SWITCH_REG1 {
				regulator-name = "vcc3v3_s3";
				regulator-always-on;
				regulator-boot-on;
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc3v3_s0: SWITCH_REG2 {
				regulator-name = "vcc3v3_s0";
				regulator-always-on;
				regulator-boot-on;
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};
		};
	};

	vdd_cpu_b: regulator@40 {
		compatible = "silergy,syr827";
		reg = <0x40>;
		fcs,suspend-voltage-selector = <1>;
		regulator-name = "vdd_cpu_b";
		regulator-min-microvolt = <712500>;
		regulator-max-microvolt = <1500000>;
		regulator-ramp-delay = <1000>;
		regulator-always-on;
		regulator-boot-on;
		vin-supply = <&vcc_sys>;

		regulator-state-mem {
			regulator-off-in-suspend;
		};
	};

	vdd_gpu: regulator@41 {
		compatible = "silergy,syr828";
		reg = <0x41>;
		fcs,suspend-voltage-selector = <1>;
		regulator-name = "vdd_gpu";
		regulator-min-microvolt = <712500>;
		regulator-max-microvolt = <1500000>;
		regulator-ramp-delay = <1000>;
		regulator-always-on;
		regulator-boot-on;
		vin-supply = <&vcc_sys>;

		regulator-state-mem {
			regulator-off-in-suspend;
		};
	};
};

&i2c4 {
	status = "okay";
	i2c-scl-rising-time-ns = <475>;
	i2c-scl-falling-time-ns = <26>;

	usbc0: fusb302@22 {
		compatible = "fcs,fusb302";
		reg = <0x22>;
		interrupt-parent = <&gpio1>;
		interrupts = <RK_PA2 IRQ_TYPE_LEVEL_LOW>;
		pinctrl-names = "default";
		pinctrl-0 = <&usbc0_int>;
		vbus-supply = <&vcc5v0_typec0>;
		status = "okay";

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				usbc0_role_sw: endpoint@0 {
					remote-endpoint = <&dwc3_0_role_switch>;
				};
			};
		};

		usb_con: connector {
			compatible = "usb-c-connector";
			label = "USB-C";
			data-role = "dual";
			power-role = "dual";
			try-power-role = "sink";
			op-sink-microwatt = <1000000>;
			sink-pdos =
				<PDO_FIXED(5000, 1000, PDO_FIXED_USB_COMM)>;
			source-pdos =
				<PDO_FIXED(5000, 3000, PDO_FIXED_USB_COMM)>;

			displayport = <&cdn_dp>;

			altmodes {
				#address-cells = <1>;
				#size-cells = <0>;

				altmode@0 {
					reg = <0>;
					svid = <0xff01>;
					vdo = <0xffffffff>;
				};
			};

			ports {
				#address-cells = <1>;
				#size-cells = <0>;

				port@0 {
					reg = <0>;
					usbc0_orien_sw: endpoint {
						remote-endpoint = <&tcphy0_orientation_switch>;
					};
				};
				port@1 {
					reg = <1>;
					dp_mode_sw: endpoint {
						remote-endpoint = <&tcphy_dp_altmode_switch>;
					};
				};
			};
		};
	};
};

&i2s2 {
	status = "okay";
};

&io_domains {
	status = "okay";

	bt656-supply = <&vcc_3v0>;
	audio-supply = <&vcca1v8_codec>;
	sdmmc-supply = <&vcc_sdio>;
	gpio1830-supply = <&vcc_3v0>;
};

&pmu_io_domains {
	pmu1830-supply = <&vcc_3v0>;
	status = "okay";
};

&pinctrl {
	buttons {
		pwr_btn: pwr-btn {
			rockchip,pins = <0 RK_PA5 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	fan {
		motor_pwr: motor-pwr {
			rockchip,pins =
				<1 RK_PC2 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	pmic {
		pmic_int_l: pmic-int-l {
			rockchip,pins =
				<1 RK_PC5 RK_FUNC_GPIO &pcfg_pull_up>;
		};

		vsel1_pin: vsel1-pin {
			rockchip,pins = <1 RK_PC1 RK_FUNC_GPIO &pcfg_pull_down>;
		};

		vsel2_pin: vsel2-pin {
			rockchip,pins = <1 RK_PB6 RK_FUNC_GPIO &pcfg_pull_down>;
		};
	};

	sd {
		sdmmc0_pwr_h: sdmmc0-pwr-h {
			rockchip,pins =
				<0 RK_PA1 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	usb2 {
		vcc5v0_host_en: vcc5v0-host-en {
			rockchip,pins =
				<4 RK_PD1 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	usb-typec {
		usbc0_int: usbc0-int {
			rockchip,pins = <1 RK_PA2 RK_FUNC_GPIO &pcfg_pull_up>;
		};

		vcc5v0_typec0_en: vcc5v0-typec0-en {
			rockchip,pins =
				<2 RK_PA0 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};
};

&pwm0 {
	status = "okay";
};

&pwm2 {
	status = "okay";
	pinctrl-names = "active";
	pinctrl-0 = <&pwm2_pin_pull_down>;
};

&saradc {
	vref-supply = <&vcca1v8_s3>;
	status = "okay";
};

&sdhci {
	bus-width = <8>;
	mmc-hs400-1_8v;
	mmc-hs400-enhanced-strobe;
	non-removable;
	status = "okay";
};

&sdmmc {
	broken-cd;
	bus-width = <4>;
	cap-mmc-highspeed;
	cap-sd-highspeed;
	clock-frequency = <150000000>;
	disable-wp;
	max-frequency = <150000000>;
	pinctrl-names = "default";
	pinctrl-0 = <&sdmmc_clk &sdmmc_cmd &sdmmc_cd &sdmmc_bus4>;
	vmmc-supply = <&vcc3v0_sd>;
	vqmmc-supply = <&vcc_sdio>;
	status = "okay";
};

&tcphy0 {
	status = "okay";
	svid = <0xff01>;
	orientation-switch;

	port {
		#address-cells = <1>;
		#size-cells = <0>;
		tcphy0_orientation_switch: endpoint@0 {
			reg = <0>;
			remote-endpoint = <&usbc0_orien_sw>;
		};
		tcphy_dp_altmode_switch: endpoint@1 {
			reg = <1>;
			remote-endpoint = <&dp_mode_sw>;
		};
	};
};

&tcphy1 {
	status = "okay";
};

&tsadc {
	/* tshut mode 0:CRU 1:GPIO */
	rockchip,hw-tshut-mode = <1>;
	/* tshut polarity 0:LOW 1:HIGH */
	rockchip,hw-tshut-polarity = <1>;
	status = "okay";
};

&u2phy0 {
	status = "okay";

	u2phy0_otg: otg-port {
		status = "okay";
	};

	u2phy0_host: host-port {
		phy-supply = <&vcc5v0_host>;
		status = "okay";
	};
};

&u2phy1 {
	status = "okay";

	u2phy1_otg: otg-port {
		status = "okay";
	};

	u2phy1_host: host-port {
		phy-supply = <&vcc5v0_host>;
		status = "okay";
	};
};

&uart0 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart0_xfer &uart0_cts>;
	status = "okay";
};

&uart2 {
	status = "okay";
};

&usb_host0_ehci {
	status = "okay";
};

&usb_host0_ohci {
	status = "okay";
};

&usb_host1_ehci {
	status = "okay";
};

&usb_host1_ohci {
	status = "okay";
};

&usbdrd3_0 {
	status = "okay";
};

&usbdrd_dwc3_0 {
	status = "okay";
	dr_mode = "otg";
	usb-role-switch;
	port {
		#address-cells = <1>;
		#size-cells = <0>;
		dwc3_0_role_switch: endpoint@0 {
			reg = <0>;
			remote-endpoint = <&usbc0_role_sw>;
		};
	};
};

&usbdrd3_1 {
	status = "okay";
};

&usbdrd_dwc3_1 {
	status = "okay";
	dr_mode = "host";
};

&vopb {
	status = "okay";
};

&vopb_mmu {
	status = "okay";
};

&vopl {
	status = "okay";
};

&vopl_mmu {
	status = "okay";
};