// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Copyright (c) 2016 Fuzhou Rockchip Electronics Co., Ltd
 */

#include <dt-bindings/clock/rk3399-cru.h>
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/interrupt-controller/arm-gic.h>
#include <dt-bindings/interrupt-controller/irq.h>
#include <dt-bindings/pinctrl/rockchip.h>
#include <dt-bindings/power/rk3399-power.h>
#include <dt-bindings/soc/rockchip,boot-mode.h>
#include <dt-bindings/soc/rockchip-system-status.h>
#include <dt-bindings/suspend/rockchip-rk3399.h>
#include <dt-bindings/thermal/thermal.h>

#include "rk3399-dram-default-timing.dtsi"

/ {
	compatible = "rockchip,rk3399";

	interrupt-parent = <&gic>;
	#address-cells = <2>;
	#size-cells = <2>;

	aliases {
		dsi0 = &dsi;
		dsi1 = &dsi1;
		ethernet0 = &gmac;
		gpio0 = &gpio0;
		gpio1 = &gpio1;
		gpio2 = &gpio2;
		gpio3 = &gpio3;
		gpio4 = &gpio4;
		i2c0 = &i2c0;
		i2c1 = &i2c1;
		i2c2 = &i2c2;
		i2c3 = &i2c3;
		i2c4 = &i2c4;
		i2c5 = &i2c5;
		i2c6 = &i2c6;
		i2c7 = &i2c7;
		i2c8 = &i2c8;
		mmc0 = &sdio0;
		mmc1 = &sdmmc;
		mmc2 = &sdhci;
		serial0 = &uart0;
		serial1 = &uart1;
		serial2 = &uart2;
		serial3 = &uart3;
		serial4 = &uart4;
	};

	cpus {
		#address-cells = <2>;
		#size-cells = <0>;

		cpu-map {
			cluster0 {
				core0 {
					cpu = <&cpu_l0>;
				};
				core1 {
					cpu = <&cpu_l1>;
				};
				core2 {
					cpu = <&cpu_l2>;
				};
				core3 {
					cpu = <&cpu_l3>;
				};
			};

			cluster1 {
				core0 {
					cpu = <&cpu_b0>;
				};
				core1 {
					cpu = <&cpu_b1>;
				};
			};
		};

		cpu_l0: cpu@0 {
			device_type = "cpu";
			compatible = "arm,cortex-a53";
			reg = <0x0 0x0>;
			enable-method = "psci";
			capacity-dmips-mhz = <485>;
			clocks = <&cru ARMCLKL>;
			#cooling-cells = <2>; /* min followed by max */
			dynamic-power-coefficient = <100>;
			cpu-idle-states = <&CPU_SLEEP &CLUSTER_SLEEP>;
		};

		cpu_l1: cpu@1 {
			device_type = "cpu";
			compatible = "arm,cortex-a53";
			reg = <0x0 0x1>;
			enable-method = "psci";
			capacity-dmips-mhz = <485>;
			clocks = <&cru ARMCLKL>;
			#cooling-cells = <2>; /* min followed by max */
			dynamic-power-coefficient = <100>;
			cpu-idle-states = <&CPU_SLEEP &CLUSTER_SLEEP>;
		};

		cpu_l2: cpu@2 {
			device_type = "cpu";
			compatible = "arm,cortex-a53";
			reg = <0x0 0x2>;
			enable-method = "psci";
			capacity-dmips-mhz = <485>;
			clocks = <&cru ARMCLKL>;
			#cooling-cells = <2>; /* min followed by max */
			dynamic-power-coefficient = <100>;
			cpu-idle-states = <&CPU_SLEEP &CLUSTER_SLEEP>;
		};

		cpu_l3: cpu@3 {
			device_type = "cpu";
			compatible = "arm,cortex-a53";
			reg = <0x0 0x3>;
			enable-method = "psci";
			capacity-dmips-mhz = <485>;
			clocks = <&cru ARMCLKL>;
			#cooling-cells = <2>; /* min followed by max */
			dynamic-power-coefficient = <100>;
			cpu-idle-states = <&CPU_SLEEP &CLUSTER_SLEEP>;
		};

		cpu_b0: cpu@100 {
			device_type = "cpu";
			compatible = "arm,cortex-a72";
			reg = <0x0 0x100>;
			enable-method = "psci";
			capacity-dmips-mhz = <1024>;
			clocks = <&cru ARMCLKB>;
			#cooling-cells = <2>; /* min followed by max */
			dynamic-power-coefficient = <436>;
			cpu-idle-states = <&CPU_SLEEP &CLUSTER_SLEEP>;
		};

		cpu_b1: cpu@101 {
			device_type = "cpu";
			compatible = "arm,cortex-a72";
			reg = <0x0 0x101>;
			enable-method = "psci";
			capacity-dmips-mhz = <1024>;
			clocks = <&cru ARMCLKB>;
			#cooling-cells = <2>; /* min followed by max */
			dynamic-power-coefficient = <436>;
			cpu-idle-states = <&CPU_SLEEP &CLUSTER_SLEEP>;
		};

		idle-states {
			entry-method = "psci";

			CPU_SLEEP: cpu-sleep {
				compatible = "arm,idle-state";
				local-timer-stop;
				arm,psci-suspend-param = <0x0010000>;
				entry-latency-us = <120>;
				exit-latency-us = <250>;
				min-residency-us = <900>;
			};

			CLUSTER_SLEEP: cluster-sleep {
				compatible = "arm,idle-state";
				local-timer-stop;
				arm,psci-suspend-param = <0x1010000>;
				entry-latency-us = <400>;
				exit-latency-us = <500>;
				min-residency-us = <2000>;
			};
		};
	};

	display_subsystem: display-subsystem {
		compatible = "rockchip,display-subsystem";
		ports = <&vopl_out>, <&vopb_out>;
		clocks = <&cru PLL_VPLL>, <&cru PLL_CPLL>;
		clock-names = "hdmi-tmds-pll", "default-vop-pll";
	};

	pmu_a53 {
		compatible = "arm,cortex-a53-pmu";
		interrupts = <GIC_PPI 7 IRQ_TYPE_LEVEL_LOW &ppi_cluster0>;
	};

	pmu_a72 {
		compatible = "arm,cortex-a72-pmu";
		interrupts = <GIC_PPI 7 IRQ_TYPE_LEVEL_LOW &ppi_cluster1>;
	};

	psci {
		compatible = "arm,psci-1.0";
		method = "smc";
	};

	timer {
		compatible = "arm,armv8-timer";
		interrupts = <GIC_PPI 13 IRQ_TYPE_LEVEL_LOW 0>,
			     <GIC_PPI 14 IRQ_TYPE_LEVEL_LOW 0>,
			     <GIC_PPI 11 IRQ_TYPE_LEVEL_LOW 0>,
			     <GIC_PPI 10 IRQ_TYPE_LEVEL_LOW 0>;
		arm,no-tick-in-suspend;
	};

	xin24m: xin24m {
		compatible = "fixed-clock";
		clock-frequency = <24000000>;
		clock-output-names = "xin24m";
		#clock-cells = <0>;
	};

	dummy_cpll: dummy_cpll {
		compatible = "fixed-clock";
		clock-frequency = <0>;
		clock-output-names = "dummy_cpll";
		#clock-cells = <0>;
	};

	dummy_vpll: dummy_vpll {
		compatible = "fixed-clock";
		clock-frequency = <0>;
		clock-output-names = "dummy_vpll";
		#clock-cells = <0>;
	};

	amba: bus {
		compatible = "simple-bus";
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;

		dmac_bus: dma-controller@ff6d0000 {
			compatible = "arm,pl330", "arm,primecell";
			reg = <0x0 0xff6d0000 0x0 0x4000>;
			interrupts = <GIC_SPI 5 IRQ_TYPE_LEVEL_HIGH 0>,
				     <GIC_SPI 6 IRQ_TYPE_LEVEL_HIGH 0>;
			#dma-cells = <1>;
			arm,pl330-periph-burst;
			clocks = <&cru ACLK_DMAC0_PERILP>;
			clock-names = "apb_pclk";
		};

		dmac_peri: dma-controller@ff6e0000 {
			compatible = "arm,pl330", "arm,primecell";
			reg = <0x0 0xff6e0000 0x0 0x4000>;
			interrupts = <GIC_SPI 7 IRQ_TYPE_LEVEL_HIGH 0>,
				     <GIC_SPI 8 IRQ_TYPE_LEVEL_HIGH 0>;
			#dma-cells = <1>;
			arm,pl330-periph-burst;
			clocks = <&cru ACLK_DMAC1_PERILP>;
			clock-names = "apb_pclk";
		};
	};

	pcie0: pcie@f8000000 {
		compatible = "rockchip,rk3399-pcie";
		reg = <0x0 0xf8000000 0x0 0x2000000>,
		      <0x0 0xfd000000 0x0 0x1000000>;
		reg-names = "axi-base", "apb-base";
		device_type = "pci";
		#address-cells = <3>;
		#size-cells = <2>;
		#interrupt-cells = <1>;
		aspm-no-l0s;
		bus-range = <0x0 0x1f>;
		clocks = <&cru ACLK_PCIE>, <&cru ACLK_PERF_PCIE>,
			 <&cru PCLK_PCIE>, <&cru SCLK_PCIE_PM>;
		clock-names = "aclk", "aclk-perf",
			      "hclk", "pm";
		interrupts = <GIC_SPI 49 IRQ_TYPE_LEVEL_HIGH 0>,
			     <GIC_SPI 50 IRQ_TYPE_LEVEL_HIGH 0>,
			     <GIC_SPI 51 IRQ_TYPE_LEVEL_HIGH 0>;
		interrupt-names = "sys", "legacy", "client";
		interrupt-map-mask = <0 0 0 7>;
		interrupt-map = <0 0 0 1 &pcie0_intc 0>,
				<0 0 0 2 &pcie0_intc 1>,
				<0 0 0 3 &pcie0_intc 2>,
				<0 0 0 4 &pcie0_intc 3>;
		max-link-speed = <1>;
		msi-map = <0x0 &its 0x0 0x1000>;
		phys = <&pcie_phy 0>, <&pcie_phy 1>,
		       <&pcie_phy 2>, <&pcie_phy 3>;
		phy-names = "pcie-phy-0", "pcie-phy-1",
			    "pcie-phy-2", "pcie-phy-3";
		power-domains = <&power RK3399_PD_PERIHP>;
		ranges = <0x83000000 0x0 0xfa000000 0x0 0xfa000000 0x0 0x1e00000
			  0x81000000 0x0 0xfbe00000 0x0 0xfbe00000 0x0 0x100000>;
		resets = <&cru SRST_PCIE_CORE>, <&cru SRST_PCIE_MGMT>,
			 <&cru SRST_PCIE_MGMT_STICKY>, <&cru SRST_PCIE_PIPE>,
			 <&cru SRST_PCIE_PM>, <&cru SRST_P_PCIE>,
			 <&cru SRST_A_PCIE>;
		reset-names = "core", "mgmt", "mgmt-sticky", "pipe",
			      "pm", "pclk", "aclk";
		status = "disabled";

		pcie0_intc: interrupt-controller {
			interrupt-controller;
			#address-cells = <0>;
			#interrupt-cells = <1>;
		};
	};

	gmac: ethernet@fe300000 {
		compatible = "rockchip,rk3399-gmac";
		reg = <0x0 0xfe300000 0x0 0x10000>;
		interrupts = <GIC_SPI 12 IRQ_TYPE_LEVEL_HIGH 0>;
		interrupt-names = "macirq";
		clocks = <&cru SCLK_MAC>, <&cru SCLK_MAC_RX>,
			 <&cru SCLK_MAC_TX>, <&cru SCLK_MACREF>,
			 <&cru SCLK_MACREF_OUT>, <&cru ACLK_GMAC>,
			 <&cru PCLK_GMAC>;
		clock-names = "stmmaceth", "mac_clk_rx",
			      "mac_clk_tx", "clk_mac_ref",
			      "clk_mac_refout", "aclk_mac",
			      "pclk_mac";
		power-domains = <&power RK3399_PD_GMAC>;
		resets = <&cru SRST_A_GMAC>;
		reset-names = "stmmaceth";
		rockchip,grf = <&grf>;
		snps,txpbl = <0x4>;
		status = "disabled";
	};

	sdio0: mmc@fe310000 {
		compatible = "rockchip,rk3399-dw-mshc",
			     "rockchip,rk3288-dw-mshc";
		reg = <0x0 0xfe310000 0x0 0x4000>;
		interrupts = <GIC_SPI 64 IRQ_TYPE_LEVEL_HIGH 0>;
		max-frequency = <150000000>;
		clocks = <&cru HCLK_SDIO>, <&cru SCLK_SDIO>,
			 <&cru SCLK_SDIO_DRV>, <&cru SCLK_SDIO_SAMPLE>;
		clock-names = "biu", "ciu", "ciu-drive", "ciu-sample";
		fifo-depth = <0x100>;
		power-domains = <&power RK3399_PD_SDIOAUDIO>;
		resets = <&cru SRST_SDIO0>;
		reset-names = "reset";
		status = "disabled";
	};

	sdmmc: mmc@fe320000 {
		compatible = "rockchip,rk3399-dw-mshc",
			     "rockchip,rk3288-dw-mshc";
		reg = <0x0 0xfe320000 0x0 0x4000>;
		interrupts = <GIC_SPI 65 IRQ_TYPE_LEVEL_HIGH 0>;
		max-frequency = <150000000>;
		assigned-clocks = <&cru HCLK_SD>;
		assigned-clock-rates = <200000000>;
		clocks = <&cru HCLK_SDMMC>, <&cru SCLK_SDMMC>,
			 <&cru SCLK_SDMMC_DRV>, <&cru SCLK_SDMMC_SAMPLE>;
		clock-names = "biu", "ciu", "ciu-drive", "ciu-sample";
		fifo-depth = <0x100>;
		power-domains = <&power RK3399_PD_SD>;
		resets = <&cru SRST_SDMMC>;
		reset-names = "reset";
		status = "disabled";
	};

	sdhci: sdhci@fe330000 {
		compatible = "rockchip,rk3399-sdhci-5.1", "arasan,sdhci-5.1";
		reg = <0x0 0xfe330000 0x0 0x10000>;
		interrupts = <GIC_SPI 11 IRQ_TYPE_LEVEL_HIGH 0>;
		arasan,soc-ctl-syscon = <&grf>;
		assigned-clocks = <&cru SCLK_EMMC>;
		assigned-clock-rates = <200000000>;
		clocks = <&cru SCLK_EMMC>, <&cru ACLK_EMMC>;
		clock-names = "clk_xin", "clk_ahb";
		clock-output-names = "emmc_cardclock";
		#clock-cells = <0>;
		phys = <&emmc_phy>;
		phy-names = "phy_arasan";
		power-domains = <&power RK3399_PD_EMMC>;
		disable-cqe-dcmd;
		disable-cqe;
		status = "disabled";
	};

	usb_host0_ehci: usb@fe380000 {
		compatible = "generic-ehci";
		reg = <0x0 0xfe380000 0x0 0x20000>;
		interrupts = <GIC_SPI 26 IRQ_TYPE_LEVEL_HIGH 0>;
		clocks = <&cru HCLK_HOST0>, <&cru HCLK_HOST0_ARB>,
			 <&u2phy0>;
		phys = <&u2phy0_host>;
		phy-names = "usb";
		status = "disabled";
	};

	usb_host0_ohci: usb@fe3a0000 {
		compatible = "generic-ohci";
		reg = <0x0 0xfe3a0000 0x0 0x20000>;
		interrupts = <GIC_SPI 28 IRQ_TYPE_LEVEL_HIGH 0>;
		clocks = <&cru HCLK_HOST0>, <&cru HCLK_HOST0_ARB>,
			 <&u2phy0>;
		phys = <&u2phy0_host>;
		phy-names = "usb";
		status = "disabled";
	};

	usb_host1_ehci: usb@fe3c0000 {
		compatible = "generic-ehci";
		reg = <0x0 0xfe3c0000 0x0 0x20000>;
		interrupts = <GIC_SPI 30 IRQ_TYPE_LEVEL_HIGH 0>;
		clocks = <&cru HCLK_HOST1>, <&cru HCLK_HOST1_ARB>,
			 <&u2phy1>;
		phys = <&u2phy1_host>;
		phy-names = "usb";
		status = "disabled";
	};

	usb_host1_ohci: usb@fe3e0000 {
		compatible = "generic-ohci";
		reg = <0x0 0xfe3e0000 0x0 0x20000>;
		interrupts = <GIC_SPI 32 IRQ_TYPE_LEVEL_HIGH 0>;
		clocks = <&cru HCLK_HOST1>, <&cru HCLK_HOST1_ARB>,
			 <&u2phy1>;
		phys = <&u2phy1_host>;
		phy-names = "usb";
		status = "disabled";
	};

	usbdrd3_0: usb@fe800000 {
		compatible = "rockchip,rk3399-dwc3";
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;
		clocks = <&cru SCLK_USB3OTG0_REF>, <&cru SCLK_USB3OTG0_SUSPEND>,
			 <&cru ACLK_USB3OTG0>, <&cru ACLK_USB3_RKSOC_AXI_PERF>,
			 <&cru ACLK_USB3>, <&cru ACLK_USB3_GRF>;
		clock-names = "ref_clk", "suspend_clk",
			      "bus_clk", "aclk_usb3_rksoc_axi_perf",
			      "aclk_usb3", "grf_clk";
		status = "disabled";

		usbdrd_dwc3_0: usb@fe800000 {
			compatible = "snps,dwc3";
			reg = <0x0 0xfe800000 0x0 0x100000>;
			interrupts = <GIC_SPI 105 IRQ_TYPE_LEVEL_HIGH 0>;
			clocks = <&cru SCLK_USB3OTG0_REF>, <&cru ACLK_USB3OTG0>,
				 <&cru SCLK_USB3OTG0_SUSPEND>;
			clock-names = "ref", "bus_early", "suspend";
			resets = <&cru SRST_A_USB3_OTG0>;
			reset-names = "usb3-otg";
			dr_mode = "otg";
			phys = <&u2phy0_otg>, <&tcphy0_usb3>;
			phy-names = "usb2-phy", "usb3-phy";
			phy_type = "utmi_wide";
			snps,dis_enblslpm_quirk;
			snps,dis-u1-entry-quirk;
			snps,dis-u2-entry-quirk;
			snps,dis-u2-freeclk-exists-quirk;
			snps,dis_u2_susphy_quirk;
			snps,dis-del-phy-power-chg-quirk;
			snps,dis-tx-ipgap-linecheck-quirk;
			snps,parkmode-disable-hs-quirk;
			snps,parkmode-disable-ss-quirk;
			power-domains = <&power RK3399_PD_USB3>;
			status = "disabled";
		};
	};

	usbdrd3_1: usb@fe900000 {
		compatible = "rockchip,rk3399-dwc3";
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;
		clocks = <&cru SCLK_USB3OTG1_REF>, <&cru SCLK_USB3OTG1_SUSPEND>,
			 <&cru ACLK_USB3OTG1>, <&cru ACLK_USB3_RKSOC_AXI_PERF>,
			 <&cru ACLK_USB3>, <&cru ACLK_USB3_GRF>;
		clock-names = "ref_clk", "suspend_clk",
			      "bus_clk", "aclk_usb3_rksoc_axi_perf",
			      "aclk_usb3", "grf_clk";
		status = "disabled";

		usbdrd_dwc3_1: usb@fe900000 {
			compatible = "snps,dwc3";
			reg = <0x0 0xfe900000 0x0 0x100000>;
			interrupts = <GIC_SPI 110 IRQ_TYPE_LEVEL_HIGH 0>;
			clocks = <&cru SCLK_USB3OTG1_REF>, <&cru ACLK_USB3OTG1>,
				 <&cru SCLK_USB3OTG1_SUSPEND>;
			clock-names = "ref", "bus_early", "suspend";
			resets = <&cru SRST_A_USB3_OTG1>;
			reset-names = "usb3-otg";
			dr_mode = "otg";
			phys = <&u2phy1_otg>, <&tcphy1_usb3>;
			phy-names = "usb2-phy", "usb3-phy";
			phy_type = "utmi_wide";
			snps,dis_enblslpm_quirk;
			snps,dis-u2-freeclk-exists-quirk;
			snps,dis_u2_susphy_quirk;
			snps,dis-del-phy-power-chg-quirk;
			snps,dis-tx-ipgap-linecheck-quirk;
			snps,parkmode-disable-hs-quirk;
			snps,parkmode-disable-ss-quirk;
			power-domains = <&power RK3399_PD_USB3>;
			status = "disabled";
		};
	};

	cdn_dp: dp@fec00000 {
		compatible = "rockchip,rk3399-cdn-dp";
		reg = <0x0 0xfec00000 0x0 0x100000>;
		interrupts = <GIC_SPI 9 IRQ_TYPE_LEVEL_HIGH 0>;
		assigned-clocks = <&cru SCLK_DP_CORE>, <&cru SCLK_SPDIF_REC_DPTX>;
		assigned-clock-rates = <100000000>, <200000000>;
		clocks = <&cru SCLK_DP_CORE>, <&cru PCLK_DP_CTRL>,
			 <&cru SCLK_SPDIF_REC_DPTX>, <&cru PCLK_VIO_GRF>;
		clock-names = "core-clk", "pclk", "spdif", "grf";
		phys = <&tcphy0_dp>, <&tcphy1_dp>;
		power-domains = <&power RK3399_PD_HDCP>;
		resets = <&cru SRST_DPTX_SPDIF_REC>, <&cru SRST_P_UPHY0_DPTX>,
			 <&cru SRST_P_UPHY0_APB>, <&cru SRST_DP_CORE>;
		reset-names = "spdif", "dptx", "apb", "core";
		rockchip,grf = <&grf>;
		#sound-dai-cells = <1>;
		status = "disabled";

		ports {
			dp_in: port {
				#address-cells = <1>;
				#size-cells = <0>;

				dp_in_vopb: endpoint@0 {
					reg = <0>;
					remote-endpoint = <&vopb_out_dp>;
				};

				dp_in_vopl: endpoint@1 {
					reg = <1>;
					remote-endpoint = <&vopl_out_dp>;
				};
			};
		};
	};

	gic: interrupt-controller@fee00000 {
		compatible = "arm,gic-v3";
		#interrupt-cells = <4>;
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;
		interrupt-controller;

		reg = <0x0 0xfee00000 0 0x10000>, /* GICD */
		      <0x0 0xfef00000 0 0xc0000>, /* GICR */
		      <0x0 0xfff00000 0 0x10000>, /* GICC */
		      <0x0 0xfff10000 0 0x10000>, /* GICH */
		      <0x0 0xfff20000 0 0x10000>; /* GICV */
		interrupts = <GIC_PPI 9 IRQ_TYPE_LEVEL_HIGH 0>;
		its: interrupt-controller@fee20000 {
			compatible = "arm,gic-v3-its";
			msi-controller;
			#msi-cells = <1>;
			reg = <0x0 0xfee20000 0x0 0x20000>;
		};

		ppi-partitions {
			ppi_cluster0: interrupt-partition-0 {
				affinity = <&cpu_l0 &cpu_l1 &cpu_l2 &cpu_l3>;
			};

			ppi_cluster1: interrupt-partition-1 {
				affinity = <&cpu_b0 &cpu_b1>;
			};
		};
	};

	saradc: saradc@ff100000 {
		compatible = "rockchip,rk3399-saradc";
		reg = <0x0 0xff100000 0x0 0x100>;
		interrupts = <GIC_SPI 62 IRQ_TYPE_LEVEL_HIGH 0>;
		#io-channel-cells = <1>;
		clocks = <&cru SCLK_SARADC>, <&cru PCLK_SARADC>;
		clock-names = "saradc", "apb_pclk";
		resets = <&cru SRST_P_SARADC>;
		reset-names = "saradc-apb";
		status = "disabled";
	};

	i2c1: i2c@ff110000 {
		compatible = "rockchip,rk3399-i2c";
		reg = <0x0 0xff110000 0x0 0x1000>;
		assigned-clocks = <&cru SCLK_I2C1>;
		assigned-clock-rates = <200000000>;
		clocks = <&cru SCLK_I2C1>, <&cru PCLK_I2C1>;
		clock-names = "i2c", "pclk";
		interrupts = <GIC_SPI 59 IRQ_TYPE_LEVEL_HIGH 0>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2c1_xfer>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	i2c2: i2c@ff120000 {
		compatible = "rockchip,rk3399-i2c";
		reg = <0x0 0xff120000 0x0 0x1000>;
		assigned-clocks = <&cru SCLK_I2C2>;
		assigned-clock-rates = <200000000>;
		clocks = <&cru SCLK_I2C2>, <&cru PCLK_I2C2>;
		clock-names = "i2c", "pclk";
		interrupts = <GIC_SPI 35 IRQ_TYPE_LEVEL_HIGH 0>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2c2_xfer>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	i2c3: i2c@ff130000 {
		compatible = "rockchip,rk3399-i2c";
		reg = <0x0 0xff130000 0x0 0x1000>;
		assigned-clocks = <&cru SCLK_I2C3>;
		assigned-clock-rates = <200000000>;
		clocks = <&cru SCLK_I2C3>, <&cru PCLK_I2C3>;
		clock-names = "i2c", "pclk";
		interrupts = <GIC_SPI 34 IRQ_TYPE_LEVEL_HIGH 0>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2c3_xfer>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	i2c5: i2c@ff140000 {
		compatible = "rockchip,rk3399-i2c";
		reg = <0x0 0xff140000 0x0 0x1000>;
		assigned-clocks = <&cru SCLK_I2C5>;
		assigned-clock-rates = <200000000>;
		clocks = <&cru SCLK_I2C5>, <&cru PCLK_I2C5>;
		clock-names = "i2c", "pclk";
		interrupts = <GIC_SPI 38 IRQ_TYPE_LEVEL_HIGH 0>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2c5_xfer>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	i2c6: i2c@ff150000 {
		compatible = "rockchip,rk3399-i2c";
		reg = <0x0 0xff150000 0x0 0x1000>;
		assigned-clocks = <&cru SCLK_I2C6>;
		assigned-clock-rates = <200000000>;
		clocks = <&cru SCLK_I2C6>, <&cru PCLK_I2C6>;
		clock-names = "i2c", "pclk";
		interrupts = <GIC_SPI 37 IRQ_TYPE_LEVEL_HIGH 0>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2c6_xfer>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	i2c7: i2c@ff160000 {
		compatible = "rockchip,rk3399-i2c";
		reg = <0x0 0xff160000 0x0 0x1000>;
		assigned-clocks = <&cru SCLK_I2C7>;
		assigned-clock-rates = <200000000>;
		clocks = <&cru SCLK_I2C7>, <&cru PCLK_I2C7>;
		clock-names = "i2c", "pclk";
		interrupts = <GIC_SPI 36 IRQ_TYPE_LEVEL_HIGH 0>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2c7_xfer>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	uart0: serial@ff180000 {
		compatible = "rockchip,rk3399-uart", "snps,dw-apb-uart";
		reg = <0x0 0xff180000 0x0 0x100>;
		clocks = <&cru SCLK_UART0>, <&cru PCLK_UART0>;
		clock-names = "baudclk", "apb_pclk";
		interrupts = <GIC_SPI 99 IRQ_TYPE_LEVEL_HIGH 0>;
		reg-shift = <2>;
		reg-io-width = <4>;
		pinctrl-names = "default";
		pinctrl-0 = <&uart0_xfer>;
		status = "disabled";
	};

	uart1: serial@ff190000 {
		compatible = "rockchip,rk3399-uart", "snps,dw-apb-uart";
		reg = <0x0 0xff190000 0x0 0x100>;
		clocks = <&cru SCLK_UART1>, <&cru PCLK_UART1>;
		clock-names = "baudclk", "apb_pclk";
		interrupts = <GIC_SPI 98 IRQ_TYPE_LEVEL_HIGH 0>;
		reg-shift = <2>;
		reg-io-width = <4>;
		pinctrl-names = "default";
		pinctrl-0 = <&uart1_xfer>;
		status = "disabled";
	};

	uart2: serial@ff1a0000 {
		compatible = "rockchip,rk3399-uart", "snps,dw-apb-uart";
		reg = <0x0 0xff1a0000 0x0 0x100>;
		clocks = <&cru SCLK_UART2>, <&cru PCLK_UART2>;
		clock-names = "baudclk", "apb_pclk";
		interrupts = <GIC_SPI 100 IRQ_TYPE_LEVEL_HIGH 0>;
		reg-shift = <2>;
		reg-io-width = <4>;
		pinctrl-names = "default";
		pinctrl-0 = <&uart2c_xfer>;
		status = "disabled";
	};

	uart3: serial@ff1b0000 {
		compatible = "rockchip,rk3399-uart", "snps,dw-apb-uart";
		reg = <0x0 0xff1b0000 0x0 0x100>;
		clocks = <&cru SCLK_UART3>, <&cru PCLK_UART3>;
		clock-names = "baudclk", "apb_pclk";
		interrupts = <GIC_SPI 101 IRQ_TYPE_LEVEL_HIGH 0>;
		reg-shift = <2>;
		reg-io-width = <4>;
		pinctrl-names = "default";
		pinctrl-0 = <&uart3_xfer>;
		status = "disabled";
	};

	spi0: spi@ff1c0000 {
		compatible = "rockchip,rk3399-spi", "rockchip,rk3066-spi";
		reg = <0x0 0xff1c0000 0x0 0x1000>;
		clocks = <&cru SCLK_SPI0>, <&cru PCLK_SPI0>;
		clock-names = "spiclk", "apb_pclk";
		interrupts = <GIC_SPI 68 IRQ_TYPE_LEVEL_HIGH 0>;
		dmas = <&dmac_peri 10>, <&dmac_peri 11>;
		dma-names = "tx", "rx";
		pinctrl-names = "default";
		pinctrl-0 = <&spi0_clk &spi0_tx &spi0_rx &spi0_cs0>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	spi1: spi@ff1d0000 {
		compatible = "rockchip,rk3399-spi", "rockchip,rk3066-spi";
		reg = <0x0 0xff1d0000 0x0 0x1000>;
		clocks = <&cru SCLK_SPI1>, <&cru PCLK_SPI1>;
		clock-names = "spiclk", "apb_pclk";
		interrupts = <GIC_SPI 53 IRQ_TYPE_LEVEL_HIGH 0>;
		dmas = <&dmac_peri 12>, <&dmac_peri 13>;
		dma-names = "tx", "rx";
		pinctrl-names = "default";
		pinctrl-0 = <&spi1_clk &spi1_tx &spi1_rx &spi1_cs0>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	spi2: spi@ff1e0000 {
		compatible = "rockchip,rk3399-spi", "rockchip,rk3066-spi";
		reg = <0x0 0xff1e0000 0x0 0x1000>;
		clocks = <&cru SCLK_SPI2>, <&cru PCLK_SPI2>;
		clock-names = "spiclk", "apb_pclk";
		interrupts = <GIC_SPI 52 IRQ_TYPE_LEVEL_HIGH 0>;
		dmas = <&dmac_peri 14>, <&dmac_peri 15>;
		dma-names = "tx", "rx";
		pinctrl-names = "default";
		pinctrl-0 = <&spi2_clk &spi2_tx &spi2_rx &spi2_cs0>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	spi4: spi@ff1f0000 {
		compatible = "rockchip,rk3399-spi", "rockchip,rk3066-spi";
		reg = <0x0 0xff1f0000 0x0 0x1000>;
		clocks = <&cru SCLK_SPI4>, <&cru PCLK_SPI4>;
		clock-names = "spiclk", "apb_pclk";
		interrupts = <GIC_SPI 67 IRQ_TYPE_LEVEL_HIGH 0>;
		dmas = <&dmac_peri 18>, <&dmac_peri 19>;
		dma-names = "tx", "rx";
		pinctrl-names = "default";
		pinctrl-0 = <&spi4_clk &spi4_tx &spi4_rx &spi4_cs0>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	spi5: spi@ff200000 {
		compatible = "rockchip,rk3399-spi", "rockchip,rk3066-spi";
		reg = <0x0 0xff200000 0x0 0x1000>;
		clocks = <&cru SCLK_SPI5>, <&cru PCLK_SPI5>;
		clock-names = "spiclk", "apb_pclk";
		interrupts = <GIC_SPI 132 IRQ_TYPE_LEVEL_HIGH 0>;
		dmas = <&dmac_bus 8>, <&dmac_bus 9>;
		dma-names = "tx", "rx";
		pinctrl-names = "default";
		pinctrl-0 = <&spi5_clk &spi5_tx &spi5_rx &spi5_cs0>;
		power-domains = <&power RK3399_PD_SDIOAUDIO>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	thermal_zones: thermal-zones {
		soc_thermal: cpu_thermal: cpu-thermal {
			polling-delay-passive = <20>;
			polling-delay = <1000>;
			sustainable-power = <1000>; /* milliwatts */

			thermal-sensors = <&tsadc 0>;

			trips {
				threshold: cpu_alert0: cpu_alert0 {
					temperature = <70000>;
					hysteresis = <2000>;
					type = "passive";
				};
				target: cpu_alert1: cpu_alert1 {
					temperature = <85000>;
					hysteresis = <2000>;
					type = "passive";
				};
				soc_crit: cpu_crit: cpu_crit {
					temperature = <115000>; /* millicelsius */
					hysteresis = <2000>; /* millicelsius */
					type = "critical";
				};
			};

			cooling-maps {
				map0 {
					trip = <&target>;
					cooling-device =
						<&cpu_l0 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
					contribution = <4096>;
				};
				map1 {
					trip = <&target>;
					cooling-device =
						<&cpu_b0 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
					contribution = <1024>;
				};
				map2 {
					trip = <&target>;
					cooling-device =
						<&gpu THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
					contribution = <4096>;
				};
			};
		};

		gpu_thermal: gpu-thermal {
			polling-delay-passive = <100>;
			polling-delay = <1000>;

			thermal-sensors = <&tsadc 1>;
		};
	};

	tsadc: tsadc@ff260000 {
		compatible = "rockchip,rk3399-tsadc";
		reg = <0x0 0xff260000 0x0 0x100>;
		interrupts = <GIC_SPI 97 IRQ_TYPE_LEVEL_HIGH 0>;
		assigned-clocks = <&cru SCLK_TSADC>;
		assigned-clock-rates = <750000>;
		clocks = <&cru SCLK_TSADC>, <&cru PCLK_TSADC>;
		clock-names = "tsadc", "apb_pclk";
		resets = <&cru SRST_TSADC>;
		reset-names = "tsadc-apb";
		rockchip,grf = <&grf>;
		rockchip,hw-tshut-temp = <95000>;
		pinctrl-names = "gpio", "otpout";
		pinctrl-0 = <&otp_pin>;
		pinctrl-1 = <&otp_out>;
		#thermal-sensor-cells = <1>;
		status = "disabled";
	};

	qos_emmc: qos@ffa58000 {
		compatible = "syscon";
		reg = <0x0 0xffa58000 0x0 0x20>;
	};

	qos_gmac: qos@ffa5c000 {
		compatible = "syscon";
		reg = <0x0 0xffa5c000 0x0 0x20>;
	};

	qos_pcie: qos@ffa60080 {
		compatible = "syscon";
		reg = <0x0 0xffa60080 0x0 0x20>;
	};

	qos_usb_host0: qos@ffa60100 {
		compatible = "syscon";
		reg = <0x0 0xffa60100 0x0 0x20>;
	};

	qos_usb_host1: qos@ffa60180 {
		compatible = "syscon";
		reg = <0x0 0xffa60180 0x0 0x20>;
	};

	qos_usb_otg0: qos@ffa70000 {
		compatible = "syscon";
		reg = <0x0 0xffa70000 0x0 0x20>;
	};

	qos_usb_otg1: qos@ffa70080 {
		compatible = "syscon";
		reg = <0x0 0xffa70080 0x0 0x20>;
	};

	qos_sd: qos@ffa74000 {
		compatible = "syscon";
		reg = <0x0 0xffa74000 0x0 0x20>;
	};

	qos_sdioaudio: qos@ffa76000 {
		compatible = "syscon";
		reg = <0x0 0xffa76000 0x0 0x20>;
	};

	qos_hdcp: qos@ffa90000 {
		compatible = "syscon";
		reg = <0x0 0xffa90000 0x0 0x20>;
	};

	qos_iep: qos@ffa98000 {
		compatible = "syscon";
		reg = <0x0 0xffa98000 0x0 0x20>;
	};

	qos_isp0_m0: qos@ffaa0000 {
		compatible = "syscon";
		reg = <0x0 0xffaa0000 0x0 0x20>;
	};

	qos_isp0_m1: qos@ffaa0080 {
		compatible = "syscon";
		reg = <0x0 0xffaa0080 0x0 0x20>;
	};

	qos_isp1_m0: qos@ffaa8000 {
		compatible = "syscon";
		reg = <0x0 0xffaa8000 0x0 0x20>;
	};

	qos_isp1_m1: qos@ffaa8080 {
		compatible = "syscon";
		reg = <0x0 0xffaa8080 0x0 0x20>;
	};

	qos_rga_r: qos@ffab0000 {
		compatible = "syscon";
		reg = <0x0 0xffab0000 0x0 0x20>;
	};

	qos_rga_w: qos@ffab0080 {
		compatible = "syscon";
		reg = <0x0 0xffab0080 0x0 0x20>;
	};

	qos_video_m0: qos@ffab8000 {
		compatible = "syscon";
		reg = <0x0 0xffab8000 0x0 0x20>;
	};

	qos_video_m1_r: qos@ffac0000 {
		compatible = "syscon";
		reg = <0x0 0xffac0000 0x0 0x20>;
	};

	qos_video_m1_w: qos@ffac0080 {
		compatible = "syscon";
		reg = <0x0 0xffac0080 0x0 0x20>;
	};

	qos_vop_big_r: qos@ffac8000 {
		compatible = "syscon";
		reg = <0x0 0xffac8000 0x0 0x20>;
	};

	qos_vop_big_w: qos@ffac8080 {
		compatible = "syscon";
		reg = <0x0 0xffac8080 0x0 0x20>;
	};

	qos_vop_little: qos@ffad0000 {
		compatible = "syscon";
		reg = <0x0 0xffad0000 0x0 0x20>;
	};

	qos_perihp: qos@ffad8080 {
		compatible = "syscon";
		reg = <0x0 0xffad8080 0x0 0x20>;
	};

	qos_gpu: qos@ffae0000 {
		compatible = "syscon";
		reg = <0x0 0xffae0000 0x0 0x20>;
	};

	pmu: power-management@ff310000 {
		compatible = "rockchip,rk3399-pmu", "syscon", "simple-mfd";
		reg = <0x0 0xff310000 0x0 0x1000>;

		/*
		 * Note: RK3399 supports 6 voltage domains including VD_CORE_L,
		 * VD_CORE_B, VD_CENTER, VD_GPU, VD_LOGIC and VD_PMU.
		 * Some of the power domains are grouped together for every
		 * voltage domain.
		 * The detail contents as below.
		 */
		power: power-controller {
			compatible = "rockchip,rk3399-power-controller";
			#power-domain-cells = <1>;
			#address-cells = <1>;
			#size-cells = <0>;

			/* These power domains are grouped by VD_CENTER */
			power-domain@RK3399_PD_IEP {
				reg = <RK3399_PD_IEP>;
				clocks = <&cru ACLK_IEP>,
					 <&cru HCLK_IEP>;
				pm_qos = <&qos_iep>;
			};
			power-domain@RK3399_PD_RGA {
				reg = <RK3399_PD_RGA>;
				clocks = <&cru ACLK_RGA>,
					 <&cru HCLK_RGA>;
				pm_qos = <&qos_rga_r>,
					 <&qos_rga_w>;
			};
			power-domain@RK3399_PD_VCODEC {
				reg = <RK3399_PD_VCODEC>;
				clocks = <&cru ACLK_VCODEC>,
					 <&cru HCLK_VCODEC>;
				pm_qos = <&qos_video_m0>;
			};
			power-domain@RK3399_PD_VDU {
				reg = <RK3399_PD_VDU>;
				clocks = <&cru ACLK_VDU>,
					 <&cru HCLK_VDU>;
				pm_qos = <&qos_video_m1_r>,
					 <&qos_video_m1_w>;
			};

			/* These power domains are grouped by VD_GPU */
			power-domain@RK3399_PD_GPU {
				reg = <RK3399_PD_GPU>;
				clocks = <&cru ACLK_GPU>;
				pm_qos = <&qos_gpu>;
			};

			/* These power domains are grouped by VD_LOGIC */
			power-domain@RK3399_PD_EDP {
				reg = <RK3399_PD_EDP>;
				clocks = <&cru PCLK_EDP_CTRL>;
			};
			power-domain@RK3399_PD_EMMC {
				reg = <RK3399_PD_EMMC>;
				clocks = <&cru ACLK_EMMC>;
				pm_qos = <&qos_emmc>;
			};
			power-domain@RK3399_PD_GMAC {
				reg = <RK3399_PD_GMAC>;
				clocks = <&cru ACLK_GMAC>,
					 <&cru PCLK_GMAC>;
				pm_qos = <&qos_gmac>;
			};
			power-domain@RK3399_PD_PERIHP {
				reg = <RK3399_PD_PERIHP>;
				#address-cells = <1>;
				#size-cells = <0>;
				clocks = <&cru ACLK_PERIHP>;
				pm_qos = <&qos_perihp>,
					 <&qos_pcie>,
					 <&qos_usb_host0>,
					 <&qos_usb_host1>;

				power-domain@RK3399_PD_SD {
					reg = <RK3399_PD_SD>;
					clocks = <&cru HCLK_SDMMC>,
						 <&cru SCLK_SDMMC>;
					pm_qos = <&qos_sd>;
				};
			};
			power-domain@RK3399_PD_SDIOAUDIO {
				reg = <RK3399_PD_SDIOAUDIO>;
				clocks = <&cru HCLK_SDIO>;
				pm_qos = <&qos_sdioaudio>;
			};
			power-domain@RK3399_PD_TCPD0 {
				reg = <RK3399_PD_TCPD0>;
				clocks = <&cru SCLK_UPHY0_TCPDCORE>,
					 <&cru SCLK_UPHY0_TCPDPHY_REF>;
			};
			power-domain@RK3399_PD_TCPD1 {
				reg = <RK3399_PD_TCPD1>;
				clocks = <&cru SCLK_UPHY1_TCPDCORE>,
					 <&cru SCLK_UPHY1_TCPDPHY_REF>;
			};
			power-domain@RK3399_PD_USB3 {
				reg = <RK3399_PD_USB3>;
				clocks = <&cru ACLK_USB3>;
				pm_qos = <&qos_usb_otg0>,
					 <&qos_usb_otg1>;
			};
			power-domain@RK3399_PD_VIO {
				reg = <RK3399_PD_VIO>;
				#address-cells = <1>;
				#size-cells = <0>;

				power-domain@RK3399_PD_HDCP {
					reg = <RK3399_PD_HDCP>;
					clocks = <&cru ACLK_HDCP>,
						 <&cru HCLK_HDCP>,
						 <&cru PCLK_HDCP>;
					pm_qos = <&qos_hdcp>;
				};
				power-domain@RK3399_PD_ISP0 {
					reg = <RK3399_PD_ISP0>;
					clocks = <&cru ACLK_ISP0>,
						 <&cru HCLK_ISP0>;
					pm_qos = <&qos_isp0_m0>,
						 <&qos_isp0_m1>;
				};
				power-domain@RK3399_PD_ISP1 {
					reg = <RK3399_PD_ISP1>;
					clocks = <&cru ACLK_ISP1>,
						 <&cru HCLK_ISP1>;
					pm_qos = <&qos_isp1_m0>,
						 <&qos_isp1_m1>;
				};
				power-domain@RK3399_PD_VO {
					reg = <RK3399_PD_VO>;
					#address-cells = <1>;
					#size-cells = <0>;

					power-domain@RK3399_PD_VOPB {
						reg = <RK3399_PD_VOPB>;
						clocks = <&cru ACLK_VOP0>,
							 <&cru HCLK_VOP0>;
						pm_qos = <&qos_vop_big_r>,
							 <&qos_vop_big_w>;
					};
					power-domain@RK3399_PD_VOPL {
						reg = <RK3399_PD_VOPL>;
						clocks = <&cru ACLK_VOP1>,
							 <&cru HCLK_VOP1>;
						pm_qos = <&qos_vop_little>;
					};
				};
			};
		};
	};

	pmugrf: syscon@ff320000 {
		compatible = "rockchip,rk3399-pmugrf", "syscon", "simple-mfd";
		reg = <0x0 0xff320000 0x0 0x1000>;

		pmu_io_domains: io-domains {
			compatible = "rockchip,rk3399-pmu-io-voltage-domain";
			status = "disabled";
		};

		reboot_mode: reboot-mode {
			compatible = "syscon-reboot-mode";
			offset = <0x300>;
			mode-charge = <BOOT_CHARGING>;
			mode-fastboot = <BOOT_FASTBOOT>;
			mode-loader = <BOOT_BL_DOWNLOAD>;
			mode-normal = <BOOT_NORMAL>;
			mode-panic = <BOOT_PANIC>;
			mode-recovery = <BOOT_RECOVERY>;
			mode-ums = <BOOT_UMS>;
		};

		pmu_pvtm: pmu-pvtm {
			compatible = "rockchip,rk3399-pmu-pvtm";
			#address-cells = <1>;
			#size-cells = <0>;
			status = "disabled";

			pvtm@4 {
				reg = <4>;
				clocks = <&pmucru SCLK_PVTM_PMU>;
				clock-names = "clk";
				resets = <&pmucru SRST_PVTM>;
				reset-names = "rst";
			};
		};
	};

	spi3: spi@ff350000 {
		compatible = "rockchip,rk3399-spi", "rockchip,rk3066-spi";
		reg = <0x0 0xff350000 0x0 0x1000>;
		clocks = <&pmucru SCLK_SPI3_PMU>, <&pmucru PCLK_SPI3_PMU>;
		clock-names = "spiclk", "apb_pclk";
		interrupts = <GIC_SPI 60 IRQ_TYPE_LEVEL_HIGH 0>;
		pinctrl-names = "default";
		pinctrl-0 = <&spi3_clk &spi3_tx &spi3_rx &spi3_cs0>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	uart4: serial@ff370000 {
		compatible = "rockchip,rk3399-uart", "snps,dw-apb-uart";
		reg = <0x0 0xff370000 0x0 0x100>;
		clocks = <&pmucru SCLK_UART4_PMU>, <&pmucru PCLK_UART4_PMU>;
		clock-names = "baudclk", "apb_pclk";
		interrupts = <GIC_SPI 102 IRQ_TYPE_LEVEL_HIGH 0>;
		reg-shift = <2>;
		reg-io-width = <4>;
		pinctrl-names = "default";
		pinctrl-0 = <&uart4_xfer>;
		status = "disabled";
	};

	i2c0: i2c@ff3c0000 {
		compatible = "rockchip,rk3399-i2c";
		reg = <0x0 0xff3c0000 0x0 0x1000>;
		assigned-clocks = <&pmucru SCLK_I2C0_PMU>;
		assigned-clock-rates = <200000000>;
		clocks = <&pmucru SCLK_I2C0_PMU>, <&pmucru PCLK_I2C0_PMU>;
		clock-names = "i2c", "pclk";
		interrupts = <GIC_SPI 57 IRQ_TYPE_LEVEL_HIGH 0>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2c0_xfer>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	i2c4: i2c@ff3d0000 {
		compatible = "rockchip,rk3399-i2c";
		reg = <0x0 0xff3d0000 0x0 0x1000>;
		assigned-clocks = <&pmucru SCLK_I2C4_PMU>;
		assigned-clock-rates = <200000000>;
		clocks = <&pmucru SCLK_I2C4_PMU>, <&pmucru PCLK_I2C4_PMU>;
		clock-names = "i2c", "pclk";
		interrupts = <GIC_SPI 56 IRQ_TYPE_LEVEL_HIGH 0>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2c4_xfer>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	i2c8: i2c@ff3e0000 {
		compatible = "rockchip,rk3399-i2c";
		reg = <0x0 0xff3e0000 0x0 0x1000>;
		assigned-clocks = <&pmucru SCLK_I2C8_PMU>;
		assigned-clock-rates = <200000000>;
		clocks = <&pmucru SCLK_I2C8_PMU>, <&pmucru PCLK_I2C8_PMU>;
		clock-names = "i2c", "pclk";
		interrupts = <GIC_SPI 58 IRQ_TYPE_LEVEL_HIGH 0>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2c8_xfer>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	pwm0: pwm@ff420000 {
		compatible = "rockchip,rk3399-pwm", "rockchip,rk3288-pwm";
		reg = <0x0 0xff420000 0x0 0x10>;
		#pwm-cells = <3>;
		pinctrl-names = "active";
		pinctrl-0 = <&pwm0_pin>;
		clocks = <&pmucru PCLK_RKPWM_PMU>;
		clock-names = "pwm";
		status = "disabled";
	};

	pwm1: pwm@ff420010 {
		compatible = "rockchip,rk3399-pwm", "rockchip,rk3288-pwm";
		reg = <0x0 0xff420010 0x0 0x10>;
		#pwm-cells = <3>;
		pinctrl-names = "active";
		pinctrl-0 = <&pwm1_pin>;
		clocks = <&pmucru PCLK_RKPWM_PMU>;
		clock-names = "pwm";
		status = "disabled";
	};

	pwm2: pwm@ff420020 {
		compatible = "rockchip,rk3399-pwm", "rockchip,rk3288-pwm";
		reg = <0x0 0xff420020 0x0 0x10>;
		#pwm-cells = <3>;
		pinctrl-names = "active";
		pinctrl-0 = <&pwm2_pin>;
		clocks = <&pmucru PCLK_RKPWM_PMU>;
		clock-names = "pwm";
		status = "disabled";
	};

	pwm3: pwm@ff420030 {
		compatible = "rockchip,rk3399-pwm", "rockchip,rk3288-pwm";
		reg = <0x0 0xff420030 0x0 0x10>;
		#pwm-cells = <3>;
		pinctrl-names = "active";
		pinctrl-0 = <&pwm3a_pin>;
		clocks = <&pmucru PCLK_RKPWM_PMU>;
		clock-names = "pwm";
		status = "disabled";
	};

	dfi: dfi@ff630000 {
		reg = <0x00 0xff630000 0x00 0x4000>;
		compatible = "rockchip,rk3399-dfi";
		rockchip,pmu = <&pmugrf>;
		clocks = <&cru PCLK_DDR_MON>;
		clock-names = "pclk_ddr_mon";
		status = "disabled";
	};

	dmc: dmc {
		compatible = "rockchip,rk3399-dmc";
		devfreq-events = <&dfi>;
		interrupts = <GIC_SPI 1 IRQ_TYPE_LEVEL_HIGH 0>;
		clocks = <&cru SCLK_DDRC>;
		clock-names = "dmc_clk";
		ddr_timing = <&ddr_timing>;
		status = "disabled";
	};

	mpp_srv: mpp-srv {
		compatible = "rockchip,mpp-service";
		rockchip,taskqueue-count = <2>;
		rockchip,resetgroup-count = <2>;
		status = "disabled";
	};

	vpu: video-codec@ff650000 {
		compatible = "rockchip,rk3399-vpu";
		reg = <0x0 0xff650000 0x0 0x800>;
		interrupts = <GIC_SPI 114 IRQ_TYPE_LEVEL_HIGH 0>,
			     <GIC_SPI 113 IRQ_TYPE_LEVEL_HIGH 0>;
		interrupt-names = "vepu", "vdpu";
		clocks = <&cru ACLK_VCODEC>, <&cru HCLK_VCODEC>;
		clock-names = "aclk", "hclk";
		iommus = <&vpu_mmu>;
		power-domains = <&power RK3399_PD_VCODEC>;
		status = "disabled";
	};

	vepu: vepu@ff650000 {
		compatible = "rockchip,vpu-encoder-v2";
		reg = <0x0 0xff650000 0x0 0x400>;
		interrupts = <GIC_SPI 114 IRQ_TYPE_LEVEL_HIGH 0>;
		interrupt-names = "irq_enc";
		clocks = <&cru ACLK_VCODEC>, <&cru HCLK_VCODEC>;
		clock-names = "aclk_vcodec", "hclk_vcodec";
		resets = <&cru SRST_H_VCODEC>, <&cru SRST_A_VCODEC>;
		reset-names = "shared_video_h", "shared_video_a";
		iommus = <&vpu_mmu>;
		rockchip,srv = <&mpp_srv>;
		rockchip,taskqueue-node = <0>;
		rockchip,resetgroup-node = <0>;
		power-domains = <&power RK3399_PD_VCODEC>;
		status = "disabled";
	};

	vdpu: vdpu@ff650400 {
		compatible = "rockchip,vpu-decoder-v2";
		reg = <0x0 0xff650400 0x0 0x400>;
		interrupts = <GIC_SPI 113 IRQ_TYPE_LEVEL_HIGH 0>;
		interrupt-names = "irq_dec";
		clocks = <&cru ACLK_VCODEC>, <&cru HCLK_VCODEC>;
		clock-names = "aclk_vcodec", "hclk_vcodec";
		resets = <&cru SRST_H_VCODEC>, <&cru SRST_A_VCODEC>;
		reset-names = "shared_video_h", "shared_video_a";
		iommus = <&vpu_mmu>;
		power-domains = <&power RK3399_PD_VCODEC>;
		rockchip,srv = <&mpp_srv>;
		rockchip,taskqueue-node = <0>;
		rockchip,resetgroup-node = <0>;
		status = "disabled";
	};

	vpu_mmu: iommu@ff650800 {
		compatible = "rockchip,iommu";
		reg = <0x0 0xff650800 0x0 0x40>;
		interrupts = <GIC_SPI 115 IRQ_TYPE_LEVEL_HIGH 0>;
		interrupt-names = "vpu_mmu";
		clocks = <&cru ACLK_VCODEC>, <&cru HCLK_VCODEC>;
		clock-names = "aclk", "iface";
		#iommu-cells = <0>;
		power-domains = <&power RK3399_PD_VCODEC>;
		status = "disabled";
	};

	vdec: video-codec@ff660000 {
		compatible = "rockchip,rk3399-vdec";
		reg = <0x0 0xff660000 0x0 0x400>;
		interrupts = <GIC_SPI 116 IRQ_TYPE_LEVEL_HIGH 0>;
		clocks = <&cru ACLK_VDU>, <&cru HCLK_VDU>,
			 <&cru SCLK_VDU_CA>, <&cru SCLK_VDU_CORE>;
		clock-names = "axi", "ahb", "cabac", "core";
		iommus = <&vdec_mmu>;
		power-domains = <&power RK3399_PD_VDU>;
		status = "disabled";
	};

	rkvdec: rkvdec@ff660000 {
		compatible = "rockchip,rkv-decoder-rk3399";
		reg = <0x0 0xff660000 0x0 0x400>;
		interrupts = <GIC_SPI 116 IRQ_TYPE_LEVEL_HIGH 0>;
		interrupt-names = "irq_dec";
		clocks = <&cru ACLK_VDU>, <&cru HCLK_VDU>,
			 <&cru SCLK_VDU_CA>, <&cru SCLK_VDU_CORE>;
		clock-names = "aclk_vcodec", "hclk_vcodec",
			      "clk_cabac", "clk_core";
		resets = <&cru SRST_H_VDU>, <&cru SRST_A_VDU>,
				 <&cru SRST_H_VDU_NOC>, <&cru SRST_A_VDU_NOC>,
				 <&cru SRST_VDU_CA>, <&cru SRST_VDU_CORE>;
		reset-names = "video_h", "video_a", "niu_h", "niu_a",
			"video_cabac", "video_core";
		iommus = <&vdec_mmu>;
		rockchip,srv = <&mpp_srv>;
		rockchip,taskqueue-node = <1>;
		rockchip,resetgroup-node = <1>;
		power-domains = <&power RK3399_PD_VDU>;
		status = "disabled";
	};

	vdec_mmu: iommu@ff660480 {
		compatible = "rockchip,iommu";
		reg = <0x0 0xff660480 0x0 0x40>, <0x0 0xff6604c0 0x0 0x40>;
		interrupts = <GIC_SPI 117 IRQ_TYPE_LEVEL_HIGH 0>;
		interrupt-names = "vdec_mmu";
		clocks = <&cru ACLK_VDU>, <&cru HCLK_VDU>;
		clock-names = "aclk", "iface";
		power-domains = <&power RK3399_PD_VDU>;
		#iommu-cells = <0>;
		status = "disabled";
	};

	iep: iep@ff670000 {
		compatible = "rockchip,iep";
		iommu_enabled = <1>;
		iommus = <&iep_mmu>;
		reg = <0x0 0xff670000 0x0 0x800>;
		interrupts = <GIC_SPI 42 IRQ_TYPE_LEVEL_HIGH 0>;
		clocks = <&cru ACLK_IEP>, <&cru HCLK_IEP>;
		clock-names = "aclk_iep", "hclk_iep";
		power-domains = <&power RK3399_PD_IEP>;
		allocator = <1>;
		version = <2>;
		status = "disabled";
	};

	iep_mmu: iommu@ff670800 {
		compatible = "rockchip,iommu";
		reg = <0x0 0xff670800 0x0 0x40>;
		interrupts = <GIC_SPI 42 IRQ_TYPE_LEVEL_HIGH 0>;
		interrupt-names = "iep_mmu";
		clocks = <&cru ACLK_IEP>, <&cru HCLK_IEP>;
		clock-names = "aclk", "iface";
		power-domains = <&power RK3399_PD_IEP>;
		#iommu-cells = <0>;
		status = "disabled";
	};

	rga: rga@ff680000 {
		compatible = "rockchip,rk3399-rga";
		reg = <0x0 0xff680000 0x0 0x10000>;
		interrupts = <GIC_SPI 55 IRQ_TYPE_LEVEL_HIGH 0>;
		clocks = <&cru ACLK_RGA>, <&cru HCLK_RGA>, <&cru SCLK_RGA_CORE>;
		clock-names = "aclk", "hclk", "sclk";
		resets = <&cru SRST_RGA_CORE>, <&cru SRST_A_RGA>, <&cru SRST_H_RGA>;
		reset-names = "core", "axi", "ahb";
		power-domains = <&power RK3399_PD_RGA>;
	};

	efuse0: efuse@ff690000 {
		compatible = "rockchip,rk3399-efuse";
		reg = <0x0 0xff690000 0x0 0x80>;
		#address-cells = <1>;
		#size-cells = <1>;
		clocks = <&cru PCLK_EFUSE1024NS>;
		clock-names = "pclk_efuse";

		/* Data cells */
		specification_serial_number: specification-serial-number@6 {
			reg = <0x06 0x1>;
			bits = <0 5>;
		};
		cpu_id: cpu-id@7 {
			reg = <0x07 0x10>;
		};
		cpub_leakage: cpu-leakage@17 {
			reg = <0x17 0x1>;
		};
		gpu_leakage: gpu-leakage@18 {
			reg = <0x18 0x1>;
		};
		center_leakage: center-leakage@19 {
			reg = <0x19 0x1>;
		};
		cpul_leakage: cpu-leakage@1a {
			reg = <0x1a 0x1>;
		};
		logic_leakage: logic-leakage@1b {
			reg = <0x1b 0x1>;
		};
		wafer_info: wafer-info@1c {
			reg = <0x1c 0x1>;
		};
		customer_demand: customer-demand@22 {
			reg = <0x22 0x1>;
			bits = <4 4>;
		};
	};

	pmucru: pmu-clock-controller@ff750000 {
		compatible = "rockchip,rk3399-pmucru";
		reg = <0x0 0xff750000 0x0 0x1000>;
		rockchip,grf = <&pmugrf>;
		#clock-cells = <1>;
		#reset-cells = <1>;
		assigned-clocks = <&pmucru PLL_PPLL>;
		assigned-clock-rates = <676000000>;
	};

	cru: clock-controller@ff760000 {
		compatible = "rockchip,rk3399-cru";
		reg = <0x0 0xff760000 0x0 0x1000>;
		rockchip,grf = <&grf>;
		#clock-cells = <1>;
		#reset-cells = <1>;
		assigned-clocks =
			<&cru PLL_GPLL>, <&cru PLL_CPLL>,
			<&cru PLL_NPLL>,
			<&cru ACLK_PERIHP>, <&cru HCLK_PERIHP>,
			<&cru PCLK_PERIHP>,
			<&cru ACLK_PERILP0>, <&cru HCLK_PERILP0>,
			<&cru PCLK_PERILP0>, <&cru ACLK_CCI>,
			<&cru HCLK_PERILP1>, <&cru PCLK_PERILP1>,
			<&cru ACLK_VIO>, <&cru ACLK_HDCP>,
			<&cru ACLK_GIC_PRE>,
			<&cru PCLK_DDR>;
		assigned-clock-rates =
			 <594000000>,  <800000000>,
			<1000000000>,
			 <150000000>,   <75000000>,
			  <37500000>,
			 <100000000>,  <100000000>,
			  <50000000>, <600000000>,
			 <100000000>,   <50000000>,
			 <400000000>, <400000000>,
			 <200000000>,
			 <200000000>;
	};

	grf: syscon@ff770000 {
		compatible = "rockchip,rk3399-grf", "syscon", "simple-mfd";
		reg = <0x0 0xff770000 0x0 0x10000>;
		#address-cells = <1>;
		#size-cells = <1>;

		io_domains: io-domains {
			compatible = "rockchip,rk3399-io-voltage-domain";
			status = "disabled";
		};

		mipi_dphy_rx0: mipi-dphy-rx0 {
			compatible = "rockchip,rk3399-mipi-dphy";
			clocks = <&cru SCLK_MIPIDPHY_REF>,
				 <&cru SCLK_DPHY_RX0_CFG>,
				 <&cru PCLK_VIO_GRF>;
			clock-names = "dphy-ref", "dphy-cfg", "grf";
			power-domains = <&power RK3399_PD_VIO>;
			#phy-cells = <0>;
			status = "disabled";
		};

		u2phy0: usb2-phy@e450 {
			compatible = "rockchip,rk3399-usb2phy";
			reg = <0xe450 0x10>;
			clocks = <&cru SCLK_USB2PHY0_REF>;
			clock-names = "phyclk";
			#clock-cells = <0>;
			clock-output-names = "clk_usbphy0_480m";
			status = "disabled";

			u2phy0_host: host-port {
				#phy-cells = <0>;
				interrupts = <GIC_SPI 27 IRQ_TYPE_LEVEL_HIGH 0>;
				interrupt-names = "linestate";
				status = "disabled";
			};

			u2phy0_otg: otg-port {
				#phy-cells = <0>;
				interrupts = <GIC_SPI 103 IRQ_TYPE_LEVEL_HIGH 0>,
					     <GIC_SPI 104 IRQ_TYPE_LEVEL_HIGH 0>,
					     <GIC_SPI 106 IRQ_TYPE_LEVEL_HIGH 0>;
				interrupt-names = "otg-bvalid", "otg-id",
						  "linestate";
				status = "disabled";
			};
		};

		u2phy1: usb2-phy@e460 {
			compatible = "rockchip,rk3399-usb2phy";
			reg = <0xe460 0x10>;
			clocks = <&cru SCLK_USB2PHY1_REF>;
			clock-names = "phyclk";
			#clock-cells = <0>;
			clock-output-names = "clk_usbphy1_480m";
			status = "disabled";

			u2phy1_host: host-port {
				#phy-cells = <0>;
				interrupts = <GIC_SPI 31 IRQ_TYPE_LEVEL_HIGH 0>;
				interrupt-names = "linestate";
				status = "disabled";
			};

			u2phy1_otg: otg-port {
				#phy-cells = <0>;
				interrupts = <GIC_SPI 108 IRQ_TYPE_LEVEL_HIGH 0>,
					     <GIC_SPI 109 IRQ_TYPE_LEVEL_HIGH 0>,
					     <GIC_SPI 111 IRQ_TYPE_LEVEL_HIGH 0>;
				interrupt-names = "otg-bvalid", "otg-id",
						  "linestate";
				status = "disabled";
			};
		};

		emmc_phy: phy@f780 {
			compatible = "rockchip,rk3399-emmc-phy";
			reg = <0xf780 0x24>;
			clocks = <&sdhci>;
			clock-names = "emmcclk";
			drive-impedance-ohm = <50>;
			#phy-cells = <0>;
			status = "disabled";
		};

		pcie_phy: pcie-phy {
			compatible = "rockchip,rk3399-pcie-phy";
			clocks = <&cru SCLK_PCIEPHY_REF>;
			clock-names = "refclk";
			#phy-cells = <1>;
			resets = <&cru SRST_PCIEPHY>;
			reset-names = "phy";
			status = "disabled";
		};

		pvtm: pvtm {
			compatible = "rockchip,rk3399-pvtm";
			#address-cells = <1>;
			#size-cells = <0>;
			status = "disabled";

			pvtm@0 {
				reg = <0>;
				clocks = <&cru SCLK_PVTM_CORE_L>;
				clock-names = "clk";
				resets = <&cru SRST_PVTM_CORE_L>;
				reset-names = "rst";
			};
			pvtm@1 {
				reg = <1>;
				clocks = <&cru SCLK_PVTM_CORE_B>;
				clock-names = "clk";
				resets = <&cru SRST_PVTM_CORE_B>;
				reset-names = "rst";
			};
			pvtm@2 {
				reg = <2>;
				clocks = <&cru SCLK_PVTM_DDR>;
				clock-names = "clk";
				resets = <&cru SRST_PVTM_DDR>;
				reset-names = "rst";
			};
			pvtm@3 {
				reg = <3>;
				clocks = <&cru SCLK_PVTM_GPU>;
				clock-names = "clk";
				resets = <&cru SRST_PVTM_GPU>;
				reset-names = "rst";
			};
		};
	};

	tcphy0: phy@ff7c0000 {
		compatible = "rockchip,rk3399-typec-phy";
		reg = <0x0 0xff7c0000 0x0 0x40000>;
		clocks = <&cru SCLK_UPHY0_TCPDCORE>,
			 <&cru SCLK_UPHY0_TCPDPHY_REF>;
		clock-names = "tcpdcore", "tcpdphy-ref";
		assigned-clocks = <&cru SCLK_UPHY0_TCPDCORE>;
		assigned-clock-rates = <50000000>;
		power-domains = <&power RK3399_PD_TCPD0>;
		resets = <&cru SRST_UPHY0>,
			 <&cru SRST_UPHY0_PIPE_L00>,
			 <&cru SRST_P_UPHY0_TCPHY>;
		reset-names = "uphy", "uphy-pipe", "uphy-tcphy";
		rockchip,grf = <&grf>;
		status = "disabled";

		tcphy0_dp: dp-port {
			#phy-cells = <0>;
		};

		tcphy0_usb3: usb3-port {
			#phy-cells = <0>;
		};
	};

	tcphy1: phy@ff800000 {
		compatible = "rockchip,rk3399-typec-phy";
		reg = <0x0 0xff800000 0x0 0x40000>;
		clocks = <&cru SCLK_UPHY1_TCPDCORE>,
			 <&cru SCLK_UPHY1_TCPDPHY_REF>;
		clock-names = "tcpdcore", "tcpdphy-ref";
		assigned-clocks = <&cru SCLK_UPHY1_TCPDCORE>;
		assigned-clock-rates = <50000000>;
		power-domains = <&power RK3399_PD_TCPD1>;
		resets = <&cru SRST_UPHY1>,
			 <&cru SRST_UPHY1_PIPE_L00>,
			 <&cru SRST_P_UPHY1_TCPHY>;
		reset-names = "uphy", "uphy-pipe", "uphy-tcphy";
		rockchip,grf = <&grf>;
		status = "disabled";

		tcphy1_dp: dp-port {
			#phy-cells = <0>;
		};

		tcphy1_usb3: usb3-port {
			#phy-cells = <0>;
		};
	};

	watchdog@ff848000 {
		compatible = "snps,dw-wdt";
		reg = <0x0 0xff848000 0x0 0x100>;
		clocks = <&cru PCLK_WDT>;
		interrupts = <GIC_SPI 120 IRQ_TYPE_LEVEL_HIGH 0>;
	};

	rktimer: rktimer@ff850000 {
		compatible = "rockchip,rk3399-timer";
		reg = <0x0 0xff850000 0x0 0x1000>;
		interrupts = <GIC_SPI 81 IRQ_TYPE_LEVEL_HIGH 0>;
		clocks = <&cru PCLK_TIMER0>, <&cru SCLK_TIMER00>;
		clock-names = "pclk", "timer";
	};

	spdif: spdif@ff870000 {
		compatible = "rockchip,rk3399-spdif";
		reg = <0x0 0xff870000 0x0 0x1000>;
		interrupts = <GIC_SPI 66 IRQ_TYPE_LEVEL_HIGH 0>;
		dmas = <&dmac_bus 7>;
		dma-names = "tx";
		clock-names = "mclk", "hclk";
		clocks = <&cru SCLK_SPDIF_8CH>, <&cru HCLK_SPDIF>;
		pinctrl-names = "default";
		pinctrl-0 = <&spdif_bus>;
		power-domains = <&power RK3399_PD_SDIOAUDIO>;
		#sound-dai-cells = <0>;
		status = "disabled";
	};

	i2s0: i2s@ff880000 {
		compatible = "rockchip,rk3399-i2s", "rockchip,rk3066-i2s";
		reg = <0x0 0xff880000 0x0 0x1000>;
		rockchip,grf = <&grf>;
		interrupts = <GIC_SPI 39 IRQ_TYPE_LEVEL_HIGH 0>;
		dmas = <&dmac_bus 0>, <&dmac_bus 1>;
		dma-names = "tx", "rx";
		clock-names = "i2s_clk", "i2s_hclk";
		clocks = <&cru SCLK_I2S0_8CH>, <&cru HCLK_I2S0_8CH>;
		resets = <&cru SRST_I2S0_8CH>, <&cru SRST_H_I2S0_8CH>;
		reset-names = "reset-m", "reset-h";
		pinctrl-names = "default";
		pinctrl-0 = <&i2s0_8ch_bus>;
		power-domains = <&power RK3399_PD_SDIOAUDIO>;
		#sound-dai-cells = <0>;
		status = "disabled";
	};

	i2s1: i2s@ff890000 {
		compatible = "rockchip,rk3399-i2s", "rockchip,rk3066-i2s";
		reg = <0x0 0xff890000 0x0 0x1000>;
		interrupts = <GIC_SPI 40 IRQ_TYPE_LEVEL_HIGH 0>;
		dmas = <&dmac_bus 2>, <&dmac_bus 3>;
		dma-names = "tx", "rx";
		clock-names = "i2s_clk", "i2s_hclk";
		clocks = <&cru SCLK_I2S1_8CH>, <&cru HCLK_I2S1_8CH>;
		resets = <&cru SRST_I2S1_8CH>, <&cru SRST_H_I2S1_8CH>;
		reset-names = "reset-m", "reset-h";
		pinctrl-names = "default";
		pinctrl-0 = <&i2s1_2ch_bus>;
		power-domains = <&power RK3399_PD_SDIOAUDIO>;
		#sound-dai-cells = <0>;
		status = "disabled";
	};

	i2s2: i2s@ff8a0000 {
		compatible = "rockchip,rk3399-i2s", "rockchip,rk3066-i2s";
		reg = <0x0 0xff8a0000 0x0 0x1000>;
		interrupts = <GIC_SPI 41 IRQ_TYPE_LEVEL_HIGH 0>;
		dmas = <&dmac_bus 4>, <&dmac_bus 5>;
		dma-names = "tx", "rx";
		clock-names = "i2s_clk", "i2s_hclk";
		clocks = <&cru SCLK_I2S2_8CH>, <&cru HCLK_I2S2_8CH>;
		resets = <&cru SRST_I2S2_8CH>, <&cru SRST_H_I2S2_8CH>;
		reset-names = "reset-m", "reset-h";
		power-domains = <&power RK3399_PD_SDIOAUDIO>;
		#sound-dai-cells = <0>;
		status = "disabled";
	};

	rng: rng@ff8b8000 {
		compatible = "rockchip,cryptov1-rng";
		reg = <0x0 0xff8b8000 0x0 0x1000>;
		clocks = <&cru SCLK_CRYPTO1>, <&cru HCLK_S_CRYPTO1>;
		clock-names = "clk_crypto", "hclk_crypto";
		assigned-clocks = <&cru SCLK_CRYPTO1>, <&cru HCLK_S_CRYPTO1>;
		assigned-clock-rates = <150000000>, <100000000>;
		status = "disabled";
	};

	vopl: vop@ff8f0000 {
		compatible = "rockchip,rk3399-vop-lit";
		reg = <0x0 0xff8f0000 0x0 0x600>,
		      <0x0 0xff8f1c00 0x0 0x200>,
		      <0x0 0xff8f2000 0x0 0x400>;
		reg-names = "regs", "cabc_lut", "gamma_lut";
		interrupts = <GIC_SPI 119 IRQ_TYPE_LEVEL_HIGH 0>;
		clocks = <&cru ACLK_VOP1>, <&cru DCLK_VOP1>, <&cru HCLK_VOP1>, <&cru DCLK_VOP1_DIV>;
		clock-names = "aclk_vop", "dclk_vop", "hclk_vop", "dclk_source";
		iommus = <&vopl_mmu>;
		power-domains = <&power RK3399_PD_VOPL>;
		resets = <&cru SRST_A_VOP1>, <&cru SRST_H_VOP1>, <&cru SRST_D_VOP1>;
		reset-names = "axi", "ahb", "dclk";
		status = "disabled";

		vopl_out: port {
			#address-cells = <1>;
			#size-cells = <0>;

			vopl_out_dsi: endpoint@0 {
				reg = <0>;
				remote-endpoint = <&dsi_in_vopl>;
			};

			vopl_out_edp: endpoint@1 {
				reg = <1>;
				remote-endpoint = <&edp_in_vopl>;
			};

			vopl_out_hdmi: endpoint@2 {
				reg = <2>;
				remote-endpoint = <&hdmi_in_vopl>;
			};

			vopl_out_dsi1: endpoint@3 {
				reg = <3>;
				remote-endpoint = <&dsi1_in_vopl>;
			};

			vopl_out_dp: endpoint@4 {
				reg = <4>;
				remote-endpoint = <&dp_in_vopl>;
			};
		};
	};

	vop1_pwm: voppwm@ff8f01a0 {
		compatible = "rockchip,vop-pwm";
		reg = <0x0 0xff8f01a0 0x0 0x10>;
		#pwm-cells = <3>;
		pinctrl-names = "active";
		pinctrl-0 = <&vop1_pwm_pin>;
		clocks = <&cru SCLK_VOP1_PWM>;
		clock-names = "pwm";
		status = "disabled";
	};

	vopl_mmu: iommu@ff8f3f00 {
		compatible = "rockchip,iommu";
		reg = <0x0 0xff8f3f00 0x0 0x100>;
		interrupts = <GIC_SPI 119 IRQ_TYPE_LEVEL_HIGH 0>;
		interrupt-names = "vopl_mmu";
		clocks = <&cru ACLK_VOP1>, <&cru HCLK_VOP1>;
		clock-names = "aclk", "iface";
		power-domains = <&power RK3399_PD_VOPL>;
		#iommu-cells = <0>;
		rockchip,disable-device-link-resume;
		status = "disabled";
	};

	vopb: vop@ff900000 {
		compatible = "rockchip,rk3399-vop-big";
		reg = <0x0 0xff900000 0x0 0x600>,
		      <0x0 0xff901c00 0x0 0x200>,
		      <0x0 0xff902000 0x0 0x1000>;
		reg-names = "regs", "cabc_lut", "gamma_lut";
		interrupts = <GIC_SPI 118 IRQ_TYPE_LEVEL_HIGH 0>;
		clocks = <&cru ACLK_VOP0>, <&cru DCLK_VOP0>, <&cru HCLK_VOP0>, <&cru DCLK_VOP0_DIV>;
		clock-names = "aclk_vop", "dclk_vop", "hclk_vop", "dclk_source";
		iommus = <&vopb_mmu>;
		power-domains = <&power RK3399_PD_VOPB>;
		resets = <&cru SRST_A_VOP0>, <&cru SRST_H_VOP0>, <&cru SRST_D_VOP0>;
		reset-names = "axi", "ahb", "dclk";
		status = "disabled";

		vopb_out: port {
			#address-cells = <1>;
			#size-cells = <0>;

			vopb_out_edp: endpoint@0 {
				reg = <0>;
				remote-endpoint = <&edp_in_vopb>;
			};

			vopb_out_dsi: endpoint@1 {
				reg = <1>;
				remote-endpoint = <&dsi_in_vopb>;
			};

			vopb_out_hdmi: endpoint@2 {
				reg = <2>;
				remote-endpoint = <&hdmi_in_vopb>;
			};

			vopb_out_dsi1: endpoint@3 {
				reg = <3>;
				remote-endpoint = <&dsi1_in_vopb>;
			};

			vopb_out_dp: endpoint@4 {
				reg = <4>;
				remote-endpoint = <&dp_in_vopb>;
			};
		};
	};

	vop0_pwm: voppwm@ff9001a0 {
		compatible = "rockchip,vop-pwm";
		reg = <0x0 0xff9001a0 0x0 0x10>;
		#pwm-cells = <3>;
		pinctrl-names = "active";
		pinctrl-0 = <&vop0_pwm_pin>;
		clocks = <&cru SCLK_VOP0_PWM>;
		clock-names = "pwm";
		status = "disabled";
	};

	vopb_mmu: iommu@ff903f00 {
		compatible = "rockchip,iommu";
		reg = <0x0 0xff903f00 0x0 0x100>;
		interrupts = <GIC_SPI 118 IRQ_TYPE_LEVEL_HIGH 0>;
		interrupt-names = "vopb_mmu";
		clocks = <&cru ACLK_VOP0>, <&cru HCLK_VOP0>;
		clock-names = "aclk", "iface";
		power-domains = <&power RK3399_PD_VOPB>;
		#iommu-cells = <0>;
		rockchip,disable-device-link-resume;
		status = "disabled";
	};

	rkisp1_0: rkisp1@ff910000 {
		compatible = "rockchip,rk3399-rkisp1";
		reg = <0x0 0xff910000 0x0 0x4000>;
		interrupts = <GIC_SPI 43 IRQ_TYPE_LEVEL_HIGH 0>;
		interrupt-names = "isp_irq";
		clocks = <&cru SCLK_ISP0>,
			 <&cru ACLK_ISP0>, <&cru HCLK_ISP0>,
			 <&cru ACLK_ISP0_WRAPPER>, <&cru HCLK_ISP0_WRAPPER>;
		clock-names = "clk_isp",
			 "aclk_isp", "hclk_isp",
			 "aclk_isp_wrap", "hclk_isp_wrap";
		devfreq = <&dmc>;
		power-domains = <&power RK3399_PD_ISP0>;
		iommus = <&isp0_mmu>;
		status = "disabled";
	};

	isp0_mmu: iommu@ff914000 {
		compatible = "rockchip,iommu";
		reg = <0x0 0xff914000 0x0 0x100>, <0x0 0xff915000 0x0 0x100>;
		interrupts = <GIC_SPI 43 IRQ_TYPE_LEVEL_HIGH 0>;
		interrupt-names = "isp0_mmu";
		clocks = <&cru ACLK_ISP0_WRAPPER>, <&cru HCLK_ISP0_WRAPPER>;
		clock-names = "aclk", "iface";
		#iommu-cells = <0>;
		power-domains = <&power RK3399_PD_ISP0>;
		rockchip,disable-mmu-reset;
		status = "disabled";
	};

	rkisp1_1: rkisp1@ff920000 {
		compatible = "rockchip,rk3399-rkisp1";
		reg = <0x0 0xff920000 0x0 0x4000>;
		interrupts = <GIC_SPI 44 IRQ_TYPE_LEVEL_HIGH 0>;
		interrupt-names = "isp_irq";
		clocks = <&cru SCLK_ISP1>,
			 <&cru ACLK_ISP1>, <&cru HCLK_ISP1>,
			 <&cru ACLK_ISP1_WRAPPER>, <&cru HCLK_ISP1_WRAPPER>,
			 <&cru PCLK_ISP1_WRAPPER>;
		clock-names = "clk_isp",
			 "aclk_isp", "hclk_isp",
			 "aclk_isp_wrap", "hclk_isp_wrap",
			 "pclk_isp_wrap";
		devfreq = <&dmc>;
		power-domains = <&power RK3399_PD_ISP1>;
		iommus = <&isp1_mmu>;
		status = "disabled";
	};

	isp1_mmu: iommu@ff924000 {
		compatible = "rockchip,iommu";
		reg = <0x0 0xff924000 0x0 0x100>, <0x0 0xff925000 0x0 0x100>;
		interrupts = <GIC_SPI 44 IRQ_TYPE_LEVEL_HIGH 0>;
		interrupt-names = "isp1_mmu";
		clocks = <&cru ACLK_ISP1_WRAPPER>, <&cru HCLK_ISP1_WRAPPER>;
		clock-names = "aclk", "iface";
		#iommu-cells = <0>;
		power-domains = <&power RK3399_PD_ISP1>;
		rockchip,disable-mmu-reset;
		status = "disabled";
	};

	hdmi_sound: hdmi-sound {
		compatible = "simple-audio-card";
		simple-audio-card,format = "i2s";
		simple-audio-card,mclk-fs = <256>;
		simple-audio-card,name = "hdmi-sound";
		status = "disabled";

		simple-audio-card,cpu {
			sound-dai = <&i2s2>;
		};
		simple-audio-card,codec {
			sound-dai = <&hdmi>;
		};
	};

	hdmi: hdmi@ff940000 {
		compatible = "rockchip,rk3399-dw-hdmi";
		reg = <0x0 0xff940000 0x0 0x20000>;
		interrupts = <GIC_SPI 23 IRQ_TYPE_LEVEL_HIGH 0>;
		clocks = <&cru PCLK_HDMI_CTRL>,
			 <&cru SCLK_HDMI_SFR>,
			 <&cru SCLK_HDMI_CEC>,
			 <&cru PCLK_VIO_GRF>,
			 <&cru PLL_VPLL>;
		clock-names = "iahb", "isfr", "cec", "grf", "vpll";
		power-domains = <&power RK3399_PD_HDCP>;
		reg-io-width = <4>;
		rockchip,grf = <&grf>;
		#sound-dai-cells = <0>;
		pinctrl-names = "default";
		pinctrl-0 = <&hdmi_i2c_xfer>;
		status = "disabled";

		ports {
			hdmi_in: port {
				#address-cells = <1>;
				#size-cells = <0>;

				hdmi_in_vopb: endpoint@0 {
					reg = <0>;
					remote-endpoint = <&vopb_out_hdmi>;
				};
				hdmi_in_vopl: endpoint@1 {
					reg = <1>;
					remote-endpoint = <&vopl_out_hdmi>;
				};
			};
		};
	};

	dsi: mipi_dsi: dsi@ff960000 {
		compatible = "rockchip,rk3399-mipi-dsi", "snps,dw-mipi-dsi";
		reg = <0x0 0xff960000 0x0 0x8000>;
		interrupts = <GIC_SPI 45 IRQ_TYPE_LEVEL_HIGH 0>;
		clocks = <&cru SCLK_DPHY_PLL>, <&cru PCLK_MIPI_DSI0>,
			 <&cru SCLK_DPHY_TX0_CFG>, <&cru PCLK_VIO_GRF>;
		clock-names = "ref", "pclk", "phy_cfg", "grf";
		power-domains = <&power RK3399_PD_VIO>;
		resets = <&cru SRST_P_MIPI_DSI0>;
		reset-names = "apb";
		rockchip,grf = <&grf>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				#address-cells = <1>;
				#size-cells = <0>;

				dsi_in_vopb: endpoint@0 {
					reg = <0>;
					remote-endpoint = <&vopb_out_dsi>;
				};
				dsi_in_vopl: endpoint@1 {
					reg = <1>;
					remote-endpoint = <&vopl_out_dsi>;
				};
			};
		};
	};

	dsi1: mipi_dsi1: dsi@ff968000 {
		compatible = "rockchip,rk3399-mipi-dsi", "snps,dw-mipi-dsi";
		reg = <0x0 0xff968000 0x0 0x8000>;
		interrupts = <GIC_SPI 46 IRQ_TYPE_LEVEL_HIGH 0>;
		clocks = <&cru SCLK_DPHY_PLL>, <&cru PCLK_MIPI_DSI1>,
			 <&cru SCLK_DPHY_TX1RX1_CFG>, <&cru PCLK_VIO_GRF>;
		clock-names = "ref", "pclk", "phy_cfg", "grf";
		power-domains = <&power RK3399_PD_VIO>;
		resets = <&cru SRST_P_MIPI_DSI1>;
		reset-names = "apb";
		rockchip,grf = <&grf>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				#address-cells = <1>;
				#size-cells = <0>;

				dsi1_in_vopb: endpoint@0 {
					reg = <0>;
					remote-endpoint = <&vopb_out_dsi1>;
				};

				dsi1_in_vopl: endpoint@1 {
					reg = <1>;
					remote-endpoint = <&vopl_out_dsi1>;
				};
			};
		};
	};

	mipi_dphy_tx1rx1: mipi-dphy-tx1rx1@ff968000 {
		compatible = "rockchip,rk3399-mipi-dphy";
		reg = <0x0 0xff968000 0x0 0x8000>;
		clocks = <&cru SCLK_MIPIDPHY_REF>,
			 <&cru SCLK_DPHY_TX1RX1_CFG>,
			 <&cru PCLK_VIO_GRF>,
			 <&cru PCLK_MIPI_DSI1>;
		clock-names = "dphy-ref", "dphy-cfg",
			"grf", "pclk_mipi_dsi";
		rockchip,grf = <&grf>;
		power-domains = <&power RK3399_PD_VIO>;
		status = "disabled";
	};

	edp: edp@ff970000 {
		compatible = "rockchip,rk3399-edp";
		reg = <0x0 0xff970000 0x0 0x8000>;
		interrupts = <GIC_SPI 10 IRQ_TYPE_LEVEL_HIGH 0>;
		clocks = <&cru PCLK_EDP>, <&cru PCLK_EDP_CTRL>, <&cru PCLK_VIO_GRF>;
		clock-names = "dp", "pclk", "grf";
		pinctrl-names = "default";
		pinctrl-0 = <&edp_hpd>;
		power-domains = <&power RK3399_PD_EDP>;
		resets = <&cru SRST_P_EDP_CTRL>;
		reset-names = "dp";
		rockchip,grf = <&grf>;
		status = "disabled";

		ports {
			#address-cells = <1>;
			#size-cells = <0>;
			edp_in: port@0 {
				reg = <0>;
				#address-cells = <1>;
				#size-cells = <0>;

				edp_in_vopb: endpoint@0 {
					reg = <0>;
					remote-endpoint = <&vopb_out_edp>;
				};

				edp_in_vopl: endpoint@1 {
					reg = <1>;
					remote-endpoint = <&vopl_out_edp>;
				};
			};
		};
	};

	gpu: gpu@ff9a0000 {
		compatible = "arm,malit860",
			     "arm,malit86x",
			     "arm,malit8xx",
			     "arm,mali-midgard";
		reg = <0x0 0xff9a0000 0x0 0x10000>;
		interrupts = <GIC_SPI 20 IRQ_TYPE_LEVEL_HIGH 0>,
			     <GIC_SPI 21 IRQ_TYPE_LEVEL_HIGH 0>,
			     <GIC_SPI 19 IRQ_TYPE_LEVEL_HIGH 0>;
		interrupt-names = "job", "mmu", "gpu";
		clocks = <&cru ACLK_GPU>;
		clock-names = "clk_mali";
		#cooling-cells = <2>;
		power-domains = <&power RK3399_PD_GPU>;
		power-off-delay-ms = <200>;
		upthreshold = <40>;
		downdifferential = <10>;
		status = "disabled";

		gpu_power_model: power_model {
			compatible = "arm,mali-simple-power-model";
			static-coefficient = <411000>;
			dynamic-coefficient = <733>;
			ts = <32000 4700 (-80) 2>;
			thermal-zone = "gpu-thermal";
		};
	};

	nocp_cci_msch0: nocp-cci-msch0@ffa86000 {
		compatible = "rockchip,rk3399-nocp";
		reg = <0x0 0xffa86000 0x0 0x400>;
	};

	nocp_gpu_msch0: nocp-gpu-msch0@ffa86400 {
		compatible = "rockchip,rk3399-nocp";
		reg = <0x0 0xffa86400 0x0 0x400>;
	};

	nocp_hp_msch0: nocp-hp-msch0@ffa86800 {
		compatible = "rockchip,rk3399-nocp";
		reg = <0x0 0xffa86800 0x0 0x400>;
	};

	nocp_lp_msch0: nocp-lp-msch0@ffa86c00 {
		compatible = "rockchip,rk3399-nocp";
		reg = <0x0 0xffa86c00 0x0 0x400>;
	};

	nocp_video_msch0: nocp-video-msch0@ffa87000 {
		compatible = "rockchip,rk3399-nocp";
		reg = <0x0 0xffa87000 0x0 0x400>;
	};

	nocp_vio0_msch0: nocp-vio0-msch0@ffa87400 {
		compatible = "rockchip,rk3399-nocp";
		reg = <0x0 0xffa87400 0x0 0x400>;
	};

	nocp_vio1_msch0: nocp-vio1-msch0@ffa87800 {
		compatible = "rockchip,rk3399-nocp";
		reg = <0x0 0xffa87800 0x0 0x400>;
	};

	nocp_cci_msch1: nocp-cci-msch1@ffa8e000 {
		compatible = "rockchip,rk3399-nocp";
		reg = <0x0 0xffa8e000 0x0 0x400>;
	};

	nocp_gpu_msch1: nocp-gpu-msch1@ffa8e400 {
		compatible = "rockchip,rk3399-nocp";
		reg = <0x0 0xffa8e400 0x0 0x400>;
	};

	nocp_hp_msch1: nocp-hp-msch1@ffa8e800 {
		compatible = "rockchip,rk3399-nocp";
		reg = <0x0 0xffa8e800 0x0 0x400>;
	};

	nocp_lp_msch1: nocp-lp-msch1@ffa8ec00 {
		compatible = "rockchip,rk3399-nocp";
		reg = <0x0 0xffa8ec00 0x0 0x400>;
	};

	nocp_video_msch1: nocp-video-msch1@ffa8f000 {
		compatible = "rockchip,rk3399-nocp";
		reg = <0x0 0xffa8f000 0x0 0x400>;
	};

	nocp_vio0_msch1: nocp-vio0-msch1@ffa8f400 {
		compatible = "rockchip,rk3399-nocp";
		reg = <0x0 0xffa8f400 0x0 0x400>;
	};

	nocp_vio1_msch1: nocp-vio1-msch1@ffa8f800 {
		compatible = "rockchip,rk3399-nocp";
		reg = <0x0 0xffa8f800 0x0 0x400>;
	};

	rockchip_system_monitor: rockchip-system-monitor {
		compatible = "rockchip,system-monitor";

		rockchip,thermal-zone = "soc-thermal";
		rockchip,polling-delay = <200>; /* milliseconds */
	};

	pinctrl: pinctrl {
		compatible = "rockchip,rk3399-pinctrl";
		rockchip,grf = <&grf>;
		rockchip,pmu = <&pmugrf>;
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;

		gpio0: gpio0@ff720000 {
			compatible = "rockchip,gpio-bank";
			reg = <0x0 0xff720000 0x0 0x100>;
			clocks = <&pmucru PCLK_GPIO0_PMU>;
			interrupts = <GIC_SPI 14 IRQ_TYPE_LEVEL_HIGH 0>;

			gpio-controller;
			#gpio-cells = <0x2>;

			interrupt-controller;
			#interrupt-cells = <0x2>;
		};

		gpio1: gpio1@ff730000 {
			compatible = "rockchip,gpio-bank";
			reg = <0x0 0xff730000 0x0 0x100>;
			clocks = <&pmucru PCLK_GPIO1_PMU>;
			interrupts = <GIC_SPI 15 IRQ_TYPE_LEVEL_HIGH 0>;

			gpio-controller;
			#gpio-cells = <0x2>;

			interrupt-controller;
			#interrupt-cells = <0x2>;
		};

		gpio2: gpio2@ff780000 {
			compatible = "rockchip,gpio-bank";
			reg = <0x0 0xff780000 0x0 0x100>;
			clocks = <&cru PCLK_GPIO2>;
			interrupts = <GIC_SPI 16 IRQ_TYPE_LEVEL_HIGH 0>;

			gpio-controller;
			#gpio-cells = <0x2>;

			interrupt-controller;
			#interrupt-cells = <0x2>;
		};

		gpio3: gpio3@ff788000 {
			compatible = "rockchip,gpio-bank";
			reg = <0x0 0xff788000 0x0 0x100>;
			clocks = <&cru PCLK_GPIO3>;
			interrupts = <GIC_SPI 17 IRQ_TYPE_LEVEL_HIGH 0>;

			gpio-controller;
			#gpio-cells = <0x2>;

			interrupt-controller;
			#interrupt-cells = <0x2>;
		};

		gpio4: gpio4@ff790000 {
			compatible = "rockchip,gpio-bank";
			reg = <0x0 0xff790000 0x0 0x100>;
			clocks = <&cru PCLK_GPIO4>;
			interrupts = <GIC_SPI 18 IRQ_TYPE_LEVEL_HIGH 0>;

			gpio-controller;
			#gpio-cells = <0x2>;

			interrupt-controller;
			#interrupt-cells = <0x2>;
		};

		pcfg_pull_up: pcfg-pull-up {
			bias-pull-up;
		};

		pcfg_pull_down: pcfg-pull-down {
			bias-pull-down;
		};

		pcfg_pull_none: pcfg-pull-none {
			bias-disable;
		};

		pcfg_pull_none_10ma: pcfg-pull-none-10ma {
			bias-disable;
			drive-strength = <10>;
		};

		pcfg_pull_none_12ma: pcfg-pull-none-12ma {
			bias-disable;
			drive-strength = <12>;
		};

		pcfg_pull_none_13ma: pcfg-pull-none-13ma {
			bias-disable;
			drive-strength = <13>;
		};

		pcfg_pull_none_18ma: pcfg-pull-none-18ma {
			bias-disable;
			drive-strength = <18>;
		};

		pcfg_pull_none_20ma: pcfg-pull-none-20ma {
			bias-disable;
			drive-strength = <20>;
		};

		pcfg_pull_up_2ma: pcfg-pull-up-2ma {
			bias-pull-up;
			drive-strength = <2>;
		};

		pcfg_pull_up_8ma: pcfg-pull-up-8ma {
			bias-pull-up;
			drive-strength = <8>;
		};

		pcfg_pull_up_10ma: pcfg-pull-up-10ma {
			bias-pull-up;
			drive-strength = <10>;
		};

		pcfg_pull_up_18ma: pcfg-pull-up-18ma {
			bias-pull-up;
			drive-strength = <18>;
		};

		pcfg_pull_up_20ma: pcfg-pull-up-20ma {
			bias-pull-up;
			drive-strength = <20>;
		};

		pcfg_pull_down_4ma: pcfg-pull-down-4ma {
			bias-pull-down;
			drive-strength = <4>;
		};

		pcfg_pull_down_8ma: pcfg-pull-down-8ma {
			bias-pull-down;
			drive-strength = <8>;
		};

		pcfg_pull_down_12ma: pcfg-pull-down-12ma {
			bias-pull-down;
			drive-strength = <12>;
		};

		pcfg_pull_down_18ma: pcfg-pull-down-18ma {
			bias-pull-down;
			drive-strength = <18>;
		};

		pcfg_pull_down_20ma: pcfg-pull-down-20ma {
			bias-pull-down;
			drive-strength = <20>;
		};

		pcfg_output_high: pcfg-output-high {
			output-high;
		};

		pcfg_output_low: pcfg-output-low {
			output-low;
		};

		clock {
			clk_32k: clk-32k {
				rockchip,pins = <0 RK_PA0 2 &pcfg_pull_none>;
			};
		};

		edp {
			edp_hpd: edp-hpd {
				rockchip,pins =
					<4 RK_PC7 2 &pcfg_pull_none>;
			};
		};

		gmac {
			rgmii_pins: rgmii-pins {
				rockchip,pins =
					/* mac_txclk */
					<3 RK_PC1 1 &pcfg_pull_none_13ma>,
					/* mac_rxclk */
					<3 RK_PB6 1 &pcfg_pull_none>,
					/* mac_mdio */
					<3 RK_PB5 1 &pcfg_pull_none>,
					/* mac_txen */
					<3 RK_PB4 1 &pcfg_pull_none_13ma>,
					/* mac_clk */
					<3 RK_PB3 1 &pcfg_pull_none>,
					/* mac_rxdv */
					<3 RK_PB1 1 &pcfg_pull_none>,
					/* mac_mdc */
					<3 RK_PB0 1 &pcfg_pull_none>,
					/* mac_rxd1 */
					<3 RK_PA7 1 &pcfg_pull_none>,
					/* mac_rxd0 */
					<3 RK_PA6 1 &pcfg_pull_none>,
					/* mac_txd1 */
					<3 RK_PA5 1 &pcfg_pull_none_13ma>,
					/* mac_txd0 */
					<3 RK_PA4 1 &pcfg_pull_none_13ma>,
					/* mac_rxd3 */
					<3 RK_PA3 1 &pcfg_pull_none>,
					/* mac_rxd2 */
					<3 RK_PA2 1 &pcfg_pull_none>,
					/* mac_txd3 */
					<3 RK_PA1 1 &pcfg_pull_none_13ma>,
					/* mac_txd2 */
					<3 RK_PA0 1 &pcfg_pull_none_13ma>;
			};

			rmii_pins: rmii-pins {
				rockchip,pins =
					/* mac_mdio */
					<3 RK_PB5 1 &pcfg_pull_none>,
					/* mac_txen */
					<3 RK_PB4 1 &pcfg_pull_none_13ma>,
					/* mac_clk */
					<3 RK_PB3 1 &pcfg_pull_none>,
					/* mac_rxer */
					<3 RK_PB2 1 &pcfg_pull_none>,
					/* mac_rxdv */
					<3 RK_PB1 1 &pcfg_pull_none>,
					/* mac_mdc */
					<3 RK_PB0 1 &pcfg_pull_none>,
					/* mac_rxd1 */
					<3 RK_PA7 1 &pcfg_pull_none>,
					/* mac_rxd0 */
					<3 RK_PA6 1 &pcfg_pull_none>,
					/* mac_txd1 */
					<3 RK_PA5 1 &pcfg_pull_none_13ma>,
					/* mac_txd0 */
					<3 RK_PA4 1 &pcfg_pull_none_13ma>;
			};
		};

		i2c0 {
			i2c0_xfer: i2c0-xfer {
				rockchip,pins =
					<1 RK_PB7 2 &pcfg_pull_none>,
					<1 RK_PC0 2 &pcfg_pull_none>;
			};
		};

		i2c1 {
			i2c1_xfer: i2c1-xfer {
				rockchip,pins =
					<4 RK_PA2 1 &pcfg_pull_none>,
					<4 RK_PA1 1 &pcfg_pull_none>;
			};
		};

		i2c2 {
			i2c2_xfer: i2c2-xfer {
				rockchip,pins =
					<2 RK_PA1 2 &pcfg_pull_none_12ma>,
					<2 RK_PA0 2 &pcfg_pull_none_12ma>;
			};
		};

		i2c3 {
			i2c3_xfer: i2c3-xfer {
				rockchip,pins =
					<4 RK_PC1 1 &pcfg_pull_none>,
					<4 RK_PC0 1 &pcfg_pull_none>;
			};

			i2c3_gpio: i2c3_gpio {
				rockchip,pins =
					<4 RK_PC1 RK_FUNC_GPIO &pcfg_pull_none>,
					<4 RK_PC0 RK_FUNC_GPIO &pcfg_pull_none>;
			};

		};

		i2c4 {
			i2c4_xfer: i2c4-xfer {
				rockchip,pins =
					<1 RK_PB4 1 &pcfg_pull_none>,
					<1 RK_PB3 1 &pcfg_pull_none>;
			};
		};

		i2c5 {
			i2c5_xfer: i2c5-xfer {
				rockchip,pins =
					<3 RK_PB3 2 &pcfg_pull_none>,
					<3 RK_PB2 2 &pcfg_pull_none>;
			};
		};

		i2c6 {
			i2c6_xfer: i2c6-xfer {
				rockchip,pins =
					<2 RK_PB2 2 &pcfg_pull_none>,
					<2 RK_PB1 2 &pcfg_pull_none>;
			};
		};

		i2c7 {
			i2c7_xfer: i2c7-xfer {
				rockchip,pins =
					<2 RK_PB0 2 &pcfg_pull_none>,
					<2 RK_PA7 2 &pcfg_pull_none>;
			};
		};

		i2c8 {
			i2c8_xfer: i2c8-xfer {
				rockchip,pins =
					<1 RK_PC5 1 &pcfg_pull_none>,
					<1 RK_PC4 1 &pcfg_pull_none>;
			};
		};

		i2s0 {
			i2s0_2ch_bus: i2s0-2ch-bus {
				rockchip,pins =
					<3 RK_PD0 1 &pcfg_pull_none>,
					<3 RK_PD1 1 &pcfg_pull_none>,
					<3 RK_PD2 1 &pcfg_pull_none>,
					<3 RK_PD3 1 &pcfg_pull_none>,
					<3 RK_PD7 1 &pcfg_pull_none>,
					<4 RK_PA0 1 &pcfg_pull_none>;
			};

			i2s0_8ch_bus: i2s0-8ch-bus {
				rockchip,pins =
					<3 RK_PD0 1 &pcfg_pull_none>,
					<3 RK_PD1 1 &pcfg_pull_none>,
					<3 RK_PD2 1 &pcfg_pull_none>,
					<3 RK_PD3 1 &pcfg_pull_none>,
					<3 RK_PD4 1 &pcfg_pull_none>,
					<3 RK_PD5 1 &pcfg_pull_none>,
					<3 RK_PD6 1 &pcfg_pull_none>,
					<3 RK_PD7 1 &pcfg_pull_none>;
			};

			i2s_8ch_mclk: i2s-8ch-mclk {
				rockchip,pins =
					<4 RK_PA0 1 &pcfg_pull_none>;
			};
		};

		i2s1 {
			i2s1_2ch_bus: i2s1-2ch-bus {
				rockchip,pins =
					<4 RK_PA3 1 &pcfg_pull_none>,
					<4 RK_PA4 1 &pcfg_pull_none>,
					<4 RK_PA5 1 &pcfg_pull_none>,
					<4 RK_PA6 1 &pcfg_pull_none>,
					<4 RK_PA7 1 &pcfg_pull_none>;
			};
		};

		sdio0 {
			sdio0_bus1: sdio0-bus1 {
				rockchip,pins =
					<2 RK_PC4 1 &pcfg_pull_up>;
			};

			sdio0_bus4: sdio0-bus4 {
				rockchip,pins =
					<2 RK_PC4 1 &pcfg_pull_up>,
					<2 RK_PC5 1 &pcfg_pull_up>,
					<2 RK_PC6 1 &pcfg_pull_up>,
					<2 RK_PC7 1 &pcfg_pull_up>;
			};

			sdio0_cmd: sdio0-cmd {
				rockchip,pins =
					<2 RK_PD0 1 &pcfg_pull_up>;
			};

			sdio0_clk: sdio0-clk {
				rockchip,pins =
					<2 RK_PD1 1 &pcfg_pull_none>;
			};

			sdio0_cd: sdio0-cd {
				rockchip,pins =
					<2 RK_PD2 1 &pcfg_pull_up>;
			};

			sdio0_pwr: sdio0-pwr {
				rockchip,pins =
					<2 RK_PD3 1 &pcfg_pull_up>;
			};

			sdio0_bkpwr: sdio0-bkpwr {
				rockchip,pins =
					<2 RK_PD4 1 &pcfg_pull_up>;
			};

			sdio0_wp: sdio0-wp {
				rockchip,pins =
					<0 RK_PA3 1 &pcfg_pull_up>;
			};

			sdio0_int: sdio0-int {
				rockchip,pins =
					<0 RK_PA4 1 &pcfg_pull_up>;
			};
		};

		sdmmc {
			sdmmc_bus1: sdmmc-bus1 {
				rockchip,pins =
					<4 RK_PB0 1 &pcfg_pull_up>;
			};

			sdmmc_bus4: sdmmc-bus4 {
				rockchip,pins =
					<4 RK_PB0 1 &pcfg_pull_up>,
					<4 RK_PB1 1 &pcfg_pull_up>,
					<4 RK_PB2 1 &pcfg_pull_up>,
					<4 RK_PB3 1 &pcfg_pull_up>;
			};

			sdmmc_clk: sdmmc-clk {
				rockchip,pins =
					<4 RK_PB4 1 &pcfg_pull_none>;
			};

			sdmmc_cmd: sdmmc-cmd {
				rockchip,pins =
					<4 RK_PB5 1 &pcfg_pull_up>;
			};

			sdmmc_cd: sdmmc-cd {
				rockchip,pins =
					<0 RK_PA7 1 &pcfg_pull_up>;
			};

			sdmmc_wp: sdmmc-wp {
				rockchip,pins =
					<0 RK_PB0 1 &pcfg_pull_up>;
			};
		};

		suspend {
			ap_pwroff: ap-pwroff {
				rockchip,pins = <1 RK_PA5 1 &pcfg_pull_none>;
			};

			ddrio_pwroff: ddrio-pwroff {
				rockchip,pins = <0 RK_PA1 1 &pcfg_pull_none>;
			};
		};

		spdif {
			spdif_bus: spdif-bus {
				rockchip,pins =
					<4 RK_PC5 1 &pcfg_pull_none>;
			};

			spdif_bus_1: spdif-bus-1 {
				rockchip,pins =
					<3 RK_PC0 3 &pcfg_pull_none>;
			};
		};

		spi0 {
			spi0_clk: spi0-clk {
				rockchip,pins =
					<3 RK_PA6 2 &pcfg_pull_up>;
			};
			spi0_cs0: spi0-cs0 {
				rockchip,pins =
					<3 RK_PA7 2 &pcfg_pull_up>;
			};
			spi0_cs1: spi0-cs1 {
				rockchip,pins =
					<3 RK_PB0 2 &pcfg_pull_up>;
			};
			spi0_tx: spi0-tx {
				rockchip,pins =
					<3 RK_PA5 2 &pcfg_pull_up>;
			};
			spi0_rx: spi0-rx {
				rockchip,pins =
					<3 RK_PA4 2 &pcfg_pull_up>;
			};
		};

		spi1 {
			spi1_clk: spi1-clk {
				rockchip,pins =
					<1 RK_PB1 2 &pcfg_pull_up>;
			};
			spi1_cs0: spi1-cs0 {
				rockchip,pins =
					<1 RK_PB2 2 &pcfg_pull_up>;
			};
			spi1_rx: spi1-rx {
				rockchip,pins =
					<1 RK_PA7 2 &pcfg_pull_up>;
			};
			spi1_tx: spi1-tx {
				rockchip,pins =
					<1 RK_PB0 2 &pcfg_pull_up>;
			};
		};

		spi2 {
			spi2_clk: spi2-clk {
				rockchip,pins =
					<2 RK_PB3 1 &pcfg_pull_up>;
			};
			spi2_cs0: spi2-cs0 {
				rockchip,pins =
					<2 RK_PB4 1 &pcfg_pull_up>;
			};
			spi2_rx: spi2-rx {
				rockchip,pins =
					<2 RK_PB1 1 &pcfg_pull_up>;
			};
			spi2_tx: spi2-tx {
				rockchip,pins =
					<2 RK_PB2 1 &pcfg_pull_up>;
			};
		};

		spi3 {
			spi3_clk: spi3-clk {
				rockchip,pins =
					<1 RK_PC1 1 &pcfg_pull_up>;
			};
			spi3_cs0: spi3-cs0 {
				rockchip,pins =
					<1 RK_PC2 1 &pcfg_pull_up>;
			};
			spi3_rx: spi3-rx {
				rockchip,pins =
					<1 RK_PB7 1 &pcfg_pull_up>;
			};
			spi3_tx: spi3-tx {
				rockchip,pins =
					<1 RK_PC0 1 &pcfg_pull_up>;
			};
		};

		spi4 {
			spi4_clk: spi4-clk {
				rockchip,pins =
					<3 RK_PA2 2 &pcfg_pull_up>;
			};
			spi4_cs0: spi4-cs0 {
				rockchip,pins =
					<3 RK_PA3 2 &pcfg_pull_up>;
			};
			spi4_rx: spi4-rx {
				rockchip,pins =
					<3 RK_PA0 2 &pcfg_pull_up>;
			};
			spi4_tx: spi4-tx {
				rockchip,pins =
					<3 RK_PA1 2 &pcfg_pull_up>;
			};
		};

		spi5 {
			spi5_clk: spi5-clk {
				rockchip,pins =
					<2 RK_PC6 2 &pcfg_pull_up>;
			};
			spi5_cs0: spi5-cs0 {
				rockchip,pins =
					<2 RK_PC7 2 &pcfg_pull_up>;
			};
			spi5_rx: spi5-rx {
				rockchip,pins =
					<2 RK_PC4 2 &pcfg_pull_up>;
			};
			spi5_tx: spi5-tx {
				rockchip,pins =
					<2 RK_PC5 2 &pcfg_pull_up>;
			};
		};

		testclk {
			test_clkout0: test-clkout0 {
				rockchip,pins =
					<0 RK_PA0 1 &pcfg_pull_none>;
			};

			test_clkout1: test-clkout1 {
				rockchip,pins =
					<2 RK_PD1 2 &pcfg_pull_none>;
			};

			test_clkout2: test-clkout2 {
				rockchip,pins =
					<0 RK_PB0 3 &pcfg_pull_none>;
			};
		};

		tsadc {
			otp_pin: otp-pin {
				rockchip,pins = <1 RK_PA6 RK_FUNC_GPIO &pcfg_pull_none>;
			};

			otp_out: otp-out {
				rockchip,pins = <1 RK_PA6 1 &pcfg_pull_none>;
			};
		};

		uart0 {
			uart0_xfer: uart0-xfer {
				rockchip,pins =
					<2 RK_PC0 1 &pcfg_pull_up>,
					<2 RK_PC1 1 &pcfg_pull_up>;
			};

			uart0_cts: uart0-cts {
				rockchip,pins =
					<2 RK_PC2 1 &pcfg_pull_none>;
			};

			uart0_rts: uart0-rts {
				rockchip,pins =
					<2 RK_PC3 1 &pcfg_pull_none>;
			};
		};

		uart1 {
			uart1_xfer: uart1-xfer {
				rockchip,pins =
					<3 RK_PB4 2 &pcfg_pull_up>,
					<3 RK_PB5 2 &pcfg_pull_up>;
			};
		};

		uart2a {
			uart2a_xfer: uart2a-xfer {
				rockchip,pins =
					<4 RK_PB0 2 &pcfg_pull_up>,
					<4 RK_PB1 2 &pcfg_pull_up>;
			};
		};

		uart2b {
			uart2b_xfer: uart2b-xfer {
				rockchip,pins =
					<4 RK_PC0 2 &pcfg_pull_up>,
					<4 RK_PC1 2 &pcfg_pull_up>;
			};
		};

		uart2c {
			uart2c_xfer: uart2c-xfer {
				rockchip,pins =
					<4 RK_PC3 1 &pcfg_pull_up>,
					<4 RK_PC4 1 &pcfg_pull_up>;
			};
		};

		uart3 {
			uart3_xfer: uart3-xfer {
				rockchip,pins =
					<3 RK_PB6 2 &pcfg_pull_up>,
					<3 RK_PB7 2 &pcfg_pull_up>;
			};

			uart3_cts: uart3-cts {
				rockchip,pins =
					<3 RK_PC0 2 &pcfg_pull_none>;
			};

			uart3_rts: uart3-rts {
				rockchip,pins =
					<3 RK_PC1 2 &pcfg_pull_none>;
			};
		};

		uart4 {
			uart4_xfer: uart4-xfer {
				rockchip,pins =
					<1 RK_PA7 1 &pcfg_pull_up>,
					<1 RK_PB0 1 &pcfg_pull_up>;
			};
		};

		uarthdcp {
			uarthdcp_xfer: uarthdcp-xfer {
				rockchip,pins =
					<4 RK_PC5 2 &pcfg_pull_up>,
					<4 RK_PC6 2 &pcfg_pull_up>;
			};
		};

		pwm0 {
			pwm0_pin: pwm0-pin {
				rockchip,pins =
					<4 RK_PC2 1 &pcfg_pull_none>;
			};

			pwm0_pin_pull_down: pwm0-pin-pull-down {
				rockchip,pins =
					<4 RK_PC2 1 &pcfg_pull_down>;
			};

			vop0_pwm_pin: vop0-pwm-pin {
				rockchip,pins =
					<4 RK_PC2 2 &pcfg_pull_none>;
			};

			vop1_pwm_pin: vop1-pwm-pin {
				rockchip,pins =
					<4 RK_PC2 3 &pcfg_pull_none>;
			};
		};

		pwm1 {
			pwm1_pin: pwm1-pin {
				rockchip,pins =
					<4 RK_PC6 1 &pcfg_pull_none>;
			};

			pwm1_pin_pull_down: pwm1-pin-pull-down {
				rockchip,pins =
					<4 RK_PC6 1 &pcfg_pull_down>;
			};
		};

		pwm2 {
			pwm2_pin: pwm2-pin {
				rockchip,pins =
					<1 RK_PC3 1 &pcfg_pull_none>;
			};

			pwm2_pin_pull_down: pwm2-pin-pull-down {
				rockchip,pins =
					<1 RK_PC3 1 &pcfg_pull_down>;
			};
		};

		pwm3a {
			pwm3a_pin: pwm3a-pin {
				rockchip,pins =
					<0 RK_PA6 1 &pcfg_pull_none>;
			};

			pwm3a_pin_pull_down: pwm3a-pin-pull-down {
				rockchip,pins =
					<0 RK_PA6 1 &pcfg_pull_down>;
			};
		};

		pwm3b {
			pwm3b_pin: pwm3b-pin {
				rockchip,pins =
					<1 RK_PB6 1 &pcfg_pull_none>;
			};

			pwm3b_pin_pull_down: pwm3b-pin-pull-down {
				rockchip,pins =
					<1 RK_PB6 1 &pcfg_pull_down>;
			};
		};

		hdmi {
			hdmi_i2c_xfer: hdmi-i2c-xfer {
				rockchip,pins =
					<4 RK_PC1 3 &pcfg_pull_none>,
					<4 RK_PC0 3 &pcfg_pull_none>;
			};

			hdmi_cec: hdmi-cec {
				rockchip,pins =
					<4 RK_PC7 1 &pcfg_pull_none>;
			};
		};

		pcie {
			pcie_clkreqn_cpm: pci-clkreqn-cpm {
				rockchip,pins =
					<2 RK_PD2 RK_FUNC_GPIO &pcfg_pull_none>;
			};

			pcie_clkreqnb_cpm: pci-clkreqnb-cpm {
				rockchip,pins =
					<4 RK_PD0 RK_FUNC_GPIO &pcfg_pull_none>;
			};
		};

	};

	rockchip_suspend: rockchip-suspend {
		compatible = "rockchip,pm-rk3399";
		status = "disabled";
		rockchip,sleep-debug-en = <0>;
		rockchip,virtual-poweroff = <0>;
		rockchip,sleep-mode-config = <
			(0
			| RKPM_SLP_ARMPD
			| RKPM_SLP_PERILPPD
			| RKPM_SLP_DDR_RET
			| RKPM_SLP_PLLPD
			| RKPM_SLP_OSC_DIS
			| RKPM_SLP_CENTER_PD
			| RKPM_SLP_AP_PWROFF
			)
		>;
		rockchip,wakeup-config = <
			(0
			| RKPM_GPIO_WKUP_EN
			)
		>;
	};
};
