#include <dt-bindings/display/media-bus-format.h>
#include "rp-lcd-hdmi.dtsi"
#define RP_SINGLE_LCD

&lvds_panel {
	status = "okay";
	compatible = "simple-panel";
	enable-delay-ms = <20>;
	prepare-delay-ms = <20>;
	unprepare-delay-ms = <20>;
	disable-delay-ms = <20>;
	bus-format = <MEDIA_BUS_FMT_RGB888_2X12_BE>;
	width-mm = <217>;
	height-mm = <136>;
		
		/*
		 * power-supply = <>;
		 * reset-gpios = <>;
		 *
		 * lcd reset pin and power supply
		 * please refer to ***-lcd-gpio.dtsi
		 * that included in main dts.
		 */
		
	display-timings {
		native-mode = <&timing0>;

		timing0: timing0 {
			clock-frequency = <72000000>;
			hactive = <1280>;
			vactive = <800>;
			hback-porch = <138>;
			hfront-porch = <136>;
			vback-porch = <10>;
			vfront-porch = <10>;
			hsync-len = <20>;
			vsync-len = <3>;
			hsync-active = <0>;
			vsync-active = <0>;
			de-active = <0>;
			pixelclk-active = <0>;
		};
	};

	ports {
		#address-cells = <1>;
		#size-cells = <0>;

		port@0 {
			reg = <0>;
			dual-lvds-even-pixels;
			panel_in_lvds: endpoint {
				remote-endpoint = <&lvds_out_panel>;
			};
		};
	};
};

&lvds {
	status = "okay";
	ports {
		port@1 {
			reg = <1>;

			lvds_out_panel: endpoint {
				remote-endpoint = <&panel_in_lvds>;
			};
		};
	};
};




&rpdzkj {
        compatible = "rp_config";
        user_version = "rpdzkj";
        system_rotate = "0";
				csi_camera_rotate = "0"; //all csi camera rotation //0 90 180 270 //no effect
				csi_camera_facing = "0"; //0:auto  1:all front   2:all back //no effect
				usb_camera_rotate = "0"; //all usb camera rotation //0 90 180 270 
				usb_camera_facing = "0"; //0:auto  1:all front   2:all back
        lcd_density = "180";
        language = "zh-CN";   //zh-CN //en-US
        time_zone = "Asia/Shanghai"; //Asia/Shanghai = +8   //Europe/London  = +1       //Africa/Casablanca     = +0;
        not_navigation_bar = "false";
        not_status_bar = "false";
        default_launcher = "true";
        has_root = "true";
        usb_not_permission = "true";
        gps_use = "false";
        gps_serial_port = "/dev/ttyS4";
        primary_device = "DSI";
        extend_device = "HDMI-A";
        extend_rotate = "0";
        rotation_efull = "false";
        home_apk = "null";
        status = "okay";
};


&pwm4 {
	status = "okay";
};

&dsi0 {
	status = "disabled";
};

&dsi0_in_vp0 {
	status = "disabled";
};

&dsi0_in_vp1 {
	status = "disabled";
};

&video_phy0 {
	status = "okay";
};

&lvds_in_vp1 {
	status = "okay";
};

&lvds_in_vp2 {
	status = "disabled";
};

&route_lvds {
	status = "okay";
	connect = <&vp1_out_lvds>;
};


&gt9xx {
        status = "okay";

        compatible = "goodix,gt9xx";
        reg = <0x5d>;
        gtp_resolution_x = <1280>;
        gtp_resolution_y = <800>;
        gtp_int_tarigger = <1>;
        gtp_change_x2y = <0>;
        gtp_overturn_x = <0>;
        gtp_overturn_y = <0>;
        gtp_send_cfg = <1>;
        gtp_touch_wakeup = <1>;

		/**
		 * goodix_rst_gpio = <>;
		 * goodix_irq_gpio = <>;
		 *
		 * touch panel interrupt and reset pin
		 * please refer to ***-lcd-gpio.dtsi
		 * that included in main dts.
		 */
        goodix,cfg-group3 = [
	       5A 00 05 20 03 02 0D 00 01 0A 28
	       0A 50 32 03 05 00 00 00 00 00 00
	       08 00 00 00 00 8C 2E 0E 30 32 34
	       06 00 00 00 82 02 1D 00 01 00 00
	       00 00 00 00 00 00 00 24 60 94 C5
	       02 07 00 00 04 97 27 00 80 30 00
	       6D 3B 00 60 47 00 54 57 00 54 00
	       00 00 00 00 00 00 00 00 00 00 00
	       00 00 00 00 00 00 00 00 00 00 00
	       00 00 00 00 00 00 00 00 00 00 00
	       00 00 1C 1A 18 16 14 12 10 0E 0C
	       0A 08 06 04 02 00 00 00 00 00 00
	       00 00 00 00 00 00 00 00 00 00 2A
	       29 28 26 24 22 21 20 1F 1E 1D 1C
	       18 16 14 13 12 10 0F 0C 0A 08 06
	       04 02 00 00 00 00 00 00 00 00 00
	       00 00 00 00 00 00 00 00 D4 01
];
	goodix,cfg-group2 = [
	       5A 00 05 20 03 02 0D 00 01 0A 28
	       0A 50 32 03 05 00 00 00 00 00 00
	       08 00 00 00 00 8C 2E 0E 30 32 34
	       06 00 00 00 82 02 1D 00 01 00 00
	       00 00 00 00 00 00 00 24 60 94 C5
	       02 07 00 00 04 97 27 00 80 30 00
	       6D 3B 00 60 47 00 54 57 00 54 00
	       00 00 00 00 00 00 00 00 00 00 00
	       00 00 00 00 00 00 00 00 00 00 00
	       00 00 00 00 00 00 00 00 00 00 00
	       00 00 1C 1A 18 16 14 12 10 0E 0C
	       0A 08 06 04 02 00 00 00 00 00 00
	       00 00 00 00 00 00 00 00 00 00 2A
	       29 28 26 24 22 21 20 1F 1E 1D 1C
	       18 16 14 13 12 10 0F 0C 0A 08 06
	       04 02 00 00 00 00 00 00 00 00 00
	       00 00 00 00 00 00 00 00 D4 01
               ];
};

