


&gmac1 {
        phy-mode = "rgmii";
        clock_in_out = "input";

        snps,reset-gpio = <&gpio3 RK_PB4 GPIO_ACTIVE_LOW>;
        snps,reset-active-low;
        /* Reset time is 20ms, 100ms for rtl8211f */
        snps,reset-delays-us = <0 20000 100000>;

        assigned-clocks = <&cru SCLK_GMAC1_RX_TX>, <&cru SCLK_GMAC1>, <&cru CLK_MAC1_OUT>;
        assigned-clock-parents = <&cru SCLK_GMAC1_RGMII_SPEED>,<&gmac1_clkin>;
        assigned-clock-rates = <0>, <125000000>, <25000000>;

        pinctrl-names = "default";
        pinctrl-0 = <&gmac1m0_miim
                     &gmac1m0_tx_bus2
                     &gmac1m0_rx_bus2
                     &gmac1m0_rgmii_clk
                     &gmac1m0_rgmii_bus
                        &gmac1m0_clkinout
            &eth1m0_pins>;

        tx_delay = <0x3a>;
        rx_delay = <0x29>;
        phy-handle = <&rgmii_phy1>;
        status = "okay";
};

&mdio1 {
        rgmii_phy1: phy@0 {
                compatible = "ethernet-phy-ieee802.3-c22";
                reg = <0x0>;
        clocks = <&cru CLK_MAC1_OUT>;
        };
};

