// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Copyright (c) 2020 Rockchip Electronics Co., Ltd.
 *
 */

/dts-v1/;

//rk3566-evb1-ddr4-v10
//#include "rk3566-evb1-ddr4-v10.dtsi"

#include "rk3566-evb-rpdzkj-rk809-tcs4525.dtsi"


#include "../rk3568-linux.dtsi"
/*************************camera***********************/
#include "rp-mipi-camera-gc2093-rk3566.dtsi"
/***************************************************/


/*************************adc key***********************/
#include "rp-adc-key.dtsi"
/***************************************************/

/*************************gmac***********************/
#include "rp-gmac1-m0-pro-rk3566.dtsi"
/***************************************************/


/*************************SATA***********************/
#include "rk3568-sata2.dtsi"
/***************************************************/

/****************** SINGLE LCD ***************/
#include "pro-rk3566-single-lcd-gpio.dtsi"

/* HDMI */
//#include "rp-lcd-hdmi.dtsi"

/* MIPI0 */
//#include "rp-lcd-mipi0-5-720-1280-v2-boxTP.dtsi"
//#include "rp-lcd-mipi0-5.5-720-1280.dtsi"
//#include "rp-lcd-mipi0-5.5-720-1280-v2.dtsi"
//#include "rp-lcd-mipi0-5.5-1080-1920.dtsi"
#include "rp-lcd-mipi0-7-1024-600.dtsi"
//#include "rp-lcd-mipi0-7-720-1280.dtsi"
//#include "rp-lcd-mipi0-7-1200-1920.dtsi"
//#include "rp-lcd-mipi0-8-800-1280.dtsi"
//#include "rp-lcd-mipi0-8-800-1280-v2.dtsi"
//#include "rp-lcd-mipi0-8-800-1280-v3.dtsi"
//#include "rp-lcd-mipi0-8-1200-1920.dtsi"
//#include "rp-lcd-mipi0-10-800-1280.dtsi"
//#include "rp-lcd-mipi0-10-800-1280-v2.dtsi"
//#include "rp-lcd-mipi0-10-800-1280-v3.dtsi"
//#include "rp-lcd-mipi0-10-1920-1200.dtsi"

/* MIPI1 */
//#include "rp-lcd-mipi1-7-1024-600.dtsi"

/* LVDS */
//#include "rp-lcd-lvds-10-1024-600.dtsi"
//#include "rp-lcd-lvds-7-1024-600-v2.dtsi"
//#include "rp-lcd-lvds-10-1280-800.dtsi"
/* EDP */
//#include "rp-lcd-edp-13-1920-1080.dtsi"






/ {
    model = "pro-rk3566";
    compatible = "rpdzkj,pro-rk3566", "rockchip,rk3566";

        
        rp_power{
                status = "okay";
                compatible = "rp_power";
                rp_not_deep_sleep = <1>;

//#define GPIO_FUNCTION_OUTPUT 0
//#define GPIO_FUNCTION_INPUT 1
//#define GPIO_FUNCTION_IRQ 2
//#define GPIO_FUNCTION_FLASH 3
//#define GPIO_FUNCTION_OUTPUT_CTRL 4

                pwr_5v_3v3 {    //3.3v 5v enable
                        gpio_num = <&gpio2 RK_PB3 GPIO_ACTIVE_HIGH>;
                        gpio_function = <0>;
                };
                
                led {       //system led
                        gpio_num = <&gpio3 RK_PC2 GPIO_ACTIVE_HIGH>;
                        gpio_function = <3>;
                };
                
                usb_pwr { // usb host power
                        gpio_num = <&gpio0 RK_PA6 GPIO_ACTIVE_HIGH>;
                        gpio_function = <4>;
                };

                otg_pwr {
                        gpio_num = <&gpio0 RK_PA5 GPIO_ACTIVE_HIGH>;
                        gpio_function = <4>;
                };

                usb_rst {       //usb hub reset
                        gpio_num = <&gpio0 RK_PB0 GPIO_ACTIVE_HIGH>;
                        gpio_function = <4>;
                };

                spk_en {       //SPK ENABLE
                        gpio_num = <&gpio4 RK_PC4 GPIO_ACTIVE_HIGH>;
                        gpio_function = <4>;
                };

                spk_mute {       //SPK MUTE
                        gpio_num = <&gpio0 RK_PA0 GPIO_ACTIVE_LOW>;
                        gpio_function = <4>;
                };
                usb_mode {       //OTG SWITCH
                        gpio_num = <&gpio0 RK_PC2 GPIO_ACTIVE_LOW>;
                        gpio_function = <0>;
                };
};



        rp_gpio{
                status = "okay";
                compatible = "rp_gpio";

/***** SPI_FLASH ********/
                gpio1d0 {      
                        gpio_num = <&gpio1 RK_PD0 GPIO_ACTIVE_HIGH>;
                        gpio_function = <0>;
                };
                gpio1d1 {       
                        gpio_num = <&gpio1 RK_PD1 GPIO_ACTIVE_HIGH>;
                        gpio_function = <0>;
                };

                gpio1d2 {       
                        gpio_num = <&gpio1 RK_PD2 GPIO_ACTIVE_HIGH>;
                        gpio_function = <0>;
                };
                gpio1d3 {       
                        gpio_num = <&gpio1 RK_PD3 GPIO_ACTIVE_HIGH>;
                        gpio_function = <0>;
                };

                gpio1d4 {       
                        gpio_num = <&gpio1 RK_PD4 GPIO_ACTIVE_HIGH>;
                        gpio_function = <0>;
                };

/***** PDM ********/

                gpio4a0 {
                        gpio_num = <&gpio4 RK_PA0 GPIO_ACTIVE_HIGH>;
                        gpio_function = <0>;
                };

                gpio4a1 {
                        gpio_num = <&gpio4 RK_PA1 GPIO_ACTIVE_HIGH>;
                        gpio_function = <0>;
                };
                gpio4a2 {
                        gpio_num = <&gpio4 RK_PA2 GPIO_ACTIVE_HIGH>;
                        gpio_function = <0>;
                };

                gpio4a3 {
                        gpio_num = <&gpio4 RK_PA3 GPIO_ACTIVE_HIGH>;
                        gpio_function = <0>;
                };
                gpio1a4 {
                        gpio_num = <&gpio1 RK_PA4 GPIO_ACTIVE_HIGH>;
                        gpio_function = <0>;
                };
                gpio3c1 {
                        gpio_num = <&gpio3 RK_PC1 GPIO_ACTIVE_HIGH>;
                        gpio_function = <0>;
                };
    };
    
    test-power {
        /** disable for use rk809-battery */
        status = "disabled";
    };
    charge-animation {
        compatible = "rockchip,uboot-charge";
        rockchip,uboot-charge-on = <0>;
        rockchip,android-charge-on = <0>;
        rockchip,uboot-low-power-voltage = <7000>;
        rockchip,screen-on-voltage = <7000>;
        status = "okay";
    };

    fiq-debugger {
        compatible = "rockchip,fiq-debugger";
        rockchip,serial-id = <2>;
        rockchip,wake-irq = <0>;
        /* If enable uart uses irq instead of fiq */
        rockchip,irq-mode-enable = <1>;
        rockchip,baudrate = <115200>;  /* Only 115200 and 1500000 */
        interrupts = <GIC_SPI 252 IRQ_TYPE_LEVEL_LOW>;
        pinctrl-names = "default";
        pinctrl-0 = <&uart2m0_xfer>;
        status = "okay";
    };
};


&pmu_io_domains {
        status = "okay";
        pmuio2-supply = <&vcc3v3_pmu>;
        vccio1-supply = <&vccio_acodec>;
        vccio3-supply = <&vccio_sd>;
        vccio4-supply = <&vcc_3v3>;
        vccio5-supply = <&vcc_3v3>;
        vccio6-supply = <&vcc_1v8>;
        vccio7-supply = <&vcc_3v3>;
};



&cpu0_opp_table {

        opp-408000000 {
            opp-hz = /bits/ 64 <408000000>;
            opp-microvolt = <825000 825000 1150000>;
            opp-microvolt-L0 = <825000 825000 1150000>;
            opp-microvolt-L1 = <800000 800000 1150000>;
            opp-microvolt-L2 = <800000 800000 1150000>;
            clock-latency-ns = <40000>;
        };
        opp-600000000 {
            opp-hz = /bits/ 64 <600000000>;
            opp-microvolt = <850000 850000 1150000>;
            opp-microvolt-L0 = <850000 850000 1150000>;
            opp-microvolt-L1 = <825000 825000 1150000>;
            opp-microvolt-L2 = <825000 825000 1150000>;
            clock-latency-ns = <40000>;
        };
        opp-816000000 {
            opp-hz = /bits/ 64 <816000000>;
            opp-microvolt = <900000 900000 1150000>;
            opp-microvolt-L0 = <900000 900000 1150000>;
            opp-microvolt-L1 = <875000 875000 1150000>;
            opp-microvolt-L2 = <875000 875000 1150000>;
            clock-latency-ns = <40000>;
            opp-suspend;
        };
        opp-1104000000 {
            opp-hz = /bits/ 64 <1104000000>;
            opp-microvolt = <950000 950000 1150000>;
            opp-microvolt-L0 = <950000 950000 1150000>;
            opp-microvolt-L1 = <925000 925000 1150000>;
            opp-microvolt-L2 = <925000 925000 1150000>;
            clock-latency-ns = <40000>;
        };
        opp-1416000000 {
            opp-hz = /bits/ 64 <1416000000>;
            opp-microvolt = <1000000 1000000 1150000>;
            opp-microvolt-L0 = <1000000 1000000 1150000>;
            opp-microvolt-L1 = <975000 975000 1150000>;
            opp-microvolt-L2 = <975000 975000 1150000>;
            clock-latency-ns = <40000>;
        };
        opp-1608000000 {
            opp-hz = /bits/ 64 <1608000000>;
            opp-microvolt = <1050000 1050000 1150000>;
            opp-microvolt-L0 = <1050000 1050000 1150000>;
            opp-microvolt-L1 = <1025000 1025000 1150000>;
            opp-microvolt-L2 = <1025000 1025000 1150000>;
            clock-latency-ns = <40000>;
        };

        opp-1800000000 {
            opp-hz = /bits/ 64 <1800000000>;
            opp-microvolt = <1100000 1100000 1150000>;
            opp-microvolt-L0 = <1100000 1100000 1150000>;
            opp-microvolt-L1 = <1075000 1075000 1150000>;
            opp-microvolt-L2 = <1075000 1075000 1150000>;
            clock-latency-ns = <40000>;
        };

};


&i2c1 {
    status = "okay";
};

&i2c4 {
    status = "okay";
    pinctrl-names = "default";
    pinctrl-0 = <&i2c4m1_xfer>;

        rtc@51 {
                status = "okay";
                compatible = "rtc,hym8563";
                reg = <0x51>;
        };
};

&uart3 {
    status = "okay";
    pinctrl-names = "default";
    pinctrl-0 = <&uart3m0_xfer>;
};

&uart6 {
        status = "okay";
        pinctrl-names = "default";
        pinctrl-0 = <&uart6m0_xfer>;
};

&uart7 {
        status = "okay";
        pinctrl-names = "default";
        pinctrl-0 = <&uart7m0_xfer>;
};

&uart9 {
        status = "okay";
        pinctrl-names = "default";
        pinctrl-0 = <&uart9m0_xfer>;
};

&spi1 {
    status = "okay";

    spi1_dev@0 {
        compatible = "rockchip,spidev";
        reg = <0>;
        spi-max-frequency = <12000000>;
        spi-lsb-first;
    };

};

&spi2 {
        status = "okay";

    spi2_dev@0 {
        compatible = "rockchip,spidev";
        reg = <0>;
        spi-max-frequency = <12000000>;
        spi-lsb-first;
    };

};

&spi3 {
       status = "okay";

       num-cs = <1>;
       pinctrl-0 = <&spi3m1_cs0 &spi3m1_pins>;
       pinctrl-1 = <&spi3m1_cs0 &spi3m1_pins_hs>;

    spi3_dev@0 {
        compatible = "rockchip,spidev";
        reg = <0>;
        spi-max-frequency = <12000000>;
        spi-lsb-first;
    };
};

&edp {
    /** delete hdp gpio that pro3566 donot use */
    /delete-property/ hpd-gpios;
};

&dmc {
    status = "disabled";
};

&dfi {
    status = "disabled";
};

&rk809 {
    battery {
                compatible = "rk817,battery";
                pinctrl-names = "default";
                pinctrl-0 = <&rp_bat_pins>;

                ocv_table = < 7024 7072 7080 7096 7104 7112 7120
                              7136 7152 7168 7184 7224 7264 7320
                              7392 7512 7612 7724 7828 7928 8100>;
                design_capacity = <5000>;
                design_qmax = <5100>;
                bat_res = <100>;
                sleep_enter_current = <300>;
                sleep_exit_current = <300>;
                sleep_filter_current = <100>;
                power_off_thresd = <7024>;
                zero_algorithm_vol = <7400>;
                max_soc_offset = <60>;
                monitor_sec = <5>;
        
                sample_res = <20>;
                bat_res_up = <140>;
                bat_res_down = <20>;
                
                virtual_power = <0>;    //test mode, 1 to force report 66%
                energy_mode = <0>;
                register_chg_psy = <1>;    //rk817 report charge state
                
                plug-det-gpio = <&gpio0 RK_PC7 GPIO_ACTIVE_LOW>;   //rpdzkj add for detect charge state, need register_chg_psy = 1, active state is plugin.
                full-det-gpio = <&gpio0 RK_PC5 GPIO_ACTIVE_HIGH>;      //rpdzkj add for detect charge status whether is full.
        };
};



&sdmmc2 {
    max-frequency = <150000000>;
    supports-sdio;
    bus-width = <4>;
    disable-wp;
    cap-sd-highspeed;
    cap-sdio-irq;
    keep-power-in-suspend;
    mmc-pwrseq = <&sdio_pwrseq>;
    non-removable;
    pinctrl-names = "default";
    pinctrl-0 = <&sdmmc2m0_bus4 &sdmmc2m0_cmd &sdmmc2m0_clk>;
    sd-uhs-sdr104;
    status = "okay";
};

&uart1 {
    status = "okay";
    pinctrl-names = "default";
    pinctrl-0 = <&uart1m1_xfer &uart1m1_ctsn>;
};


&wireless_bluetooth {
    uart_rts_gpios = <&gpio4 RK_PB6 GPIO_ACTIVE_LOW>;
    pinctrl-names = "default", "rts_gpio";
    pinctrl-0 = <&uart1m1_rtsn>;
    pinctrl-1 = <&uart1_gpios>;
    BT,reset_gpio    = <&gpio4 RK_PA5 GPIO_ACTIVE_HIGH>;
    BT,wake_gpio     = <&gpio4 RK_PA6 GPIO_ACTIVE_HIGH>;
    BT,wake_host_irq = <&gpio4 RK_PB1 GPIO_ACTIVE_HIGH>;
    status = "okay";
};

&wireless_wlan {
    pinctrl-names = "default";
    pinctrl-0 = <&wifi_host_wake_irq>;
    WIFI,host_wake_irq = <&gpio3 RK_PD4 GPIO_ACTIVE_HIGH>;
};


        
&rk_headset {
        status = "okay";
    pinctrl-names = "default";
    pinctrl-0 = <&hp_det>;
    headset_gpio = <&gpio3 RK_PA1 GPIO_ACTIVE_HIGH>;
    };



&pinctrl {
    rp-pins {
        rp_bat_pins: rp-bat-pins {
            rockchip,pins =
                <0 RK_PC7 RK_FUNC_GPIO &pcfg_pull_up>,
                <0 RK_PC5 RK_FUNC_GPIO &pcfg_pull_none>;
        };
    };
    
    
    headphone {
        hp_det: hp-det {
            rockchip,pins = <3 RK_PA1 RK_FUNC_GPIO &pcfg_pull_down>;
        };
    };

    
    wireless-wlan {
        wifi_host_wake_irq: wifi-host-wake-irq {
            rockchip,pins = <3 RK_PD4 RK_FUNC_GPIO &pcfg_pull_down>;
        };
    };

    wireless-bluetooth {
        uart1_gpios: uart1-gpios {
            rockchip,pins = <4 RK_PB6 RK_FUNC_GPIO &pcfg_pull_none>;
        };
    };
};

&rk809_codec {
    mic-in-differential;
};
