/ {
    backlight: backlight {
        status = "okay";
        compatible = "pwm-backlight";
        pwms = <&pwm0 0 25000 0>;
        brightness-levels = <
              0   1   2   3   4   5   6   7
              8   9  10  11  12  13  14  15
             16  17  18  19  20  21  22  23
             24  25  26  27  28  29  30  31
             32  33  34  35  36  37  38  39
             40  41  42  43  44  45  46  47
             48  49  50  51  52  53  54  55
             56  57  58  59  60  61  62  63
             64  65  66  67  68  69  70  71
             72  73  74  75  76  77  78  79
             80  81  82  83  84  85  86  87
             88  89  90  91  92  93  94  95
             96  97  98  99 100 101 102 103
            104 105 106 107 108 109 110 111
            112 113 114 115 116 117 118 119
            120 121 122 123 124 125 126 127
            128 129 130 131 132 133 134 135
            136 137 138 139 140 141 142 143
            144 145 146 147 148 149 150 151
            152 153 154 155 156 157 158 159
            160 161 162 163 164 165 166 167
            168 169 170 171 172 173 174 175
            176 177 178 179 180 181 182 183
            184 185 186 187 188 189 190 191
            192 193 194 195 196 197 198 199
            200 201 202 203 204 205 206 207
            208 209 210 211 212 213 214 215
            216 217 218 219 220 221 222 223
            224 225 226 227 228 229 230 231
            232 233 234 235 236 237 238 239
            240 241 242 243 244 245 246 247
            248 249 250 251 252 253 254 255>;
        default-brightness-level = <255>;
    };

    //bill  
        rpdzkj_config {
                compatible = "rp_config";
                user_version = "rpdzkj";
                system_rotate = "270";
                back_camera_rotate = "0";
                front_camera_rotate = "0";
                lcd_density = "190";
                language = "zh-CN";   //zh-CN //en-US
                time_zone = "Asia/Shanghai"; //Asia/Shanghai = +8   //Europe/London  = +1    //Africa/Casablanca    = +0;
                not_navigation_bar = "false";
                not_status_bar = "false";
                default_launcher = "true";
                has_root = "true";  //true//false
                usb_not_permission = "true";  
                usb_camera_only_front = "false";
                gps_use = "false";
                /* 
                 * UART*, please check board
                 * whether have this uart,
                 * otherwish system may not run
                 */
                gps_serial_port = "/dev/ttyS4"; 
                primary_device = "DSI";
                extend_device = "HDMI-A";
                extend_rotate = "0";
                rotation_efull = "true";
                home_apk = "null";
                
                status = "okay";
        };
};


&hdmi {
    #address-cells = <1>;
    #size-cells = <0>;
    #sound-dai-cells = <0>;
    ddc-i2c-scl-high-time-ns = <9625>;
    ddc-i2c-scl-low-time-ns = <10000>;
    status = "okay";
};

&pwm0 {
    status = "okay";
};

&display_subsystem {
    status = "okay";

    ports = <&vopb_out>, <&vopl_out>;
    logo-memory-region = <&drm_logo>;

    route {
        route_hdmi: route-hdmi {
            status = "okay";
            logo,uboot = "logo.bmp";
            logo,kernel = "logo_kernel.bmp";
            logo,mode = "center";
            charge_logo,mode = "center";
            connect = <&vopl_out_hdmi>;
        };

        route_dsi: route-dsi {

            status = "okay";
            // status = "disabled";
            logo,uboot = "logo.bmp";
            logo,kernel = "logo_kernel.bmp";
            logo,mode = "center";
            charge_logo,mode = "center";
            connect = <&vopb_out_dsi>;
        };

        route_dsi1: route-dsi1 {
            status = "disabled";
            logo,uboot = "logo.bmp";
            logo,kernel = "logo_kernel.bmp";
            logo,mode = "center";
            charge_logo,mode = "center";
            connect = <&vopl_out_dsi1>;
        };

        route_edp: route-edp {
            status = "disabled";
            logo,uboot = "logo.bmp";
            logo,kernel = "logo_kernel.bmp";
            logo,mode = "center";
            charge_logo,mode = "center";
            connect = <&vopb_out_edp>;
        };
    };
};

&dsi {
        status = "okay";
//    rockchip,lane-rate = <410>;

        panel {
                 compatible ="simple-panel-dsi";
                status = "okay";
                reg = <0>;
                power-supply = <&vcc3v3_sys>;
                backlight = <&backlight>;
                cmd_later_reset = <0>;
                enable-gpios = <&gpio1 13 GPIO_ACTIVE_HIGH>;
                reset-gpios  = <&gpio1 0 GPIO_ACTIVE_LOW>;
                dsi,flags = <(MIPI_DSI_MODE_VIDEO | MIPI_DSI_MODE_VIDEO_BURST |
                // MIPI_DSI_MODE_VIDEO_SYNC_PULSE)>;
                MIPI_DSI_MODE_LPM | MIPI_DSI_MODE_EOT_PACKET)>;    /** 7inch 720x1280 must this mode */
                dsi,format = <MIPI_DSI_FMT_RGB888>;
                //        bus-format = <MEDIA_BUS_FMT_RGB666_1X24>;
                dsi,lanes = <4>;
                reset-delay-ms = <100>;
                init-delay-ms = <100>;
                enable-delay-ms = <120>;
                disable-delay-ms = <50>;
                unprepare-delay-ms = <20>;
                
                width-mm = <68>;
                height-mm = <121>;
                panel-init-sequence = [
                    //test
                    05 78 01 01
                    39 00 04 B9 F1 12 83
                    39 00 1C BA 33 81 05 F9 0E 0E 20 00 00 00 00 00 00 00 44 25 00 91 0A 00 00 02 4F D1 00 00 37
                    39 00 02 B8 26
                    39 00 04 BF 02 10 00
                    39 00 0B B3 07 0B 1E 1E 03 FF 00 00 00 00
                    39 00 0A C0 73 73 50 50 00 00 08 70 00
                    39 00 02 BC 46
                    39 00 02 CC 0B
                    39 00 02 B4 80
                    39 00 04 B2 C8 12 A0
                    39 00 0F E3 07 07 0B 0B 03 0B 00 00 00 00 FF 80 C0 10
                    39 00 0D C1 53 00 32 32 77 F1 FF FF CC CC 77 77
                    39 00 03 B5 09 09
                    39 00 03 B6 B7 B7
                    39 00 40 E9 C2 10 0A 00 00 81 80 12 30 00 37 86 81 80 37 18 00 05 00 00 00 00 00 05 00 00 00 00 F8 BA 46 02 08 28 88 88 88 88 88 F8 BA 57 13 18 38 88 88 88 88 88 00 00 00 03 00 00 00 00 00 00 00 00 00
                    39 00 3E EA 07 12 01 01 02 3C 00 00 00 00 00 00 8F BA 31 75 38 18 88 88 88 88 88 8F BA 20 64 28 08 88 88 88 88 88 23 10 00 00 04 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
                    39 00 23 E0 00 02 04 1A 23 3F 2C 28 05 09 0B 10 11 10 12 12 19 00 02 04 1A 23 3F 2C 28 05 09 0B 10 11 10 12 12 19
                    05 ff 01 11 ////Sleep Out
                    05 32 01 29 ///Display On
                ];

                panel-exit-sequence = [
                        05 78 01 28
                        05 78 01 10
                ];

                display-timings {
                        native-mode = <&timing0>;
                        timing0: timing0 {
                                clock-frequency = <60000000>;
                                hactive = <720>;
                                vactive = <1280>;
                                hback-porch = <40>;
                                hfront-porch = <40>;
                                vback-porch = <11>;
                                vfront-porch = <16>;
                                hsync-len = <10>;
                                vsync-len = <3>;
                                hsync-active = <0>;
                                vsync-active = <0>;
                                de-active = <0>;
                                pixelclk-active = <0>;
                        };

                };
                
                                ports {
                                    #address-cells = <1>;
                                    #size-cells = <0>;
                        
                                    port@0 {
                                        reg = <0>;
                                        panel_in_dsi: endpoint {
                                            remote-endpoint = <&dsi_out_panel>;
                                        };
                                    };
                                };
                                
        };
        
            ports {
                        #address-cells = <1>;
                        #size-cells = <0>;
                
                        port@1 {
                            reg = <1>;
                            dsi_out_panel: endpoint {
                                remote-endpoint = <&panel_in_dsi>;
                            };
                        };
                    };
                    
};


&vopb {
        assigned-clocks = <&cru DCLK_VOP0_DIV>;
        assigned-clock-parents = <&cru PLL_CPLL>;
        //assigned-clock-parents = <&cru PLL_VPLL>;
        status = "okay";
};

&vopb_mmu {
        status = "okay";
};

&vopl {
        assigned-clocks = <&cru DCLK_VOP1_DIV>;
        assigned-clock-parents = <&cru PLL_VPLL>;
        //assigned-clock-parents = <&cru PLL_CPLL>;
        status = "okay";
};

&vopl_mmu {
        status = "okay";
};

&dsi_in_vopl {
        status = "disabled";
};

&dsi_in_vopb { 
        status = "okay"; 
}; 
 
&hdmi_in_vopb {
        status = "disabled";
};

&hdmi_in_vopl { 
        status = "okay"; 
}; 
 

&edp_in_vopb { 
        status = "disabled"; 
}; 
&edp_in_vopl { 
        status = "disabled"; 
}; 

&dsi1_in_vopb { 
        status = "disabled"; 
}; 
&dsi1_in_vopl { 
        status = "disabled"; 
}; 

&route_hdmi {
    status = "okay";
    connect = <&vopl_out_hdmi>;
};

&route_dsi {
    status = "okay";
    connect = <&vopb_out_dsi>;
};


&i2c4 {
        status = "okay";
    goodix_ts@5d {
        compatible = "goodix,gt9xx";
        reg = <0x5d>;
        gtp_resolution_x = <720>;
        gtp_resolution_y = <1280>;
        gtp_int_tarigger = <1>;
        gtp_change_x2y = <0>;
        gtp_overturn_x = <0>;
        gtp_overturn_y = <0>;
        gtp_send_cfg = <1>;
        gtp_touch_wakeup = <1>;
        goodix_rst_gpio = <&gpio1 4 GPIO_ACTIVE_HIGH>;
            goodix_irq_gpio = <&gpio1 22 IRQ_TYPE_EDGE_FALLING>;
    
         	  goodix,cfg-group0 = [
                        46 D0 02 00 05 05 35 01 01 08 1E 0F 5A 3C
                        03 05 00 00 00 00 11 11 00 19 1B 1E 14 89
                        29 0A 41 43 D3 07 00 00 00 9A 02 11 00 01
                        05 00 00 00 00 09 11 00 00 36 4A 94 45 00
                        00 00 00 00 94 37 00 8B 3B 00 83 3F 00 7C
                        43 00 76 47 00 76 10 30 48 00 F0 4A 3A FF
                        FF 27 00 00 00 00 00 00 00 00 00 00 00 00
                        00 00 00 00 00 00 00 00 00 00 00 00 00 00
                        08 0A 0C 0E 10 12 14 16 18 1A 00 00 00 00
                        00 00 00 00 00 00 00 00 00 00 00 00 00 00
                        00 00 0E 0C 0A 08 06 05 04 02 00 1D 1E 1F
                        20 22 24 28 29 2A 00 00 00 00 00 00 00 00
                        00 00 00 00 00 00 00 00 00 00 00 00 00 00
                        00 00 84 01];


    };
};
