// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
// Copyright (c) 2020 Fuzhou Rockchip Electronics Co., Ltd

/dts-v1/;
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/pinctrl/rockchip.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/display/drm_mipi_dsi.h>
#include <dt-bindings/sensor-dev.h>
#include <dt-bindings/pwm/pwm.h>
#include "dt-bindings/usb/pd.h"
#include "rk3399pro.dtsi"
#include "rk3399-linux.dtsi"
#include "rk3399-opp.dtsi"
#include "rk3399-vop-clk-set.dtsi"

/ {
	compatible = "rockchip,rk3399pro-evb-v11-linux", "rockchip,rk3399pro";

	adc-keys {
		compatible = "adc-keys";
		io-channels = <&saradc 2>;
		io-channel-names = "buttons";
		poll-interval = <100>;
		keyup-threshold-microvolt = <1800000>;

		esc-key {
			linux,code = <KEY_ESC>;
			label = "esc";
			press-threshold-microvolt = <1310000>;
		};

		menu-key {
			linux,code = <KEY_MENU>;
			label = "menu";
			press-threshold-microvolt = <987000>;
		};

		home-key {
			linux,code = <KEY_HOME>;
			label = "home";
			press-threshold-microvolt = <624000>;
		};

		vol-down-key {
			linux,code = <KEY_VOLUMEDOWN>;
			label = "volume down";
			press-threshold-microvolt = <300000>;
		};

		vol-up-key {
			linux,code = <KEY_VOLUMEUP>;
			label = "volume up";
			press-threshold-microvolt = <17000>;
		};
	};

	backlight: backlight {
		compatible = "pwm-backlight";
		pwms = <&pwm0 0 25000 0>;
		brightness-levels = <
			  0  20  20  21  21  22  22  23
			 23  24  24  25  25  26  26  27
			 27  28  28  29  29  30  30  31
			 31  32  32  33  33  34  34  35
			 35  36  36  37  37  38  38  39
			 40  41  42  43  44  45  46  47
			 48  49  50  51  52  53  54  55
			 56  57  58  59  60  61  62  63
			 64  65  66  67  68  69  70  71
			 72  73  74  75  76  77  78  79
			 80  81  82  83  84  85  86  87
			 88  89  90  91  92  93  94  95
			 96  97  98  99 100 101 102 103
			104 105 106 107 108 109 110 111
			112 113 114 115 116 117 118 119
			120 121 122 123 124 125 126 127
			128 129 130 131 132 133 134 135
			136 137 138 139 140 141 142 143
			144 145 146 147 148 149 150 151
			152 153 154 155 156 157 158 159
			160 161 162 163 164 165 166 167
			168 169 170 171 172 173 174 175
			176 177 178 179 180 181 182 183
			184 185 186 187 188 189 190 191
			192 193 194 195 196 197 198 199
			200 201 202 203 204 205 206 207
			208 209 210 211 212 213 214 215
			216 217 218 219 220 221 222 223
			224 225 226 227 228 229 230 231
			232 233 234 235 236 237 238 239
			240 241 242 243 244 245 246 247
			248 249 250 251 252 253 254 255
		>;
		default-brightness-level = <200>;
		enable-gpios = <&gpio1 RK_PB5 GPIO_ACTIVE_HIGH>;
	};

	clkin_gmac: external-gmac-clock {
		compatible = "fixed-clock";
		clock-frequency = <125000000>;
		clock-output-names = "clkin_gmac";
		#clock-cells = <0>;
	};

	fiq_debugger: fiq-debugger {
		compatible = "rockchip,fiq-debugger";
		rockchip,serial-id = <2>;
		rockchip,wake-irq = <0>;
		rockchip,irq-mode-enable = <0>;  /* If enable uart uses irq instead of fiq */
		rockchip,baudrate = <1500000>;  /* Only 115200 and 1500000 */
		pinctrl-names = "default";
		pinctrl-0 = <&uart2c_xfer>;
		interrupts = <GIC_SPI 150 IRQ_TYPE_LEVEL_HIGH 0>;
	};

	hdmi_sound: hdmi-sound {
		status = "okay";
		compatible = "simple-audio-card";
		simple-audio-card,format = "i2s";
		simple-audio-card,mclk-fs = <256>;
		simple-audio-card,name = "rockchip,hdmi";

		simple-audio-card,cpu {
			sound-dai = <&i2s2>;
		};
		simple-audio-card,codec {
			sound-dai = <&hdmi>;
		};
	};

	panel: panel {
		compatible = "simple-panel";
		backlight = <&backlight>;
		enable-gpios = <&gpio4 RK_PD6 GPIO_ACTIVE_HIGH>;
		prepare-delay-ms = <20>;
		enable-delay-ms = <20>;
		reset-delay-ms = <20>;
		width-mm = <120>;
		height-mm = <160>;

		display-timings {
			native-mode = <&timing0>;

			timing0: timing0 {
				clock-frequency = <200000000>;
				hactive = <1536>;
				vactive = <2048>;
				hfront-porch = <12>;
				hsync-len = <16>;
				hback-porch = <48>;
				vfront-porch = <8>;
				vsync-len = <4>;
				vback-porch = <8>;
				hsync-active = <0>;
				vsync-active = <0>;
				de-active = <0>;
				pixelclk-active = <0>;
			};
		};

		ports {
			panel_in: endpoint {
				remote-endpoint = <&edp_out>;
			};
		};
	};

	rk809_sound: rk809-sound {
		compatible = "rockchip,multicodecs-card";
		rockchip,card-name = "rockchip,rk809-codec";
		rockchip,codec-hp-det;
		rockchip,mclk-fs = <256>;
		rockchip,cpu = <&i2s1>;
		rockchip,codec = <&rk809_codec>;
	};

	rk_headset: rk-headset {
		compatible = "rockchip_headset";
		headset_gpio = <&gpio0 RK_PB5 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&hp_det>;
		io-channels = <&saradc 3>;
	};

	sdio_pwrseq: sdio-pwrseq {
		compatible = "mmc-pwrseq-simple";
		clocks = <&rk809 1>;
		clock-names = "ext_clock";
		pinctrl-names = "default";
		pinctrl-0 = <&wifi_enable_h>;

		/*
		 * On the module itself this is one of these (depending
		 * on the actual card populated):
		 * - SDIO_RESET_L_WL_REG_ON
		 * - PDN (power down when low)
		 */
		reset-gpios = <&gpio2 RK_PD3 GPIO_ACTIVE_LOW>;
	};

	usbacm_video_control: usbacm-video-control {
		compatible = "rockchip,usbacm-video-control";
		status = "disabled";
	};

	vcc_phy: vcc-phy-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vcc_phy";
		regulator-always-on;
		regulator-boot-on;
	};

	vbus_typec: vbus-typec-regulator {
		compatible = "regulator-fixed";
		enable-active-high;
		gpio = <&gpio1 18 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&vcc5v0_typec0_en>;
		regulator-name = "vbus_typec";
		vin-supply = <&vcc5v0_sys>;
	};

	vcc5v0_sys: vccsys {
		compatible = "regulator-fixed";
		regulator-name = "vcc5v0_sys";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
	};

	wireless-wlan {
		compatible = "wlan-platdata";
		rockchip,grf = <&grf>;
		wifi_chip_type = "ap6398s";
		sdio_vref = <1800>;
		WIFI,host_wake_irq = <&gpio0 RK_PA3 GPIO_ACTIVE_HIGH>;
		status = "okay";
	};

	wireless-bluetooth {
		compatible = "bluetooth-platdata";
		clocks = <&rk809 1>;
		clock-names = "ext_clock";
		uart_rts_gpios = <&gpio2 RK_PC3 GPIO_ACTIVE_LOW>;
		pinctrl-names = "default", "rts_gpio";
		pinctrl-0 = <&uart0_rts>, <&bt_irq_gpio>;
		pinctrl-1 = <&uart0_gpios>;
		BT,reset_gpio    = <&gpio2 RK_PD4 GPIO_ACTIVE_HIGH>;
		BT,wake_gpio     = <&gpio2 RK_PD2 GPIO_ACTIVE_HIGH>;
		BT,wake_host_irq = <&gpio0 RK_PA5 GPIO_ACTIVE_HIGH>;
		status = "okay";
	};
};

&cdn_dp {
	status = "okay";
	phys = <&tcphy0_dp>;
};

&cpu_l0 {
	cpu-supply = <&vdd_cpu_l>;
};

&cpu_l1 {
	cpu-supply = <&vdd_cpu_l>;
};

&cpu_l2 {
	cpu-supply = <&vdd_cpu_l>;
};

&cpu_l3 {
	cpu-supply = <&vdd_cpu_l>;
};

&cpu_b0 {
	cpu-supply = <&vdd_cpu_b>;
};

&cpu_b1 {
	cpu-supply = <&vdd_cpu_b>;
};

&display_subsystem {
	status = "okay";
};

&dfi {
	status = "okay";
};

&dmc {
	status = "okay";
	center-supply = <&vdd_center>;
	upthreshold = <40>;
	downdifferential = <20>;
	system-status-freq = <
		/*system status         freq(KHz)*/
		SYS_STATUS_NORMAL       856000
		SYS_STATUS_REBOOT       856000
		SYS_STATUS_SUSPEND      328000
		SYS_STATUS_VIDEO_1080P  666000
		SYS_STATUS_VIDEO_4K     856000
		SYS_STATUS_VIDEO_4K_10B 856000
		SYS_STATUS_PERFORMANCE  856000
		SYS_STATUS_BOOST        856000
		SYS_STATUS_DUALVIEW     856000
		SYS_STATUS_ISP          856000
	>;
	vop-bw-dmc-freq = <
	/* min_bw(MB/s) max_bw(MB/s) freq(KHz) */
		0       762      416000
		763     3012     666000
		3013    99999    856000
	>;

	vop-pn-msch-readlatency = <
		0	0x20
		4	0x20
	>;

	auto-min-freq = <328000>;
	auto-freq-en = <0>;
};

&dmc_opp_table {
		compatible = "operating-points-v2";

		opp-200000000 {
			opp-hz = /bits/ 64 <200000000>;
			opp-microvolt = <900000>;
			status = "disabled";
		};
		opp-300000000 {
			opp-hz = /bits/ 64 <300000000>;
			opp-microvolt = <900000>;
			status = "disabled";
		};
		opp-328000000 {
			opp-hz = /bits/ 64 <328000000>;
			opp-microvolt = <900000>;
		};
		opp-400000000 {
			opp-hz = /bits/ 64 <400000000>;
			opp-microvolt = <900000>;
			status = "disabled";
		};
		opp-416000000 {
			opp-hz = /bits/ 64 <416000000>;
			opp-microvolt = <900000>;
		};
		opp-528000000 {
			opp-hz = /bits/ 64 <528000000>;
			opp-microvolt = <900000>;
			status = "disabled";
		};
		opp-600000000 {
			opp-hz = /bits/ 64 <600000000>;
			opp-microvolt = <900000>;
			status = "disabled";
		};
		opp-666000000 {
			opp-hz = /bits/ 64 <666000000>;
			opp-microvolt = <900000>;
		};
		opp-800000000 {
			opp-hz = /bits/ 64 <800000000>;
			opp-microvolt = <900000>;
			status = "disabled";
		};
		opp-856000000 {
			opp-hz = /bits/ 64 <856000000>;
			opp-microvolt = <900000>;
		};
		opp-928000000 {
			opp-hz = /bits/ 64 <928000000>;
			opp-microvolt = <900000>;
			status = "disabled";
		};
};

&dp_in_vopb {
	status = "disabled";
};

&edp {
	status = "okay";
	force-hpd;

	ports {
		port@1 {
			reg = <1>;

			edp_out: endpoint {
				remote-endpoint = <&panel_in>;
			};
		};
	};
};

&edp_in_vopb {
	status = "disabled";
};

&emmc_phy {
	status = "okay";
};

&fiq_debugger {
	pinctrl-0 = <&uart2a_xfer>;
};

&gmac {
	phy-supply = <&vcc_phy>;
	phy-mode = "rgmii";
	clock_in_out = "input";
	snps,reset-gpio = <&gpio3 RK_PB7 GPIO_ACTIVE_LOW>;
	snps,reset-active-low;
	snps,reset-delays-us = <0 10000 50000>;
	assigned-clocks = <&cru SCLK_RMII_SRC>;
	assigned-clock-parents = <&clkin_gmac>;
	pinctrl-names = "default";
	pinctrl-0 = <&rgmii_pins>;
	tx_delay = <0x28>;
	rx_delay = <0x11>;
	status = "okay";
};

&gpu {
	status = "okay";
	mali-supply = <&vdd_gpu>;
};

&hdmi {
	status = "okay";
	#sound-dai-cells = <0>;
	rockchip,phy-table =
		<74250000  0x8009 0x0004 0x0272>,
		<165000000 0x802b 0x0004 0x0209>,
		<297000000 0x8039 0x0005 0x028d>,
		<594000000 0x8039 0x0000 0x00f6>,
		<000000000 0x0000 0x0000 0x0000>;
};

&hdmi_in_vopl {
	status = "disabled";
};

&i2c0 {
	status = "okay";
	i2c-scl-rising-time-ns = <180>;
	i2c-scl-falling-time-ns = <30>;
	clock-frequency = <400000>;

	rk809: pmic@20 {
		compatible = "rockchip,rk809";
		reg = <0x20>;
		interrupt-parent = <&gpio1>;
		interrupts = <RK_PC2 IRQ_TYPE_LEVEL_LOW>;
		pinctrl-names = "default", "pmic-sleep",
				"pmic-power-off", "pmic-reset";
		pinctrl-0 = <&pmic_int_l>;
		pinctrl-1 = <&soc_slppin_slp>, <&rk809_slppin_slp>;
		pinctrl-2 = <&soc_slppin_gpio>, <&rk809_slppin_pwrdn>;
		pinctrl-3 = <&soc_slppin_gpio>, <&rk809_slppin_null>;
		rockchip,system-power-controller;
		pmic-reset-func = <0>;
		wakeup-source;
		#clock-cells = <1>;
		clock-output-names = "rk808-clkout1", "rk808-clkout2";

		vcc1-supply = <&vcc5v0_sys>;
		vcc2-supply = <&vcc5v0_sys>;
		vcc3-supply = <&vcc5v0_sys>;
		vcc4-supply = <&vcc5v0_sys>;
		vcc5-supply = <&vcc_buck5>;
		vcc6-supply = <&vcc_buck5>;
		vcc7-supply = <&vcc3v3_sys>;
		vcc8-supply = <&vcc3v3_sys>;
		vcc9-supply = <&vcc5v0_sys>;

		pwrkey {
			status = "okay";
		};

		rtc {
			status = "okay";
		};

		pinctrl_rk8xx: pinctrl_rk8xx {
			gpio-controller;
			#gpio-cells = <2>;

			rk809_slppin_null: rk809_slppin_null {
				pins = "gpio_slp";
				function = "pin_fun0";
			};

			rk809_slppin_slp: rk809_slppin_slp {
				pins = "gpio_slp";
				function = "pin_fun1";
			};

			rk809_slppin_pwrdn: rk809_slppin_pwrdn {
				pins = "gpio_slp";
				function = "pin_fun2";
			};

			rk809_slppin_rst: rk809_slppin_rst {
				pins = "gpio_slp";
				function = "pin_fun3";
			};
		};

		regulators {
			vdd_center: DCDC_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <750000>;
				regulator-max-microvolt = <1350000>;
				regulator-initial-mode = <0x2>;
				regulator-name = "vdd_center";
				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <900000>;
				};
			};

			vdd_cpu_l: DCDC_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <750000>;
				regulator-max-microvolt = <1350000>;
				regulator-ramp-delay = <6001>;
				regulator-initial-mode = <0x2>;
				regulator-name = "vdd_cpu_l";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_ddr: DCDC_REG3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vcc_ddr";
				regulator-initial-mode = <0x2>;
				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};

			vcc3v3_sys: DCDC_REG4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-initial-mode = <0x2>;
				regulator-name = "vcc3v3_sys";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vcc_buck5: DCDC_REG5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <2200000>;
				regulator-max-microvolt = <2200000>;
				regulator-name = "vcc_buck5";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <2200000>;
				};
			};

			vcca_0v9: LDO_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <900000>;
				regulator-max-microvolt = <900000>;
				regulator-name = "vcca_0v9";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_1v8: LDO_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;

				regulator-name = "vcc_1v8";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vcc0v9_soc: LDO_REG3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <900000>;
				regulator-max-microvolt = <900000>;

				regulator-name = "vcc0v9_soc";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <900000>;
				};
			};

			vcca_1v8: LDO_REG4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;

				regulator-name = "vcca_1v8";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd1v5_dvp: LDO_REG5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1500000>;
				regulator-max-microvolt = <1500000>;

				regulator-name = "vdd1v5_dvp";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_1v5: LDO_REG6 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1500000>;
				regulator-max-microvolt = <1500000>;

				regulator-name = "vcc_1v5";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_3v0: LDO_REG7 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3000000>;
				regulator-max-microvolt = <3000000>;

				regulator-name = "vcc_3v0";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vccio_sd: LDO_REG8 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;

				regulator-name = "vccio_sd";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_sd: LDO_REG9 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;

				regulator-name = "vcc_sd";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc5v0_usb: SWITCH_REG1 {
				regulator-name = "vcc5v0_usb";
				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};

			vccio_3v3: SWITCH_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vccio_3v3";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};
		};

		rk809_codec: codec {
			#sound-dai-cells = <0>;
			compatible = "rockchip,rk809-codec", "rockchip,rk817-codec";
			clocks = <&cru SCLK_I2S_8CH_OUT>;
			clock-names = "mclk";
			pinctrl-names = "default";
			pinctrl-0 = <&i2s_8ch_mclk>;
			hp-volume = <20>;
			spk-volume = <3>;
			status = "okay";
		};
	};

	vdd_cpu_b: tcs4525@1c {
		compatible = "tcs,tcs4525";
		reg = <0x1c>;
		vin-supply = <&vcc5v0_sys>;
		regulator-compatible = "fan53555-reg";
		pinctrl-0 = <&vsel1_gpio>;
		vsel-gpios = <&gpio1 RK_PC1 GPIO_ACTIVE_HIGH>;
		regulator-name = "vdd_cpu_b";
		regulator-min-microvolt = <712500>;
		regulator-max-microvolt = <1500000>;
		regulator-ramp-delay = <2300>;
		fcs,suspend-voltage-selector = <1>;
		regulator-always-on;
		regulator-boot-on;
		regulator-initial-state = <3>;
		regulator-state-mem {
			regulator-off-in-suspend;
		};
	};

	vdd_gpu: tcs4526@10 {
		compatible = "tcs,tcs4526";
		reg = <0x10>;
		vin-supply = <&vcc5v0_sys>;
		regulator-compatible = "fan53555-reg";
		pinctrl-0 = <&vsel2_gpio>;
		vsel-gpios = <&gpio1 RK_PB6 GPIO_ACTIVE_HIGH>;
		regulator-name = "vdd_gpu";
		regulator-min-microvolt = <735000>;
		regulator-max-microvolt = <1400000>;
		regulator-ramp-delay = <1000>;
		fcs,suspend-voltage-selector = <1>;
		regulator-always-on;
		regulator-boot-on;
		regulator-initial-state = <3>;
		regulator-state-mem {
			regulator-off-in-suspend;
		};
	};

	bq25700: bq25700@6b {
		compatible = "ti,bq25703";
		reg = <0x6b>;
		interrupt-parent = <&gpio1>;
		interrupts = <RK_PA1 IRQ_TYPE_LEVEL_LOW>;
		pinctrl-names = "default";
		pinctrl-0 = <&charger_ok_int>;
		ti,charge-current = <1500000>;
		ti,max-charge-voltage = <8704000>;
		ti,max-input-voltage = <20000000>;
		ti,max-input-current = <6000000>;
		ti,input-current-sdp = <500000>;
		ti,input-current-dcp = <2000000>;
		ti,input-current-cdp = <2000000>;
		ti,input-current-dc = <2000000>;
		ti,minimum-sys-voltage = <6700000>;
		ti,otg-voltage = <5000000>;
		ti,otg-current = <500000>;
		ti,input-current = <500000>;
		pd-charge-only = <0>;
		status = "disabled";
	};
};

&i2c1 {
	status = "okay";
	i2c-scl-rising-time-ns = <140>;
	i2c-scl-falling-time-ns = <30>;

	mpu6500@68 {
		status = "okay";
		compatible = "invensense,mpu6500";
		reg = <0x68>;
		irq-gpio = <&gpio3 RK_PD2 IRQ_TYPE_EDGE_RISING>;
		mpu-int_config = <0x10>;
		mpu-level_shifter = <0>;
		mpu-orientation = <0 1 0 1 0 0 0 0 1>;
		orientation-x= <1>;
		orientation-y= <0>;
		orientation-z= <0>;
		mpu-debug = <1>;
	};

	sensor@d {
		status = "okay";
		compatible = "ak8963";
		reg = <0x0d>;
		type = <SENSOR_TYPE_COMPASS>;
		irq-gpio = <&gpio3 RK_PD7 IRQ_TYPE_EDGE_RISING>;
		irq_enable = <0>;
		poll_delay_ms = <30>;
		layout = <3>;
	};

	ov13850: ov13850@10 {
		compatible = "ovti,ov13850";
		status = "okay";
		reg = <0x10>;
		clocks = <&cru SCLK_CIF_OUT>;
		clock-names = "xvclk";

		/* conflict with csi-ctl-gpios */
		reset-gpios = <&gpio4 26 GPIO_ACTIVE_HIGH>;
		pwdn-gpios = <&gpio4 25 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "rockchip,camera_default";
		pinctrl-0 = <&cif_clkout>;

		port {
			ucam_out0: endpoint {
				remote-endpoint = <&mipi_in_ucam0>;
				data-lanes = <1 2>;
			};
		};
	};

	imx327: imx327@1a {
		compatible = "sony,imx327";
		status = "okay";
		reg = <0x1a>;
		clocks = <&cru SCLK_CIF_OUT>;
		clock-names = "xvclk";
		/* conflict with csi-ctl-gpios */
		reset-gpios = <&gpio4 26 GPIO_ACTIVE_HIGH>;
		pwdn-gpios = <&gpio4 25 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&cif_clkout>;
		rockchip,camera-module-index = <0>;
		rockchip,camera-module-facing = "back";
		rockchip,camera-module-name = "TongJu";
		rockchip,camera-module-lens-name = "CHT842-MD";
		port {
			ucam_out2: endpoint {
				remote-endpoint = <&mipi_in_ucam2>;
				data-lanes = <1 2>;
			};
		};
	};

};

&i2c4 {
	status = "okay";
	i2c-scl-rising-time-ns = <345>;
	i2c-scl-falling-time-ns = <11>;

	gsl3673: gsl3673@40 {
		compatible = "GSL,GSL3673";
		reg = <0x40>;
		screen_max_x = <1536>;
		screen_max_y = <2048>;
		irq_gpio_number = <&gpio4 RK_PC3 IRQ_TYPE_LEVEL_LOW>;
		rst_gpio_number = <&gpio4 RK_PC6 GPIO_ACTIVE_HIGH>;
	};
};

&i2c8 {
	status = "okay";
	i2c-scl-rising-time-ns = <345>;
	i2c-scl-falling-time-ns = <11>;
	clock-frequency = <100000>;

	fusb0: fusb30x@22 {
		compatible = "fairchild,fusb302";
		reg = <0x22>;
		pinctrl-names = "default";
		pinctrl-0 = <&fusb0_int>;
		int-n-gpios = <&gpio1 RK_PA2 GPIO_ACTIVE_HIGH>;
		vbus-5v-gpios = <&gpio0 RK_PA1 GPIO_ACTIVE_LOW>;
		status = "okay";
	};

};

&i2s1 {
	status = "okay";
	#sound-dai-cells = <0>;
};

&i2s2 {
	#sound-dai-cells = <0>;
	status = "okay";
};

&io_domains {
	status = "okay";
	bt656-supply = <&vcca_1v8>;
	audio-supply = <&vcca_1v8>;
	sdmmc-supply = <&vccio_sd>;
	gpio1830-supply = <&vcc_3v0>;
};

&isp0_mmu {
	status = "okay";
};

&isp1_mmu {
	status = "okay";
};

&mipi_dphy_tx1rx1 {
	status = "okay";

	ports {
		#address-cells = <1>;
		#size-cells = <0>;

		port@0 {
			reg = <0>;
			#address-cells = <1>;
			#size-cells = <0>;

			mipi_in_ucam1: endpoint@1 {
				reg = <1>;
				/* Unlinked camera */
				//remote-endpoint = <&ucam_out1>;
				data-lanes = <1 2>;
			};
		};

		port@1 {
			reg = <1>;
			#address-cells = <1>;
			#size-cells = <0>;

			dphy_tx1rx1_out: endpoint@0 {
				reg = <0>;
				remote-endpoint = <&isp1_mipi_in>;
			};
		};
	};
};

&mipi_dphy_rx0 {
	status = "okay";

	ports {
		#address-cells = <1>;
		#size-cells = <0>;

		port@0 {
			reg = <0>;
			#address-cells = <1>;
			#size-cells = <0>;

			mipi_in_ucam0: endpoint@1 {
				reg = <1>;
				remote-endpoint = <&ucam_out0>;
				data-lanes = <1 2>;
			};
			mipi_in_ucam2: endpoint@2 {
				reg = <2>;
				remote-endpoint = <&ucam_out2>;
				data-lanes = <1 2>;
			};
		};

		port@1 {
			reg = <1>;
			#address-cells = <1>;
			#size-cells = <0>;

			dphy_rx0_out: endpoint@0 {
				reg = <0>;
				remote-endpoint = <&isp0_mipi_in>;
			};
		};
	};
};

&pcie_phy {
	status = "okay";
};

&pcie0 {
	status = "okay";
};

&pmu_io_domains {
	status = "okay";
	pmu1830-supply = <&vcc_1v8>;
};

&pwm0 {
	status = "okay";
};

&pwm2 {
	status = "okay";
};

&rkisp1_0 {
	status = "okay";
	assigned-clocks = <&cru PLL_NPLL>, <&cru SCLK_CIF_OUT_SRC>, <&cru SCLK_CIF_OUT>;
	assigned-clock-rates = <594000000>, <594000000>, <37125000>;
	port {
		#address-cells = <1>;
		#size-cells = <0>;

		isp0_mipi_in: endpoint@0 {
			reg = <0>;
			remote-endpoint = <&dphy_rx0_out>;
		};
	};
};

&rkisp1_1 {
	status = "okay";

	port {
		#address-cells = <1>;
		#size-cells = <0>;

		isp1_mipi_in: endpoint@0 {
			reg = <0>;
			remote-endpoint = <&dphy_tx1rx1_out>;
		};
	};
};

&rockchip_suspend {
	status = "okay";
	rockchip,sleep-debug-en = <1>;
	rockchip,sleep-mode-config = <
		(0
		| RKPM_SLP_ARMPD
		| RKPM_SLP_PERILPPD
		| RKPM_SLP_DDR_RET
		| RKPM_SLP_PLLPD
		| RKPM_SLP_CENTER_PD
		| RKPM_SLP_OSC_DIS
		| RKPM_SLP_AP_PWROFF
		)
	>;
	rockchip,wakeup-config = <RKPM_GPIO_WKUP_EN>;
	rockchip,pwm-regulator-config = <PWM2_REGULATOR_EN>;
	rockchip,power-ctrl =
		<&gpio1 RK_PC1 GPIO_ACTIVE_HIGH>,
		<&gpio1 RK_PB6 GPIO_ACTIVE_HIGH>;
};

&route_edp {
	status = "okay";
};

&saradc {
	status = "okay";
	vref-supply = <&vcc_1v8>;
};

&sdmmc {
	sd-uhs-sdr12;
	sd-uhs-sdr25;
	sd-uhs-sdr50;
	sd-uhs-sdr104;
};

&spi1 {
	status = "okay";
	max-freq = <48000000>; /* spi internal clk, don't modify */
	spi_dev@0 {
		compatible = "rockchip,spidev";
		reg = <0>;
		spi-max-frequency = <12000000>;
		spi-lsb-first;
	};
};

&tcphy0 {
	status = "okay";
	orientation-switch;
	port {
		#address-cells = <1>;
		#size-cells = <0>;
		tcphy0_orientation_switch: endpoint@0 {
			reg = <0>;
			remote-endpoint = <&usbc0_orien_sw>;
		};
	};
};

&tcphy1 {
	status = "okay";
};

&tsadc {
	rockchip,hw-tshut-mode = <1>; /* tshut mode 0:CRU 1:GPIO */
	rockchip,hw-tshut-polarity = <1>; /* tshut polarity 0:LOW 1:HIGH */
	status = "okay";
};

&u2phy0 {
	status = "okay";
	extcon = <&fusb0>;

	u2phy0_otg: otg-port {
		status = "okay";
	};

	u2phy0_host: host-port {
		phy-supply = <&vcc5v0_usb>;
		status = "okay";
	};
};

&u2phy1 {
	status = "okay";

	u2phy1_otg: otg-port {
		status = "okay";
	};

	u2phy1_host: host-port {
		phy-supply = <&vcc5v0_usb>;
		status = "okay";
	};
};

&uart0 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart0_xfer &uart0_cts>;
	status = "okay";
};

&usb_host0_ehci {
	status = "okay";
};

&usb_host1_ehci {
	status = "okay";
};
&usb_host0_ohci {
	status = "okay";
};

&usb_host1_ohci {
	status = "okay";
};

&usbdrd3_0 {
	status = "okay";
};

&usbdrd3_1 {
	status = "okay";
};

&usbdrd_dwc3_0 {
	status = "okay";
	usb-role-switch;
	port {
		#address-cells = <1>;
		#size-cells = <0>;
		dwc3_0_role_switch: endpoint@0 {
			reg = <0>;
			remote-endpoint = <&usbc0_role_sw>;
		};
	};
};

&usbdrd_dwc3_1 {
	status = "okay";
};

&vopb {
	status = "okay";
};

&vopb_mmu {
	status = "okay";
};

&vopl {
	status = "okay";
};

&vopl_mmu {
	status = "okay";
};

&pinctrl {
	pinctrl-names = "default";
	pinctrl-0 = <&npu_ref_clk>;

	bq2570 {
		charger_ok_int: charger-ok-int {
			rockchip,pins =
				<1 RK_PA1 RK_FUNC_GPIO &pcfg_pull_up>;
			};
	};

	headphone {
		hp_det: hp-det {
			rockchip,pins =
				<0 RK_PB5 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	lcd_rst {
		lcd_rst_gpio: lcd-rst-gpio {
			rockchip,pins =
				<3 RK_PA4 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	npu_clk {
		npu_ref_clk: npu-ref-clk {
		     rockchip,pins =
			     <0 RK_PA2 1 &pcfg_pull_none>;
	     };
	};

	pmic {
		pmic_int_l: pmic-int-l {
			rockchip,pins =
				<1 RK_PC2 RK_FUNC_GPIO &pcfg_pull_up>;
		};
		vsel1_gpio: vsel1-gpio {
			rockchip,pins =
				<1 RK_PC1 RK_FUNC_GPIO &pcfg_pull_down>;
		};
		vsel2_gpio: vsel2-gpio {
			rockchip,pins =
				<1 RK_PB6 RK_FUNC_GPIO &pcfg_pull_down>;
		};

		soc_slppin_gpio: soc-slppin-gpio {
			rockchip,pins =
				<1 RK_PA5 RK_FUNC_GPIO &pcfg_output_low>;
		};

		soc_slppin_slp: soc-slppin-slp {
			rockchip,pins =
				<1 RK_PA5 1 &pcfg_pull_down>;
		};

		soc_slppin_rst: soc-slppin-rst {
			rockchip,pins =
				<1 RK_PA5 2 &pcfg_pull_none>;
		};
	};

	sdio-pwrseq {
		wifi_enable_h: wifi-enable-h {
			rockchip,pins =
				<2 RK_PD3 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	sdmmc {
		sdmmc_bus1: sdmmc-bus1 {
			rockchip,pins =
				<4 RK_PB0 1 &pcfg_pull_up_10ma>;
		};

		sdmmc_bus4: sdmmc-bus4 {
			rockchip,pins =
				<4 RK_PB0 1 &pcfg_pull_up_10ma>,
				<4 RK_PB1 1 &pcfg_pull_up_10ma>,
				<4 RK_PB2 1 &pcfg_pull_up_10ma>,
				<4 RK_PB3 1 &pcfg_pull_up_10ma>;
		};

		sdmmc_clk: sdmmc-clk {
			rockchip,pins =
				<4 RK_PB4 1 &pcfg_pull_none_10ma>;
		};

		sdmmc_cmd: sdmmc-cmd {
			rockchip,pins =
				<4 RK_PB5 1 &pcfg_pull_up_10ma>;
		};
	};

	tp_irq {
		tp_irq_gpio: tp-irq-gpio {
			rockchip,pins =
				<3 RK_PB0 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	usb-typec {
		usbc0_int: usbc0-int {
			rockchip,pins = <1 RK_PA2 RK_FUNC_GPIO &pcfg_pull_up>;
		};

	vcc5v0_typec0_en: vcc5v0-typec0-en {
		rockchip,pins = <1 RK_PC2 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	wireless-bluetooth {
		bt_irq_gpio: bt-irq-gpio {
			rockchip,pins =
				<0 RK_PA5 RK_FUNC_GPIO &pcfg_pull_down>;
		};

		uart0_gpios: uart0-gpios {
			rockchip,pins =
				<2 RK_PC3 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};
};

/* DON'T PUT ANYTHING BELOW HERE.  PUT IT ABOVE PINCTRL */
/* DON'T PUT ANYTHING BELOW HERE.  PUT IT ABOVE PINCTRL */
/* DON'T PUT ANYTHING BELOW HERE.  PUT IT ABOVE PINCTRL */
