// SPDX-License-Identifier: GPL-2.0
/*
 * Copyright (c) 2018 Fuzhou Rockchip Electronics Co., Ltd
 */

/dts-v1/;
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/pinctrl/rockchip.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/display/drm_mipi_dsi.h>
#include <dt-bindings/sensor-dev.h>
#include "px30.dtsi"
#include "px30-android.dtsi"

/ {
	model = "Rockchip PX30 AD D6 board";
	compatible = "rockchip,px30-ad-d6", "rockchip,px30";

	dvdd12_anx: dvdd12-anx {
		compatible = "regulator-fixed";
		regulator-name = "dvdd12-anx";
		regulator-boot-on;
		gpio = <&gpio1 RK_PB5 GPIO_ACTIVE_HIGH>;
		enable-active-high;

		regulator-state-mem {
			regulator-off-in-suspend;
		};
	};

	adc-keys {
		compatible = "adc-keys";
		io-channels = <&saradc 2>;
		io-channel-names = "buttons";
		poll-interval = <100>;
		keyup-threshold-microvolt = <1800000>;

		esc-key {
			linux,code = <KEY_ESC>;
			label = "esc";
			press-threshold-microvolt = <1310000>;
		};

		home-key {
			linux,code = <KEY_HOME>;
			label = "home";
			press-threshold-microvolt = <624000>;
		};

		menu-key {
			linux,code = <KEY_MENU>;
			label = "menu";
			press-threshold-microvolt = <987000>;
		};

		vol-down-key {
			linux,code = <KEY_VOLUMEDOWN>;
			label = "volume down";
			press-threshold-microvolt = <300000>;
		};

		vol-up-key {
			linux,code = <KEY_VOLUMEUP>;
			label = "volume up";
			press-threshold-microvolt = <17000>;
		};
	};

	backlight: backlight {
		compatible = "pwm-backlight";
		pwms = <&pwm1 0 25000 0>;
		brightness-levels = <
			  0   1   2   3   4   5   6   7
			  8   9  10  11  12  13  14  15
			 16  17  18  19  20  21  22  23
			 24  25  26  27  28  29  30  31
			 32  33  34  35  36  37  38  39
			 40  41  42  43  44  45  46  47
			 48  49  50  51  52  53  54  55
			 56  57  58  59  60  61  62  63
			 64  65  66  67  68  69  70  71
			 72  73  74  75  76  77  78  79
			 80  81  82  83  84  85  86  87
			 88  89  90  91  92  93  94  95
			 96  97  98  99 100 101 102 103
			104 105 106 107 108 109 110 111
			112 113 114 115 116 117 118 119
			120 121 122 123 124 125 126 127
			128 129 130 131 132 133 134 135
			136 137 138 139 140 141 142 143
			144 145 146 147 148 149 150 151
			152 153 154 155 156 157 158 159
			160 161 162 163 164 165 166 167
			168 169 170 171 172 173 174 175
			176 177 178 179 180 181 182 183
			184 185 186 187 188 189 190 191
			192 193 194 195 196 197 198 199
			200 201 202 203 204 205 206 207
			208 209 210 211 212 213 214 215
			216 217 218 219 220 221 222 223
			224 225 226 227 228 229 230 231
			232 233 234 235 236 237 238 239
			240 241 242 243 244 245 246 247
			248 249 250 251 252 253 254 255>;
		default-brightness-level = <200>;
		enable-gpios = <&gpio0 RK_PB7 GPIO_ACTIVE_HIGH>;
	};

	sdio_pwrseq: sdio-pwrseq {
		compatible = "mmc-pwrseq-simple";
		pinctrl-names = "default";
		pinctrl-0 = <&wifi_enable_h>;

		/*
		 * On the module itself this is one of these (depending
		 * on the actual card populated):
		 * - SDIO_RESET_L_WL_REG_ON
		 * - PDN (power down when low)
		 */
		reset-gpios = <&gpio0 RK_PA2 GPIO_ACTIVE_LOW>;
	};

	vcc_phy: vcc-phy-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vcc_phy";
		regulator-always-on;
		regulator-boot-on;
	};

	vcc5v0_sys: vccsys {
		compatible = "regulator-fixed";
		regulator-name = "vcc5v0_sys";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
	};
};

&bus_apll {
	bus-supply = <&vdd_logic>;
	status = "okay";
};

&cpu0 {
	cpu-supply = <&vdd_arm>;
};

&dfi {
	status = "okay";
};

&dmc {
	auto-freq-en = <0>;
	center-supply = <&vdd_logic>;
	status = "okay";
};

&emmc {
	bus-width = <8>;
	cap-mmc-highspeed;
	mmc-hs200-1_8v;
	no-sdio;
	no-sd;
	disable-wp;
	non-removable;
	num-slots = <1>;
	status = "okay";
};

&gpu {
	mali-supply = <&vdd_logic>;
	status = "okay";
};

&i2c0 {
	status = "okay";

	rk809: pmic@20 {
		compatible = "rockchip,rk809";
		reg = <0x20>;
		interrupt-parent = <&gpio0>;
		interrupts = <7 IRQ_TYPE_LEVEL_LOW>;
		pinctrl-names = "default", "pmic-sleep",
				"pmic-power-off", "pmic-reset";
		pinctrl-0 = <&pmic_int>;
		pinctrl-1 = <&soc_slppin_slp>, <&rk817_slppin_slp>;
		pinctrl-2 = <&soc_slppin_gpio>, <&rk817_slppin_pwrdn>;
		pinctrl-3 = <&soc_slppin_rst>, <&rk817_slppin_rst>;
		rockchip,system-power-controller;
		wakeup-source;
		#clock-cells = <1>;
		clock-output-names = "rk808-clkout1", "rk808-clkout2";
		pmic-reset-func = <1>;

		vcc1-supply = <&vcc5v0_sys>;
		vcc2-supply = <&vcc5v0_sys>;
		vcc3-supply = <&vcc5v0_sys>;
		vcc4-supply = <&vcc5v0_sys>;
		vcc5-supply = <&vcc3v3_sys>;
		vcc6-supply = <&vcc3v3_sys>;
		vcc7-supply = <&vcc3v3_sys>;
		vcc8-supply = <&vcc3v3_sys>;
		vcc9-supply = <&vcc5v0_sys>;

		pwrkey {
			status = "okay";
		};

		pinctrl_rk8xx: pinctrl_rk8xx {
			gpio-controller;
			#gpio-cells = <2>;

			rk817_slppin_null: rk817_slppin_null {
				pins = "gpio_slp";
				function = "pin_fun0";
			};

			rk817_slppin_slp: rk817_slppin_slp {
				pins = "gpio_slp";
				function = "pin_fun1";
			};

			rk817_slppin_pwrdn: rk817_slppin_pwrdn {
				pins = "gpio_slp";
				function = "pin_fun2";
			};

			rk817_slppin_rst: rk817_slppin_rst {
				pins = "gpio_slp";
				function = "pin_fun3";
			};
		};

		regulators {
			vdd_logic: DCDC_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <850000>;
				regulator-max-microvolt = <1350000>;
				regulator-ramp-delay = <6001>;
				regulator-initial-mode = <0x2>;
				regulator-name = "vdd_logic";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <950000>;
				};
			};

			vdd_arm: DCDC_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <850000>;
				regulator-max-microvolt = <1350000>;
				regulator-ramp-delay = <6001>;
				regulator-initial-mode = <0x2>;
				regulator-name = "vdd_arm";

				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <950000>;
				};
			};

			vcc_ddr: DCDC_REG3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vcc_ddr";
				regulator-initial-mode = <0x2>;

				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};

			vcc_3v0: DCDC_REG4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3000000>;
				regulator-max-microvolt = <3000000>;
				regulator-initial-mode = <0x2>;
				regulator-name = "vcc_3v0";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3000000>;
				};
			};

			vcc_1v0: LDO_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <1000000>;
				regulator-name = "vcc_1v0";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1000000>;
				};
			};

			vcc1v8_soc: LDO_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc1v8_soc";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vdd1v0_soc: LDO_REG3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <1000000>;
				regulator-name = "vcc1v0_soc";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1000000>;
				};
			};

			vcc3v0_pmu: LDO_REG4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vcc3v0_pmu";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;

				};
			};

			vccio_sd: LDO_REG5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vccio_sd";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vcc_sd: LDO_REG6 {
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vcc_sd";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;

				};
			};

			vcc2v8_dvp: LDO_REG7 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <2800000>;
				regulator-max-microvolt = <2800000>;
				regulator-name = "vcc2v8_dvp";

				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <2800000>;
				};
			};

			vcc1v8_dvp: LDO_REG8 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc1v8_dvp";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vdd1v5_dvp: LDO_REG9 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1500000>;
				regulator-max-microvolt = <1500000>;
				regulator-name = "vdd1v5_dvp";

				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <1500000>;
				};
			};

			vcc3v3_sys: DCDC_REG5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vcc3v3_sys";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vcc5v0_host: SWITCH_REG1 {
				regulator-name = "vcc5v0_host";
			};

			vcc3v3_lcd: SWITCH_REG2 {
				regulator-boot-on;
				regulator-name = "vcc3v3_lcd";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};
		};
	};
};

&io_domains {
	vccio1-supply = <&vcc1v8_soc>;
	vccio2-supply = <&vccio_sd>;
	vccio3-supply = <&vcc_3v0>;
	vccio4-supply = <&vcc3v0_pmu>;
	vccio5-supply = <&vcc_3v0>;
	status = "okay";
};

&nandc0 {
	status = "okay";
};

&pmu_io_domains {
	pmuio1-supply = <&vcc3v0_pmu>;
	pmuio2-supply = <&vcc3v0_pmu>;
	status = "okay";
};

&pwm1 {
	status = "okay";
};

&rk_rga {
	status = "okay";
};

&rockchip_suspend {
	rockchip,sleep-debug-en = <1>;
	status = "okay";
};

&saradc {
	vref-supply = <&vcc1v8_soc>;
	status = "okay";
};

&sdmmc {
	bus-width = <4>;
	cap-mmc-highspeed;
	cap-sd-highspeed;
	no-sdio;
	no-mmc;
	card-detect-delay = <800>;
	ignore-pm-notify;
	sd-uhs-sdr12;
	sd-uhs-sdr25;
	sd-uhs-sdr50;
	sd-uhs-sdr104;
	vqmmc-supply = <&vccio_sd>;
	vmmc-supply = <&vcc_sd>;
	status = "okay";
};

&sdio {
	bus-width = <4>;
	cap-sd-highspeed;
	no-sd;
	no-mmc;
	ignore-pm-notify;
	keep-power-in-suspend;
	non-removable;
	mmc-pwrseq = <&sdio_pwrseq>;
	sd-uhs-sdr104;
	status = "okay";
};

&tsadc {
	pinctrl-names = "init", "default";
	pinctrl-0 = <&tsadc_otp_gpio>;
	pinctrl-1 = <&tsadc_otp_out>;
	status = "okay";
};

&uart1 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart1_xfer &uart1_cts>;
	status = "okay";
};

&u2phy {
	status = "okay";

	u2phy_host: host-port {
		status = "okay";
	};

	u2phy_otg: otg-port {
		status = "okay";
	};
};

&usb20_otg {
	status = "okay";
};

&usb_host0_ehci {
	status = "okay";
};

&usb_host0_ohci {
	status = "okay";
};

&display_subsystem {
	status = "okay";
};

&vopb {
	status = "okay";
};

&vopb_mmu {
	status = "okay";
};

&vopl {
	status = "okay";
};

&vopl_mmu {
	status = "okay";
};

&mpp_srv {
	status = "okay";
};

&vdpu {
	status = "okay";
};

&vepu {
	status = "okay";
};

&vpu_mmu {
	status = "okay";
};

&hevc {
	status = "okay";
};

&hevc_mmu {
	status = "okay";
};

&i2c1 {
	status = "okay";

	anx6345@38 {
		compatible = "analogix,anx6345";
		reg = <0x38>;
		reset-gpios = <&gpio1 RK_PB0 GPIO_ACTIVE_LOW>;
		panel-supply = <&vcc3v3_lcd>;
		dvdd25-supply = <&vcc3v3_lcd>;
		dvdd12-supply = <&dvdd12_anx>;

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;

				anx6345_in_rgb: endpoint {
					remote-endpoint = <&rgb_out_anx6345>;
				};
			};
		};
	};
};

&rgb {
	pinctrl-names = "default", "sleep";
	pinctrl-0 = <&lcdc_rgb_pins>;
	pinctrl-1 = <&lcdc_sleep_pins>;
	status = "okay";

	ports {
		port@1 {
			reg = <1>;

			rgb_out_anx6345: endpoint {
				remote-endpoint = <&anx6345_in_rgb>;
			};
		};
	};
};

&rgb_in_vopb {
	status = "okay";
};

&rgb_in_vopl {
	status = "disabled";
};

&route_rgb {
	connect = <&vopb_out_rgb>;
	status = "okay";
};

&pinctrl {
	lcdc {
		lcdc_rgb_pins: lcdc-rgb-pins {
			rockchip,pins =
				<3 RK_PA0 1 &pcfg_pull_none_8ma>, /* LCDC_DCLK */
				<3 RK_PA1 1 &pcfg_pull_none_8ma>, /* LCDC_HSYNC */
				<3 RK_PA2 1 &pcfg_pull_none_8ma>, /* LCDC_VSYNC */
				<3 RK_PA3 1 &pcfg_pull_none_8ma>, /* LCDC_DEN */
				<3 RK_PD3 1 &pcfg_pull_none_8ma>, /* LCDC_D23 */
				<3 RK_PD2 1 &pcfg_pull_none_8ma>, /* LCDC_D22 */
				<3 RK_PD1 1 &pcfg_pull_none_8ma>, /* LCDC_D21 */
				<3 RK_PD0 1 &pcfg_pull_none_8ma>, /* LCDC_D20 */
				<3 RK_PC7 1 &pcfg_pull_none_8ma>, /* LCDC_D19 */
				<3 RK_PC6 1 &pcfg_pull_none_8ma>, /* LCDC_D18 */
				<3 RK_PC5 1 &pcfg_pull_none_8ma>, /* LCDC_D17 */
				<3 RK_PC4 1 &pcfg_pull_none_8ma>, /* LCDC_D16 */
				<3 RK_PC3 1 &pcfg_pull_none_8ma>, /* LCDC_D15 */
				<3 RK_PC2 1 &pcfg_pull_none_8ma>, /* LCDC_D14 */
				<3 RK_PC1 1 &pcfg_pull_none_8ma>, /* LCDC_D13 */
				<3 RK_PC0 1 &pcfg_pull_none_8ma>, /* LCDC_D12 */
				<3 RK_PB7 1 &pcfg_pull_none_8ma>, /* LCDC_D11 */
				<3 RK_PB6 1 &pcfg_pull_none_8ma>, /* LCDC_D10 */
				<3 RK_PB5 1 &pcfg_pull_none_8ma>, /* LCDC_D9 */
				<3 RK_PB4 1 &pcfg_pull_none_8ma>, /* LCDC_D8 */
				<3 RK_PB3 1 &pcfg_pull_none_8ma>, /* LCDC_D7 */
				<3 RK_PB2 1 &pcfg_pull_none_8ma>, /* LCDC_D6 */
				<3 RK_PB1 1 &pcfg_pull_none_8ma>, /* LCDC_D5 */
				<3 RK_PB0 1 &pcfg_pull_none_8ma>, /* LCDC_D4 */
				<3 RK_PA7 1 &pcfg_pull_none_8ma>, /* LCDC_D3 */
				<3 RK_PA6 1 &pcfg_pull_none_8ma>, /* LCDC_D2 */
				<3 RK_PA5 1 &pcfg_pull_none_8ma>, /* LCDC_D1 */
				<3 RK_PA4 1 &pcfg_pull_none_8ma>; /* LCDC_D0 */
		};

		lcdc_sleep_pins: lcdc-sleep-pins {
			rockchip,pins =
				<3 RK_PA0 RK_FUNC_GPIO &pcfg_pull_none>, /* LCDC_DCLK */
				<3 RK_PA1 RK_FUNC_GPIO &pcfg_pull_none>, /* LCDC_HSYNC */
				<3 RK_PA2 RK_FUNC_GPIO &pcfg_pull_none>, /* LCDC_VSYNC */
				<3 RK_PA3 RK_FUNC_GPIO &pcfg_pull_none>, /* LCDC_DEN */
				<3 RK_PD3 RK_FUNC_GPIO &pcfg_pull_none>, /* LCDC_D23 */
				<3 RK_PD2 RK_FUNC_GPIO &pcfg_pull_none>, /* LCDC_D22 */
				<3 RK_PD1 RK_FUNC_GPIO &pcfg_pull_none>, /* LCDC_D21 */
				<3 RK_PD0 RK_FUNC_GPIO &pcfg_pull_none>, /* LCDC_D20 */
				<3 RK_PC7 RK_FUNC_GPIO &pcfg_pull_none>, /* LCDC_D19 */
				<3 RK_PC6 RK_FUNC_GPIO &pcfg_pull_none>, /* LCDC_D18 */
				<3 RK_PC5 RK_FUNC_GPIO &pcfg_pull_none>, /* LCDC_D17 */
				<3 RK_PC4 RK_FUNC_GPIO &pcfg_pull_none>, /* LCDC_D16 */
				<3 RK_PC3 RK_FUNC_GPIO &pcfg_pull_none>, /* LCDC_D15 */
				<3 RK_PC2 RK_FUNC_GPIO &pcfg_pull_none>, /* LCDC_D14 */
				<3 RK_PC1 RK_FUNC_GPIO &pcfg_pull_none>, /* LCDC_D13 */
				<3 RK_PC0 RK_FUNC_GPIO &pcfg_pull_none>, /* LCDC_D12 */
				<3 RK_PB7 RK_FUNC_GPIO &pcfg_pull_none>, /* LCDC_D11 */
				<3 RK_PB6 RK_FUNC_GPIO &pcfg_pull_none>, /* LCDC_D10 */
				<3 RK_PB5 RK_FUNC_GPIO &pcfg_pull_none>, /* LCDC_D9 */
				<3 RK_PB4 RK_FUNC_GPIO &pcfg_pull_none>, /* LCDC_D8 */
				<3 RK_PB3 RK_FUNC_GPIO &pcfg_pull_none>, /* LCDC_D7 */
				<3 RK_PB2 RK_FUNC_GPIO &pcfg_pull_none>, /* LCDC_D6 */
				<3 RK_PB1 RK_FUNC_GPIO &pcfg_pull_none>, /* LCDC_D5 */
				<3 RK_PB0 RK_FUNC_GPIO &pcfg_pull_none>, /* LCDC_D4 */
				<3 RK_PA7 RK_FUNC_GPIO &pcfg_pull_none>, /* LCDC_D3 */
				<3 RK_PA6 RK_FUNC_GPIO &pcfg_pull_none>, /* LCDC_D2 */
				<3 RK_PA5 RK_FUNC_GPIO &pcfg_pull_none>, /* LCDC_D1 */
				<3 RK_PA4 RK_FUNC_GPIO &pcfg_pull_none>; /* LCDC_D0 */
		};
	};

	pmic {
		pmic_int: pmic_int {
			rockchip,pins =
				<0 RK_PA7 RK_FUNC_GPIO &pcfg_pull_up>;
		};

		soc_slppin_gpio: soc_slppin_gpio {
			rockchip,pins =
				<0 RK_PA4 RK_FUNC_GPIO &pcfg_output_low>;
		};

		soc_slppin_slp: soc_slppin_slp {
			rockchip,pins =
				<0 RK_PA4 1 &pcfg_pull_none>;
		};

		soc_slppin_rst: soc_slppin_rst {
			rockchip,pins =
				<0 RK_PA4 2 &pcfg_pull_none>;
		};
	};

	sdio-pwrseq {
		wifi_enable_h: wifi-enable-h {
			rockchip,pins = <0 RK_PA2 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};
};

&firmware_android {
	compatible = "android,firmware";

	fstab {
		compatible = "android,fstab";

		system {
			compatible = "android,system";
			dev = "/dev/block/by-name/system";
			type = "ext4";
			mnt_flags = "ro,barrier=1,inode_readahead_blks=8";
			fsmgr_flags = "wait";
		};

		vendor {
			compatible = "android,vendor";
			dev = "/dev/block/by-name/vendor";
			type = "ext4";
			mnt_flags = "ro,barrier=1,inode_readahead_blks=8";
			fsmgr_flags = "wait";
		};
	};
};
