// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Copyright (c) 2022 Rockchip Electronics Co., Ltd.
 */

#include <dt-bindings/clock/rk3528-cru.h>
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/interrupt-controller/arm-gic.h>
#include <dt-bindings/interrupt-controller/irq.h>
#include <dt-bindings/phy/phy.h>
#include <dt-bindings/pinctrl/rockchip.h>
#include <dt-bindings/power/rk3528-power.h>
#include <dt-bindings/soc/rockchip,boot-mode.h>
#include <dt-bindings/soc/rockchip-system-status.h>
#include <dt-bindings/suspend/rockchip-rk3528.h>
#include <dt-bindings/thermal/thermal.h>
#include <dt-bindings/display/rockchip-tve.h>

/ {
	compatible = "rockchip,rk3528";

	interrupt-parent = <&gic>;
	#address-cells = <2>;
	#size-cells = <2>;

	aliases {
		ethernet0 = &gmac0;
		ethernet1 = &gmac1;
		gpio0 = &gpio0;
		gpio1 = &gpio1;
		gpio2 = &gpio2;
		gpio3 = &gpio3;
		gpio4 = &gpio4;
		i2c0 = &i2c0;
		i2c1 = &i2c1;
		i2c2 = &i2c2;
		i2c3 = &i2c3;
		i2c4 = &i2c4;
		i2c5 = &i2c5;
		i2c6 = &i2c6;
		i2c7 = &i2c7;
		serial0 = &uart0;
		serial1 = &uart1;
		serial2 = &uart2;
		serial3 = &uart3;
		serial4 = &uart4;
		serial5 = &uart5;
		serial6 = &uart6;
		serial7 = &uart7;
		spi0 = &spi0;
		spi1 = &spi1;
		spi2 = &sfc;
	};

	clocks {
		compatible = "simple-bus";
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;

		xin24m: xin24m {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <24000000>;
			clock-output-names = "xin24m";
		};

		mclkin_sai0: mclkin-sai0 {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <0>;
			clock-output-names = "i2s0_mclkin";
		};

		mclkin_sai1: mclkin-sai1 {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <0>;
			clock-output-names = "i2s1_mclkin";
		};

		mclkout_sai0: mclkout-sai0@ff340014 {
			compatible = "rockchip,clk-out";
			reg = <0 0xff340014 0 0x4>;
			clocks = <&cru MCLK_SAI_I2S0>;
			#clock-cells = <0>;
			clock-output-names = "mclk_sai0_to_io";
			rockchip,bit-shift = <1>;
			rockchip,bit-set-to-disable;
		};

		mclkout_sai1: mclkout-sai1@ff320004 {
			compatible = "rockchip,clk-out";
			reg = <0 0xff320004 0 0x4>;
			clocks = <&cru MCLK_SAI_I2S1>;
			#clock-cells = <0>;
			clock-output-names = "mclk_sai1_to_io";
			rockchip,bit-shift = <14>;
			rockchip,bit-set-to-disable;
		};
	};

	cpus {
		#address-cells = <2>;
		#size-cells = <0>;

		cpu-map {
			cluster0 {
				core0 {
					cpu = <&cpu0>;
				};
				core1 {
					cpu = <&cpu1>;
				};
				core2 {
					cpu = <&cpu2>;
				};
				core3 {
					cpu = <&cpu3>;
				};
			};
		};

		cpu0: cpu@0 {
			device_type = "cpu";
			compatible = "arm,cortex-a53";
			reg = <0x0 0x0>;
			enable-method = "psci";
			clocks = <&scmi_clk SCMI_CLK_CPU>;
			#cooling-cells = <2>; /* min followed by max */
			dynamic-power-coefficient = <147>;
			operating-points-v2 = <&cpu0_opp_table>;
			cpu-idle-states = <&CPU_SLEEP0>;
		};

		cpu1: cpu@1 {
			device_type = "cpu";
			compatible = "arm,cortex-a53";
			reg = <0x0 0x1>;
			enable-method = "psci";
			clocks = <&scmi_clk SCMI_CLK_CPU>;
			operating-points-v2 = <&cpu0_opp_table>;
			cpu-idle-states = <&CPU_SLEEP0>;
		};

		cpu2: cpu@2 {
			device_type = "cpu";
			compatible = "arm,cortex-a53";
			reg = <0x0 0x2>;
			enable-method = "psci";
			clocks = <&scmi_clk SCMI_CLK_CPU>;
			operating-points-v2 = <&cpu0_opp_table>;
			cpu-idle-states = <&CPU_SLEEP1>;
		};

		cpu3: cpu@3 {
			device_type = "cpu";
			compatible = "arm,cortex-a53";
			reg = <0x0 0x3>;
			enable-method = "psci";
			clocks = <&scmi_clk SCMI_CLK_CPU>;
			operating-points-v2 = <&cpu0_opp_table>;
			cpu-idle-states = <&CPU_SLEEP1>;
		};

		idle-states {
			entry-method = "psci";

			CPU_SLEEP0: cpu-sleep0 {
				compatible = "arm,idle-state";
				local-timer-stop;
				arm,psci-suspend-param = <0x0010000>;
				entry-latency-us = <120>;
				exit-latency-us = <250>;
				min-residency-us = <900>;
				status = "disabled";
			};

			CPU_SLEEP1: cpu-sleep {
				compatible = "arm,idle-state";
				local-timer-stop;
				arm,psci-suspend-param = <0x0010000>;
				entry-latency-us = <120>;
				exit-latency-us = <250>;
				min-residency-us = <900>;
				status = "okay";
			};
		};
	};

	cpu0_opp_table: cpu0-opp-table {
		compatible = "operating-points-v2";
		opp-shared;

		mbist-vmin = <825000 925000 975000>;
		nvmem-cells = <&cpu_leakage>, <&cpu_opp_info>, <&cpu_mbist_vmin>;
		nvmem-cell-names = "leakage", "opp-info", "mbist-vmin";

		rockchip,video-4k-freq = <1200000>;
		rockchip,pvtm-voltage-sel = <
			0	1320	0
			1321	1350	1
			1351	1375	2
			1376	1405	3
			1406	1435	4
			1436	1470	5
			1471	1505	6
			1506	1540	7
			1541	1575	8
			1576	1610	9
			1611	1640	10
			1641	9999	11
		>;
		rockchip,pvtm-pvtpll;
		rockchip,pvtm-offset = <0x18>;
		rockchip,pvtm-sample-time = <1100>;
		rockchip,pvtm-freq = <1608000>;
		rockchip,pvtm-volt = <900000>;
		rockchip,pvtm-ref-temp = <40>;
		rockchip,pvtm-temp-prop = <0 0>;
		rockchip,pvtm-thermal-zone = "soc-thermal";
		rockchip,grf = <&grf>;
		rockchip,temp-hysteresis = <5000>;
		rockchip,low-temp = <10000>;
		rockchip,low-temp-min-volt = <900000>;

		opp-408000000 {
			opp-hz = /bits/ 64 <408000000>;
			opp-microvolt = <825000 825000 1100000>;
			opp-microvolt-L0 = <875000 875000 1100000>;
			opp-microvolt-L1 = <875000 875000 1100000>;
			opp-microvolt-L2 = <875000 875000 1100000>;
			opp-microvolt-L3 = <875000 875000 1100000>;
			opp-microvolt-L4 = <875000 875000 1100000>;
			opp-microvolt-L5 = <850000 850000 1100000>;
			clock-latency-ns = <40000>;
			opp-suspend;
		};
		opp-600000000 {
			opp-hz = /bits/ 64 <600000000>;
			opp-microvolt = <825000 825000 1100000>;
			opp-microvolt-L0 = <875000 875000 1100000>;
			opp-microvolt-L1 = <875000 875000 1100000>;
			opp-microvolt-L2 = <875000 875000 1100000>;
			opp-microvolt-L3 = <875000 875000 1100000>;
			opp-microvolt-L4 = <875000 875000 1100000>;
			opp-microvolt-L5 = <850000 850000 1100000>;
			clock-latency-ns = <40000>;
		};
		opp-816000000 {
			opp-hz = /bits/ 64 <816000000>;
			opp-microvolt = <825000 825000 1100000>;
			opp-microvolt-L0 = <875000 875000 1100000>;
			opp-microvolt-L1 = <875000 875000 1100000>;
			opp-microvolt-L2 = <875000 875000 1100000>;
			opp-microvolt-L3 = <875000 875000 1100000>;
			opp-microvolt-L4 = <875000 875000 1100000>;
			opp-microvolt-L5 = <850000 850000 1100000>;
			clock-latency-ns = <40000>;
		};
		opp-1008000000 {
			opp-hz = /bits/ 64 <1008000000>;
			opp-microvolt = <825000 825000 1100000>;
			opp-microvolt-L0 = <875000 875000 1100000>;
			opp-microvolt-L1 = <875000 875000 1100000>;
			opp-microvolt-L2 = <875000 875000 1100000>;
			opp-microvolt-L3 = <875000 875000 1100000>;
			opp-microvolt-L4 = <875000 875000 1100000>;
			opp-microvolt-L5 = <850000 850000 1100000>;
			clock-latency-ns = <40000>;
		};
		opp-1200000000 {
			opp-hz = /bits/ 64 <1200000000>;
			opp-microvolt = <825000 825000 1100000>;
			opp-microvolt-L0 = <900000 900000 1100000>;
			opp-microvolt-L1 = <887500 887500 1100000>;
			opp-microvolt-L2 = <875000 875000 1100000>;
			opp-microvolt-L3 = <875000 875000 1100000>;
			opp-microvolt-L4 = <875000 875000 1100000>;
			opp-microvolt-L5 = <862500 862500 1100000>;
			opp-microvolt-L6 = <850000 850000 1100000>;
			clock-latency-ns = <40000>;
		};
		opp-1416000000 {
			opp-hz = /bits/ 64 <1416000000>;
			opp-microvolt = <962500 962500 1100000>;
			opp-microvolt-L1 = <950000 950000 1100000>;
			opp-microvolt-L2 = <950000 950000 1100000>;
			opp-microvolt-L3 = <937500 937500 1100000>;
			opp-microvolt-L4 = <925000 925000 1100000>;
			opp-microvolt-L5 = <912500 912500 1100000>;
			opp-microvolt-L6 = <900000 900000 1100000>;
			opp-microvolt-L7 = <887500 887000 1100000>;
			opp-microvolt-L8 = <875000 875000 1100000>;
			opp-microvolt-L9 = <862500 862500 1100000>;
			opp-microvolt-L10 = <850000 850000 1100000>;
			opp-microvolt-L11 = <850000 850000 1100000>;
			clock-latency-ns = <40000>;
		};
		opp-1608000000 {
			opp-hz = /bits/ 64 <1608000000>;
			opp-microvolt = <1012500 1012500 1100000>;
			opp-microvolt-L2 = <1000000 1000000 1100000>;
			opp-microvolt-L3 = <987500 987500 1100000>;
			opp-microvolt-L4 = <975000 975000 1100000>;
			opp-microvolt-L5 = <962500 962500 1100000>;
			opp-microvolt-L6 = <950000 950000 1100000>;
			opp-microvolt-L7 = <937500 937500 1100000>;
			opp-microvolt-L8 = <925000 925000 1100000>;
			opp-microvolt-L9 = <912500 912500 1100000>;
			opp-microvolt-L10 = <900000 900000 1100000>;
			opp-microvolt-L11 = <887500 887500 1100000>;
			clock-latency-ns = <40000>;
		};
		opp-1800000000 {
			opp-hz = /bits/ 64 <1800000000>;
			opp-microvolt = <1062500 1062500 1100000>;
			opp-microvolt-L1 = <1050000 1050000 1100000>;
			opp-microvolt-L2 = <1037500 1037500 1100000>;
			opp-microvolt-L3 = <1025000 1025000 1100000>;
			opp-microvolt-L4 = <1012500 1012500 1100000>;
			opp-microvolt-L5 = <1000000 1000000 1100000>;
			opp-microvolt-L6 = <987500 987500 1100000>;
			opp-microvolt-L7 = <975000 975000 1100000>;
			opp-microvolt-L8 = <962500 962500 1100000>;
			opp-microvolt-L9 = <950000 950000 1100000>;
			opp-microvolt-L10 = <937500 937500 1100000>;
			opp-microvolt-L11 = <925000 925000 1100000>;
			clock-latency-ns = <40000>;
		};
		opp-2016000000 {
			opp-hz = /bits/ 64 <2016000000>;
			opp-microvolt = <1100000 1100000 1100000>;
			opp-microvolt-L1 = <1087500 1087500 1100000>;
			opp-microvolt-L2 = <1075000 1075000 1100000>;
			opp-microvolt-L3 = <1062500 1062500 1100000>;
			opp-microvolt-L4 = <1050000 1050000 1100000>;
			opp-microvolt-L5 = <1037500 1037500 1100000>;
			opp-microvolt-L6 = <1025000 1025000 1100000>;
			opp-microvolt-L7 = <1012500 1012500 1100000>;
			opp-microvolt-L8 = <1000000 1000000 1100000>;
			opp-microvolt-L9 = <987500 987500 1100000>;
			opp-microvolt-L10 = <975000 975000 1100000>;
			opp-microvolt-L11 = <962500 962500 1100000>;
			clock-latency-ns = <40000>;
		};
	};

	arm-pmu {
		compatible = "arm,cortex-a53-pmu";
		interrupts = <GIC_SPI 171 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 172 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 173 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 174 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-affinity = <&cpu0>, <&cpu1>, <&cpu2>, <&cpu3>;
	};

	cpuinfo {
		compatible = "rockchip,cpuinfo";
		nvmem-cells = <&otp_id>, <&otp_cpu_version>, <&cpu_code>;
		nvmem-cell-names = "id", "cpu-version", "cpu-code";
	};

	display_subsystem: display-subsystem {
		compatible = "rockchip,display-subsystem";
		ports = <&vop_out>;
		status = "disabled";
	};

	dmc: dmc {
		compatible = "rockchip,rk3528-dmc";
		interrupts = <GIC_SPI 17 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "complete";
		devfreq-events = <&dfi>;
		clocks = <&scmi_clk SCMI_CLK_DDR>;
		clock-names = "dmc_clk";
		operating-points-v2 = <&dmc_opp_table>;
		upthreshold = <40>;
		downdifferential = <20>;
		system-status-level = <
			/* system status	freq level */
			SYS_STATUS_NORMAL	DMC_FREQ_LEVEL_HIGH
		>;
		auto-min-freq = <324000>;
		auto-freq-en = <0>;
		status = "disabled";
	};

	dmc_opp_table: dmc-opp-table {
		compatible = "operating-points-v2";

		mbist-vmin = <850000 900000>;
		nvmem-cells = <&log_leakage>, <&dmc_opp_info>, <&logic_mbist_vmin>;
		nvmem-cell-names = "leakage", "opp-info", "mbist-vmin";

		rockchip,temp-hysteresis = <5000>;
		rockchip,low-temp = <10000>;
		rockchip,low-temp-min-volt = <900000>;

		rockchip,leakage-voltage-sel = <
			1   10   0
			11  14   1
			15  22   2
			23  28   3
			29  254  4
		>;

		opp-920000000 {
			opp-hz = /bits/ 64 <920000000>;
			opp-microvolt = <850000 850000 1000000>;
		};
		opp-1056000000 {
			opp-hz = /bits/ 64 <1056000000>;
			opp-microvolt = <850000 850000 1000000>;
			opp-microvolt-L0 = <875000 875000 1000000>;
			opp-microvolt-L1 = <850000 850000 1000000>;
			opp-microvolt-L2 = <850000 850000 1000000>;
			opp-microvolt-L3 = <850000 850000 1000000>;
			opp-microvolt-L4 = <850000 850000 1000000>;
		};
		opp-1184000000 {
			opp-hz = /bits/ 64 <1184000000>;
			opp-microvolt = <900000 900000 1000000>;
			opp-microvolt-L0 = <950000 950000 1000000>;
			opp-microvolt-L1 = <925000 925000 1000000>;
			opp-microvolt-L2 = <900000 900000 1000000>;
			opp-microvolt-L3 = <875000 875000 1000000>;
			opp-microvolt-L4 = <862500 862500 1000000>;
			status = "disabled";
		};
	};

	firmware {
		scmi: scmi {
			compatible = "arm,scmi-smc";
			shmem = <&scmi_shmem>;
			arm,smc-id = <0x82000010>;
			#address-cells = <1>;
			#size-cells = <0>;

			scmi_clk: protocol@14 {
				reg = <0x14>;
				#clock-cells = <1>;

				assigned-clocks = <&scmi_clk SCMI_CLK_CPU>;
				assigned-clock-rates = <1200000000>;
			};
		};
	};

	mpp_srv: mpp-srv {
		compatible = "rockchip,mpp-service";
		rockchip,taskqueue-count = <5>;
		rockchip,resetgroup-count = <5>;
		status = "disabled";
	};

	psci {
		compatible = "arm,psci-1.0";
		method = "smc";
	};

	rkvtunnel: rkvtunnel {
		compatible = "rockchip,video-tunnel";
		status = "disabled";
	};

	rockchip_suspend: rockchip-suspend {
		compatible = "rockchip,pm-rk3528";
		status = "disabled";
		rockchip,sleep-debug-en = <0>;
		rockchip,sleep-mode-config = <
			(0
			| RKPM_SLP_ARMPD
			)
		>;
		rockchip,wakeup-config = <
			(0
			| RKPM_CPU0_WKUP_EN
			| RKPM_GPIO_WKUP_EN
			)
		>;
	};

	rockchip_system_monitor: rockchip-system-monitor {
		compatible = "rockchip,system-monitor";

		rockchip,thermal-zone = "soc-thermal";
		rockchip,polling-delay = <200>; /* milliseconds */
		rockchip,temp-hysteresis = <5000>; /* millicelsius */
		rockchip,offline-cpu-temp = <105000>; /* millicelsius */
		rockchip,temp-offline-cpus = "2-3";
	};

	secure_otp: secure-otp {
		compatible = "rockchip,secure-otp";
		rockchip,otp-size = <32>;
		status = "disabled";
	};

	thermal_zones: thermal-zones {
		soc_thermal: soc-thermal {
			polling-delay-passive = <20>; /* milliseconds */
			polling-delay = <1000>; /* milliseconds */
			sustainable-power = <638>; /* milliwatts */

			thermal-sensors = <&tsadc 0>;

			trips {
				threshold: trip-point-0 {
					temperature = <95000>;
					hysteresis = <2000>;
					type = "passive";
				};
				target: trip-point-1 {
					temperature = <110000>;
					hysteresis = <2000>;
					type = "passive";
				};
				soc_crit: soc-crit {
					temperature = <120000>; /* millicelsius */
					hysteresis = <2000>; /* millicelsius */
					type = "critical";
				};
			};

			cooling-maps {
				map0 {
					trip = <&target>;
					cooling-device =
						<&cpu0 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
					contribution = <1024>;
				};
				map1 {
					trip = <&target>;
					cooling-device =
						<&gpu THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
					contribution = <1024>;
				};
			};

		};
	};

	timer {
		compatible = "arm,armv8-timer";
		interrupts = <GIC_PPI 13 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
			     <GIC_PPI 14 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
			     <GIC_PPI 11 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
			     <GIC_PPI 10 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>;
	};

	scmi_shmem: scmi-shmem@10f000 {
		compatible = "arm,scmi-shmem";
		reg = <0x0 0x0010f000 0x0 0x100>;
	};

	sram: sram@fe480000 {
		compatible = "mmio-sram";
		reg = <0x0 0xfe480000 0x0 0xc000>;

		#address-cells = <1>;
		#size-cells = <1>;
		ranges = <0x0 0x0 0xfe480000 0xc000>;

		/* start address and size should be 4k algin */
		rkvdec_sram: rkvdec-sram@0 {
			reg = <0x0 0xc000>;
		};
	};

	pcie2x1: pcie@fe4f0000 {
		compatible = "rockchip,rk3528-pcie", "snps,dw-pcie";
		#address-cells = <3>;
		#size-cells = <2>;
		bus-range = <0x0 0xff>;
		clocks = <&cru ACLK_PCIE>, <&cru HCLK_PCIE_SLV>,
			 <&cru HCLK_PCIE_DBI>, <&cru PCLK_CRU_PCIE>,
			 <&cru CLK_PCIE_AUX>, <&cru PCLK_PCIE>,
			 <&cru PCLK_PCIE_PHY>;
		clock-names = "aclk", "hclk_slv",
			      "hclk_dbi", "pclk_cru",
			      "aux", "pclk",
			      "pipe";
		device_type = "pci";
		interrupts = <GIC_SPI 158 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 157 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 156 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 155 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 154 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 153 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "msi", "pmc", "sys", "legacy", "msg", "err";
		#interrupt-cells = <1>;
		interrupt-map-mask = <0 0 0 7>;
		interrupt-map = <0 0 0 1 &pcie2x1_intc 0>,
				<0 0 0 2 &pcie2x1_intc 1>,
				<0 0 0 3 &pcie2x1_intc 2>,
				<0 0 0 4 &pcie2x1_intc 3>;
		linux,pci-domain = <0>;
		num-ib-windows = <8>;
		num-ob-windows = <8>;
		num-viewport = <4>;
		max-link-speed = <2>;
		num-lanes = <1>;
		phys = <&combphy_pu PHY_TYPE_PCIE>;
		phy-names = "pcie-phy";
		ranges = <0x00000800 0x0 0xfc000000 0x0 0xfc000000 0x0 0x100000
			  0x81000000 0x0 0xfc100000 0x0 0xfc100000 0x0 0x100000
			  0x82000000 0x0 0xfc200000 0x0 0xfc200000 0x0 0x1e00000
			  0xc3000000 0x1 0x00000000 0x1 0x00000000 0x0 0x40000000>;
		reg = <0x0 0xfe4f0000 0x0 0x10000>,
		      <0x1 0x40000000 0x0 0x400000>;
		reg-names = "pcie-apb", "pcie-dbi";
		resets = <&cru SRST_RESETN_PCIE_POWER_UP>, <&cru SRST_PRESETN_PCIE>,
			 <&cru SRST_PRESETN_CRU_PCIE>;
		reset-names = "pcie", "periph", "preset_cru";
		status = "disabled";

		pcie2x1_intc: legacy-interrupt-controller {
			interrupt-controller;
			#address-cells = <0>;
			#interrupt-cells = <1>;
			interrupt-parent = <&gic>;
			interrupts = <GIC_SPI 155 IRQ_TYPE_EDGE_RISING>;
		};
	};

	usbdrd30: usbdrd {
		compatible = "rockchip,rk3528-dwc3", "rockchip,rk3399-dwc3";
		clocks = <&cru CLK_REF_USB3OTG>, <&cru CLK_SUSPEND_USB3OTG>,
			 <&cru ACLK_USB3OTG>;
		clock-names = "ref_clk", "suspend_clk",
			      "bus_clk";
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;
		status = "disabled";

		usbdrd_dwc3: dwc3@fe500000 {
			compatible = "snps,dwc3";
			reg = <0x0 0xfe500000 0x0 0x400000>;
			interrupts = <GIC_SPI 152 IRQ_TYPE_LEVEL_HIGH>;
			dr_mode = "otg";
			phys = <&u2phy_otg>, <&combphy_pu PHY_TYPE_USB3>;
			phy-names = "usb2-phy", "usb3-phy";
			phy_type = "utmi_wide";
			resets = <&cru SRST_ARESETN_USB3OTG>;
			reset-names = "usb3-otg";
			snps,dis_enblslpm_quirk;
			snps,dis-u1-entry-quirk;
			snps,dis-u2-entry-quirk;
			snps,dis-u2-freeclk-exists-quirk;
			snps,dis-del-phy-power-chg-quirk;
			snps,dis-tx-ipgap-linecheck-quirk;
			snps,dis_rxdet_inp3_quirk;
			snps,parkmode-disable-hs-quirk;
			snps,parkmode-disable-ss-quirk;
			quirk-skip-phy-init;
			status = "disabled";
		};
	};

	gic: interrupt-controller@fed01000 {
		compatible = "arm,gic-400";
		#interrupt-cells = <3>;
		#address-cells = <0>;
		interrupt-controller;
		reg = <0x0 0xfed01000 0 0x1000>,
		      <0x0 0xfed02000 0 0x2000>,
		      <0x0 0xfed04000 0 0x2000>,
		      <0x0 0xfed06000 0 0x2000>;
		interrupts = <GIC_PPI 9 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>;
	};

	usb_host0_ehci: usb@ff100000 {
		compatible = "generic-ehci";
		reg = <0x0 0xff100000 0x0 0x40000>;
		interrupts = <GIC_SPI 143 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru HCLK_USBHOST>,
			 <&cru HCLK_USBHOST_ARB>,
			 <&usb2phy>;
		clock-names = "usbhost", "arbiter", "utmi";
		phys = <&u2phy_host>;
		phy-names = "usb2-phy";
		status = "disabled";
	};

	usb_host0_ohci: usb@ff140000 {
		compatible = "generic-ohci";
		reg = <0x0 0xff140000 0x0 0x40000>;
		interrupts = <GIC_SPI 144 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru HCLK_USBHOST>,
			 <&cru HCLK_USBHOST_ARB>,
			 <&usb2phy>;
		clock-names = "usbhost", "arbiter", "utmi";
		phys = <&u2phy_host>;
		phy-names = "usb2-phy";
		status = "disabled";
	};

	debug: debug@ff190000 {
		compatible = "rockchip,debug";
		reg = <0x0 0xff190000 0x0 0x1000>,
		      <0x0 0xff192000 0x0 0x1000>,
		      <0x0 0xff194000 0x0 0x1000>,
		      <0x0 0xff196000 0x0 0x1000>;
	};

	qos_crypto_a: qos@ff200000 {
		compatible = "syscon";
		reg = <0x0 0xff200000 0x0 0x20>;
	};

	qos_crypto_p: qos@ff200080 {
		compatible = "syscon";
		reg = <0x0 0xff200080 0x0 0x20>;
	};

	qos_dcf: qos@ff200100 {
		compatible = "syscon";
		reg = <0x0 0xff200100 0x0 0x20>;
	};

	qos_dft2apb: qos@ff200200 {
		compatible = "syscon";
		reg = <0x0 0xff200200 0x0 0x20>;
	};

	qos_dma2ddr: qos@ff200280 {
		compatible = "syscon";
		reg = <0x0 0xff200280 0x0 0x20>;
	};

	qos_dmac: qos@ff200300 {
		compatible = "syscon";
		reg = <0x0 0xff200300 0x0 0x20>;
	};

	qos_keyreader: qos@ff200380 {
		compatible = "syscon";
		reg = <0x0 0xff200380 0x0 0x20>;
	};

	qos_cpu: qos@ff210000 {
		compatible = "syscon";
		reg = <0x0 0xff210000 0x0 0x20>;
	};

	qos_debug: qos@ff210080 {
		compatible = "syscon";
		reg = <0x0 0xff210080 0x0 0x20>;
	};

	qos_gpu_m0: qos@ff220000 {
		compatible = "syscon";
		reg = <0x0 0xff220000 0x0 0x20>;
	};

	qos_gpu_m1: qos@ff220080 {
		compatible = "syscon";
		reg = <0x0 0xff220080 0x0 0x20>;
	};

	qos_pmu_mcu: qos@ff240000 {
		compatible = "syscon";
		reg = <0x0 0xff240000 0x0 0x20>;
	};

	qos_rkvdec: qos@ff250000 {
		compatible = "syscon";
		reg = <0x0 0xff250000 0x0 0x20>;
	};

	qos_rkvenc: qos@ff260000 {
		compatible = "syscon";
		reg = <0x0 0xff260000 0x0 0x20>;
	};

	qos_gmac0: qos@ff270000 {
		compatible = "syscon";
		reg = <0x0 0xff270000 0x0 0x20>;
	};

	qos_hdcp: qos@ff270080 {
		compatible = "syscon";
		reg = <0x0 0xff270080 0x0 0x20>;
	};

	qos_jpegdec: qos@ff270100 {
		compatible = "syscon";
		reg = <0x0 0xff270100 0x0 0x20>;
	};

	qos_rga2_m0ro: qos@ff270200 {
		compatible = "syscon";
		reg = <0x0 0xff270200 0x0 0x20>;
	};

	qos_rga2_m0wo: qos@ff270280 {
		compatible = "syscon";
		reg = <0x0 0xff270280 0x0 0x20>;
	};

	qos_sdmmc0: qos@ff270300 {
		compatible = "syscon";
		reg = <0x0 0xff270300 0x0 0x20>;
	};

	qos_usb2host: qos@ff270380 {
		compatible = "syscon";
		reg = <0x0 0xff270380 0x0 0x20>;
	};

	qos_vdpp: qos@ff270480 {
		compatible = "syscon";
		reg = <0x0 0xff270480 0x0 0x20>;
	};

	qos_vop: qos@ff270500 {
		compatible = "syscon";
		reg = <0x0 0xff270500 0x0 0x20>;
	};

	qos_emmc: qos@ff280000 {
		compatible = "syscon";
		reg = <0x0 0xff280000 0x0 0x20>;
	};

	qos_fspi: qos@ff280080 {
		compatible = "syscon";
		reg = <0x0 0xff280080 0x0 0x20>;
	};

	qos_gmac1: qos@ff280100 {
		compatible = "syscon";
		reg = <0x0 0xff280100 0x0 0x20>;
	};

	qos_pcie: qos@ff280180 {
		compatible = "syscon";
		reg = <0x0 0xff280180 0x0 0x20>;
	};

	qos_sdio0: qos@ff280200 {
		compatible = "syscon";
		reg = <0x0 0xff280200 0x0 0x20>;
	};

	qos_sdio1: qos@ff280280 {
		compatible = "syscon";
		reg = <0x0 0xff280280 0x0 0x20>;
	};

	qos_tsp: qos@ff280300 {
		compatible = "syscon";
		reg = <0x0 0xff280300 0x0 0x20>;
	};

	qos_usb3otg: qos@ff280380 {
		compatible = "syscon";
		reg = <0x0 0xff280380 0x0 0x20>;
	};

	qos_vpu: qos@ff280400 {
		compatible = "syscon";
		reg = <0x0 0xff280400 0x0 0x20>;
	};

	/*
	 * Merge all GRF, each independent GRF offset is shown as bellow:
	 * CORE_GRF:		0xff300000
	 * GPU_GRF:		0xff310000
	 * RKVENC_GRF:		0xff320000
	 * DDR_GRF:		0xff330000
	 * VPU_GRF:		0xff340000
	 * COMBO_PIPE_PHY_GRF:	0xff348000
	 * RKVDEC_GRF:		0xff350000
	 * VO_GRF:		0xff360000
	 * PMU_GRF:		0xff370000
	 * SYS_GRF:		0xff380000
	 */
	grf: syscon@ff300000 {
		compatible = "rockchip,rk3528-grf", "syscon", "simple-mfd";
		reg = <0x0 0xff300000 0x0 0x90000>;

		grf_cru: grf-clock-controller {
			compatible = "rockchip,rk3528-grf-cru";
			#clock-cells = <1>;
		};

		reboot_mode: reboot-mode {
			compatible = "syscon-reboot-mode";
			offset = <0x70200>;
			mode-bootloader = <BOOT_BL_DOWNLOAD>;
			mode-charge = <BOOT_CHARGING>;
			mode-fastboot = <BOOT_FASTBOOT>;
			mode-loader = <BOOT_BL_DOWNLOAD>;
			mode-normal = <BOOT_NORMAL>;
			mode-recovery = <BOOT_RECOVERY>;
			mode-ums = <BOOT_UMS>;
			mode-panic = <BOOT_PANIC>;
			mode-watchdog = <BOOT_WATCHDOG>;
		};
	};

	cru: clock-controller@ff4a0000 {
		compatible = "rockchip,rk3528-cru";
		reg = <0x0 0xff4a0000 0x0 0x30000>;
		rockchip,grf = <&grf>;
		#clock-cells = <1>;
		#reset-cells = <1>;

		assigned-clocks =
			<&cru XIN_OSC0_DIV>,
			<&cru PLL_GPLL>,
			<&cru PLL_PPLL>,
			<&cru PLL_CPLL>,
			<&cru CLK_MATRIX_250M_SRC>,
			<&cru CLK_MATRIX_500M_SRC>,
			<&cru CLK_MATRIX_50M_SRC>,
			<&cru CLK_MATRIX_100M_SRC>,
			<&cru CLK_MATRIX_150M_SRC>,
			<&cru CLK_MATRIX_200M_SRC>,
			<&cru CLK_MATRIX_300M_SRC>,
			<&cru CLK_MATRIX_339M_SRC>,
			<&cru CLK_MATRIX_400M_SRC>,
			<&cru CLK_MATRIX_600M_SRC>,
			<&cru CLK_PPLL_50M_MATRIX>,
			<&cru CLK_PPLL_100M_MATRIX>,
			<&cru CLK_PPLL_125M_MATRIX>,
			<&cru ACLK_BUS_VOPGL_ROOT>,
			<&cru ACLK_VO_ROOT>,
			<&cru ACLK_VPU_ROOT>,
			<&cru ACLK_VPU_L_ROOT>;

		assigned-clock-rates =
			<32768>,
			<1188000000>,
			<1000000000>,
			<996000000>,
			<250000000>,
			<500000000>,
			<50000000>,
			<100000000>,
			<150000000>,
			<200000000>,
			<300000000>,
			<340000000>,
			<400000000>,
			<600000000>,
			<50000000>,
			<100000000>,
			<125000000>,
			<500000000>,
			<340000000>,
			<300000000>,
			<200000000>;
	};

	ioc_grf: syscon@ff540000 {
		compatible = "rockchip,rk3528-ioc-grf", "syscon";
		reg = <0x0 0xff540000 0x0 0x40000>;
	};

	pmu: power-management@ff600000 {
		compatible = "rockchip,rk3528-pmu", "syscon", "simple-mfd";
		reg = <0x0 0xff600000 0x0 0x2000>;

		power: power-controller {
			compatible = "rockchip,rk3528-power-controller";
			#power-domain-cells = <1>;
			#address-cells = <1>;
			#size-cells = <0>;
			status = "okay";

			/* These power domains are grouped by VD_GPU */
			pd_gpu@RK3528_PD_GPU {
				reg = <RK3528_PD_GPU>;
				clocks = <&cru ACLK_GPU_MALI>,
					 <&cru PCLK_GPU_ROOT>;
				pm_qos = <&qos_gpu_m0>,
					 <&qos_gpu_m1>;
			};
			/* These power domains are grouped by VD_LOGIC */
			pd_rkvdec@RK3528_PD_RKVDEC {
				reg = <RK3528_PD_RKVDEC>;
			};
			pd_rkvenc@RK3528_PD_RKVENC {
				reg = <RK3528_PD_RKVENC>;
			};
			pd_vo@RK3528_PD_VO {
				reg = <RK3528_PD_VO>;
			};
			pd_vpu@RK3528_PD_VPU {
				reg = <RK3528_PD_VPU>;
			};
		};
	};

	mailbox: mailbox@ff630000 {
		compatible = "rockchip,rk3528-mailbox",
			     "rockchip,rk3368-mailbox";
		reg = <0x0 0xff630000 0x0 0x200>;
		interrupts = <GIC_SPI 60 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru PCLK_PMU_MAILBOX>;
		clock-names = "pclk_mailbox";
		#mbox-cells = <1>;
		status = "disabled";
	};

	gpu: gpu@ff700000 {
		compatible = "arm,mali-450";
		reg = <0x0 0xff700000 0x0 0x40000>;

		interrupts = <GIC_SPI 88 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 89 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 86 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 92 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 93 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 90 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 91 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "Mali_GP_IRQ",
				  "Mali_GP_MMU_IRQ",
				  "IRQPP",
				  "Mali_PP0_IRQ",
				  "Mali_PP0_MMU_IRQ",
				  "Mali_PP1_IRQ",
				  "Mali_PP1_MMU_IRQ";
		clocks = <&scmi_clk SCMI_CLK_GPU>, <&cru ACLK_GPU_MALI>,
			 <&cru PCLK_GPU_ROOT>;
		clock-names = "clk_mali", "aclk_gpu_mali", "pclk_gpu";
		assigned-clocks = <&scmi_clk SCMI_CLK_GPU>;
		assigned-clock-rates = <300000000>;
		power-domains = <&power RK3528_PD_GPU>;
		operating-points-v2 = <&gpu_opp_table>;
		#cooling-cells = <2>;
		rockchip,grf = <&grf>;
		status = "disabled";

		gpu_power_model: power-model {
			compatible = "simple-power-model";
			leakage-range= <1 3>;
			ls = <(-15658) 67354 0>;
			static-coefficient = <10000>;
			dynamic-coefficient = <724>;
			ts = <3156546 120154 (-2506) 39>;
			thermal-zone = "soc-thermal";
		};
	};

	gpu_opp_table: gpu-opp-table {
		compatible = "operating-points-v2";

		mbist-vmin = <825000 925000>;
		nvmem-cells = <&gpu_leakage>, <&gpu_opp_info>, <&gpu_mbist_vmin>;
		nvmem-cell-names = "leakage", "opp-info", "mbist-vmin";

		rockchip,pvtm-voltage-sel = <
			0	750	0
			751	770	1
			771	790	2
			791	810	3
			811	830	4
			831	850	5
			851	870	6
			871	890	7
			891	9999	8
		>;
		rockchip,pvtm-pvtpll;
		rockchip,pvtm-offset = <0x10018>;
		rockchip,pvtm-sample-time = <1100>;
		rockchip,pvtm-freq = <800000>;
		rockchip,pvtm-volt = <900000>;
		rockchip,pvtm-ref-temp = <40>;
		rockchip,pvtm-temp-prop = <0 0>;
		rockchip,pvtm-thermal-zone = "soc-thermal";
		rockchip,grf = <&grf>;
		rockchip,temp-hysteresis = <5000>;
		rockchip,low-temp = <10000>;
		rockchip,low-temp-min-volt = <900000>;

		opp-300000000 {
			opp-hz = /bits/ 64 <300000000>;
			opp-microvolt = <875000 875000 1000000>;
			opp-microvolt-L5 = <850000 850000 1000000>;
			opp-microvolt-L6 = <837500 837500 1000000>;
			opp-microvolt-L7 = <825000 825000 1000000>;
			opp-microvolt-L8 = <825000 825000 1000000>;
		};
		opp-500000000 {
			opp-hz = /bits/ 64 <500000000>;
			opp-microvolt = <875000 875000 1000000>;
			opp-microvolt-L5 = <850000 850000 1000000>;
			opp-microvolt-L6 = <837500 837500 1000000>;
			opp-microvolt-L7 = <825000 825000 1000000>;
			opp-microvolt-L8 = <825000 825000 1000000>;
		};
		opp-600000000 {
			opp-hz = /bits/ 64 <600000000>;
			opp-microvolt = <875000 875000 1000000>;
			opp-microvolt-L5 = <850000 850000 1000000>;
			opp-microvolt-L6 = <837500 837500 1000000>;
			opp-microvolt-L7 = <825000 825000 1000000>;
			opp-microvolt-L8 = <825000 825000 1000000>;
		};
		opp-700000000 {
			opp-hz = /bits/ 64 <700000000>;
			opp-microvolt = <900000 900000 1000000>;
			opp-microvolt-L1 = <887500 887500 1000000>;
			opp-microvolt-L2 = <875000 875000 1000000>;
			opp-microvolt-L3 = <875000 875000 1000000>;
			opp-microvolt-L4 = <875000 875000 1000000>;
			opp-microvolt-L5 = <850000 850000 1000000>;
			opp-microvolt-L6 = <837500 837500 1000000>;
			opp-microvolt-L7 = <825000 825000 1000000>;
			opp-microvolt-L8 = <825000 825000 1000000>;
			clock-latency-ns = <40000>;
		};
		opp-800000000 {
			opp-hz = /bits/ 64 <800000000>;
			opp-microvolt = <950000 950000 1000000>;
			opp-microvolt-L1 = <937500 937500 1000000>;
			opp-microvolt-L2 = <925000 925000 1000000>;
			opp-microvolt-L3 = <912500 912500 1000000>;
			opp-microvolt-L4 = <900000 900000 1000000>;
			opp-microvolt-L5 = <887500 887500 1000000>;
			opp-microvolt-L6 = <875000 875000 1000000>;
			opp-microvolt-L7 = <862500 862500 1000000>;
			opp-microvolt-L8 = <850000 850000 1000000>;
			clock-latency-ns = <40000>;
		};
	};

	gpu_bus: gpu-bus {
		compatible = "rockchip,rk3528-bus";
		rockchip,busfreq-policy = "clkfreq";
		clocks = <&scmi_clk SCMI_CLK_GPU>;
		clock-names = "bus";
		operating-points-v2 = <&gpu_bus_opp_table>;
		status = "disabled";
	};

	gpu_bus_opp_table: gpu-bus-opp-table {
		compatible = "operating-points-v2";

		nvmem-cells = <&log_leakage>;
		nvmem-cell-names = "leakage";

		rockchip,leakage-voltage-sel = <
			1   22   0
			23  254  1
		>;

		opp-700000000 {
			opp-hz = /bits/ 64 <700000000>;
			opp-microvolt = <850000 850000 1000000>;
		};
		opp-800000000 {
			opp-hz = /bits/ 64 <800000000>;
			opp-microvolt = <875000 875000 1000000>;
			opp-microvolt-L1 = <850000 850000 1000000>;
		};
	};

	rkvdec: rkvdec@ff740100 {
		compatible = "rockchip,rkv-decoder-rk3528", "rockchip,rkv-decoder-v2";
		reg = <0x0 0xff740100 0x0 0x400>, <0x0 0xff740000 0x0 0x100>;
		reg-names = "regs", "link";
		interrupts = <GIC_SPI 94 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "irq_dec";
		clocks = <&cru ACLK_RKVDEC>, <&cru HCLK_RKVDEC>, <&cru CLK_HEVC_CA_RKVDEC>;
		clock-names = "aclk_vcodec", "hclk_vcodec","clk_hevc_cabac";
		rockchip,normal-rates = <340000000>, <0>, <600000000>;
		assigned-clocks = <&cru ACLK_RKVDEC>, <&cru CLK_HEVC_CA_RKVDEC>;
		assigned-clock-rates = <340000000>, <600000000>;
		resets = <&cru SRST_ARESETN_RKVDEC>, <&cru SRST_HRESETN_RKVDEC>,
			 <&cru SRST_RESETN_HEVC_CA_RKVDEC>;
		reset-names = "video_a", "video_h", "video_hevc_cabac";
		iommus = <&rkvdec_mmu>;
		rockchip,srv = <&mpp_srv>;
		rockchip,taskqueue-node = <0>;
		rockchip,resetgroup-node = <0>;
		rockchip,task-capacity = <16>;
		rockchip,sram = <&rkvdec_sram>;
		/* rcb_iova: start and size */
		rockchip,rcb-iova = <0x10000000 65536>;
		rockchip,rcb-min-width = <512>;
		status = "disabled";
	};

	rkvdec_mmu: iommu@ff740800 {
		compatible = "rockchip,iommu-v2";
		reg = <0x0 0xff740800 0x0 0x40>, <0x0 0xff740900 0x0 0x40>;
		interrupts = <GIC_SPI 95 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "rkvdec_mmu";
		clocks = <&cru ACLK_RKVDEC>, <&cru HCLK_RKVDEC>, <&cru CLK_HEVC_CA_RKVDEC>;
		clock-names = "aclk", "iface", "clk_hevc_cabac";
		#iommu-cells = <0>;
		rockchip,shootdown-entire;
		status = "disabled";
	};

	rkvenc: rkvenc@ff780000 {
		compatible = "rockchip,rkv-encoder-rk3528", "rockchip,rkv-encoder-v2";
		reg = <0x0 0xff780000 0x0 0x6000>;
		interrupts = <GIC_SPI 97 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "irq_rkvenc";
		clocks = <&cru ACLK_RKVENC>, <&cru HCLK_RKVENC>, <&cru CLK_CORE_RKVENC>;
		clock-names = "aclk_vcodec", "hclk_vcodec", "clk_core";
		rockchip,normal-rates = <300000000>, <0>, <300000000>;
		resets = <&cru SRST_ARESETN_RKVENC>, <&cru SRST_HRESETN_RKVENC>,
			 <&cru SRST_RESETN_CORE_RKVENC>;
		reset-names = "video_a", "video_h", "video_core";
		assigned-clocks = <&cru ACLK_RKVENC>, <&cru CLK_CORE_RKVENC>;
		assigned-clock-rates = <300000000>, <300000000>;
		iommus = <&rkvenc_mmu>;
		rockchip,srv = <&mpp_srv>;
		rockchip,grf = <&grf>;
		rockchip,grf-mem-offset = <0x20010>;
		rockchip,grf-mem-values = <0x00000021>, <0xffff0021>;
		rockchip,taskqueue-node = <1>;
		rockchip,resetgroup-node = <1>;
		status = "disabled";
	};

	rkvenc_mmu: iommu@ff78f000 {
		compatible = "rockchip,iommu-v2";
		reg = <0x0 0xff78f000 0x0 0x40>;
		interrupts = <GIC_SPI 96 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "rkvenc_mmu";
		clocks = <&cru ACLK_RKVENC>, <&cru HCLK_RKVENC>;
		clock-names = "aclk", "iface";
		#iommu-cells = <0>;
		rockchip,shootdown-entire;
		status = "disabled";
	};

	vdpu: vdpu@ff7c0400 {
		compatible = "rockchip,vpu-decoder-v2";
		reg = <0x0 0xff7c0400 0x0 0x400>;
		interrupts = <GIC_SPI 98 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "irq_dec";
		clocks = <&cru ACLK_VPU>, <&cru HCLK_VPU>;
		clock-names = "aclk_vcodec", "hclk_vcodec";
		rockchip,normal-rates = <300000000>, <0>;
		assigned-clocks = <&cru ACLK_VPU>;
		assigned-clock-rates = <300000000>;
		resets = <&cru SRST_ARESETN_VPU>, <&cru SRST_HRESETN_VPU>;
		reset-names = "shared_video_a", "shared_video_h";
		iommus = <&vdpu_mmu>;
		rockchip,srv = <&mpp_srv>;
		rockchip,grf = <&grf>;
		rockchip,grf-mem-offset = <0x40034>;
		rockchip,grf-mem-values = <0x0f040000>, <0x0f040f04>;
		rockchip,taskqueue-node = <2>;
		rockchip,resetgroup-node = <2>;
		rockchip,disable-auto-freq;
		status = "disabled";
	};

	vdpu_mmu: iommu@ff7c0800 {
		compatible = "rockchip,iommu-v2";
		reg = <0x0 0xff7c0800 0x0 0x40>;
		interrupts = <GIC_SPI 99 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "vdpu_mmu";
		clock-names = "aclk", "iface";
		clocks = <&cru ACLK_VPU>, <&cru HCLK_VPU>;
		#iommu-cells = <0>;
		rockchip,shootdown-entire;
		status = "disabled";
	};

	avsd: avsd_plus@ff7c1000 {
		compatible = "rockchip,avs-plus-decoder";
		reg = <0x0 0xff7c1000 0x0 0x200>;
		interrupts = <GIC_SPI 98 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "irq_dec";
		clocks = <&cru ACLK_VPU>, <&cru HCLK_VPU>;
		clock-names = "aclk_vcodec", "hclk_vcodec";
		rockchip,normal-rates = <300000000>, <0>;
		assigned-clocks = <&cru ACLK_VPU>;
		assigned-clock-rates = <300000000>;
		resets = <&cru SRST_ARESETN_VPU>, <&cru SRST_HRESETN_VPU>;
		reset-names = "shared_video_a", "shared_video_h";
		iommus = <&vdpu_mmu>;
		rockchip,srv = <&mpp_srv>;
		rockchip,taskqueue-node = <2>;
		rockchip,resetgroup-node = <2>;
		rockchip,disable-auto-freq;
		status = "disabled";
	};

	vop: vop@ff840000 {
		compatible = "rockchip,rk3528-vop";
		reg = <0x0 0xff840000 0x0 0x3000>,
		      <0x0 0xff845000 0x0 0x1000>,
		      <0x0 0xff846400 0x0 0x800>;
		reg-names = "regs",
			    "gamma_lut",
			    "acm_regs";
		interrupts = <GIC_SPI 109 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru ACLK_VOP>,
			 <&cru HCLK_VOP>,
			 <&cru DCLK_VOP0>,
			 <&cru DCLK_VOP1>;
		clock-names = "aclk_vop",
			      "hclk_vop",
			      "dclk_vp0",
			      "dclk_vp1";
		assigned-clocks = <&cru DCLK_VOP0>;
		assigned-clock-parents = <&inno_hdmiphy_clk>;
		iommus = <&vop_mmu>;
		rockchip,grf = <&grf>;
		status = "disabled";

		vop_out: ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				#address-cells = <1>;
				#size-cells = <0>;
				reg = <0>;

				vp0_out_hdmi: endpoint@0 {
					reg = <0>;
					remote-endpoint = <&hdmi_in_vp0>;
				};
			};

			port@1 {
				#address-cells = <1>;
				#size-cells = <0>;
				reg = <1>;

				vp1_out_tve: endpoint@0 {
					reg = <0>;
					remote-endpoint = <&tve_in_vp1>;
				};
			};
		};
	};

	vop_mmu: iommu@ff847e00 {
		compatible = "rockchip,iommu-v2";
		reg = <0x0 0xff847e00 0x0 0x100>;
		interrupts = <GIC_SPI 109 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "vop_mmu";
		clocks = <&cru ACLK_VOP>, <&cru HCLK_VOP>;
		clock-names = "aclk", "iface";
		#iommu-cells = <0>;
		rockchip,disable-device-link-resume;
		rockchip,shootdown-entire;
		status = "disabled";
	};

	rga2: rga@ff850000 {
		compatible = "rockchip,rga2_core0";
		reg = <0x0 0xff850000 0x0 0x1000>;
		interrupts = <GIC_SPI 105 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "rga2_irq";
		clocks = <&cru ACLK_RGA2E>, <&cru HCLK_RGA2E>, <&cru CLK_CORE_RGA2E>;
		clock-names = "aclk_rga2", "hclk_rga2", "clk_rga2";
		iommus = <&rga2_mmu>;
		rockchip,grf = <&grf>;
		rockchip,grf-offset = <0x600e0>;
		rockchip,grf-values = <0x0ff10000>, <0x0ff10ff1>;
		status = "disabled";
	};

	rga2_mmu: iommu@ff850f00 {
		compatible = "rockchip,iommu-v2";
		reg = <0x0 0xff850f00 0x0 0x100>;
		interrupts = <GIC_SPI 105 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "rga2_mmu";
		clocks = <&cru ACLK_RGA2E>, <&cru HCLK_RGA2E>;
		clock-names = "aclk", "iface";
		#iommu-cells = <0>;
		status = "disabled";
	};

	iep: iep@ff860000 {
		compatible = "rockchip,iep-v2";
		reg = <0x0 0xff860000 0x0 0x500>;
		interrupts = <GIC_SPI 106 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru ACLK_VDPP>, <&cru HCLK_VDPP>, <&cru CLK_CORE_VDPP>;
		clock-names = "aclk", "hclk", "sclk";
		rockchip,normal-rates = <340000000>, <0>, <340000000>;
		assigned-clocks = <&cru ACLK_VDPP>, <&cru CLK_CORE_VDPP>;
		assigned-clock-rates = <340000000>, <340000000>;
		resets = <&cru SRST_ARESETN_VDPP>, <&cru SRST_HRESETN_VDPP>,
			 <&cru SRST_RESETN_CORE_VDPP>;
		reset-names = "shared_rst_a", "shared_rst_h", "shared_rst_s";
		rockchip,srv = <&mpp_srv>;
		rockchip,taskqueue-node = <3>;
		rockchip,resetgroup-node = <3>;
		iommus = <&iep_mmu>;
		status = "disabled";
	};

	iep_mmu: iommu@ff860800 {
		compatible = "rockchip,iommu-v2";
		reg = <0x0 0xff860800 0x0 0x100>;
		interrupts = <GIC_SPI 106 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "iep_mmu";
		clocks = <&cru ACLK_VDPP>, <&cru HCLK_VDPP>;
		clock-names = "aclk", "iface";
		#iommu-cells = <0>;
		rockchip,shootdown-entire;
		status = "disabled";
	};

	vdpp: vdpp@ff861000 {
		compatible = "rockchip,vdpp-v1";
		reg = <0x0 0xff861000 0x0 0x100>,  <0x0 0xff862000 0x0 0x900>;
		reg-names = "vdpp_regs", "zme_regs";
		interrupts = <GIC_SPI 106 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru ACLK_VDPP>, <&cru HCLK_VDPP>, <&cru CLK_CORE_VDPP>;
		clock-names = "aclk", "hclk", "sclk";
		rockchip,normal-rates = <340000000>, <0>, <340000000>;
		assigned-clocks = <&cru ACLK_VDPP>, <&cru CLK_CORE_VDPP>;
		assigned-clock-rates = <340000000>, <340000000>;
		resets = <&cru SRST_ARESETN_VDPP>, <&cru SRST_HRESETN_VDPP>,
			 <&cru SRST_RESETN_CORE_VDPP>;
		reset-names = "shared_rst_a", "shared_rst_h", "shared_rst_s";
		rockchip,srv = <&mpp_srv>;
		rockchip,grf = <&grf>;
		rockchip,grf-mem-offset = <0x600e0>;
		rockchip,grf-mem-values = <0xf0040000>, <0xf004f004>;
		rockchip,taskqueue-node = <3>;
		rockchip,resetgroup-node = <3>;
		rockchip,disable-auto-freq;
		iommus = <&iep_mmu>;
		status = "disabled";
	};

	jpegd: jpegd@ff870000 {
		compatible = "rockchip,rkv-jpeg-decoder-v1";
		reg = <0x0 0xff870000 0x0 0x400>;
		interrupts = <GIC_SPI 107 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru ACLK_JPEG_DECODER>, <&cru HCLK_JPEG_DECODER>;
		clock-names = "aclk_vcodec", "hclk_vcodec";
		rockchip,normal-rates = <340000000>, <0>;
		assigned-clocks = <&cru ACLK_JPEG_DECODER>;
		assigned-clock-rates = <340000000>;
		rockchip,disable-auto-freq;
		resets = <&cru SRST_ARESETN_JPEG_DECODER>, <&cru SRST_HRESETN_JPEG_DECODER>;
		reset-names = "video_a", "video_h";
		iommus = <&jpegd_mmu>;
		rockchip,srv = <&mpp_srv>;
		rockchip,taskqueue-node = <4>;
		rockchip,resetgroup-node = <4>;
		status = "disabled";
	};

	jpegd_mmu: iommu@ff870480 {
		compatible = "rockchip,iommu-v2";
		reg = <0x0 0xff870480 0x0 0x40>;
		interrupts = <GIC_SPI 108 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "jpegd_mmu";
		clock-names = "aclk", "iface";
		clocks = <&cru ACLK_JPEG_DECODER>, <&cru HCLK_JPEG_DECODER>;
		#iommu-cells = <0>;
		rockchip,shootdown-entire;
		status = "disabled";
	};

	tve: tve@ff880000 {
		compatible = "rockchip,rk3528-tve";
		reg = <0x0 0xff880000 0x0 0x4000>,
		      <0x0 0xffde0000 0x0 0x300>;
		interrupts = <GIC_SPI 112 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru HCLK_CVBS>,
			 <&cru PCLK_VCDCPHY>,
			 <&cru DCLK_CVBS>,
			 <&cru DCLK_4X_CVBS>;
		clock-names = "hclk",
			      "pclk_vdac",
			      "dclk",
			      "dclk_4x";
		rockchip,lumafilter0 = <0x0ff80006>;
		rockchip,lumafilter1 = <0x00090010>;
		rockchip,lumafilter2 = <0x0ffb0fd8>;
		rockchip,lumafilter3 = <0x00080057>;
		rockchip,lumafilter4 = <0x0fef0f64>;
		rockchip,lumafilter5 = <0x0016010a>;
		rockchip,lumafilter6 = <0x0f830df7>;
		rockchip,lumafilter7 = <0x08de055f>;
		rockchip,tve-upsample = <DCLK_UPSAMPLEx4>;
		rockchip,grf = <&grf>;
		nvmem-cells = <&vdac_out_current>, <&test_version>;
		nvmem-cell-names = "out-current", "version";
		status = "disabled";

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				#address-cells = <1>;
				#size-cells = <0>;

				tve_in_vp1: endpoint@0 {
					reg = <0>;
					remote-endpoint = <&vp1_out_tve>;
					status = "disabled";
				};
			};
		};
	};

	hdcp2: hdcp2@ff8c0000 {
		compatible = "rockchip,rk3528-hdmi-hdcp2";
		reg = <0x0 0xff8c0000 0x0 0x2000>;
		interrupts = <GIC_SPI 104 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru ACLK_HDCP>, <&cru PCLK_HDCP>,
			 <&cru HCLK_HDCP>;
		clock-names ="aclk_hdcp2", "pclk_hdcp2", "hdcp2_clk_hdmi";
		status = "disabled";
	};

	hdmi: hdmi@ff8d0000 {
		compatible = "rockchip,rk3528-dw-hdmi";
		reg = <0x0 0xff8d0000 0x0 0x20000>,
		      <0x0 0xff610000 0x0 0x200>;
		interrupts = <GIC_SPI 102 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 103 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "hdmi", "hdmi_wakeup";
		clocks = <&cru PCLK_HDMI>,
			 <&cru CLK_SFR_HDMI>,
			 <&cru CLK_CEC_HDMI>,
			 <&inno_hdmiphy_clk>;
		clock-names = "iahb", "isfr", "cec", "dclk_vp0";
		ddc-i2c-scl-high-time-ns = <9625>;
		ddc-i2c-scl-low-time-ns = <10000>;
		reg-io-width = <4>;
		rockchip,grf = <&grf>;
		pinctrl-names = "default";
		pinctrl-0 = <&hdmi_pins>;
		phys = <&hdmiphy>;
		phy-names = "hdmi";
		#sound-dai-cells = <0>;
		hpd-gpios = <&gpio0 RK_PA2 GPIO_ACTIVE_HIGH>;
		status = "disabled";

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				#address-cells = <1>;
				#size-cells = <0>;

				hdmi_in_vp0: endpoint@0 {
					reg = <0>;
					remote-endpoint = <&vp0_out_hdmi>;
					status = "disabled";
				};
			};
		};
	};

	dfi: dfi@ff930000 {
		reg = <0x0 0xff930000 0x0 0x400>;
		compatible = "rockchip,rk3528-dfi";
		rockchip,grf = <&grf>;
		status = "disabled";
	};

	spi0: spi@ff9c0000 {
		compatible = "rockchip,rk3066-spi";
		reg = <0x0 0xff9c0000 0x0 0x1000>;
		interrupts = <GIC_SPI 131 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&cru CLK_SPI0>, <&cru PCLK_SPI0>, <&cru SCLK_IN_SPI0>;
		clock-names = "spiclk", "apb_pclk", "sclk_in";
		dmas = <&dmac 25>, <&dmac 24>;
		dma-names = "tx", "rx";
		pinctrl-names = "default";
		pinctrl-0 = <&spi0_csn0 &spi0_csn1 &spi0_pins>;
		status = "disabled";
	};

	spi1: spi@ff9d0000 {
		compatible = "rockchip,rk3066-spi";
		reg = <0x0 0xff9d0000 0x0 0x1000>;
		interrupts = <GIC_SPI 132 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&cru CLK_SPI1>, <&cru PCLK_SPI1>, <&cru SCLK_IN_SPI1>;
		clock-names = "spiclk", "apb_pclk", "sclk_in";
		dmas = <&dmac 31>, <&dmac 30>;
		dma-names = "tx", "rx";
		pinctrl-names = "default";
		pinctrl-0 = <&spi1_csn0 &spi1_csn1 &spi1_pins>;
		status = "disabled";
	};

	uart0: serial@ff9f0000 {
		compatible = "rockchip,rk3528-uart", "snps,dw-apb-uart";
		reg = <0x0 0xff9f0000 0x0 0x100>;
		interrupts = <GIC_SPI 40 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_UART0>, <&cru PCLK_UART0>;
		clock-names = "baudclk", "apb_pclk";
		reg-shift = <2>;
		reg-io-width = <4>;
		dmas = <&dmac 9>, <&dmac 8>;
		status = "disabled";
	};

	uart1: serial@ff9f8000 {
		compatible = "rockchip,rk3528-uart", "snps,dw-apb-uart";
		reg = <0x0 0xff9f8000 0x0 0x100>;
		interrupts = <GIC_SPI 41 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_UART1>, <&cru PCLK_UART1>;
		clock-names = "baudclk", "apb_pclk";
		reg-shift = <2>;
		reg-io-width = <4>;
		dmas = <&dmac 11>, <&dmac 10>;
		status = "disabled";
	};

	uart2: serial@ffa00000 {
		compatible = "rockchip,rk3528-uart", "snps,dw-apb-uart";
		reg = <0x0 0xffa00000 0x0 0x100>;
		interrupts = <GIC_SPI 42 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_UART2>, <&cru PCLK_UART2>;
		clock-names = "baudclk", "apb_pclk";
		reg-shift = <2>;
		reg-io-width = <4>;
		dmas = <&dmac 13>, <&dmac 12>;
		status = "disabled";
	};

	uart3: serial@ffa08000 {
		compatible = "rockchip,rk3528-uart", "snps,dw-apb-uart";
		reg = <0x0 0xffa08000 0x0 0x100>;
		interrupts = <GIC_SPI 43 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_UART3>, <&cru PCLK_UART3>;
		clock-names = "baudclk", "apb_pclk";
		reg-shift = <2>;
		reg-io-width = <4>;
		dmas = <&dmac 15>, <&dmac 14>;
		status = "disabled";
	};

	uart4: serial@ffa10000 {
		compatible = "rockchip,rk3528-uart", "snps,dw-apb-uart";
		reg = <0x0 0xffa10000 0x0 0x100>;
		interrupts = <GIC_SPI 44 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_UART4>, <&cru PCLK_UART4>;
		clock-names = "baudclk", "apb_pclk";
		reg-shift = <2>;
		reg-io-width = <4>;
		dmas = <&dmac 17>, <&dmac 16>;
		status = "disabled";
	};

	uart5: serial@ffa18000 {
		compatible = "rockchip,rk3528-uart", "snps,dw-apb-uart";
		reg = <0x0 0xffa18000 0x0 0x100>;
		interrupts = <GIC_SPI 45 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_UART5>, <&cru PCLK_UART5>;
		clock-names = "baudclk", "apb_pclk";
		reg-shift = <2>;
		reg-io-width = <4>;
		dmas = <&dmac 19>, <&dmac 18>;
		status = "disabled";
	};

	uart6: serial@ffa20000 {
		compatible = "rockchip,rk3528-uart", "snps,dw-apb-uart";
		reg = <0x0 0xffa20000 0x0 0x100>;
		interrupts = <GIC_SPI 46 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_UART6>, <&cru PCLK_UART6>;
		clock-names = "baudclk", "apb_pclk";
		reg-shift = <2>;
		reg-io-width = <4>;
		dmas = <&dmac 21>, <&dmac 20>;
		status = "disabled";
	};

	uart7: serial@ffa28000 {
		compatible = "rockchip,rk3528-uart", "snps,dw-apb-uart";
		reg = <0x0 0xffa28000 0x0 0x100>;
		interrupts = <GIC_SPI 47 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_UART7>, <&cru PCLK_UART7>;
		clock-names = "baudclk", "apb_pclk";
		reg-shift = <2>;
		reg-io-width = <4>;
		dmas = <&dmac 23>, <&dmac 22>;
		status = "disabled";
	};

	i2c0: i2c@ffa50000 {
		compatible = "rockchip,rk3528-i2c", "rockchip,rk3399-i2c";
		reg = <0x0 0xffa50000 0x0 0x1000>;
		clocks = <&cru CLK_I2C0>, <&cru PCLK_I2C0>;
		clock-names = "i2c", "pclk";
		interrupts = <GIC_SPI 61 IRQ_TYPE_LEVEL_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2c0m0_xfer>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	i2c1: i2c@ffa58000 {
		compatible = "rockchip,rk3528-i2c", "rockchip,rk3399-i2c";
		reg = <0x0 0xffa58000 0x0 0x1000>;
		clocks = <&cru CLK_I2C1>, <&cru PCLK_I2C1>;
		clock-names = "i2c", "pclk";
		interrupts = <GIC_SPI 62 IRQ_TYPE_LEVEL_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2c1m0_xfer>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	i2c2: i2c@ffa60000 {
		compatible = "rockchip,rk3528-i2c", "rockchip,rk3399-i2c";
		reg = <0x0 0xffa60000 0x0 0x1000>;
		clocks = <&cru CLK_I2C2>, <&cru PCLK_I2C2>;
		clock-names = "i2c", "pclk";
		interrupts = <GIC_SPI 63 IRQ_TYPE_LEVEL_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2c2m0_xfer>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	i2c3: i2c@ffa68000 {
		compatible = "rockchip,rk3528-i2c", "rockchip,rk3399-i2c";
		reg = <0x0 0xffa68000 0x0 0x1000>;
		clocks = <&cru CLK_I2C3>, <&cru PCLK_I2C3>;
		clock-names = "i2c", "pclk";
		interrupts = <GIC_SPI 64 IRQ_TYPE_LEVEL_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2c3m0_xfer>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	i2c4: i2c@ffa70000 {
		compatible = "rockchip,rk3528-i2c", "rockchip,rk3399-i2c";
		reg = <0x0 0xffa70000 0x0 0x1000>;
		clocks = <&cru CLK_I2C4>, <&cru PCLK_I2C4>;
		clock-names = "i2c", "pclk";
		interrupts = <GIC_SPI 65 IRQ_TYPE_LEVEL_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2c4_xfer>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	i2c5: i2c@ffa78000 {
		compatible = "rockchip,rk3528-i2c", "rockchip,rk3399-i2c";
		reg = <0x0 0xffa78000 0x0 0x1000>;
		clocks = <&cru CLK_I2C5>, <&cru PCLK_I2C5>;
		clock-names = "i2c", "pclk";
		interrupts = <GIC_SPI 66 IRQ_TYPE_LEVEL_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2c5m0_xfer>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	i2c6: i2c@ffa80000 {
		compatible = "rockchip,rk3528-i2c", "rockchip,rk3399-i2c";
		reg = <0x0 0xffa80000 0x0 0x1000>;
		clocks = <&cru CLK_I2C6>, <&cru PCLK_I2C6>;
		clock-names = "i2c", "pclk";
		interrupts = <GIC_SPI 67 IRQ_TYPE_LEVEL_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2c6m0_xfer>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	i2c7: i2c@ffa88000 {
		compatible = "rockchip,rk3528-i2c", "rockchip,rk3399-i2c";
		reg = <0x0 0xffa88000 0x0 0x1000>;
		clocks = <&cru CLK_I2C7>, <&cru PCLK_I2C7>;
		clock-names = "i2c", "pclk";
		interrupts = <GIC_SPI 68 IRQ_TYPE_LEVEL_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2c7_xfer>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	pwm0: pwm@ffa90000 {
		compatible = "rockchip,rk3528-pwm", "rockchip,rk3328-pwm";
		reg = <0x0 0xffa90000 0x0 0x10>;
		interrupts = <GIC_SPI 53 IRQ_TYPE_LEVEL_HIGH>;
		#pwm-cells = <3>;
		pinctrl-names = "active";
		pinctrl-0 = <&pwm0m0_pins>;
		clocks = <&cru CLK_PWM0>, <&cru PCLK_PWM0>;
		clock-names = "pwm", "pclk";
		status = "disabled";
	};

	pwm1: pwm@ffa90010 {
		compatible = "rockchip,rk3528-pwm", "rockchip,rk3328-pwm";
		reg = <0x0 0xffa90010 0x0 0x10>;
		interrupts = <GIC_SPI 53 IRQ_TYPE_LEVEL_HIGH>;
		#pwm-cells = <3>;
		pinctrl-names = "active";
		pinctrl-0 = <&pwm1m0_pins>;
		clocks = <&cru CLK_PWM0>, <&cru PCLK_PWM0>;
		clock-names = "pwm", "pclk";
		status = "disabled";
	};

	pwm2: pwm@ffa90020 {
		compatible = "rockchip,rk3528-pwm", "rockchip,rk3328-pwm";
		reg = <0x0 0xffa90020 0x0 0x10>;
		interrupts = <GIC_SPI 53 IRQ_TYPE_LEVEL_HIGH>;
		#pwm-cells = <3>;
		pinctrl-names = "active";
		pinctrl-0 = <&pwm2m0_pins>;
		clocks = <&cru CLK_PWM0>, <&cru PCLK_PWM0>;
		clock-names = "pwm", "pclk";
		status = "disabled";
	};

	pwm3: pwm@ffa90030 {
		compatible = "rockchip,rk3528-pwm", "rockchip,rk3328-pwm";
		reg = <0x0 0xffa90030 0x0 0x10>;
		interrupts = <GIC_SPI 53 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 54 IRQ_TYPE_LEVEL_HIGH>;
		#pwm-cells = <3>;
		pinctrl-names = "active";
		pinctrl-0 = <&pwm3m0_pins>;
		clocks = <&cru CLK_PWM0>, <&cru PCLK_PWM0>;
		clock-names = "pwm", "pclk";
		status = "disabled";
	};

	pwm4: pwm@ffa98000 {
		compatible = "rockchip,rk3528-pwm", "rockchip,rk3328-pwm";
		reg = <0x0 0xffa98000 0x0 0x10>;
		interrupts = <GIC_SPI 55 IRQ_TYPE_LEVEL_HIGH>;
		#pwm-cells = <3>;
		pinctrl-names = "active";
		pinctrl-0 = <&pwm4m0_pins>;
		clocks = <&cru CLK_PWM1>, <&cru PCLK_PWM1>;
		clock-names = "pwm", "pclk";
		status = "disabled";
	};

	pwm5: pwm@ffa98010 {
		compatible = "rockchip,rk3528-pwm", "rockchip,rk3328-pwm";
		reg = <0x0 0xffa98010 0x0 0x10>;
		interrupts = <GIC_SPI 55 IRQ_TYPE_LEVEL_HIGH>;
		#pwm-cells = <3>;
		pinctrl-names = "active";
		pinctrl-0 = <&pwm5m0_pins>;
		clocks = <&cru CLK_PWM1>, <&cru PCLK_PWM1>;
		clock-names = "pwm", "pclk";
		status = "disabled";
	};

	pwm6: pwm@ffa98020 {
		compatible = "rockchip,rk3528-pwm", "rockchip,rk3328-pwm";
		reg = <0x0 0xffa98020 0x0 0x10>;
		interrupts = <GIC_SPI 55 IRQ_TYPE_LEVEL_HIGH>;
		#pwm-cells = <3>;
		pinctrl-names = "active";
		pinctrl-0 = <&pwm6m0_pins>;
		clocks = <&cru CLK_PWM1>, <&cru PCLK_PWM1>;
		clock-names = "pwm", "pclk";
		status = "disabled";
	};

	pwm7: pwm@ffa98030 {
		compatible = "rockchip,rk3528-pwm", "rockchip,rk3328-pwm";
		reg = <0x0 0xffa98030 0x0 0x10>;
		interrupts = <GIC_SPI 55 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 56 IRQ_TYPE_LEVEL_HIGH>;
		#pwm-cells = <3>;
		pinctrl-names = "active";
		pinctrl-0 = <&pwm7m0_pins>;
		clocks = <&cru CLK_PWM1>, <&cru PCLK_PWM1>;
		clock-names = "pwm", "pclk";
		status = "disabled";
	};

	rktimer: timer@ffab0000 {
		compatible = "rockchip,rk3528-timer", "rockchip,rk3288-timer";
		reg = <0x0 0xffab0000 0x0 0x20>;
		interrupts = <GIC_SPI 31 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru PCLK_TIMER>, <&cru CLK_TIMER0>;
		clock-names = "pclk", "timer";
	};

	wdt: watchdog@ffac0000 {
		compatible = "snps,dw-wdt";
		reg = <0x0 0xffac0000 0x0 0x100>;
		clocks = <&cru TCLK_WDT_NS>, <&cru PCLK_WDT_NS>;
		clock-names = "tclk", "pclk";
		interrupts = <GIC_SPI 28 IRQ_TYPE_LEVEL_HIGH>;
		status = "disabled";
	};

	tsadc: tsadc@ffad0000 {
		compatible = "rockchip,rk3528-tsadc";
		reg = <0x0 0xffad0000 0x0 0x400>;
		rockchip,grf = <&grf>;
		interrupts = <GIC_SPI 139 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru CLK_TSADC>, <&cru CLK_TSADC_TSEN>, <&cru PCLK_TSADC>;
		clock-names = "tsadc", "tsadc_tsen", "apb_pclk";
		assigned-clocks = <&cru CLK_TSADC>, <&cru CLK_TSADC_TSEN>;
		assigned-clock-rates = <1200000>, <12000000>;
		resets = <&cru SRST_RESETN_TSADC>, <&cru SRST_PRESETN_TSADC>;
		reset-names = "tsadc", "tsadc-apb";
		#thermal-sensor-cells = <1>;
		rockchip,hw-tshut-temp = <120000>;
		rockchip,hw-tshut-mode = <0>; /* tshut mode 0:CRU 1:GPIO */
		rockchip,hw-tshut-polarity = <0>; /* tshut polarity 0:LOW 1:HIGH */
		nvmem-cells = <&cpu_tsadc_trim_l>, <&cpu_tsadc_trim_h>;
		nvmem-cell-names = "trim_l", "trim_h";
		status = "disabled";
	};

	saradc: saradc@ffae0000 {
		compatible = "rockchip,rk3528-saradc";
		reg = <0x0 0xffae0000 0x0 0x10000>;
		interrupts = <GIC_SPI 140 IRQ_TYPE_LEVEL_HIGH>;
		#io-channel-cells = <1>;
		clocks = <&cru CLK_SARADC>, <&cru PCLK_SARADC>;
		clock-names = "saradc", "apb_pclk";
		resets = <&cru SRST_PRESETN_SARADC>;
		reset-names = "saradc-apb";
		status = "disabled";
	};

	sai3: sai@ffb70000 {
		compatible = "rockchip,rk3528-sai", "rockchip,sai-v1";
		reg = <0x0 0xffb70000 0x0 0x1000>;
		interrupts = <GIC_SPI 128 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru MCLK_SAI_I2S3>, <&cru HCLK_SAI_I2S3>;
		clock-names = "mclk", "hclk";
		dmas = <&dmac 5>;
		dma-names = "tx";
		resets = <&cru SRST_MRESETN_SAI_I2S3>, <&cru SRST_HRESETN_SAI_I2S3>;
		reset-names = "m", "h";
		#sound-dai-cells = <0>;
		status = "disabled";
	};

	sai0: sai@ffb80000 {
		compatible = "rockchip,rk3528-sai", "rockchip,sai-v1";
		reg = <0x0 0xffb80000 0x0 0x1000>;
		interrupts = <GIC_SPI 125 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru MCLK_SAI_I2S0>, <&cru HCLK_SAI_I2S0>;
		clock-names = "mclk", "hclk";
		dmas = <&dmac 1>, <&dmac 0>;
		dma-names = "tx", "rx";
		resets = <&cru SRST_MRESETN_SAI_I2S0>, <&cru SRST_HRESETN_SAI_I2S0>;
		reset-names = "m", "h";
		pinctrl-names = "default";
		pinctrl-0 = <&i2s0m0_lrck
			     &i2s0m0_sclk
			     &i2s0m0_sdi
			     &i2s0m0_sdo>;
		#sound-dai-cells = <0>;
		status = "disabled";
	};

	sai2: sai@ffb90000 {
		compatible = "rockchip,rk3528-sai", "rockchip,sai-v1";
		reg = <0x0 0xffb90000 0x0 0x1000>;
		interrupts = <GIC_SPI 127 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru MCLK_SAI_I2S2>, <&cru HCLK_SAI_I2S2>;
		clock-names = "mclk", "hclk";
		dmas = <&dmac 4>;
		dma-names = "tx";
		resets = <&cru SRST_MRESETN_SAI_I2S2>, <&cru SRST_HRESETN_SAI_I2S2>;
		reset-names = "m", "h";
		#sound-dai-cells = <0>;
		status = "disabled";
	};

	sai1: sai@ffba0000 {
		compatible = "rockchip,rk3528-sai", "rockchip,sai-v1";
		reg = <0x0 0xffba0000 0x0 0x1000>;
		interrupts = <GIC_SPI 126 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru MCLK_SAI_I2S1>, <&cru HCLK_SAI_I2S1>;
		clock-names = "mclk", "hclk";
		dmas = <&dmac 3>, <&dmac 2>;
		dma-names = "tx", "rx";
		resets = <&cru SRST_MRESETN_SAI_I2S1>, <&cru SRST_HRESETN_SAI_I2S1>;
		reset-names = "m", "h";
		pinctrl-names = "default";
		pinctrl-0 = <&i2s1_sclk
			     &i2s1_lrck
			     &i2s1_sdi0
			     &i2s1_sdi1
			     &i2s1_sdi2
			     &i2s1_sdi3
			     &i2s1_sdo0
			     &i2s1_sdo1
			     &i2s1_sdo2
			     &i2s1_sdo3>;
		#sound-dai-cells = <0>;
		status = "disabled";
	};

	pdm: pdm@ffbb0000 {
		compatible = "rockchip,rk3528-pdm", "rockchip,rk3568-pdm";
		reg = <0x0 0xffbb0000 0x0 0x1000>;
		clocks = <&cru MCLK_PDM>, <&cru HCLK_PDM>;
		clock-names = "pdm_clk", "pdm_hclk";
		dmas = <&dmac 6>;
		dma-names = "rx";
		pinctrl-names = "default";
		pinctrl-0 = <&pdm_clk0
			     &pdm_clk1
			     &pdm_sdi0
			     &pdm_sdi1
			     &pdm_sdi2
			     &pdm_sdi3>;
		#sound-dai-cells = <0>;
		status = "disabled";
	};

	spdif_8ch: spdif@ffbc0000 {
		compatible = "rockchip,rk3528-spdif", "rockchip,rk3568-spdif";
		reg = <0x0 0xffbc0000 0x0 0x1000>;
		interrupts = <GIC_SPI 130 IRQ_TYPE_LEVEL_HIGH>;
		dmas = <&dmac 7>;
		dma-names = "tx";
		clock-names = "mclk", "hclk";
		clocks = <&cru MCLK_SPDIF>, <&cru HCLK_SPDIF>;
		#sound-dai-cells = <0>;
		pinctrl-names = "default";
		pinctrl-0 = <&spdifm0_pins>;
		status = "disabled";
	};

	gmac0: ethernet@ffbd0000 {
		compatible = "rockchip,rk3528-gmac", "snps,dwmac-4.20a";
		reg = <0x0 0xffbd0000 0x0 0x10000>;
		interrupts = <GIC_SPI 113 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 116 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "macirq", "eth_wake_irq";
		rockchip,grf = <&grf>;
		clocks = <&cru CLK_GMAC0_SRC>, <&cru CLK_GMAC0_RMII_50M>,
			 <&cru CLK_GMAC0_RX>, <&cru CLK_GMAC0_TX>,
			 <&cru PCLK_MAC_VO>, <&cru ACLK_MAC_VO>;
		clock-names = "stmmaceth", "clk_mac_ref",
			      "mac_clk_rx", "mac_clk_tx",
			      "pclk_mac", "aclk_mac";
		resets = <&cru SRST_ARESETN_MAC_VO>;
		reset-names = "stmmaceth";

		snps,mixed-burst;
		snps,tso;

		snps,axi-config = <&gmac0_stmmac_axi_setup>;
		snps,mtl-rx-config = <&gmac0_mtl_rx_setup>;
		snps,mtl-tx-config = <&gmac0_mtl_tx_setup>;

		phy-mode = "rmii";
		clock_in_out = "input";
		phy-handle = <&rmii0_phy>;

		nvmem-cells = <&macphy_bgs>;
		nvmem-cell-names = "bgs";
		status = "disabled";

		mdio0: mdio {
			compatible = "snps,dwmac-mdio";
			#address-cells = <0x1>;
			#size-cells = <0x0>;
			rmii0_phy: ethernet-phy@2 {
				compatible = "ethernet-phy-id0044.1400", "ethernet-phy-ieee802.3-c22";
				reg = <2>;
				clocks = <&cru CLK_MACPHY>;
				resets = <&cru SRST_RESETN_MACPHY>;
				phy-is-integrated;
				pinctrl-names = "default";
				pinctrl-0 = <&fephym0_led_link &fephym0_led_spd>;
				nvmem-cells = <&macphy_txlevel>;
				nvmem-cell-names = "txlevel";
			};
		};

		gmac0_stmmac_axi_setup: stmmac-axi-config {
			snps,wr_osr_lmt = <4>;
			snps,rd_osr_lmt = <8>;
			snps,blen = <0 0 0 0 16 8 4>;
		};

		gmac0_mtl_rx_setup: rx-queues-config {
			snps,rx-queues-to-use = <1>;
			queue0 {};
		};

		gmac0_mtl_tx_setup: tx-queues-config {
			snps,tx-queues-to-use = <1>;
			queue0 {};
		};
	};

	gmac1: ethernet@ffbe0000 {
		compatible = "rockchip,rk3528-gmac", "snps,dwmac-4.20a";
		reg = <0x0 0xffbe0000 0x0 0x10000>;
		interrupts = <GIC_SPI 121 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 124 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "macirq", "eth_wake_irq";
		rockchip,grf = <&grf>;
		clocks = <&cru CLK_GMAC1_SRC_VPU>, <&cru CLK_GMAC1_RMII_VPU>,
			 <&cru PCLK_MAC_VPU>, <&cru ACLK_MAC_VPU>;
		clock-names = "stmmaceth", "clk_mac_ref",
			      "pclk_mac", "aclk_mac";
		resets = <&cru SRST_ARESETN_MAC>;
		reset-names = "stmmaceth";

		snps,mixed-burst;
		snps,tso;

		snps,axi-config = <&gmac1_stmmac_axi_setup>;
		snps,mtl-rx-config = <&gmac1_mtl_rx_setup>;
		snps,mtl-tx-config = <&gmac1_mtl_tx_setup>;

		status = "disabled";

		mdio1: mdio {
			compatible = "snps,dwmac-mdio";
			#address-cells = <0x1>;
			#size-cells = <0x0>;
		};

		gmac1_stmmac_axi_setup: stmmac-axi-config {
			snps,wr_osr_lmt = <4>;
			snps,rd_osr_lmt = <8>;
			snps,blen = <0 0 0 0 16 8 4>;
		};

		gmac1_mtl_rx_setup: rx-queues-config {
			snps,rx-queues-to-use = <1>;
			queue0 {};
		};

		gmac1_mtl_tx_setup: tx-queues-config {
			snps,tx-queues-to-use = <1>;
			queue0 {};
		};
	};

	sdhci: mmc@ffbf0000 {
		compatible = "rockchip,rk3528-dwcmshc";
		reg = <0x0 0xffbf0000 0x0 0x10000>;
		interrupts = <GIC_SPI 136 IRQ_TYPE_LEVEL_HIGH>;
		assigned-clocks = <&cru BCLK_EMMC>, <&cru TCLK_EMMC>, <&cru CCLK_SRC_EMMC>;
		assigned-clock-rates = <200000000>, <24000000>, <200000000>;
		clocks = <&cru CCLK_SRC_EMMC>, <&cru HCLK_EMMC>,
			 <&cru ACLK_EMMC>, <&cru BCLK_EMMC>,
			 <&cru TCLK_EMMC>;
		clock-names = "core", "bus", "axi", "block", "timer";
		resets = <&cru SRST_CRESETN_EMMC>, <&cru SRST_HRESETN_EMMC>,
			 <&cru SRST_ARESETN_EMMC>, <&cru SRST_BRESETN_EMMC>,
			 <&cru SRST_TRESETN_EMMC>;
		reset-names = "core", "bus", "axi", "block", "timer";
		max-frequency = <200000000>;
		status = "disabled";
	};

	sfc: spi@ffc00000 {
		compatible = "rockchip,sfc";
		reg = <0x0 0xffc00000 0x0 0x4000>;
		interrupts = <GIC_SPI 135 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_SFC>, <&cru HCLK_SFC>;
		clock-names = "clk_sfc", "hclk_sfc";
		assigned-clocks = <&cru SCLK_SFC>;
		assigned-clock-rates = <100000000>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	sdio0: mmc@ffc10000 {
		compatible = "rockchip,rk3528-dw-mshc",
			     "rockchip,rk3288-dw-mshc";
		reg = <0x0 0xffc10000 0x0 0x4000>;
		interrupts = <GIC_SPI 137 IRQ_TYPE_LEVEL_HIGH>;
		max-frequency = <150000000>;
		clocks = <&cru HCLK_SDIO0>, <&cru CCLK_SRC_SDIO0>,
			 <&grf_cru SCLK_SDIO0_DRV>, <&grf_cru SCLK_SDIO0_SAMPLE>;
		clock-names = "biu", "ciu", "ciu-drive", "ciu-sample";
		fifo-depth = <0x100>;
		resets = <&cru SRST_HRESETN_SDIO0>;
		reset-names = "reset";
		rockchip,use-v2-tuning;
		status = "disabled";
	};

	sdio1: mmc@ffc20000 {
		compatible = "rockchip,rk3528-dw-mshc",
			     "rockchip,rk3288-dw-mshc";
		reg = <0x0 0xffc20000 0x0 0x4000>;
		interrupts = <GIC_SPI 138 IRQ_TYPE_LEVEL_HIGH>;
		max-frequency = <150000000>;
		clocks = <&cru HCLK_SDIO1>, <&cru CCLK_SRC_SDIO1>,
			 <&grf_cru SCLK_SDIO1_DRV>, <&grf_cru SCLK_SDIO1_SAMPLE>;
		clock-names = "biu", "ciu", "ciu-drive", "ciu-sample";
		fifo-depth = <0x100>;
		resets = <&cru SRST_HRESETN_SDIO1>;
		reset-names = "reset";
		rockchip,use-v2-tuning;
		status = "disabled";
	};

	sdmmc: mmc@ffc30000 {
		compatible = "rockchip,rk3528-dw-mshc",
			     "rockchip,rk3288-dw-mshc";
		reg = <0x0 0xffc30000 0x0 0x4000>;
		interrupts = <GIC_SPI 133 IRQ_TYPE_LEVEL_HIGH>;
		max-frequency = <150000000>;
		clocks = <&cru HCLK_SDMMC0>, <&cru CCLK_SRC_SDMMC0>,
			 <&grf_cru SCLK_SDMMC_DRV>, <&grf_cru SCLK_SDMMC_SAMPLE>;
		clock-names = "biu", "ciu", "ciu-drive", "ciu-sample";
		fifo-depth = <0x100>;
		resets = <&cru SRST_HRESETN_SDMMC0>;
		reset-names = "reset";
		rockchip,use-v2-tuning;
		status = "disabled";
	};

	crypto: crypto@ffc40000 {
		compatible = "rockchip,crypto-v4";
		reg = <0x0 0xffc40000 0x0 0x2000>;
		interrupts = <GIC_SPI 19 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&scmi_clk SCMI_ACLK_CRYPTO>, <&scmi_clk SCMI_HCLK_CRYPTO>,
			 <&scmi_clk SCMI_CORE_CRYPTO>, <&scmi_clk SCMI_PKA_CRYPTO>;
		clock-names = "aclk", "hclk", "sclk", "pka";
		assigned-clocks = <&scmi_clk SCMI_CORE_CRYPTO>, <&scmi_clk SCMI_PKA_CRYPTO>;
		assigned-clock-rates = <300000000>, <300000000>;
		resets = <&cru SRST_RESETN_CORE_CRYPTO>;
		reset-names = "crypto-rst";
		status = "disabled";
	};

	rng: rng@ffc50000 {
		compatible = "rockchip,rkrng";
		reg = <0x0 0xffc50000 0x0 0x200>;
		interrupts = <GIC_SPI 23 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&scmi_clk SCMI_HCLK_TRNG>;
		clock-names = "hclk_trng";
		resets = <&cru SRST_HRESETN_TRNG_NS>;
		reset-names = "reset";
		status = "disabled";
	};

	otp: otp@ffce0000 {
		compatible = "rockchip,rk3528-otp";
		reg = <0x0 0xffce0000 0x0 0x4000>;
		#address-cells = <1>;
		#size-cells = <1>;
		clocks = <&cru CLK_USER_OTPC_NS>, <&cru CLK_SBPI_OTPC_NS>,
			 <&cru PCLK_OTPC_NS>;
		clock-names = "usr", "sbpi", "apb";
		resets = <&cru SRST_RESETN_USER_OTPC_NS>,
			 <&cru SRST_RESETN_SBPI_OTPC_NS>,
			 <&cru SRST_PRESETN_OTPC_NS>;
		reset-names = "usr", "sbpi", "apb";

		/* Data cells */
		cpu_code: cpu-code@2 {
			reg = <0x02 0x2>;
		};
		otp_cpu_version: cpu-version@8 {
			reg = <0x08 0x1>;
			bits = <3 3>;
		};
		cpu_mbist_vmin: cpu-mbist-vmin@9 {
			reg = <0x09 0x1>;
			bits = <0 3>;
		};
		gpu_mbist_vmin: gpu-mbist-vmin@9 {
			reg = <0x09 0x1>;
			bits = <3 2>;
		};
		logic_mbist_vmin: logic-mbist-vmin@9 {
			reg = <0x09 0x1>;
			bits = <5 2>;
		};
		otp_id: id@a {
			reg = <0x0a 0x10>;
		};
		cpu_leakage: cpu-leakage@1a {
			reg = <0x1a 0x1>;
		};
		log_leakage: log-leakage@1b {
			reg = <0x1b 0x1>;
		};
		gpu_leakage: gpu-leakage@1c {
			reg = <0x1c 0x1>;
		};
		test_version: test-version@29 {
			reg = <0x29 0x1>;
		};
		macphy_bgs: macphy-bgs@2d {
			reg = <0x2d 0x1>;
		};
		macphy_txlevel: macphy-txlevel@2e {
			reg = <0x2e 0x2>;
		};
		vdac_out_current: vdac-out-current@30 {
			reg = <0x30 0x1>;
		};
		cpu_opp_info: cpu-opp-info@32 {
			reg = <0x32 0x6>;
		};
		gpu_opp_info: gpu-opp-info@38 {
			reg = <0x38 0x6>;
		};
		dmc_opp_info: dmc-opp-info@3e {
			reg = <0x3e 0x6>;
		};
		cpu_tsadc_trim_l: cpu-tsadc-trim-l@44 {
			reg = <0x44 0x1>;
		};
		cpu_tsadc_trim_h: cpu-tsadc-trim-h@45 {
			reg = <0x45 0x1>;
		};
	};

	dmac: dma-controller@ffd60000 {
		compatible = "arm,pl330", "arm,primecell";
		reg = <0x0 0xffd60000 0x0 0x4000>;
		interrupts = <GIC_SPI 0 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 1 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 2 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 3 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 4 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 5 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 6 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 7 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 16 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru ACLK_DMAC>;
		clock-names = "apb_pclk";
		#dma-cells = <1>;
		arm,pl330-periph-burst;
	};

	hwlock: hwspinlock@ffd70000 {
		compatible = "rockchip,hwspinlock";
		reg = <0x0 0xffd70000 0x0 0x100>;
		#hwlock-cells = <1>;
		status = "disabled";
	};

	combphy_pu: phy@ffdc0000 {
		compatible = "rockchip,rk3528-naneng-combphy";
		reg = <0x0 0xffdc0000 0x0 0x10000>;
		#phy-cells = <1>;
		clocks = <&cru CLK_REF_PCIE_INNER_PHY>, <&cru PCLK_PCIE_PHY>, <&cru PCLK_PIPE_GRF>;
		clock-names = "refclk", "apbclk", "pipe_clk";
		assigned-clocks = <&cru CLK_REF_PCIE_INNER_PHY>;
		assigned-clock-rates = <100000000>;
		resets = <&cru SRST_PRESETN_PCIE_PHY>, <&cru SRST_RESETN_PCIE_PIPE_PHY>;
		reset-names = "combphy-apb", "combphy";
		rockchip,pipe-grf = <&grf>;
		rockchip,pipe-phy-grf = <&grf>;
		status = "disabled";
	};

	usb2phy: usb2-phy@ffdf0000 {
		compatible = "rockchip,rk3528-usb2phy";
		reg = <0x0 0xffdf0000 0x0 0x10000>;
		clocks = <&cru CLK_REF_USBPHY>, <&cru PCLK_USBPHY>;
		clock-names = "phyclk", "apb_pclk";
		#clock-cells = <0>;
		rockchip,usbgrf = <&grf>;
		status = "disabled";

		u2phy_otg: otg-port {
			#phy-cells = <0>;
			interrupts = <GIC_SPI 146 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 147 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 148 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "otg-bvalid",
					  "otg-id",
					  "linestate";
			status = "disabled";
		};

		u2phy_host: host-port {
			#phy-cells = <0>;
			interrupts = <GIC_SPI 150 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "linestate";
			status = "disabled";
		};
	};

	hdmiphy: hdmiphy@ffe00000 {
		compatible = "rockchip,rk3528-hdmi-phy";
		reg = <0x0 0xffe00000 0x0 0x10000>;
		interrupts = <GIC_SPI 101 IRQ_TYPE_LEVEL_HIGH>;
		#phy-cells = <0>;
		clocks = <&cru PCLK_HDMIPHY>, <&xin24m>;
		clock-names = "sysclk", "refclk";
		status = "disabled";

		inno_hdmiphy_clk: clk-port {
			#clock-cells = <0>;
			clock-output-names = "clk_hdmiphy_pixel_io";
			status = "okay";
		};
	};

	acodec: acodec@ffe10000 {
		compatible = "rockchip,rk3528-codec";
		reg = <0x0 0xffe10000 0x0 0x1000>;
		#sound-dai-cells = <0>;
		clocks = <&cru PCLK_ACODEC>, <&cru MCLK_ACODEC_TX>;
		clock-names = "pclk", "mclk";
		resets = <&cru SRST_PRESETN_ACODEC>;
		reset-names = "acodec";
		status = "disabled";
	};

	pinctrl: pinctrl {
		compatible = "rockchip,rk3528-pinctrl";
		rockchip,grf = <&ioc_grf>;
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;

		gpio0: gpio@ff610000 {
			compatible = "rockchip,gpio-bank";
			reg = <0x0 0xff610000 0x0 0x200>;
			interrupts = <GIC_SPI 71 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cru PCLK_GPIO0>, <&cru DBCLK_GPIO0>;
			gpio-controller;
			#gpio-cells = <2>;
			gpio-ranges = <&pinctrl 0 0 32>;
			interrupt-controller;
			#interrupt-cells = <2>;
		};

		gpio1: gpio@ffaf0000 {
			compatible = "rockchip,gpio-bank";
			reg = <0x0 0xffaf0000 0x0 0x200>;
			interrupts = <GIC_SPI 73 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cru PCLK_GPIO1>, <&cru DBCLK_GPIO1>;
			gpio-controller;
			#gpio-cells = <2>;
			gpio-ranges = <&pinctrl 0 32 32>;
			interrupt-controller;
			#interrupt-cells = <2>;
		};

		gpio2: gpio@ffb00000 {
			compatible = "rockchip,gpio-bank";
			reg = <0x0 0xffb00000 0x0 0x200>;
			interrupts = <GIC_SPI 75 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cru PCLK_GPIO2>, <&cru DBCLK_GPIO2>;
			gpio-controller;
			#gpio-cells = <2>;
			gpio-ranges = <&pinctrl 0 64 32>;
			interrupt-controller;
			#interrupt-cells = <2>;
		};

		gpio3: gpio@ffb10000 {
			compatible = "rockchip,gpio-bank";
			reg = <0x0 0xffb10000 0x0 0x200>;
			interrupts = <GIC_SPI 76 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cru PCLK_GPIO3>, <&cru DBCLK_GPIO3>;
			gpio-controller;
			#gpio-cells = <2>;
			gpio-ranges = <&pinctrl 0 96 32>;
			interrupt-controller;
			#interrupt-cells = <2>;
		};

		gpio4: gpio@ffb20000 {
			compatible = "rockchip,gpio-bank";
			reg = <0x0 0xffb20000 0x0 0x200>;
			interrupts = <GIC_SPI 78 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cru PCLK_GPIO4>, <&cru DBCLK_GPIO4>;
			gpio-controller;
			#gpio-cells = <2>;
			gpio-ranges = <&pinctrl 0 128 32>;
			interrupt-controller;
			#interrupt-cells = <2>;
		};
	};
};

#include "rk3528-pinctrl.dtsi"
