#include "rp-lcd-hdmi.dtsi"
#define RP_SINGLE_LCD
#define RP_EDP_USED


&edp_panel {
    status = "okay";
        compatible = "simple-panel";
        prepare-delay-ms = <20>;
        enable-delay-ms = <20>;
        disable-delay-ms = <20>;
        unprepare-delay-ms = <20>;
    
        /**
         * power-supply = <>;
         * reset-gpios = <>;
         *
         * lcd reset pin and power supply
         * please refer to ***-lcd-gpio.dtsi
         * that included in main dts.
         */
         
        display-timings {
                native-mode = <&timing1>;

                timing0: timing0 {//EDP 15.6
                        clock-frequency = <150000000>;
                        hactive = <1920>;
                        vactive = <1080>;
                        hfront-porch = <160>;
                        hsync-len = <32>;
                        hback-porch = <160>;
                        vfront-porch = <3>;
                        vsync-len = <5>;
                        vback-porch = <23>;
                        hsync-active = <0>;
                        vsync-active = <0>;
                        de-active = <0>;
                        pixelclk-active = <0>;
                };

                timing1: timing1 {// EDP 13.3 
                        clock-frequency = <138000000>;
                        hactive = <1920>;
                        vactive = <1080>;
                        hfront-porch = <48>;
                        hsync-len = <32>;
                        hback-porch = <80>;
                        vfront-porch = <3>;
                        vsync-len = <5>;
                        vback-porch = <23>;
                        hsync-active = <0>;
                        vsync-active = <0>;
                        de-active = <0>;
                        pixelclk-active = <0>;
                };
        };

        ports {
                    panel_in_edp: endpoint {
                            remote-endpoint = <&edp_out_panel>;
            };
    };
};



&edp {
    status = "okay";
    force-hpd;
        ports {
                port@1 {
                        reg = <1>;

                        edp_out_panel: endpoint {
                                remote-endpoint = <&panel_in_edp>;
                        };
                };
        };
};

&edp_phy {
    status = "okay";
};

&edp_in_vp0 {
    status = "okay";
};

&edp_in_vp1 {
    status = "disabled";
};

&hdmi_in_vp0 {
    status = "disabled";
};
&hdmi_in_vp1 {
    status = "okay";
};

&route_edp {
    status = "okay";
    connect = <&vp0_out_edp>;
};



&gt9xx {
    status = "okay";
    compatible = "goodix,gt9xx";
    reg = <0x5d>;
    gtp_resolution_x = <1920>;
    gtp_resolution_y = <1080>;
    gtp_int_tarigger = <1>;
    gtp_change_x2y = <0>;
    gtp_overturn_x = <0>;
    gtp_overturn_y = <0>;
    gtp_send_cfg = <1>;
    gtp_touch_wakeup = <1>;

    /**
     * goodix_rst_gpio = <>;
     * goodix_irq_gpio = <>;
     *
     * touch panel interrupt and reset pin
     * please refer to ***-lcd-gpio.dtsi
     * that included in main dts.
     */

    goodix,cfg-group0 = [
     43 80 07 38 04 0A 3D 00 01 06
     28 08 55 32 03 05 00 00 00 00
     00 00 06 18 1A 1E 14 95 35 FF
     2D 2F A6 0F 00 00 00 01 03 2C
     00 00 00 00 00 00 00 00 00 00
     00 2D 5A 94 D0 42 00 08 00 04
     79 30 00 6E 37 00 65 3F 00 5D
     49 00 57 54 00 57 00 00 00 00
     00 00 00 00 00 00 00 00 00 00
     00 00 00 00 00 00 00 00 00 00
     00 00 00 00 00 00 00 00 00 00
     00 00 1D 1C 1B 1A 19 18 17 16
     15 14 13 12 11 10 0F 0E 0D 0C
     0B 0A 09 08 07 06 05 04 03 02
     01 00 00 01 02 03 04 05 06 07
     08 09 0A 0B 0C 0D 0E 0F 10 11
     12 13 14 15 16 17 18 19 1B 1C
     1D 1E 1F 20 21 22 23 24 25 26
     27 28 29 2A 86 01
    ];
};

