/**
 * enable pcie3x2 relavent config for rk3568
 */
 
/ {
    vcc3v3_pcie3: gpio-regulator-pcie3 {
        compatible = "regulator-fixed";
        regulator-name = "vcc3v3_pcie3";
        regulator-min-microvolt = <3300000>;
        regulator-max-microvolt = <3300000>;
        enable-active-high;
        /**
         * gpio config please refer to main dts if have
         * gpio = <&gpio* ** ***>;
         */
        startup-delay-us = <5000>;
        vin-supply = <&dc_12v>;
    };
};

&pcie30phy {
    status = "okay";
};

&pcie3x2 {
    /**
     * gpio please refer to main dts:
     * reset-gpios = <&gpio* ** ***>;
     */
    status = "okay";
    vpcie3v3-supply = <&vcc3v3_pcie3>;
};
