// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
// Copyright (c) 2018 Fuzhou Rockchip Electronics Co., Ltd.

#include <dt-bindings/clock/rk1808-cru.h>
#include <dt-bindings/interrupt-controller/arm-gic.h>
#include <dt-bindings/interrupt-controller/irq.h>
#include <dt-bindings/pinctrl/rockchip.h>
#include <dt-bindings/power/rk1808-power.h>
#include <dt-bindings/phy/phy.h>
#include <dt-bindings/soc/rockchip,boot-mode.h>
#include <dt-bindings/soc/rockchip-system-status.h>
#include <dt-bindings/suspend/rockchip-rk1808.h>
#include <dt-bindings/thermal/thermal.h>
#include "rk1808-dram-default-timing.dtsi"

/ {
	compatible = "rockchip,rk1808";

	interrupt-parent = <&gic>;
	#address-cells = <2>;
	#size-cells = <2>;

	aliases {
		i2c0 = &i2c0;
		i2c1 = &i2c1;
		i2c2 = &i2c2;
		i2c3 = &i2c3;
		i2c4 = &i2c4;
		i2c5 = &i2c5;
		serial0 = &uart0;
		serial1 = &uart1;
		serial2 = &uart2;
		serial3 = &uart3;
		serial4 = &uart4;
		serial5 = &uart5;
		serial6 = &uart6;
		serial7 = &uart7;
		spi0 = &spi0;
		spi1 = &spi1;
		spi2 = &spi2;
	};

	cpus {
		#address-cells = <2>;
		#size-cells = <0>;

		cpu0: cpu@0 {
			device_type = "cpu";
			compatible = "arm,cortex-a35", "arm,armv8";
			reg = <0x0 0x0>;
			enable-method = "psci";
			clocks = <&cru ARMCLK>;
			operating-points-v2 = <&cpu0_opp_table>;
			dynamic-power-coefficient = <74>;
			#cooling-cells = <2>;
			cpu-idle-states = <&CPU_SLEEP>;
			power-model {
				compatible = "simple-power-model";
				ref-leakage = <31>;
				static-coefficient = <100000>;
				ts = <597400 241050 (-2450) 70>;
				thermal-zone = "soc-thermal";
			};
		};

		cpu1: cpu@1 {
			device_type = "cpu";
			compatible = "arm,cortex-a35", "arm,armv8";
			reg = <0x0 0x1>;
			enable-method = "psci";
			clocks = <&cru ARMCLK>;
			operating-points-v2 = <&cpu0_opp_table>;
			dynamic-power-coefficient = <74>;
			cpu-idle-states = <&CPU_SLEEP>;
		};

		idle-states {
			entry-method = "psci";

			CPU_SLEEP: cpu-sleep {
				compatible = "arm,idle-state";
				local-timer-stop;
				arm,psci-suspend-param = <0x0010000>;
				entry-latency-us = <120>;
				exit-latency-us = <250>;
				min-residency-us = <900>;
			};

			CLUSTER_SLEEP: cluster-sleep {
				compatible = "arm,idle-state";
				local-timer-stop;
				arm,psci-suspend-param = <0x1010000>;
				entry-latency-us = <400>;
				exit-latency-us = <500>;
				min-residency-us = <2000>;
			};
		};
	};

	cpu0_opp_table: cpu0-opp-table {
		compatible = "operating-points-v2";
		opp-shared;

		rockchip,temp-hysteresis = <5000>;
		rockchip,low-temp = <0>;
		rockchip,low-temp-min-volt = <800000>;
		rockchip,low-temp-adjust-volt = <
			/* MHz    MHz    uV */
			   0      1608   50000
		>;

		rockchip,max-volt = <950000>;
		rockchip,evb-irdrop = <25000>;
		nvmem-cells = <&cpu_leakage>;
		nvmem-cell-names = "leakage";

		rockchip,pvtm-voltage-sel = <
			0        69000   0
			69001    74000   1
			74001    99999   2
		>;
		rockchip,pvtm-freq = <408000>;
		rockchip,pvtm-volt = <800000>;
		rockchip,pvtm-ch = <0 0>;
		rockchip,pvtm-sample-time = <1000>;
		rockchip,pvtm-number = <10>;
		rockchip,pvtm-error = <1000>;
		rockchip,pvtm-ref-temp = <25>;
		rockchip,pvtm-temp-prop = <(-20) (-26)>;
		rockchip,thermal-zone = "soc-thermal";

		opp-408000000 {
			opp-hz = /bits/ 64 <408000000>;
			opp-microvolt = <750000 750000 950000>;
			clock-latency-ns = <40000>;
			opp-suspend;
		};
		opp-600000000 {
			opp-hz = /bits/ 64 <600000000>;
			opp-microvolt = <750000 750000 950000>;
			clock-latency-ns = <40000>;
		};
		opp-816000000 {
			opp-hz = /bits/ 64 <816000000>;
			opp-microvolt = <750000 750000 950000>;
			clock-latency-ns = <40000>;
		};
		opp-1008000000 {
			opp-hz = /bits/ 64 <1008000000>;
			opp-microvolt = <750000 750000 950000>;
			clock-latency-ns = <40000>;
		};
		opp-1200000000 {
			opp-hz = /bits/ 64 <1200000000>;
			opp-microvolt = <800000 800000 950000>;
			opp-microvolt-L0 = <800000 800000 950000>;
			opp-microvolt-L1 = <750000 750000 950000>;
			opp-microvolt-L2 = <750000 750000 950000>;
			clock-latency-ns = <40000>;
		};
		opp-1296000000 {
			opp-hz = /bits/ 64 <1296000000>;
			opp-microvolt = <825000 825000 950000>;
			opp-microvolt-L0 = <825000 825000 950000>;
			opp-microvolt-L1 = <775000 775000 950000>;
			opp-microvolt-L2 = <750000 750000 950000>;
			clock-latency-ns = <40000>;
		};
		opp-1416000000 {
			opp-hz = /bits/ 64 <1416000000>;
			opp-microvolt = <850000 850000 950000>;
			opp-microvolt-L0 = <850000 850000 950000>;
			opp-microvolt-L1 = <800000 800000 950000>;
			opp-microvolt-L2 = <775000 775000 950000>;
			clock-latency-ns = <40000>;
		};
		opp-1512000000 {
			opp-hz = /bits/ 64 <1512000000>;
			opp-microvolt = <875000 875000 950000>;
			opp-microvolt-L0 = <875000 875000 950000>;
			opp-microvolt-L1 = <825000 825000 950000>;
			opp-microvolt-L2 = <800000 800000 950000>;
			clock-latency-ns = <40000>;
		};
		opp-1608000000 {
			opp-hz = /bits/ 64 <1608000000>;
			opp-microvolt = <900000 900000 950000>;
			opp-microvolt-L0 = <900000 900000 950000>;
			opp-microvolt-L1 = <850000 850000 950000>;
			opp-microvolt-L2 = <825000 825000 950000>;
			clock-latency-ns = <40000>;
		};
	};

	arm-pmu {
		compatible = "arm,cortex-a53-pmu";
		interrupts = <GIC_SPI 228 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 229 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-affinity = <&cpu0>, <&cpu1>;
	};

	cpuinfo {
		compatible = "rockchip,cpuinfo";
		nvmem-cells = <&efuse_id>, <&efuse_cpu_version>;
		nvmem-cell-names = "id", "cpu-version";
	};

	bus_soc: bus-soc {
		compatible = "rockchip,rk1808-bus";
		rockchip,busfreq-policy = "smc";
		soc-bus0 {
			bus-id = <0>;
			cfg-val = <0x1e0>;
			enable-msk = <0x407f>;
			status = "okay";
		};
		soc-bus1 {
			bus-id = <1>;
			cfg-val = <0x12c0>;
			enable-msk = <0x41ff>;
			status = "okay";
		};
		soc-bus2 {
			bus-id = <2>;
			cfg-val = <0x12c0>;
			enable-msk = <0x4005>;
			status = "okay";
		};
		soc-bus3 {
			bus-id = <3>;
			cfg-val = <0x12c0>;
			enable-msk = <0x4001>;
			status = "okay";
		};
		soc-bus4 {
			bus-id = <4>;
			cfg-val = <0x12c0>;
			enable-msk = <0x4001>;
			status = "disabled";
		};
	};

	gmac_clkin: external-gmac-clock {
		compatible = "fixed-clock";
		clock-frequency = <125000000>;
		clock-output-names = "gmac_clkin";
		#clock-cells = <0>;
	};

	mipi_csi2: mipi-csi2 {
		compatible = "rockchip,rk1808-mipi-csi2";
		rockchip,hw = <&mipi_csi2_hw>;
		status = "disabled";
	};

	psci {
		compatible = "arm,psci-1.0";
		method = "smc";
	};

	rockchip_suspend: rockchip-suspend {
		compatible = "rockchip,pm-rk1808";
		status = "disabled";
		rockchip,sleep-debug-en = <0>;
		rockchip,sleep-mode-config = <
			(0
			| RKPM_SLP_ARMOFF
			| RKPM_SLP_PMU_PMUALIVE_32K
			| RKPM_SLP_PMU_DIS_OSC
			| RKPM_SLP_PMIC_LP
			| RKPM_SLP_32K_EXT
			)
		>;
		rockchip,wakeup-config = <
			(0
			| RKPM_GPIO_WKUP_EN
			)
		>;
	};

	timer {
		compatible = "arm,armv8-timer";
		interrupts = <GIC_PPI 13 IRQ_TYPE_LEVEL_LOW>,
			     <GIC_PPI 14 IRQ_TYPE_LEVEL_LOW>,
			     <GIC_PPI 11 IRQ_TYPE_LEVEL_LOW>,
			     <GIC_PPI 10 IRQ_TYPE_LEVEL_LOW>;
		arm,no-tick-in-suspend;
	};

	xin24m: xin24m {
		compatible = "fixed-clock";
		clock-frequency = <24000000>;
		clock-output-names = "xin24m";
		#clock-cells = <0>;
	};

	xin32k: xin32k {
		compatible = "fixed-clock";
		clock-frequency = <32768>;
		clock-output-names = "xin32k";
		#clock-cells = <0>;
		pinctrl-names = "default";
		pinctrl-0 = <&clkin_32k>;
	};

	pcie0: pcie@fc400000 {
		compatible = "rockchip,rk1808-pcie", "snps,dw-pcie";
		#address-cells = <3>;
		#size-cells = <2>;
		bus-range = <0x0 0x1f>;
		clocks = <&cru HSCLK_PCIE>, <&cru LSCLK_PCIE>,
			 <&cru ACLK_PCIE>, <&cru PCLK_PCIE>,
			 <&cru SCLK_PCIE_AUX>;
		clock-names = "hsclk", "lsclk",
			      "aclk", "pclk",
			      "sclk-aux";
		interrupts = <GIC_SPI 86 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 87 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 88 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 89 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "sys", "legacy", "msg", "err";
		linux,pci-domain = <0>;
		num-ib-windows = <6>;
		num-ob-windows = <2>;
		msi-map = <0x0 &its 0x0 0x1000>;
		num-lanes = <2>;
		phys = <&combphy PHY_TYPE_PCIE>;
		phy-names = "pcie-phy";
		pinctrl-names = "default";
		pinctrl-0 = <&pcie_clkreq>;
		power-domains = <&power RK1808_PD_PCIE>;
		ranges = <0x00000800 0x0 0xf8000000 0x0 0xf8000000 0x0 0x800000
			  0x83000000 0x0 0xf8800000 0x0 0xf8800000 0x0 0x3700000
			  0x81000000 0x0 0xfbf00000 0x0 0xfbf00000 0x0 0x100000>;
		reg = <0x0 0xfc000000 0x0 0x400000>,
		      <0x0 0xfc400000 0x0 0x10000>;
		reg-names = "pcie-dbi", "pcie-apb";
		resets = <&cru SRST_PCIE_NIU_H>, <&cru SRST_PCIE_NIU_L>,
			 <&cru SRST_PCIEGRF_P>, <&cru SRST_PCIECTL_P>,
			 <&cru SRST_PCIECTL_POWERUP>, <&cru SRST_PCIECTL_MST_A>,
			 <&cru SRST_PCIECTL_SLV_A>, <&cru SRST_PCIECTL_DBI_A>,
			 <&cru SRST_PCIECTL_BUTTON>, <&cru SRST_PCIECTL_PE>,
			 <&cru SRST_PCIECTL_CORE>, <&cru SRST_PCIECTL_NSTICKY>,
			 <&cru SRST_PCIECTL_STICKY>, <&cru SRST_PCIECTL_PWR>,
			 <&cru SRST_PCIE_NIU_A>, <&cru SRST_PCIE_NIU_P>;
		reset-names = "niu-h", "niu-l", "grf-p", "ctl-p",
			      "ctl-powerup", "ctl-mst-a", "ctl-slv-a",
			      "ctl-dbi-a", "ctl-button", "ctl-pe",
			      "ctl-core", "ctl-nsticky", "ctl-sticky",
			      "ctl-pwr", "ctl-niu-a", "ctl-niu-p";
		rockchip,usbpciegrf = <&usb_pcie_grf>;
		rockchip,pmugrf = <&pmugrf>;
		status = "disabled";
	};

	usbdrd3: usb {
		compatible = "rockchip,rk1808-dwc3", "rockchip,rk3399-dwc3";
		clocks = <&cru SCLK_USB3_OTG0_REF>, <&cru ACLK_USB3OTG>,
			 <&cru SCLK_USB3_OTG0_SUSPEND>;
		clock-names = "ref_clk", "bus_clk",
			      "suspend_clk";
		assigned-clocks = <&cru SCLK_USB3_OTG0_SUSPEND>;
		assigned-clock-rates = <24000000>;
		power-domains = <&power RK1808_PD_PCIE>;
		resets = <&cru SRST_USB3_OTG_A>;
		reset-names = "usb3-otg";
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;
		status = "disabled";

		usbdrd_dwc3: dwc3@fd000000 {
			compatible = "snps,dwc3";
			reg = <0x0 0xfd000000 0x0 0x200000>;
			interrupts = <GIC_SPI 75 IRQ_TYPE_LEVEL_HIGH>;
			dr_mode = "otg";
			phys = <&u2phy_otg>, <&combphy PHY_TYPE_USB3>;
			phy-names = "usb2-phy", "usb3-phy";
			phy_type = "utmi_wide";
			snps,dis_enblslpm_quirk;
			snps,dis-u1-entry-quirk;
			snps,dis-u2-entry-quirk;
			snps,dis-u2-freeclk-exists-quirk;
			snps,dis_u2_susphy_quirk;
			snps,dis_u3_susphy_quirk;
			snps,dis-del-phy-power-chg-quirk;
			snps,tx-ipgap-linecheck-dis-quirk;
			snps,parkmode-disable-hs-quirk;
			snps,parkmode-disable-ss-quirk;
			status = "disabled";
		};
	};

	grf: syscon@fe000000 {
		compatible = "rockchip,rk1808-grf", "syscon", "simple-mfd";
		reg = <0x0 0xfe000000 0x0 0x1000>;
		#address-cells = <1>;
		#size-cells = <1>;

		npu_pvtm: npu-pvtm {
			compatible = "rockchip,rk1808-npu-pvtm";
			#address-cells = <1>;
			#size-cells = <0>;
			status = "okay";

			pvtm@2 {
				reg = <2>;
				clocks = <&cru SCLK_PVTM_NPU>;
				clock-names = "clk";
			};
		};

		rgb: rgb {
			compatible = "rockchip,rk1808-rgb";
			status = "disabled";

			ports {
				#address-cells = <1>;
				#size-cells = <0>;

				port@0 {
					reg = <0>;

					rgb_in_vop_lite: endpoint {
						remote-endpoint = <&vop_lite_out_rgb>;
					};
				};
			};
		};
	};

	usb2phy_grf: syscon@fe010000 {
		compatible = "rockchip,rk1808-usb2phy-grf", "syscon",
			     "simple-mfd";
		reg = <0x0 0xfe010000 0x0 0x8000>;
		#address-cells = <1>;
		#size-cells = <1>;

		u2phy: usb2-phy@100 {
			compatible = "rockchip,rk1808-usb2phy";
			reg = <0x100 0x10>;
			clocks = <&cru SCLK_USBPHY_REF>;
			clock-names = "phyclk";
			#clock-cells = <0>;
			assigned-clocks = <&cru USB480M>;
			assigned-clock-parents = <&u2phy>;
			clock-output-names = "usb480m_phy";
			status = "disabled";

			u2phy_host: host-port {
				#phy-cells = <0>;
				interrupts = <GIC_SPI 79 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-names = "linestate";
				status = "disabled";
			};

			u2phy_otg: otg-port {
				#phy-cells = <0>;
				interrupts = <GIC_SPI 78 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 77 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 76 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-names = "otg-bvalid", "otg-id",
						  "linestate";
				status = "disabled";
			};
		};
	};

	combphy_grf: syscon@fe018000 {
		compatible = "rockchip,usb3phy-grf", "syscon";
		reg = <0x0 0xfe018000 0x0 0x8000>;
	};

	pmugrf: syscon@fe020000 {
		compatible = "rockchip,rk1808-pmugrf", "syscon", "simple-mfd";
		reg = <0x0 0xfe020000 0x0 0x1000>;
		#address-cells = <1>;
		#size-cells = <1>;

		pmu_pvtm: pmu-pvtm {
			compatible = "rockchip,rk1808-pmu-pvtm";
			#address-cells = <1>;
			#size-cells = <0>;
			status = "okay";

			pvtm@1 {
				reg = <1>;
				clocks = <&cru SCLK_PVTM_PMU>;
				clock-names = "clk";
			};
		};

		reboot-mode {
			compatible = "syscon-reboot-mode";
			offset = <0x200>;
			mode-bootloader = <BOOT_BL_DOWNLOAD>;
			mode-charge = <BOOT_CHARGING>;
			mode-fastboot = <BOOT_FASTBOOT>;
			mode-loader = <BOOT_BL_DOWNLOAD>;
			mode-normal = <BOOT_NORMAL>;
			mode-recovery = <BOOT_RECOVERY>;
			mode-ums = <BOOT_UMS>;
		};
	};

	usb_pcie_grf: syscon@fe040000 {
		compatible = "rockchip,usb-pcie-grf", "syscon";
		reg = <0x0 0xfe040000 0x0 0x1000>;
	};

	coregrf: syscon@fe050000 {
		compatible = "rockchip,rk1808-coregrf", "syscon", "simple-mfd";
		reg = <0x0 0xfe050000 0x0 0x1000>;
		#address-cells = <1>;
		#size-cells = <1>;

		pvtm: pvtm {
			compatible = "rockchip,rk1808-pvtm";
			#address-cells = <1>;
			#size-cells = <0>;
			status = "okay";

			pvtm@0 {
				reg = <0>;
				clocks = <&cru SCLK_PVTM_CORE>;
				clock-names = "clk";
			};
		};
	};

	qos_npu: qos@fe850000 {
		compatible = "syscon";
		reg = <0x0 0xfe850000 0x0 0x20>;
	};

	qos_pcie: qos@fe880000 {
		compatible = "syscon";
		reg = <0x0 0xfe880000 0x0 0x20>;
		status = "disabled";
	};

	qos_usb2: qos@fe890000 {
		compatible = "syscon";
		reg = <0x0 0xfe890000 0x0 0x20>;
		status = "disabled";
	};

	qos_usb3: qos@fe890080 {
		compatible = "syscon";
		reg = <0x0 0xfe890080 0x0 0x20>;
		status = "disabled";
	};

	qos_isp: qos@fe8a0000 {
		compatible = "syscon";
		reg = <0x0 0xfe8a0000 0x0 0x20>;
	};

	qos_rga_rd: qos@fe8a0080 {
		compatible = "syscon";
		reg = <0x0 0xfe8a0080 0x0 0x20>;
	};

	qos_rga_wr: qos@fe8a0100 {
		compatible = "syscon";
		reg = <0x0 0xfe8a0100 0x0 0x20>;
	};

	qos_cif: qos@fe8a0180 {
		compatible = "syscon";
		reg = <0x0 0xfe8a0180 0x0 0x20>;
	};

	qos_vop_raw: qos@fe8b0000 {
		compatible = "syscon";
		reg = <0x0 0xfe8b0000 0x0 0x20>;
	};

	qos_vop_lite: qos@fe8b0080 {
		compatible = "syscon";
		reg = <0x0 0xfe8b0080 0x0 0x20>;
	};

	qos_vpu: qos@fe8c0000 {
		compatible = "syscon";
		reg = <0x0 0xfe8c0000 0x0 0x20>;
	};

	sram: sram@fec00000 {
		compatible = "mmio-sram";
		reg = <0x0 0xfec00000 0x0 0x200000>;
		#address-cells = <1>;
		#size-cells = <1>;
		ranges = <0 0x0 0xfec00000 0x200000>;
		/* reserved for ddr dvfs and system suspend/resume */
		ddr-sram@0 {
			reg = <0x0 0x8000>;
		};
		/* reserved for vad audio buffer */
		vad_sram: vad-sram@1c0000 {
			reg = <0x1c0000 0x40000>;
		};
	};

	hwlock: hwspinlock@ff040000 {
		compatible = "rockchip,hwspinlock";
		reg = <0 0xff040000 0 0x10000>;
		#hwlock-cells = <1>;
	};

	gic: interrupt-controller@ff100000 {
		compatible = "arm,gic-v3";
		#interrupt-cells = <3>;
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;
		interrupt-controller;

		reg = <0x0 0xff100000 0 0x10000>, /* GICD */
		      <0x0 0xff140000 0 0xc0000>, /* GICR */
		      <0x0 0xff300000 0 0x10000>, /* GICC */
		      <0x0 0xff310000 0 0x10000>, /* GICH */
		      <0x0 0xff320000 0 0x10000>; /* GICV */
		interrupts = <GIC_PPI 9 IRQ_TYPE_LEVEL_HIGH>;
		its: interrupt-controller@ff120000 {
			compatible = "arm,gic-v3-its";
			msi-controller;
			reg = <0x0 0xff120000 0x0 0x20000>;
		};
	};

	efuse: efuse@ff260000 {
		compatible = "rockchip,rk1808-efuse";
		reg = <0x0 0xff3b0000 0x0 0x50>;
		#address-cells = <1>;
		#size-cells = <1>;
		clocks = <&cru SCLK_EFUSE_NS>, <&cru PCLK_EFUSE>;
		clock-names = "sclk_efuse", "pclk_efuse";
		assigned-clocks = <&cru SCLK_EFUSE_NS>;
		assigned-clock-rates = <24000000>;
		rockchip,efuse-size = <0x20>;

		/* Data cells */
		efuse_id: id@7 {
			reg = <0x07 0x10>;
		};
		cpu_leakage: cpu-leakage@17 {
			reg = <0x17 0x1>;
		};
		logic_leakage: logic-leakage@18 {
			reg = <0x18 0x1>;
		};
		npu_leakage: npu-leakage@19 {
			reg = <0x19 0x1>;
		};
		efuse_cpu_version: cpu-version@1c {
			reg = <0x1c 0x1>;
			bits = <3 3>;
		};
	};

	cru: clock-controller@ff350000 {
		compatible = "rockchip,rk1808-cru";
		reg = <0x0 0xff350000 0x0 0x5000>;
		rockchip,grf = <&grf>;
		rockchip,pmugrf = <&pmugrf>;
		#clock-cells = <1>;
		#reset-cells = <1>;

		assigned-clocks =
			<&cru SCLK_32K_IOE>,
			<&cru PLL_GPLL>, <&cru PLL_CPLL>,
			<&cru PLL_PPLL>, <&cru ARMCLK>,
			<&cru MSCLK_PERI>, <&cru LSCLK_PERI>,
			<&cru HSCLK_BUS_PRE>, <&cru MSCLK_BUS_PRE>,
			<&cru LSCLK_BUS_PRE>;
		assigned-clock-parents = <&xin32k>;
		assigned-clock-rates =
			<32768>,
			<1188000000>, <1000000000>,
			<100000000>, <816000000>,
			<200000000>, <100000000>,
			<300000000>, <200000000>,
			<100000000>;
	};

	mipi_dphy_rx: mipi-dphy-rx@ff360000 {
		compatible = "rockchip,rk1808-mipi-dphy-rx";
		reg = <0x0 0xff360000 0x0 0x4000>;
		clocks = <&cru PCLK_MIPICSIPHY>;
		clock-names = "pclk";
		power-domains = <&power RK1808_PD_VIO>;
		rockchip,grf = <&grf>;
		status = "disabled";
	};

	mipi_dphy: mipi-dphy@ff370000 {
		compatible = "rockchip,rk1808-mipi-dphy";
		reg = <0x0 0xff370000 0x0 0x500>;
		clocks = <&cru SCLK_MIPIDSIPHY_REF>, <&cru PCLK_MIPIDSIPHY>;
		clock-names = "ref", "pclk";
		clock-output-names = "mipi_dphy_pll";
		#clock-cells = <0>;
		resets = <&cru SRST_MIPIDSIPHY_P>;
		reset-names = "apb";
		#phy-cells = <0>;
		rockchip,grf = <&grf>;
		status = "disabled";
	};

	combphy: phy@ff380000 {
		compatible = "rockchip,rk1808-combphy";
		reg = <0x0 0xff380000 0x0 0x10000>;
		#phy-cells = <1>;
		clocks = <&cru SCLK_PCIEPHY_REF>;
		clock-names = "refclk";
		assigned-clocks = <&cru SCLK_PCIEPHY_REF>;
		assigned-clock-rates = <25000000>;
		resets = <&cru SRST_USB3_OTG_A>, <&cru SRST_PCIEPHY_POR>,
			 <&cru SRST_PCIEPHY_P>, <&cru SRST_PCIEPHY_PIPE>,
			 <&cru SRST_USB3PHY_GRF_P>;
		reset-names = "otg-rst", "combphy-por",
			      "combphy-apb", "combphy-pipe",
			      "usb3phy_grf_p";
		rockchip,combphygrf = <&combphy_grf>;
		rockchip,usbpciegrf = <&usb_pcie_grf>;
		status = "disabled";
	};

	thermal_zones: thermal-zones {
		soc_thermal: soc-thermal {
			polling-delay-passive = <20>; /* milliseconds */
			polling-delay = <1000>; /* milliseconds */
			sustainable-power = <977>; /* milliwatts */

			thermal-sensors = <&tsadc 0>;

			trips {
				threshold: trip-point-0 {
					/* millicelsius */
					temperature = <75000>;
					/* millicelsius */
					hysteresis = <2000>;
					type = "passive";
				};
				target: trip-point-1 {
					/* millicelsius */
					temperature = <85000>;
					/* millicelsius */
					hysteresis = <2000>;
					type = "passive";
				};
				soc_crit: soc-crit {
					/* millicelsius */
					temperature = <115000>;
					/* millicelsius */
					hysteresis = <2000>;
					type = "critical";
				};
			};

			cooling-maps {
				map0 {
					trip = <&target>;
					cooling-device =
						<&cpu0 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
					contribution = <4096>;
				};
				map1 {
					trip = <&target>;
					cooling-device =
						<&npu THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
					contribution = <1024>;
				};
			};
		};
	};

	tsadc: tsadc@ff3a0000 {
		compatible = "rockchip,rk1808-tsadc";
		reg = <0x0 0xff3a0000 0x0 0x100>;
		interrupts = <GIC_SPI 32 IRQ_TYPE_LEVEL_HIGH>;
		rockchip,grf = <&grf>;
		clocks = <&cru SCLK_TSADC>, <&cru PCLK_TSADC>;
		clock-names = "tsadc", "apb_pclk";
		assigned-clocks = <&cru SCLK_TSADC>;
		assigned-clock-rates = <650000>;
		resets = <&cru SRST_TSADC>;
		reset-names = "tsadc-apb";
		#thermal-sensor-cells = <1>;
		rockchip,hw-tshut-temp = <120000>;
		status = "disabled";
	};

	saradc: saradc@ff3c0000 {
		compatible = "rockchip,rk1808-saradc", "rockchip,rk3399-saradc";
		reg = <0x0 0xff3c0000 0x0 0x100>;
		interrupts = <GIC_SPI 64 IRQ_TYPE_LEVEL_HIGH>;
		#io-channel-cells = <1>;
		clocks = <&cru SCLK_SARADC>, <&cru PCLK_SARADC>;
		clock-names = "saradc", "apb_pclk";
		resets = <&cru SRST_SARADC_P>;
		reset-names = "saradc-apb";
		status = "disabled";
	};

	pwm0: pwm@ff3d0000 {
		compatible = "rockchip,rk1808-pwm", "rockchip,rk3328-pwm";
		reg = <0x0 0xff3d0000 0x0 0x10>;
		interrupts = <GIC_SPI 20 IRQ_TYPE_LEVEL_HIGH>;
		#pwm-cells = <3>;
		pinctrl-names = "active";
		pinctrl-0 = <&pwm0_pin>;
		clocks = <&cru SCLK_PWM0>, <&cru PCLK_PWM0>;
		clock-names = "pwm", "pclk";
		status = "disabled";
	};

	pwm1: pwm@ff3d0010 {
		compatible = "rockchip,rk1808-pwm", "rockchip,rk3328-pwm";
		reg = <0x0 0xff3d0010 0x0 0x10>;
		interrupts = <GIC_SPI 20 IRQ_TYPE_LEVEL_HIGH>;
		#pwm-cells = <3>;
		pinctrl-names = "active";
		pinctrl-0 = <&pwm1_pin>;
		clocks = <&cru SCLK_PWM0>, <&cru PCLK_PWM0>;
		clock-names = "pwm", "pclk";
		status = "disabled";
	};

	pwm2: pwm@ff3d0020 {
		compatible = "rockchip,rk1808-pwm", "rockchip,rk3328-pwm";
		reg = <0x0 0xff3d0020 0x0 0x10>;
		interrupts = <GIC_SPI 20 IRQ_TYPE_LEVEL_HIGH>;
		#pwm-cells = <3>;
		pinctrl-names = "active";
		pinctrl-0 = <&pwm2_pin>;
		clocks = <&cru SCLK_PWM0>, <&cru PCLK_PWM0>;
		clock-names = "pwm", "pclk";
		status = "disabled";
	};

	pwm3: pwm@ff3d0030 {
		compatible = "rockchip,rk1808-pwm", "rockchip,rk3328-pwm";
		reg = <0x0 0xff3d0030 0x0 0x10>;
		interrupts = <GIC_SPI 20 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 19 IRQ_TYPE_LEVEL_HIGH>;
		#pwm-cells = <3>;
		pinctrl-names = "active";
		pinctrl-0 = <&pwm3_pin>;
		clocks = <&cru SCLK_PWM0>, <&cru PCLK_PWM0>;
		clock-names = "pwm", "pclk";
		status = "disabled";
	};

	pwm4: pwm@ff3d8000 {
		compatible = "rockchip,rk1808-pwm", "rockchip,rk3328-pwm";
		reg = <0x0 0xff3d8000 0x0 0x10>;
		interrupts = <GIC_SPI 85 IRQ_TYPE_LEVEL_HIGH>;
		#pwm-cells = <3>;
		pinctrl-names = "active";
		pinctrl-0 = <&pwm4_pin>;
		clocks = <&cru SCLK_PWM1>, <&cru PCLK_PWM1>;
		clock-names = "pwm", "pclk";
		status = "disabled";
	};

	pwm5: pwm@ff3d8010 {
		compatible = "rockchip,rk1808-pwm", "rockchip,rk3328-pwm";
		reg = <0x0 0xff3d8010 0x0 0x10>;
		interrupts = <GIC_SPI 85 IRQ_TYPE_LEVEL_HIGH>;
		#pwm-cells = <3>;
		pinctrl-names = "active";
		pinctrl-0 = <&pwm5_pin>;
		clocks = <&cru SCLK_PWM1>, <&cru PCLK_PWM1>;
		clock-names = "pwm", "pclk";
		status = "disabled";
	};

	pwm6: pwm@ff3d8020 {
		compatible = "rockchip,rk1808-pwm", "rockchip,rk3328-pwm";
		reg = <0x0 0xff3d8020 0x0 0x10>;
		interrupts = <GIC_SPI 85 IRQ_TYPE_LEVEL_HIGH>;
		#pwm-cells = <3>;
		pinctrl-names = "active";
		pinctrl-0 = <&pwm6_pin>;
		clocks = <&cru SCLK_PWM1>, <&cru PCLK_PWM1>;
		clock-names = "pwm", "pclk";
		status = "disabled";
	};

	pwm7: pwm@ff3d8030 {
		compatible = "rockchip,rk1808-pwm", "rockchip,rk3328-pwm";
		reg = <0x0 0xff3d8030 0x0 0x10>;
		interrupts = <GIC_SPI 85 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 84 IRQ_TYPE_LEVEL_HIGH>;
		#pwm-cells = <3>;
		pinctrl-names = "active";
		pinctrl-0 = <&pwm7_pin>;
		clocks = <&cru SCLK_PWM1>, <&cru PCLK_PWM1>;
		clock-names = "pwm", "pclk";
		status = "disabled";
	};

	pmu: power-management@ff3e0000 {
		compatible = "rockchip,rk1808-pmu", "syscon", "simple-mfd";
		reg = <0x0 0xff3e0000 0x0 0x1000>;

		power: power-controller {
			compatible = "rockchip,rk1808-power-controller";
			#power-domain-cells = <1>;
			#address-cells = <1>;
			#size-cells = <0>;
			status = "okay";

			/* These power domains are grouped by VD_NPU */
			pd_npu@RK1808_VD_NPU {
				reg = <RK1808_VD_NPU>;
				clocks = <&cru SCLK_NPU>,
					 <&cru ACLK_NPU>,
					 <&cru HCLK_NPU>;
				pm_qos = <&qos_npu>;
			};

			/* These power domains are grouped by VD_LOGIC */
			pd_pcie@RK1808_PD_PCIE {
				reg = <RK1808_PD_PCIE>;
				clocks = <&cru HSCLK_PCIE>,
					 <&cru LSCLK_PCIE>,
					 <&cru ACLK_PCIE>,
					 <&cru ACLK_PCIE_MST>,
					 <&cru ACLK_PCIE_SLV>,
					 <&cru PCLK_PCIE>,
					 <&cru SCLK_PCIE_AUX>,
					 <&cru SCLK_PCIE_AUX>,
					 <&cru ACLK_USB3OTG>,
					 <&cru HCLK_HOST>,
					 <&cru HCLK_HOST_ARB>,
					 <&cru SCLK_USB3_OTG0_REF>,
					 <&cru SCLK_USB3_OTG0_SUSPEND>;
				pm_qos = <&qos_pcie>,
					 <&qos_usb2>,
					 <&qos_usb3>;
			};
			pd_vpu@RK1808_PD_VPU {
				reg = <RK1808_PD_VPU>;
				clocks = <&cru ACLK_VPU>,
					 <&cru HCLK_VPU>;
				pm_qos = <&qos_vpu>;
			};
			pd_vio@RK1808_PD_VIO {
				reg = <RK1808_PD_VIO>;
				clocks = <&cru HSCLK_VIO>,
					 <&cru LSCLK_VIO>,
					 <&cru ACLK_VOPRAW>,
					 <&cru HCLK_VOPRAW>,
					 <&cru ACLK_VOPLITE>,
					 <&cru HCLK_VOPLITE>,
					 <&cru PCLK_DSI_TX>,
					 <&cru PCLK_CSI_TX>,
					 <&cru ACLK_RGA>,
					 <&cru HCLK_RGA>,
					 <&cru ACLK_ISP>,
					 <&cru HCLK_ISP>,
					 <&cru ACLK_CIF>,
					 <&cru HCLK_CIF>,
					 <&cru PCLK_CSI2HOST>,
					 <&cru DCLK_VOPRAW>,
					 <&cru DCLK_VOPLITE>;
				pm_qos = <&qos_rga_rd>, <&qos_rga_wr>,
					 <&qos_isp>, <&qos_cif>,
					 <&qos_vop_raw>, <&qos_vop_lite>;
			};
		};
	};

	i2c0: i2c@ff410000 {
		compatible = "rockchip,rk3399-i2c";
		reg = <0x0 0xff410000 0x0 0x1000>;
		clocks =  <&cru SCLK_PMU_I2C0>, <&cru PCLK_I2C0_PMU>;
		clock-names = "i2c", "pclk";
		interrupts = <GIC_SPI 7 IRQ_TYPE_LEVEL_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2c0_xfer>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	dmac: dmac@ff4e0000 {
		compatible = "arm,pl330", "arm,primecell";
		reg = <0x0 0xff4e0000 0x0 0x4000>;
		interrupts = <GIC_SPI 1 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru ACLK_DMAC>;
		clock-names = "apb_pclk";
		#dma-cells = <1>;
		arm,pl330-periph-burst;
	};

	uart0: serial@ff430000 {
		compatible = "rockchip,rk1808-uart", "snps,dw-apb-uart";
		reg = <0x0 0xff430000 0x0 0x100>;
		interrupts = <GIC_SPI 13 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_UART0_PMU>, <&cru PCLK_UART0_PMU>;
		clock-names = "baudclk", "apb_pclk";
		reg-shift = <2>;
		reg-io-width = <4>;
		dmas = <&dmac 0>, <&dmac 1>;
		pinctrl-names = "default";
		pinctrl-0 = <&uart0_xfer &uart0_cts &uart0_rts>;
		status = "disabled";
	};

	i2c1: i2c@ff500000 {
		compatible = "rockchip,rk3399-i2c";
		reg = <0x0 0xff500000 0x0 0x1000>;
		clocks = <&cru SCLK_I2C1>, <&cru PCLK_I2C1>;
		clock-names = "i2c", "pclk";
		interrupts = <GIC_SPI 8 IRQ_TYPE_LEVEL_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2c1_xfer>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	i2c2: i2c@ff504000 {
		compatible = "rockchip,rk3399-i2c";
		reg = <0x0 0xff504000 0x0 0x1000>;
		clocks = <&cru SCLK_I2C2>, <&cru PCLK_I2C2>;
		clock-names = "i2c", "pclk";
		interrupts = <GIC_SPI 9 IRQ_TYPE_LEVEL_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2c2m0_xfer>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	i2c3: i2c@ff508000 {
		compatible = "rockchip,rk3399-i2c";
		reg = <0x0 0xff508000 0x0 0x1000>;
		clocks = <&cru SCLK_I2C3>, <&cru PCLK_I2C3>;
		clock-names = "i2c", "pclk";
		interrupts = <GIC_SPI 83 IRQ_TYPE_LEVEL_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2c3_xfer>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	i2c4: i2c@ff50c000 {
		compatible = "rockchip,rk3399-i2c";
		reg = <0x0 0xff50c000 0x0 0x1000>;
		clocks = <&cru SCLK_I2C4>, <&cru PCLK_I2C4>;
		clock-names = "i2c", "pclk";
		interrupts = <GIC_SPI 101 IRQ_TYPE_LEVEL_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2c4_xfer>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	i2c5: i2c@ff510000 {
		compatible = "rockchip,rk3399-i2c";
		reg = <0x0 0xff510000 0x0 0x1000>;
		clocks = <&cru SCLK_I2C5>, <&cru PCLK_I2C5>;
		clock-names = "i2c", "pclk";
		interrupts = <GIC_SPI 102 IRQ_TYPE_LEVEL_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2c5_xfer>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	spi0: spi@ff520000 {
		compatible = "rockchip,rk1808-spi", "rockchip,rk3066-spi";
		reg = <0x0 0xff520000 0x0 0x1000>;
		interrupts = <GIC_SPI 21 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&cru SCLK_SPI0>, <&cru PCLK_SPI0>;
		clock-names = "spiclk", "apb_pclk";
		dmas = <&dmac 10>, <&dmac 11>;
		pinctrl-names = "default", "high_speed";
		pinctrl-0 = <&spi0_clk &spi0_csn &spi0_miso &spi0_mosi>;
		pinctrl-1 = <&spi0_clk_hs &spi0_csn &spi0_miso_hs &spi0_mosi_hs>;
		status = "disabled";
	};

	spi1: spi@ff530000 {
		compatible = "rockchip,rk1808-spi", "rockchip,rk3066-spi";
		reg = <0x0 0xff530000 0x0 0x1000>;
		interrupts = <GIC_SPI 22 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&cru SCLK_SPI1>, <&cru PCLK_SPI1>;
		clock-names = "spiclk", "apb_pclk";
		dmas = <&dmac 12>, <&dmac 13>;
		pinctrl-names = "default", "high_speed";
		pinctrl-0 = <&spi1_clk &spi1_csn0 &spi1_csn1 &spi1_miso &spi1_mosi>;
		pinctrl-1 = <&spi1_clk_hs &spi1_csn0 &spi1_csn1 &spi1_miso_hs &spi1_mosi_hs>;
		status = "disabled";
	};

	uart1: serial@ff540000 {
		compatible = "rockchip,rk1808-uart", "snps,dw-apb-uart";
		reg = <0x0 0xff540000 0x0 0x100>;
		interrupts = <GIC_SPI 14 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_UART1>, <&cru PCLK_UART1>;
		clock-names = "baudclk", "apb_pclk";
		reg-shift = <2>;
		reg-io-width = <4>;
		dmas = <&dmac 2>, <&dmac 3>;
		pinctrl-names = "default";
		pinctrl-0 = <&uart1m0_xfer &uart1_cts &uart1_rts>;
		status = "disabled";
	};

	uart2: serial@ff550000 {
		compatible = "rockchip,rk1808-uart", "snps,dw-apb-uart";
		reg = <0x0 0xff550000 0x0 0x100>;
		interrupts = <GIC_SPI 15 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_UART2>, <&cru PCLK_UART2>;
		clock-names = "baudclk", "apb_pclk";
		reg-shift = <2>;
		reg-io-width = <4>;
		dmas = <&dmac 4>, <&dmac 5>;
		pinctrl-names = "default";
		pinctrl-0 = <&uart2m0_xfer>;
		status = "disabled";
	};

	uart3: serial@ff560000 {
		compatible = "rockchip,rk1808-uart", "snps,dw-apb-uart";
		reg = <0x0 0xff560000 0x0 0x100>;
		interrupts = <GIC_SPI 16 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_UART3>, <&cru PCLK_UART3>;
		clock-names = "baudclk", "apb_pclk";
		reg-shift = <2>;
		reg-io-width = <4>;
		dmas = <&dmac 6>, <&dmac 7>;
		pinctrl-names = "default";
		pinctrl-0 = <&uart3m0_xfer &uart3_ctsm0 &uart3_rtsm0>;
		status = "disabled";
	};

	uart4: serial@ff570000 {
		compatible = "rockchip,rk1808-uart", "snps,dw-apb-uart";
		reg = <0x0 0xff570000 0x0 0x100>;
		interrupts = <GIC_SPI 17 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_UART4>, <&cru PCLK_UART4>;
		clock-names = "baudclk", "apb_pclk";
		reg-shift = <2>;
		reg-io-width = <4>;
		dmas = <&dmac 8>, <&dmac 9>;
		pinctrl-names = "default";
		pinctrl-0 = <&uart4_xfer &uart4_cts &uart4_rts>;
		status = "disabled";
	};

	spi2: spi@ff580000 {
		compatible = "rockchip,rk1808-spi", "rockchip,rk3066-spi";
		reg = <0x0 0xff580000 0x0 0x1000>;
		interrupts = <GIC_SPI 23 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&cru SCLK_SPI2>, <&cru PCLK_SPI2>;
		clock-names = "spiclk", "apb_pclk";
		dmas = <&dmac 14>, <&dmac 15>;
		pinctrl-names = "default", "high_speed";
		pinctrl-0 = <&spi2m0_clk &spi2m0_csn &spi2m0_miso &spi2m0_mosi>;
		pinctrl-1 = <&spi2m0_clk_hs &spi2m0_csn &spi2m0_miso_hs &spi2m0_mosi_hs>;
		status = "disabled";
	};

	uart5: serial@ff5a0000 {
		compatible = "rockchip,rk1808-uart", "snps,dw-apb-uart";
		reg = <0x0 0xff5a0000 0x0 0x100>;
		interrupts = <GIC_SPI 46 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_UART5>, <&cru PCLK_UART5>;
		clock-names = "baudclk", "apb_pclk";
		reg-shift = <2>;
		reg-io-width = <4>;
		dmas = <&dmac 25>, <&dmac 26>;
		pinctrl-names = "default";
		pinctrl-0 = <&uart5_xfer>;
		status = "disabled";
	};

	uart6: serial@ff5b0000 {
		compatible = "rockchip,rk1808-uart", "snps,dw-apb-uart";
		reg = <0x0 0xff5b0000 0x0 0x100>;
		interrupts = <GIC_SPI 45 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_UART6>, <&cru PCLK_UART6>;
		clock-names = "baudclk", "apb_pclk";
		reg-shift = <2>;
		reg-io-width = <4>;
		dmas = <&dmac 27>, <&dmac 28>;
		pinctrl-names = "default";
		pinctrl-0 = <&uart6_xfer>;
		status = "disabled";
	};

	uart7: serial@ff5c0000 {
		compatible = "rockchip,rk1808-uart", "snps,dw-apb-uart";
		reg = <0x0 0xff5c0000 0x0 0x100>;
		interrupts = <GIC_SPI 44 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_UART7>, <&cru PCLK_UART7>;
		clock-names = "baudclk", "apb_pclk";
		reg-shift = <2>;
		reg-io-width = <4>;
		dmas = <&dmac 29>, <&dmac 30>;
		pinctrl-names = "default";
		pinctrl-0 = <&uart7_xfer>;
		status = "disabled";
	};

	pwm8: pwm@ff5d0000 {
		compatible = "rockchip,rk1808-pwm", "rockchip,rk3328-pwm";
		reg = <0x0 0xff5d0000 0x0 0x10>;
		interrupts = <GIC_SPI 91 IRQ_TYPE_LEVEL_HIGH>;
		#pwm-cells = <3>;
		pinctrl-names = "active";
		pinctrl-0 = <&pwm8_pin>;
		clocks = <&cru SCLK_PWM2>, <&cru PCLK_PWM2>;
		clock-names = "pwm", "pclk";
		status = "disabled";
	};

	pwm9: pwm@fff5d0010 {
		compatible = "rockchip,rk1808-pwm", "rockchip,rk3328-pwm";
		reg = <0x0 0xff5d0010 0x0 0x10>;
		interrupts = <GIC_SPI 91 IRQ_TYPE_LEVEL_HIGH>;
		#pwm-cells = <3>;
		pinctrl-names = "active";
		pinctrl-0 = <&pwm9_pin>;
		clocks = <&cru SCLK_PWM2>, <&cru PCLK_PWM2>;
		clock-names = "pwm", "pclk";
		status = "disabled";
	};

	pwm10: pwm@ff5d0020 {
		compatible = "rockchip,rk1808-pwm", "rockchip,rk3328-pwm";
		reg = <0x0 0xff5d0020 0x0 0x10>;
		interrupts = <GIC_SPI 91 IRQ_TYPE_LEVEL_HIGH>;
		#pwm-cells = <3>;
		pinctrl-names = "active";
		pinctrl-0 = <&pwm10_pin>;
		clocks = <&cru SCLK_PWM2>, <&cru PCLK_PWM2>;
		clock-names = "pwm", "pclk";
		status = "disabled";
	};

	pwm11: pwm@ff5d0030 {
		compatible = "rockchip,rk1808-pwm", "rockchip,rk3328-pwm";
		reg = <0x0 0xff5d0030 0x0 0x10>;
		interrupts = <GIC_SPI 91 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 90 IRQ_TYPE_LEVEL_HIGH>;
		#pwm-cells = <3>;
		pinctrl-names = "active";
		pinctrl-0 = <&pwm11_pin>;
		clocks = <&cru SCLK_PWM2>, <&cru PCLK_PWM2>;
		clock-names = "pwm", "pclk";
		status = "disabled";
	};

	rng: rng@ff630000 {
		compatible = "rockchip,cryptov2-rng";
		reg = <0x0 0xff630000 0x0 0x4000>;
		clocks = <&cru SCLK_CRYPTO>, <&cru SCLK_CRYPTO_APK>,
			<&cru ACLK_CRYPTO>, <&cru HCLK_CRYPTO>;
		clock-names = "clk_crypto", "clk_crypto_apk",
				"aclk_crypto", "hclk_crypto";
		resets = <&cru SRST_CRYPTO_CORE>;
		reset-names = "reset";
		status = "disabled";
	};

	dcf: dcf@ff640000 {
		compatible = "syscon";
		reg = <0x0 0xff640000 0x0 0x1000>;
	};

	rktimer: rktimer@ff700000 {
		compatible = "rockchip,rk3288-timer";
		reg = <0x0 0xff700000 0x0 0x1000>;
		interrupts = <GIC_SPI 26 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru PCLK_TIMER>, <&cru SCLK_TIMER0>;
		clock-names = "pclk", "timer";
	};

	wdt: watchdog@ff720000 {
		compatible = "snps,dw-wdt";
		reg = <0x0 0xff720000 0x0 0x100>;
		clocks = <&cru PCLK_WDT>;
		interrupts = <GIC_SPI 33 IRQ_TYPE_LEVEL_HIGH>;
		status = "okay";
	};

	i2s0: i2s@ff7e0000 {
		compatible = "rockchip,rk1808-i2s-tdm";
		reg = <0x0 0xff7e0000 0x0 0x1000>;
		interrupts = <GIC_SPI 10 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_I2S0_8CH_TX>, <&cru SCLK_I2S0_8CH_RX>, <&cru HCLK_I2S0_8CH>;
		clock-names = "mclk_tx", "mclk_rx", "hclk";
		dmas = <&dmac 16>, <&dmac 17>;
		dma-names = "tx", "rx";
		resets = <&cru SRST_I2S0_TX>, <&cru SRST_I2S0_RX>;
		reset-names = "tx-m", "rx-m";
		rockchip,cru = <&cru>;
		rockchip,grf = <&grf>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2s0_8ch_sclktx
			     &i2s0_8ch_sclkrx
			     &i2s0_8ch_lrcktx
			     &i2s0_8ch_lrckrx
			     &i2s0_8ch_sdi0
			     &i2s0_8ch_sdi1
			     &i2s0_8ch_sdi2
			     &i2s0_8ch_sdi3
			     &i2s0_8ch_sdo0
			     &i2s0_8ch_sdo1
			     &i2s0_8ch_sdo2
			     &i2s0_8ch_sdo3
			     &i2s0_8ch_mclk>;
		status = "disabled";
	};

	i2s1: i2s@ff7f0000 {
		compatible = "rockchip,rk1808-i2s", "rockchip,rk3066-i2s";
		reg = <0x0 0xff7f0000 0x0 0x1000>;
		interrupts = <GIC_SPI 11 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_I2S1_2CH>, <&cru HCLK_I2S1_2CH>;
		clock-names = "i2s_clk", "i2s_hclk";
		dmas = <&dmac 18>, <&dmac 19>;
		dma-names = "tx", "rx";
		resets = <&cru SRST_I2S1>, <&cru SRST_I2S1_H>;
		reset-names = "reset-m", "reset-h";
		pinctrl-names = "default";
		pinctrl-0 = <&i2s1_2ch_sclk
			     &i2s1_2ch_lrck
			     &i2s1_2ch_sdi
			     &i2s1_2ch_sdo>;
		status = "disabled";
	};

	pdm: pdm@ff800000 {
		compatible = "rockchip,rk1808-pdm", "rockchip,pdm";
		reg = <0x0 0xff800000 0x0 0x1000>;
		clocks = <&cru SCLK_PDM>, <&cru HCLK_PDM>;
		clock-names = "pdm_clk", "pdm_hclk";
		dmas = <&dmac 24>;
		dma-names = "rx";
		resets = <&cru SRST_PDM>;
		reset-names = "pdm-m";
		pinctrl-names = "default";
		pinctrl-0 = <&pdm_clk
			     &pdm_clk1
			     &pdm_sdi0
			     &pdm_sdi1
			     &pdm_sdi2
			     &pdm_sdi3>;
		status = "disabled";
	};

	vad: vad@ff810000 {
		compatible = "rockchip,rk1808-vad";
		reg = <0x0 0xff810000 0x0 0x10000>;
		reg-names = "vad";
		clocks = <&cru HCLK_VAD>;
		clock-names = "hclk";
		interrupts = <GIC_SPI 72 IRQ_TYPE_LEVEL_HIGH>;
		rockchip,audio-sram = <&vad_sram>;
		rockchip,audio-src = <0>;
		rockchip,det-channel = <0>;
		rockchip,mode = <1>;
		status = "disabled";
	};

	dfi: dfi@ff9c0000 {
		reg = <0x00 0xff9c0000 0x00 0x400>;
		compatible = "rockchip,rk1808-dfi";
		rockchip,pmugrf = <&pmugrf>;
		status = "disabled";
	};

	dmc: dmc {
		compatible = "rockchip,rk1808-dmc";
		dcf_reg = <&dcf>;
		interrupts = <GIC_SPI 0 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "complete_irq";
		devfreq-events = <&dfi>;
		clocks = <&cru SCLK_DDRCLK>;
		clock-names = "dmc_clk";
		operating-points-v2 = <&dmc_opp_table>;
		ddr_timing = <&ddr_timing>;
		upthreshold = <40>;
		downdifferential = <20>;
		system-status-freq = <
			/*system status         freq(KHz)*/
			SYS_STATUS_NORMAL       924000
			SYS_STATUS_REBOOT       450000
			SYS_STATUS_SUSPEND      328000
			SYS_STATUS_VIDEO_1080P  924000
			SYS_STATUS_BOOST        924000
			SYS_STATUS_ISP          924000
			SYS_STATUS_PERFORMANCE  924000
		>;
		auto-min-freq = <328000>;
		auto-freq-en = <0>;
		#cooling-cells = <2>;
		status = "disabled";
	};

	dmc_opp_table: dmc-opp-table {
		compatible = "operating-points-v2";

		rockchip,max-volt = <950000>;
		rockchip,evb-irdrop = <12500>;
		nvmem-cells = <&logic_leakage>;
		nvmem-cell-names = "leakage";
		rockchip,temp-hysteresis = <5000>;
		rockchip,low-temp = <0>;
		rockchip,low-temp-min-volt = <800000>;

		opp-192000000 {
			opp-hz = /bits/ 64 <192000000>;
			opp-microvolt = <800000>;
		};
		opp-324000000 {
			opp-hz = /bits/ 64 <324000000>;
			opp-microvolt = <800000>;
		};
		opp-450000000 {
			opp-hz = /bits/ 64 <450000000>;
			opp-microvolt = <800000>;
		};
		opp-528000000 {
			opp-hz = /bits/ 64 <528000000>;
			opp-microvolt = <800000>;
		};
		opp-664000000 {
			opp-hz = /bits/ 64 <664000000>;
			opp-microvolt = <800000>;
		};
		opp-784000000 {
			opp-hz = /bits/ 64 <784000000>;
			opp-microvolt = <800000>;
		};
		opp-924000000 {
			opp-hz = /bits/ 64 <924000000>;
			opp-microvolt = <800000>;
		};
		/* 1066M is only for ddr4 */
		opp-1066000000 {
			opp-hz = /bits/ 64 <1066000000>;
			opp-microvolt = <800000>;
			status = "disabled";
		};
	};

	rk_rga: rk_rga@ffaf0000 {
		compatible = "rockchip,rga2";
		dev_mode = <0>;
		reg = <0x0 0xffaf0000 0x0 0x1000>;
		interrupts = <GIC_SPI 60 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru ACLK_RGA>, <&cru HCLK_RGA>, <&cru SCLK_RGA>;
		clock-names = "aclk_rga", "hclk_rga", "clk_rga";
		power-domains = <&power RK1808_PD_VIO>;
		status = "disabled";
	};

	cif: cif@ffae0000 {
		compatible = "rockchip,rk1808-cif";
		reg = <0x0 0xffae0000 0x0 0x200>;
		reg-names = "cif_regs";
		interrupts = <GIC_SPI 56 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "cif-intr";
		clocks = <&cru ACLK_CIF>, <&cru DCLK_CIF>,
			 <&cru HCLK_CIF>, <&cru SCLK_CIF_OUT>;
		clock-names = "aclk_cif", "dclk_cif",
			"hclk_cif", "sclk_cif_out";
		resets = <&cru SRST_CIF_A>, <&cru SRST_CIF_H>,
			 <&cru SRST_CIF_I>, <&cru SRST_CIF_D>,
			 <&cru SRST_CIF_PCLKIN>;
		reset-names = "rst_cif_a", "rst_cif_h",
			"rst_cif_i", "rst_cif_d",
			"rst_cif_pclkin";
		power-domains = <&power RK1808_PD_VIO>;
		iommus = <&cif_mmu>;
		status = "disabled";
	};

	cif_mmu: iommu@ffae0800 {
		compatible = "rockchip,iommu";
		reg = <0x0 0xffae0800 0x0 0x100>;
		interrupts = <GIC_SPI 56 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "cif_mmu";
		clocks = <&cru ACLK_CIF>, <&cru HCLK_CIF>;
		clock-names = "aclk", "iface";
		power-domains = <&power RK1808_PD_VIO>;
		#iommu-cells = <0>;
		status = "disabled";
	};

	vop_lite: vop@ffb00000 {
		compatible = "rockchip,rk1808-vop-lit";
		reg = <0x0 0xffb00000 0x0 0x200>;
		reg-names = "regs";
		interrupts = <GIC_SPI 61 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru ACLK_VOPLITE>, <&cru DCLK_VOPLITE>,
			 <&cru HCLK_VOPLITE>;
		clock-names = "aclk_vop", "dclk_vop", "hclk_vop";
		power-domains = <&power RK1808_PD_VIO>;
		iommus = <&vopl_mmu>;
		status = "disabled";

		vop_lite_out: port {
			#address-cells = <1>;
			#size-cells = <0>;

			vop_lite_out_dsi: endpoint@0 {
				reg = <0>;
				remote-endpoint = <&dsi_in_vop_lite>;
			};

			vop_lite_out_rgb: endpoint@1 {
				reg = <1>;
				remote-endpoint = <&rgb_in_vop_lite>;
			};
		};
	};

	vopl_mmu: iommu@ffb00f00 {
		compatible = "rockchip,iommu";
		reg = <0x0 0xffb00f00 0x0 0x100>;
		interrupts = <GIC_SPI 61 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "vopl_mmu";
		clocks = <&cru ACLK_VOPLITE>, <&cru HCLK_VOPLITE>;
		clock-names = "aclk", "iface";
		power-domains = <&power RK1808_PD_VIO>;
		#iommu-cells = <0>;
		status = "disabled";
	};

	mipi_csi2_hw: mipi-csi2-hw@ffb10000 {
		compatible = "rockchip,rk1808-mipi-csi2-hw";
		reg = <0x0 0xffb10000 0x0 0x100>;
		reg-names = "csihost_regs";
		interrupts = <GIC_SPI 106 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 105 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "csi-intr1", "csi-intr2";
		clocks = <&cru PCLK_CSI2HOST>;
		clock-names = "pclk_csi2host";
		status = "disabled";
	};

	csi_tx: csi@ffb20000 {
		compatible = "rockchip,rk1808-mipi-csi";
		reg = <0x0 0xffb20000 0x0 0x500>;
		reg-names = "csi_regs";
		interrupts = <GIC_SPI 57 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru PCLK_CSI_TX>, <&mipi_dphy>;
		clock-names = "pclk", "hs_clk";
		resets = <&cru SRST_CSITX_P>,
			 <&cru SRST_CSITX_TXBYTEHS>,
			 <&cru SRST_CSITX_TXESC>,
			 <&cru SRST_CSITX_CAM>,
			 <&cru SRST_CSITX_I>;
		reset-names = "tx_apb", "tx_bytehs", "tx_esc", "tx_cam", "tx_i";
		phys = <&mipi_dphy>;
		phy-names = "mipi_dphy";
		power-domains = <&power RK1808_PD_VIO>;
		rockchip,grf = <&grf>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";

		ports {

			port {
				csi_in_vop_raw: endpoint {
					remote-endpoint = <&vop_raw_out_csi>;
				};
			};
		};
	};

	dsi: dsi@ffb30000 {
		compatible = "rockchip,rk1808-mipi-dsi";
		reg = <0x0 0xffb30000 0x0 0x500>;
		interrupts = <GIC_SPI 59 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru PCLK_DSI_TX>, <&mipi_dphy>;
		clock-names = "pclk", "hs_clk";
		resets = <&cru SRST_MIPIDSI_HOST_P>;
		reset-names = "apb";
		phys = <&mipi_dphy>;
		phy-names = "mipi_dphy";
		power-domains = <&power RK1808_PD_VIO>;
		rockchip,grf = <&grf>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";

		ports {
			port {
				dsi_in_vop_lite: endpoint {
					remote-endpoint = <&vop_lite_out_dsi>;
				};
			};
		};
	};

	vop_raw: vop@ffb40000 {
		compatible = "rockchip,rk1808-vop-raw";
		reg = <0x0 0xffb40000 0x0 0x500>;
		reg-names = "regs";
		interrupts = <GIC_SPI 62 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru ACLK_VOPRAW>, <&cru DCLK_VOPRAW>,
			 <&cru HCLK_VOPRAW>;
		clock-names = "aclk_vop", "dclk_vop", "hclk_vop";
		power-domains = <&power RK1808_PD_VIO>;
		iommus = <&vopr_mmu>;
		status = "disabled";

		vop_raw_out: port {
			#address-cells = <1>;
			#size-cells = <0>;

			vop_raw_out_csi: endpoint@0 {
				reg = <0>;
				remote-endpoint = <&csi_in_vop_raw>;
			};
		};
	};

	vopr_mmu: iommu@ffb40f00 {
		compatible = "rockchip,iommu";
		reg = <0x0 0xffb40f00 0x0 0x100>;
		interrupts = <GIC_SPI 62 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "vopr_mmu";
		clocks = <&cru ACLK_VOPRAW>, <&cru HCLK_VOPRAW>;
		clock-names = "aclk", "iface";
		power-domains = <&power RK1808_PD_VIO>;
		#iommu-cells = <0>;
		status = "disabled";
	};

	rkisp1: rkisp1@ffb50000 {
		compatible = "rockchip,rk1808-rkisp1";
		reg = <0x0 0xffb50000 0x0 0x8000>;
		interrupts = <GIC_SPI 97 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 96 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 95 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "isp_irq", "mi_irq", "mipi_irq";
		clocks = <&cru ACLK_ISP>, <&cru HCLK_ISP>,
			<&cru SCLK_ISP>, <&cru DCLK_CIF>;
		clock-names = "aclk_isp", "hclk_isp",
			"clk_isp", "pclk_isp";
		power-domains = <&power RK1808_PD_VIO>;
		iommus = <&isp_mmu>;
		rockchip,grf = <&grf>;
		status = "disabled";
	};

	isp_mmu: iommu@ffb58000 {
		compatible = "rockchip,iommu";
		reg = <0x0 0xffb58000 0x0 0x100>;
		interrupts = <GIC_SPI 97 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "isp_mmu";
		clocks = <&cru ACLK_ISP>, <&cru HCLK_ISP>,
			<&cru SCLK_ISP>;
		clock-names = "aclk", "iface", "sclk";
		power-domains = <&power RK1808_PD_VIO>;
		rk_iommu,disable_reset_quirk;
		#iommu-cells = <0>;
		status = "disabled";
	};

	vpu_service: vpu_service@ffb80000 {
		compatible = "rockchip,vpu_service";
		reg = <0x0 0xffb80000 0x0 0x800>;
		interrupts = <GIC_SPI 93 IRQ_TYPE_LEVEL_HIGH>,
				<GIC_SPI 94 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "irq_enc", "irq_dec";
		clocks = <&cru ACLK_VPU>, <&cru HCLK_VPU>;
		clock-names = "aclk_vcodec", "hclk_vcodec";
		power-domains = <&power RK1808_PD_VPU>;
		resets = <&cru SRST_VPU_A>, <&cru SRST_VPU_H>;
		reset-names = "video_a", "video_h";
		iommus = <&vpu_mmu>;
		iommu_enabled = <1>;
		allocator = <1>; /* 0 means ion, 1 means drm */
		status = "disabled";
	};

	vpu_mmu: iommu@ffb80800 {
		compatible = "rockchip,iommu";
		reg = <0x0 0xffb80800 0x0 0x100>;
		interrupts = <GIC_SPI 92 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "vpu_mmu";
		clocks = <&cru ACLK_VPU>, <&cru HCLK_VPU>;
		clock-names = "aclk", "iface";
		power-domains = <&power RK1808_PD_VPU>;
		#iommu-cells = <0>;
		status = "disabled";
	};

	sdio: dwmmc@ffc60000 {
		compatible = "rockchip,rk1808-dw-mshc", "rockchip,rk3288-dw-mshc";
		reg = <0x0 0xffc60000 0x0 0x4000>;
		clocks = <&cru HCLK_SDIO>, <&cru SCLK_SDIO>,
			 <&cru SCLK_SDIO_DRV>, <&cru SCLK_SDIO_SAMPLE>;
		clock-names = "biu", "ciu", "ciu-drive", "ciu-sample";
		max-frequency = <150000000>;
		fifo-depth = <0x100>;
		interrupts = <GIC_SPI 49 IRQ_TYPE_LEVEL_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&sdmmc1_clk &sdmmc1_cmd &sdmmc1_bus4>;
		status = "disabled";
	};

	npu: npu@ffbc0000 {
		compatible = "rockchip,npu";
		reg = <0x0 0xffbc0000 0x0 0x1000>;
		clocks =  <&cru SCLK_NPU>, <&cru ACLK_NPU>, <&cru HCLK_NPU>;
		clock-names = "sclk_npu", "aclk_npu", "hclk_npu";
		assigned-clocks = <&cru SCLK_NPU>;
		assigned-clock-rates = <800000000>;
		interrupts = <GIC_SPI 43 IRQ_TYPE_LEVEL_HIGH>;
		power-domains = <&power RK1808_VD_NPU>;
		operating-points-v2 = <&npu_opp_table>;
		#cooling-cells = <2>;
		status = "disabled";

		npu_power_model: power-model {
			compatible = "simple-power-model";
			ref-leakage = <31>;
			static-coefficient = <100000>;
			dynamic-coefficient = <3080>;
			ts = <88610 303120 (-5000) 100>;
			thermal-zone = "soc-thermal";
		};
	};

	npu_opp_table: npu-opp-table {
		compatible = "operating-points-v2";

		rockchip,thermal-zone = "soc-thermal";
		rockchip,temp-hysteresis = <5000>;
		rockchip,low-temp = <0>;
		rockchip,low-temp-min-volt = <800000>;
		rockchip,low-temp-adjust-volt = <
			/* MHz    MHz    uV */
			   0      792   50000
		>;

		rockchip,max-volt = <880000>;
		rockchip,evb-irdrop = <37500>;
		nvmem-cells = <&npu_leakage>;
		nvmem-cell-names = "leakage";

		rockchip,pvtm-voltage-sel = <
			0        69000   0
			69001    74000   1
			74001    99999   2
		>;
		rockchip,pvtm-ch = <0 0>;

		opp-200000000 {
			opp-hz = /bits/ 64 <200000000>;
			opp-microvolt = <750000 750000 880000>;
		};
		opp-297000000 {
			opp-hz = /bits/ 64 <297000000>;
			opp-microvolt = <750000 750000 880000>;
		};
		opp-400000000 {
			opp-hz = /bits/ 64 <400000000>;
			opp-microvolt = <750000 750000 880000>;
		};
		opp-594000000 {
			opp-hz = /bits/ 64 <594000000>;
			opp-microvolt = <750000 750000 880000>;
		};
		opp-792000000 {
			opp-hz = /bits/ 64 <792000000>;
			opp-microvolt = <850000 850000 880000>;
			opp-microvolt-L0 = <850000 850000 880000>;
			opp-microvolt-L1 = <825000 825000 880000>;
			opp-microvolt-L2 = <800000 800000 880000>;
		};
	};

	sfc: sfc@ffc50000 {
		compatible = "rockchip,sfc";
		reg = <0x0 0xffc50000 0x0 0x4000>;
		interrupts = <GIC_SPI 50 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru SCLK_SFC>, <&cru HCLK_SFC>;
		clock-names = "clk_sfc", "hclk_sfc";
		assigned-clocks = <&cru SCLK_SFC>;
		assigned-clock-rates = <100000000>;
		status = "disabled";
	};

	sdmmc: dwmmc@ffcf0000 {
		compatible = "rockchip,rk1808-dw-mshc", "rockchip,rk3288-dw-mshc";
		reg = <0x0 0xffcf0000 0x0 0x4000>;
		clocks = <&cru HCLK_SDMMC>, <&cru SCLK_SDMMC>,
			 <&cru SCLK_SDMMC_DRV>, <&cru SCLK_SDMMC_SAMPLE>;
		clock-names = "biu", "ciu", "ciu-drive", "ciu-sample";
		max-frequency = <150000000>;
		fifo-depth = <0x100>;
		interrupts = <GIC_SPI 48 IRQ_TYPE_LEVEL_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&sdmmc0_clk &sdmmc0_cmd &sdmmc0_bus4 &sdmmc0_detn>;
		status = "disabled";
	};

	emmc: dwmmc@ffd00000 {
		compatible = "rockchip,rk1808-dw-mshc", "rockchip,rk3288-dw-mshc";
		reg = <0x0 0xffd00000 0x0 0x4000>;
		clocks = <&cru HCLK_EMMC>, <&cru SCLK_EMMC>,
			 <&cru SCLK_EMMC_DRV>, <&cru SCLK_EMMC_SAMPLE>;
		clock-names = "biu", "ciu", "ciu-drive", "ciu-sample";
		max-frequency = <150000000>;
		fifo-depth = <0x100>;
		interrupts = <GIC_SPI 47 IRQ_TYPE_LEVEL_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&emmc_clk &emmc_cmd &emmc_bus8>;
		status = "disabled";
	};

	usb_host0_ehci: usb@ffd80000 {
		compatible = "generic-ehci";
		reg = <0x0 0xffd80000 0x0 0x10000>;
		interrupts = <GIC_SPI 53 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru HCLK_HOST>, <&cru HCLK_HOST_ARB>,
			 <&u2phy>;
		clock-names = "usbhost", "arbiter", "utmi";
		phys = <&u2phy_host>;
		phy-names = "usb";
		status = "disabled";
		power-domains = <&power RK1808_PD_PCIE>;
	};

	usb_host0_ohci: usb@ffd90000 {
		compatible = "generic-ohci";
		reg = <0x0 0xffd90000 0x0 0x10000>;
		interrupts = <GIC_SPI 54 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&cru HCLK_HOST>, <&cru HCLK_HOST_ARB>,
			 <&u2phy>;
		clock-names = "usbhost", "arbiter", "utmi";
		phys = <&u2phy_host>;
		phy-names = "usb";
		status = "disabled";
		power-domains = <&power RK1808_PD_PCIE>;
	};

	gmac: ethernet@ffdd0000 {
		compatible = "rockchip,rk1808-gmac";
		reg = <0x0 0xffdd0000 0x0 0x10000>;
		rockchip,grf = <&grf>;
		interrupts = <GIC_SPI 39 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "macirq";
		clocks = <&cru SCLK_GMAC>, <&cru SCLK_GMAC_RX_TX>,
			 <&cru SCLK_GMAC_RX_TX>, <&cru SCLK_GMAC_REF>,
			 <&cru SCLK_GMAC_REFOUT>, <&cru ACLK_GMAC>,
			 <&cru PCLK_GMAC>, <&cru SCLK_GMAC_RGMII_SPEED>;
		clock-names = "stmmaceth", "mac_clk_rx",
			      "mac_clk_tx", "clk_mac_ref",
			      "clk_mac_refout", "aclk_mac",
			      "pclk_mac", "clk_mac_speed";
		phy-mode = "rgmii";
		pinctrl-names = "default";
		pinctrl-0 = <&rgmii_pins>;
		resets = <&cru SRST_GAMC_A>;
		reset-names = "stmmaceth";
		/* power-domains = <&power RK1808_PD_GMAC>; */
		status = "disabled";
	};

	rockchip_system_monitor: rockchip-system-monitor {
		compatible = "rockchip,system-monitor";

		rockchip,thermal-zone = "soc-thermal";
		rockchip,polling-delay = <200>; /* milliseconds */
	};

	pinctrl: pinctrl {
		compatible = "rockchip,rk1808-pinctrl";
		rockchip,grf = <&grf>;
		rockchip,pmu = <&pmugrf>;
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;

		gpio0: gpio0@ff4c0000 {
			compatible = "rockchip,gpio-bank";
			reg = <0x0 0xff4c0000 0x0 0x100>;
			interrupts = <GIC_SPI 3 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cru PCLK_GPIO0_PMU>, <&cru DBCLK_PMU_GPIO0>;
			gpio-controller;
			#gpio-cells = <2>;

			interrupt-controller;
			#interrupt-cells = <2>;
		};

		gpio1: gpio1@ff690000 {
			compatible = "rockchip,gpio-bank";
			reg = <0x0 0xff690000 0x0 0x100>;
			interrupts = <GIC_SPI 4 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cru PCLK_GPIO1>, <&cru DBCLK_GPIO1>;
			gpio-controller;
			#gpio-cells = <2>;

			interrupt-controller;
			#interrupt-cells = <2>;
		};

		gpio2: gpio2@ff6a0000 {
			compatible = "rockchip,gpio-bank";
			reg = <0x0 0xff6a0000 0x0 0x100>;
			interrupts = <GIC_SPI 5 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cru PCLK_GPIO2>, <&cru DBCLK_GPIO2>;
			gpio-controller;
			#gpio-cells = <2>;

			interrupt-controller;
			#interrupt-cells = <2>;
		};

		gpio3: gpio3@ff6b0000 {
			compatible = "rockchip,gpio-bank";
			reg = <0x0 0xff6b0000 0x0 0x100>;
			interrupts = <GIC_SPI 6 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cru PCLK_GPIO3>, <&cru DBCLK_GPIO3>;
			gpio-controller;
			#gpio-cells = <2>;

			interrupt-controller;
			#interrupt-cells = <2>;
		};

		gpio4: gpio4@ff6c0000 {
			compatible = "rockchip,gpio-bank";
			reg = <0x0 0xff6c0000 0x0 0x100>;
			interrupts = <GIC_SPI 82 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cru PCLK_GPIO4>, <&cru DBCLK_GPIO4>;
			gpio-controller;
			#gpio-cells = <2>;

			interrupt-controller;
			#interrupt-cells = <2>;
		};

		pcfg_pull_up: pcfg-pull-up {
			bias-pull-up;
		};

		pcfg_pull_down: pcfg-pull-down {
			bias-pull-down;
		};

		pcfg_pull_none: pcfg-pull-none {
			bias-disable;
		};

		pcfg_pull_none_2ma: pcfg-pull-none-2ma {
			bias-disable;
			drive-strength = <2>;
		};

		pcfg_pull_up_2ma: pcfg-pull-up-2ma {
			bias-pull-up;
			drive-strength = <2>;
		};

		pcfg_pull_up_4ma: pcfg-pull-up-4ma {
			bias-pull-up;
			drive-strength = <4>;
		};

		pcfg_pull_none_4ma: pcfg-pull-none-4ma {
			bias-disable;
			drive-strength = <4>;
		};

		pcfg_pull_down_4ma: pcfg-pull-down-4ma {
			bias-pull-down;
			drive-strength = <4>;
		};

		pcfg_pull_none_8ma: pcfg-pull-none-8ma {
			bias-disable;
			drive-strength = <8>;
		};

		pcfg_pull_up_8ma: pcfg-pull-up-8ma {
			bias-pull-up;
			drive-strength = <8>;
		};

		pcfg_pull_none_12ma: pcfg-pull-none-12ma {
			bias-disable;
			drive-strength = <12>;
		};

		pcfg_pull_up_12ma: pcfg-pull-up-12ma {
			bias-pull-up;
			drive-strength = <12>;
		};

		pcfg_pull_none_smt: pcfg-pull-none-smt {
			bias-disable;
			input-schmitt-enable;
		};

		pcfg_pull_none_2ma_smt: pcfg-pull-none-2ma-smt {
			bias-disable;
			drive-strength = <2>;
			input-schmitt-enable;
		};

		pcfg_output_high: pcfg-output-high {
			output-high;
		};

		pcfg_output_low: pcfg-output-low {
			output-low;
		};

		pcfg_input_high: pcfg-input-high {
			bias-pull-up;
			input-enable;
		};

		pcfg_input: pcfg-input {
			input-enable;
		};

		pcfg_input_smt: pcfg-input-smt {
			input-enable;
			input-schmitt-enable;
		};

		cif-m0 {
			cif_clkout_m0: cif-clkout-m0 {
				rockchip,pins =
					<2 RK_PB7 1 &pcfg_pull_none>;
			};

			cif_d12d15_m0: cif-d12d15-m0 {
				rockchip,pins =
					<2 RK_PA0 1 &pcfg_pull_none>,/* cif_d12 */
					<2 RK_PA1 1 &pcfg_pull_none>,/* cif_d13 */
					<2 RK_PA2 1 &pcfg_pull_none>,/* cif_d14 */
					<2 RK_PA3 1 &pcfg_pull_none>;/* cif_d15 */
			};

			cif_d10d11_m0: cif-d10d11-m0 {
				rockchip,pins =
					<2 RK_PC2 1 &pcfg_pull_none>,/* cif_d10 */
					<2 RK_PC3 1 &pcfg_pull_none>;/* cif_d11 */
			};

			cif_d2d9_m0: cif-d2d9-m0 {
				rockchip,pins =
					<2 RK_PA4 1 &pcfg_pull_none>,/* cif_d2 */
					<2 RK_PA5 1 &pcfg_pull_none>,/* cif_d3 */
					<2 RK_PA6 1 &pcfg_pull_none>,/* cif_d4 */
					<2 RK_PA7 1 &pcfg_pull_none>,/* cif_d5 */
					<2 RK_PB0 1 &pcfg_pull_none>,/* cif_d6 */
					<2 RK_PB1 1 &pcfg_pull_none>,/* cif_d7 */
					<2 RK_PB2 1 &pcfg_pull_none>,/* cif_d8 */
					<2 RK_PB3 1 &pcfg_pull_none>,/* cif_d9 */
					<2 RK_PB4 1 &pcfg_pull_none>,/* cif_vsync */
					<2 RK_PB5 1 &pcfg_pull_none>,/* cif_href */
					<2 RK_PB6 1 &pcfg_pull_none>;/* cif_clkin */
			};

			cif_d0d1_m0: cif-d0d1-m0 {
				rockchip,pins =
					<2 RK_PC0 1 &pcfg_pull_none>,/* cif_d0 */
					<2 RK_PC1 1 &pcfg_pull_none>;/* cif_d1 */
			};
		};

		emmc {
			emmc_clk: emmc-clk {
				rockchip,pins =
					/* emmc_clkout */
					<1 RK_PB1 1 &pcfg_pull_up_4ma>;
			};

			emmc_rstnout: emmc-rstnout {
				rockchip,pins =
					/* emmc_rstn */
					<1 RK_PB3 1 &pcfg_pull_none>;
			};

			emmc_bus8: emmc-bus8 {
				rockchip,pins =
					/* emmc_d0 */
					<1 RK_PA0 1 &pcfg_pull_up_4ma>,
					/* emmc_d1 */
					<1 RK_PA1 1 &pcfg_pull_up_4ma>,
					/* emmc_d2 */
					<1 RK_PA2 1 &pcfg_pull_up_4ma>,
					/* emmc_d3 */
					<1 RK_PA3 1 &pcfg_pull_up_4ma>,
					/* emmc_d4 */
					<1 RK_PA4 1 &pcfg_pull_up_4ma>,
					/* emmc_d5 */
					<1 RK_PA5 1 &pcfg_pull_up_4ma>,
					/* emmc_d6 */
					<1 RK_PA6 1 &pcfg_pull_up_4ma>,
					/* emmc_d7 */
					<1 RK_PA7 1 &pcfg_pull_up_4ma>;
			};

			emmc_pwren: emmc-pwren {
				rockchip,pins =
					<1 RK_PB0 1 &pcfg_pull_none>;
			};

			emmc_cmd: emmc-cmd {
				rockchip,pins =
					<1 RK_PB2 1 &pcfg_pull_up_4ma>;
			};
		};

		gmac {
			rgmii_pins: rgmii-pins {
				rockchip,pins =
					/* rgmii_txen */
					<2 RK_PA1 2 &pcfg_pull_none_4ma>,
					/* rgmii_txd1 */
					<2 RK_PA2 2 &pcfg_pull_none_4ma>,
					/* rgmii_txd0 */
					<2 RK_PA3 2 &pcfg_pull_none_4ma>,
					/* rgmii_rxd0 */
					<2 RK_PA4 2 &pcfg_pull_none>,
					/* rgmii_rxd1 */
					<2 RK_PA5 2 &pcfg_pull_none>,
					/* rgmii_rxdv */
					<2 RK_PA7 2 &pcfg_pull_none>,
					/* rgmii_mdio */
					<2 RK_PB0 2 &pcfg_pull_none_2ma>,
					/* rgmii_mdc */
					<2 RK_PB2 2 &pcfg_pull_none_2ma>,
					/* rgmii_txd3 */
					<2 RK_PB3 2 &pcfg_pull_none_4ma>,
					/* rgmii_txd2 */
					<2 RK_PB4 2 &pcfg_pull_none_4ma>,
					/* rgmii_rxd2 */
					<2 RK_PB5 2 &pcfg_pull_none>,
					/* rgmii_rxd3 */
					<2 RK_PB6 2 &pcfg_pull_none>,
					/* rgmii_clk */
					<2 RK_PB7 2 &pcfg_pull_none>,
					/* rgmii_txclk */
					<2 RK_PC1 2 &pcfg_pull_none_4ma>,
					/* rgmii_rxclk */
					<2 RK_PC2 2 &pcfg_pull_none>;
			};

			rmii_pins: rmii-pins {
				rockchip,pins =
					/* rmii_txen */
					<2 RK_PA1 2 &pcfg_pull_none_4ma>,
					/* rmii_txd1 */
					<2 RK_PA2 2 &pcfg_pull_none_4ma>,
					/* rmii_txd0 */
					<2 RK_PA3 2 &pcfg_pull_none_4ma>,
					/* rmii_rxd0 */
					<2 RK_PA4 2 &pcfg_pull_none>,
					/* rmii_rxd1 */
					<2 RK_PA5 2 &pcfg_pull_none>,
					/* rmii_rxer */
					<2 RK_PA6 2 &pcfg_pull_none>,
					/* rmii_rxdv */
					<2 RK_PA7 2 &pcfg_pull_none>,
					/* rmii_mdio */
					<2 RK_PB0 2 &pcfg_pull_none_2ma>,
					/* rmii_mdc */
					<2 RK_PB2 2 &pcfg_pull_none_2ma>,
					/* rmii_clk */
					<2 RK_PB7 2 &pcfg_pull_none>;
			};
		};

		i2c0 {
			i2c0_xfer: i2c0-xfer {
				rockchip,pins =
					/* i2c0_sda */
					<0 RK_PB1 1 &pcfg_pull_none_2ma_smt>,
					/* i2c0_scl */
					<0 RK_PB0 1 &pcfg_pull_none_2ma_smt>;
			};
		};

		i2c1 {
			i2c1_xfer: i2c1-xfer {
				rockchip,pins =
					/* i2c1_sda */
					<0 RK_PC1 1 &pcfg_pull_none_2ma_smt>,
					/* i2c1_scl */
					<0 RK_PC0 1 &pcfg_pull_none_2ma_smt>;
			};
		};

		i2c2m0 {
			i2c2m0_xfer: i2c2m0-xfer {
				rockchip,pins =
					/* i2c2m0_sda */
					<3 RK_PB4 2 &pcfg_pull_none_2ma_smt>,
					/* i2c2m0_scl */
					<3 RK_PB3 2 &pcfg_pull_none_2ma_smt>;
			};
		};

		i2c2m1 {
			i2c2m1_xfer: i2c2m1-xfer {
				rockchip,pins =
					/* i2c2m1_sda */
					<1 RK_PB5 2 &pcfg_pull_none_2ma_smt>,
					/* i2c2m1_scl */
					<1 RK_PB4 2 &pcfg_pull_none_2ma_smt>;
			};
		};

		i2c3 {
			i2c3_xfer: i2c3-xfer {
				rockchip,pins =
					/* i2c3_sda */
					<2 RK_PD1 1 &pcfg_pull_none_2ma_smt>,
					/* i2c3_scl */
					<2 RK_PD0 1 &pcfg_pull_none_2ma_smt>;
			};
		};

		i2c4 {
			i2c4_xfer: i2c4-xfer {
				rockchip,pins =
					/* i2c4_sda */
					<3 RK_PC3 3 &pcfg_pull_none_2ma_smt>,
					/* i2c4_scl */
					<3 RK_PC2 3 &pcfg_pull_none_2ma_smt>;
			};
		};

		i2c5 {
			i2c5_xfer: i2c5-xfer {
				rockchip,pins =
					/* i2c5_sda */
					<4 RK_PC2 1 &pcfg_pull_none_2ma_smt>,
					/* i2c5_scl */
					<4 RK_PC1 1 &pcfg_pull_none_2ma_smt>;
			};
		};

		i2s1 {
			i2s1_2ch_lrck: i2s1-2ch-lrck {
				rockchip,pins =
					<3 RK_PA0 1 &pcfg_pull_none_2ma_smt>;
			};
			i2s1_2ch_sclk: i2s1-2ch-sclk {
				rockchip,pins =
					<3 RK_PA1 1 &pcfg_pull_none_2ma_smt>;
			};
			i2s1_2ch_mclk: i2s1-2ch-mclk {
				rockchip,pins =
					<3 RK_PA2 1 &pcfg_pull_none_2ma_smt>;
			};
			i2s1_2ch_sdo: i2s1-2ch-sdo {
				rockchip,pins =
					<3 RK_PA3 1 &pcfg_pull_none_2ma>;
			};
			i2s1_2ch_sdi: i2s1-2ch-sdi {
				rockchip,pins =
					<3 RK_PA4 1 &pcfg_pull_none_2ma>;
			};
		};

		i2s0 {
			i2s0_8ch_sdi3: i2s0-8ch-sdi3 {
				rockchip,pins =
					<3 RK_PA5 1 &pcfg_pull_none_2ma>;
			};
			i2s0_8ch_sdi2: i2s0-8ch-sdi2 {
				rockchip,pins =
					<3 RK_PA6 1 &pcfg_pull_none_2ma>;
			};
			i2s0_8ch_sdi1: i2s0-8ch-sdi1 {
				rockchip,pins =
					<3 RK_PA7 1 &pcfg_pull_none_2ma>;
			};
			i2s0_8ch_sclkrx: i2s0-8ch-sclkrx {
				rockchip,pins =
					<3 RK_PB0 1 &pcfg_pull_none_2ma_smt>;
			};
			i2s0_8ch_lrckrx: i2s0-8ch-lrckrx {
				rockchip,pins =
					<3 RK_PB1 1 &pcfg_pull_none_2ma_smt>;
			};
			i2s0_8ch_sdo3: i2s0-8ch-sdo3 {
				rockchip,pins =
					<3 RK_PB2 1 &pcfg_pull_none_2ma>;
			};
			i2s0_8ch_sdo2: i2s0-8ch-sdo2 {
				rockchip,pins =
					<3 RK_PB3 1 &pcfg_pull_none_2ma>;
			};
			i2s0_8ch_sdo1: i2s0-8ch-sdo1 {
				rockchip,pins =
					<3 RK_PB4 1 &pcfg_pull_none_2ma>;
			};
			i2s0_8ch_mclk: i2s0-8ch-mclk {
				rockchip,pins =
					<3 RK_PB5 1 &pcfg_pull_none_2ma_smt>;
			};
			i2s0_8ch_lrcktx: i2s0-8ch-lrcktx {
				rockchip,pins =
					<3 RK_PB6 1 &pcfg_pull_none_2ma_smt>;
			};
			i2s0_8ch_sclktx: i2s0-8ch-sclktx {
				rockchip,pins =
					<3 RK_PB7 1 &pcfg_pull_none_2ma_smt>;
			};
			i2s0_8ch_sdo0: i2s0-8ch-sdo0 {
				rockchip,pins =
					<3 RK_PC0 1 &pcfg_pull_none_2ma>;
			};
			i2s0_8ch_sdi0: i2s0-8ch-sdi0 {
				rockchip,pins =
					<3 RK_PC1 1 &pcfg_pull_none_2ma>;
			};
		};

		lcdc {
			lcdc_rgb_dclk_pin: lcdc-rgb-dclk-pin {
				rockchip,pins =
					/* lcdc_clkm0 */
					<2 RK_PC6 3 &pcfg_pull_none>;
			};

			lcdc_rgb_den_pin: lcdc-rgb-den-pin {
				rockchip,pins =
					/* lcdc_denm0 */
					<2 RK_PC7 3 &pcfg_pull_none>;
			};

			lcdc_rgb_m0_hsync_pin: lcdc-rgb-m0-hsync-pin {
				rockchip,pins =
					/* lcdc_hsyncm0 */
					<2 RK_PB2 3 &pcfg_pull_none>;
			};

			lcdc_rgb_m0_vsync_pin: lcdc-rgb-m0-vsync-pin {
				rockchip,pins =
					/* lcdc_vsyncm0 */
					<2 RK_PB3 3 &pcfg_pull_none>;
			};

			lcdc_rgb_m1_hsync_pin: lcdc-rgb-m1-hsync-pin {
				rockchip,pins =
					/* lcdc_hsyncm1 */
					<3 RK_PB2 3 &pcfg_pull_none>;
			};

			lcdc_rgb_m1_vsync_pin: lcdc-rgb-m1-vsync-pin {
				rockchip,pins =
					/* lcdc_vsyncm1 */
					<3 RK_PB3 3 &pcfg_pull_none>;
			};

			lcdc_rgb666_data_pins: lcdc-rgb666-data-pins {
				rockchip,pins =
					/* lcdc_d0m0 */
					<2 RK_PA2 3 &pcfg_pull_none>,
					/* lcdc_d1m0 */
					<2 RK_PA3 3 &pcfg_pull_none>,
					/* lcdc_d2m0 */
					<2 RK_PC2 3 &pcfg_pull_none>,
					/* lcdc_d3m0 */
					<2 RK_PC3 3 &pcfg_pull_none>,
					/* lcdc_d4m0 */
					<2 RK_PC4 3 &pcfg_pull_none>,
					/* lcdc_d5m0 */
					<2 RK_PC5 3 &pcfg_pull_none>,
					/* lcdc_d6m0 */
					<2 RK_PA0 3 &pcfg_pull_none>,
					/* lcdc_d7m0 */
					<2 RK_PA1 3 &pcfg_pull_none>,
					/* lcdc_d8 */
					<3 RK_PC2 1 &pcfg_pull_none>,
					/* lcdc_d9 */
					<3 RK_PC3 1 &pcfg_pull_none>,
					/* lcdc_d10 */
					<3 RK_PC4 1 &pcfg_pull_none>,
					/* lcdc_d11 */
					<3 RK_PC5 1 &pcfg_pull_none>,
					/* lcdc_d12 */
					<3 RK_PC6 1 &pcfg_pull_none>,
					/* lcdc_d13 */
					<3 RK_PC7 1 &pcfg_pull_none>,
					/* lcdc_d14 */
					<3 RK_PD0 1 &pcfg_pull_none>,
					/* lcdc_d15 */
					<3 RK_PD1 1 &pcfg_pull_none>,
					/* lcdc_d16 */
					<3 RK_PD2 1 &pcfg_pull_none>,
					/* lcdc_d17 */
					<3 RK_PD3 1 &pcfg_pull_none>;
			};

			lcdc_rgb565_data_pins: lcdc-rgb565-data-pins {
				rockchip,pins =
					/* lcdc_d0m0 */
					<2 RK_PA2 3 &pcfg_pull_none>,
					/* lcdc_d1m0 */
					<2 RK_PA3 3 &pcfg_pull_none>,
					/* lcdc_d2m0 */
					<2 RK_PC2 3 &pcfg_pull_none>,
					/* lcdc_d3m0 */
					<2 RK_PC3 3 &pcfg_pull_none>,
					/* lcdc_d4m0 */
					<2 RK_PC4 3 &pcfg_pull_none>,
					/* lcdc_d5m0 */
					<2 RK_PC5 3 &pcfg_pull_none>,
					/* lcdc_d6m0 */
					<2 RK_PA0 3 &pcfg_pull_none>,
					/* lcdc_d7m0 */
					<2 RK_PA1 3 &pcfg_pull_none>,
					/* lcdc_d8 */
					<3 RK_PC2 1 &pcfg_pull_none>,
					/* lcdc_d9 */
					<3 RK_PC3 1 &pcfg_pull_none>,
					/* lcdc_d10 */
					<3 RK_PC4 1 &pcfg_pull_none>,
					/* lcdc_d11 */
					<3 RK_PC5 1 &pcfg_pull_none>,
					/* lcdc_d12 */
					<3 RK_PC6 1 &pcfg_pull_none>,
					/* lcdc_d13 */
					<3 RK_PC7 1 &pcfg_pull_none>,
					/* lcdc_d14 */
					<3 RK_PD0 1 &pcfg_pull_none>,
					/* lcdc_d15 */
					<3 RK_PD1 1 &pcfg_pull_none>;
			};
		};

		pciusb {
			pciusb_pins: pciusb-pins {
				rockchip,pins =
					/* pciusb_debug0 */
					<4 RK_PB4 3 &pcfg_pull_none>,
					/* pciusb_debug1 */
					<4 RK_PB5 3 &pcfg_pull_none>,
					/* pciusb_debug2 */
					<4 RK_PB6 3 &pcfg_pull_none>,
					/* pciusb_debug3 */
					<4 RK_PB7 3 &pcfg_pull_none>,
					/* pciusb_debug4 */
					<4 RK_PC0 3 &pcfg_pull_none>,
					/* pciusb_debug5 */
					<4 RK_PC1 3 &pcfg_pull_none>,
					/* pciusb_debug6 */
					<4 RK_PC2 3 &pcfg_pull_none>,
					/* pciusb_debug7 */
					<4 RK_PC3 3 &pcfg_pull_none>;
			};

			pcie_clkreq: pcie-clkreq {
				rockchip,pins =
					/* pcie_clkreqn_m1 */
					<0 RK_PC6 1 &pcfg_pull_none >;
			};
		};

		pdm {
			pdm_clk: pdm-clk {
				rockchip,pins =
					/* pdm_clk0 */
					<3 RK_PB0 2 &pcfg_pull_none_2ma>;
			};

			pdm_sdi3: pdm-sdi3 {
				rockchip,pins =
					<3 RK_PA5 2 &pcfg_pull_none_2ma>;
			};

			pdm_sdi2: pdm-sdi2 {
				rockchip,pins =
					<3 RK_PA6 2 &pcfg_pull_none_2ma>;
			};

			pdm_sdi1: pdm-sdi1 {
				rockchip,pins =
					<3 RK_PA7 2 &pcfg_pull_none_2ma>;
			};

			pdm_clk1: pdm-clk1 {
				rockchip,pins =
					<3 RK_PB1 2 &pcfg_pull_none_2ma>;
			};

			pdm_sdi0: pdm-sdi0 {
				rockchip,pins =
					<3 RK_PC1 2 &pcfg_pull_none_2ma>;
			};
		};

		pwm0 {
			pwm0_pin: pwm0-pin {
				rockchip,pins =
					<0 RK_PB7 1 &pcfg_pull_none_2ma>;
			};
		};

		pwm1 {
			pwm1_pin: pwm1-pin {
				rockchip,pins =
					<0 RK_PC3 1 &pcfg_pull_none_2ma>;
			};
		};

		pwm2 {
			pwm2_pin: pwm2-pin {
				rockchip,pins =
					<0 RK_PC5 1 &pcfg_pull_none_2ma>;
			};
		};

		pwm3 {
			pwm3_pin: pwm3-pin {
				rockchip,pins =
					<0 RK_PC4 1 &pcfg_pull_none_2ma>;
			};
		};

		pwm4 {
			pwm4_pin: pwm4-pin {
				rockchip,pins =
					<1 RK_PB6 2 &pcfg_pull_none_2ma>;
			};
		};

		pwm5 {
			pwm5_pin: pwm5-pin {
				rockchip,pins =
					<1 RK_PB7 2 &pcfg_pull_none_2ma>;
			};
		};
		pwm6 {
			pwm6_pin: pwm6-pin {
				rockchip,pins =
					<3 RK_PA1 2 &pcfg_pull_none_2ma>;
			};
		};

		pwm7 {
			pwm7_pin: pwm7-pin {
				rockchip,pins =
					<3 RK_PA2 2 &pcfg_pull_none_2ma>;
			};
		};

		pwm8 {
			pwm8_pin: pwm8-pin {
				rockchip,pins =
					<3 RK_PD0 2 &pcfg_pull_none_2ma>;
			};
		};

		pwm9 {
			pwm9_pin: pwm9-pin {
				rockchip,pins =
					<3 RK_PD1 2 &pcfg_pull_none_2ma>;
			};
		};

		pwm10 {
			pwm10_pin: pwm10-pin {
				rockchip,pins =
					<3 RK_PD2 2 &pcfg_pull_none_2ma>;
			};
		};

		pwm11 {
			pwm11_pin: pwm11-pin {
				rockchip,pins =
					<3 RK_PD3 2 &pcfg_pull_none_2ma>;
			};
		};

		sdmmc0 {
			sdmmc0_bus4: sdmmc0-bus4 {
				rockchip,pins =
				/* sdmmc0_d0 */
				<4 RK_PA2 1 &pcfg_pull_up_8ma>,
				/* sdmmc0_d1 */
				<4 RK_PA3 1 &pcfg_pull_up_8ma>,
				/* sdmmc0_d2 */
				<4 RK_PA4 1 &pcfg_pull_up_8ma>,
				/* sdmmc0_d3 */
				<4 RK_PA5 1 &pcfg_pull_up_8ma>;
			};

			sdmmc0_cmd: sdmmc0-cmd {
				rockchip,pins =
					<4 RK_PA0 1 &pcfg_pull_up_8ma>;
			};

			sdmmc0_clk: sdmmc0-clk {
				rockchip,pins =
					<4 RK_PA1 1 &pcfg_pull_up_8ma>;
			};

			sdmmc0_detn: sdmmc0-detn {
				rockchip,pins =
					<0 RK_PA3 1 &pcfg_pull_none>;
			};
		};

		sdmmc1 {
			sdmmc1_bus4: sdmmc1-bus4 {
				rockchip,pins =
				/* sdmmc1_d0 */
				<4 RK_PB0 1 &pcfg_pull_up_4ma>,
				/* sdmmc1_d1 */
				<4 RK_PB1 1 &pcfg_pull_up_4ma>,
				/* sdmmc1_d2 */
				<4 RK_PB2 1 &pcfg_pull_up_4ma>,
				/* sdmmc1_d3 */
				<4 RK_PB3 1 &pcfg_pull_up_4ma>;
			};

			sdmmc1_cmd: sdmmc1-cmd {
				rockchip,pins =
					<4 RK_PA6 1 &pcfg_pull_up_4ma>;
			};

			sdmmc1_clk: sdmmc1-clk {
				rockchip,pins =
					<4 RK_PA7 1 &pcfg_pull_up_4ma>;
			};
		};

		spi0 {
			spi0_mosi: spi0-mosi {
				rockchip,pins =
					<1 RK_PB4 1 &pcfg_pull_up_2ma>;
			};

			spi0_miso: spi0-miso {
				rockchip,pins =
					<1 RK_PB5 1 &pcfg_pull_up_2ma>;
			};

			spi0_csn: spi0-csn {
				rockchip,pins =
					<1 RK_PB6 1 &pcfg_pull_up_2ma>;
			};

			spi0_clk: spi0-clk {
				rockchip,pins =
					<1 RK_PB7 1 &pcfg_pull_up_2ma>;
			};

			spi0_mosi_hs: spi0-mosi-hs {
				rockchip,pins =
					<1 RK_PB4 1 &pcfg_pull_up_2ma>;
			};

			spi0_miso_hs: spi0-miso-hs {
				rockchip,pins =
					<1 RK_PB5 1 &pcfg_pull_up_2ma>;
			};

			spi0_csn_hs: spi0-csn-hs {
				rockchip,pins =
					<1 RK_PB6 1 &pcfg_pull_up_2ma>;
			};

			spi0_clk_hs: spi0-clk-hs {
				rockchip,pins =
					<1 RK_PB7 1 &pcfg_pull_up_2ma>;
			};
		};

		spi1m0 {
			spi1_clk: spi1-clk {
				rockchip,pins =
					<4 RK_PB4 2 &pcfg_pull_up_2ma>;
			};

			spi1_mosi: spi1-mosi {
				rockchip,pins =
					<4 RK_PB5 2 &pcfg_pull_up_2ma>;
			};

			spi1_csn0: spi1-csn0 {
				rockchip,pins =
					<4 RK_PB6 2 &pcfg_pull_up_2ma>;
			};

			spi1_miso: spi1-miso {
				rockchip,pins =
					<4 RK_PB7 2 &pcfg_pull_up_2ma>;
			};

			spi1_csn1: spi1-csn1 {
				rockchip,pins =
					<4 RK_PC0 2 &pcfg_pull_up_2ma>;
			};

			spi1_clk_hs: spi1-clk-hs {
				rockchip,pins =
					<4 RK_PB4 2 &pcfg_pull_up_2ma>;
			};

			spi1_mosi_hs: spi1-mosi-hs {
				rockchip,pins =
					<4 RK_PB5 2 &pcfg_pull_up_2ma>;
			};

			spi1_csn0_hs: spi1-csn0-hs {
				rockchip,pins =
					<4 RK_PB6 2 &pcfg_pull_up_2ma>;
			};

			spi1_miso_hs: spi1-miso-hs {
				rockchip,pins =
					<4 RK_PB7 2 &pcfg_pull_up_2ma>;
			};

			spi1_csn1_hs: spi1-csn1-hs {
				rockchip,pins =
					<4 RK_PC0 2 &pcfg_pull_up_2ma>;
			};
		};

		spi1m1 {
			spi1m1_clk: spi1m1-clk {
				rockchip,pins =
					<3 RK_PC7 3 &pcfg_pull_up_2ma>;
			};

			spi1m1_mosi: spi1m1-mosi {
				rockchip,pins =
					<3 RK_PD0 3 &pcfg_pull_up_2ma>;
			};

			spi1m1_csn0: spi1m1-csn0 {
				rockchip,pins =
					<3 RK_PD1 3 &pcfg_pull_up_2ma>;
			};

			spi1m1_miso: spi1m1-miso {
				rockchip,pins =
					<3 RK_PD2 3 &pcfg_pull_up_2ma>;
			};

			spi1m1_csn1: spi1m1-csn1 {
				rockchip,pins =
					<3 RK_PD3 3 &pcfg_pull_up_2ma>;
			};

			spi1m1_clk_hs: spi1m1-clk-hs {
				rockchip,pins =
					<3 RK_PC7 3 &pcfg_pull_up_2ma>;
			};

			spi1m1_mosi_hs: spi1m1-mosi-hs {
				rockchip,pins =
					<3 RK_PD0 3 &pcfg_pull_up_2ma>;
			};

			spi1m1_csn0_hs: spi1m1-csn0-hs {
				rockchip,pins =
					<3 RK_PD1 3 &pcfg_pull_up_2ma>;
			};

			spi1m1_miso_hs: spi1m1-miso-hs {
				rockchip,pins =
					<3 RK_PD2 3 &pcfg_pull_up_2ma>;
			};

			spi1m1_csn1_hs: spi1m1-csn1-hs {
				rockchip,pins =
					<3 RK_PD3 3 &pcfg_pull_up_2ma>;
			};
		};

		spi2m0 {
			spi2m0_miso: spi2m0-miso {
				rockchip,pins =
					<1 RK_PA6 2 &pcfg_pull_up_2ma>;
			};

			spi2m0_clk: spi2m0-clk {
				rockchip,pins =
					<1 RK_PA7 2 &pcfg_pull_up_2ma>;
			};

			spi2m0_mosi: spi2m0-mosi {
				rockchip,pins =
					<1 RK_PB0 2 &pcfg_pull_up_2ma>;
			};

			spi2m0_csn: spi2m0-csn {
				rockchip,pins =
					<1 RK_PB1 2 &pcfg_pull_up_2ma>;
			};

			spi2m0_miso_hs: spi2m0-miso-hs {
				rockchip,pins =
					<1 RK_PA6 2 &pcfg_pull_up_2ma>;
			};

			spi2m0_clk_hs: spi2m0-clk-hs {
				rockchip,pins =
					<1 RK_PA7 2 &pcfg_pull_up_2ma>;
			};

			spi2m0_mosi_hs: spi2m0-mosi-hs {
				rockchip,pins =
					<1 RK_PB0 2 &pcfg_pull_up_2ma>;
			};

			spi2m0_csn_hs: spi2m0-csn-hs {
				rockchip,pins =
					<1 RK_PB1 2 &pcfg_pull_up_2ma>;
			};
		};

		spi2m1 {
			spi2m1_miso: spi2m1-miso {
				rockchip,pins =
					<2 RK_PA4 3 &pcfg_pull_up_2ma>;
			};

			spi2m1_clk: spi2m1-clk {
				rockchip,pins =
					<2 RK_PA5 3 &pcfg_pull_up_2ma>;
			};

			spi2m1_mosi: spi2m1-mosi {
				rockchip,pins =
					<2 RK_PA6 3 &pcfg_pull_up_2ma>;
			};

			spi2m1_csn: spi2m1-csn {
				rockchip,pins =
					<2 RK_PA7 3 &pcfg_pull_up_2ma>;
			};

			spi2m1_miso_hs: spi2m1-miso-hs {
				rockchip,pins =
					<2 RK_PA4 3 &pcfg_pull_up_2ma>;
			};

			spi2m1_clk_hs: spi2m1-clk-hs {
				rockchip,pins =
					<2 RK_PA5 3 &pcfg_pull_up_2ma>;
			};

			spi2m1_mosi_hs: spi2m1-mosi-hs {
				rockchip,pins =
					<2 RK_PA6 3 &pcfg_pull_up_2ma>;
			};

			spi2m1_csn_hs: spi2m1-csn-hs {
				rockchip,pins =
					<2 RK_PA7 3 &pcfg_pull_up_2ma>;
			};
		};

		uart0 {
			uart0_xfer: uart0-xfer {
				rockchip,pins =
					/* uart0_rx */
					<0 RK_PB3 1 &pcfg_pull_up_2ma>,
					/* uart0_tx */
					<0 RK_PB2 1 &pcfg_pull_up_2ma>;
			};

			uart0_cts: uart0-cts {
				rockchip,pins =
					<0 RK_PB4 1 &pcfg_pull_none>;
			};

			uart0_rts: uart0-rts {
				rockchip,pins =
					<0 RK_PB5 1 &pcfg_pull_none>;
			};
		};

		uart1 {
			uart1m0_xfer: uart1m0-xfer {
				rockchip,pins =
					/* uart1_rxm0 */
					<4 RK_PB0 2 &pcfg_pull_up_2ma>,
					/* uart1_txm0 */
					<4 RK_PB1 2 &pcfg_pull_up_2ma>;
			};

			uart1m1_xfer: uart1m1-xfer {
				rockchip,pins =
					/* uart1_rxm1 */
					<1 RK_PB4 3 &pcfg_pull_up_2ma>,
					/* uart1_txm1 */
					<1 RK_PB5 3 &pcfg_pull_up_2ma>;
			};

			uart1_cts: uart1-cts {
				rockchip,pins =
					<4 RK_PB2 2 &pcfg_pull_none>;
			};

			uart1_rts: uart1-rts {
				rockchip,pins =
					<4 RK_PB3 2 &pcfg_pull_none>;
			};
		};

		uart2 {
			uart2m0_xfer: uart2m0-xfer {
				rockchip,pins =
					/* uart2_rxm0 */
					<4 RK_PA3 2 &pcfg_pull_up_2ma>,
					/* uart2_txm0 */
					<4 RK_PA2 2 &pcfg_pull_up_2ma>;
			};

			uart2m1_xfer: uart2m1-xfer {
				rockchip,pins =
					/* uart2_rxm1 */
					<2 RK_PD1 2 &pcfg_pull_up_2ma>,
					/* uart2_txm1 */
					<2 RK_PD0 2 &pcfg_pull_up_2ma>;
			};

			uart2m2_xfer: uart2m2-xfer {
				rockchip,pins =
					/* uart2_rxm2 */
					<3 RK_PA4 2 &pcfg_pull_up_2ma>,
					/* uart2_txm2 */
					<3 RK_PA3 2 &pcfg_pull_up_2ma>;
			};
		};

		uart3 {
			uart3m0_xfer: uart3m0-xfer {
				rockchip,pins =
					/* uart3_rxm0 */
					<0 RK_PC4 2 &pcfg_pull_up_2ma>,
					/* uart3_txm0 */
					<0 RK_PC3 2 &pcfg_pull_up_2ma>;
			};

			uart3_ctsm0: uart3-ctsm0 {
				rockchip,pins =
					<0 RK_PC6 2 &pcfg_pull_none>;
			};

			uart3_rtsm0: uart3-rtsm0 {
				rockchip,pins =
					<0 RK_PC7 2 &pcfg_pull_none>;
			};
		};

		uart4 {
			uart4_xfer: uart4-xfer {
				rockchip,pins =
					/* uart4_rx */
					<4 RK_PB4 1 &pcfg_pull_up_2ma>,
					/* uart4_tx */
					<4 RK_PB5 1 &pcfg_pull_up_2ma>;
			};

			uart4_cts: uart4-cts {
				rockchip,pins =
					<4 RK_PB6 1 &pcfg_pull_none>;
			};

			uart4_rts: uart4-rts {
				rockchip,pins =
					<4 RK_PB7 1 &pcfg_pull_none>;
			};
		};

		uart5 {
			uart5_xfer: uart5-xfer {
				rockchip,pins =
					/* uart5_rx */
					<3 RK_PC3 2 &pcfg_pull_up_2ma>,
					/* uart5_tx */
					<3 RK_PC2 2 &pcfg_pull_up_2ma>;
			};
		};

		uart6 {
			uart6_xfer: uart6-xfer {
				rockchip,pins =
					/* uart6_rx */
					<3 RK_PC5 2 &pcfg_pull_up_2ma>,
					/* uart6_tx */
					<3 RK_PC4 2 &pcfg_pull_up_2ma>;
			};
		};

		uart7 {
			uart7_xfer: uart7-xfer {
				rockchip,pins =
					/* uart7_rx */
					<3 RK_PC7 2 &pcfg_pull_up_2ma>,
					/* uart7_tx */
					<3 RK_PC6 2 &pcfg_pull_up_2ma>;
			};
		};

		tsadc {
			tsadc_otp_gpio: tsadc-otp-gpio {
				rockchip,pins =
					<0 RK_PA6 RK_FUNC_GPIO &pcfg_pull_none>;
			};

			tsadc_otp_out: tsadc-otp-out {
				rockchip,pins =
					<0 RK_PA6 2 &pcfg_pull_none>;
			};
		};

		xin32k {
			clkin_32k: clkin-32k {
				rockchip,pins =
					<0 RK_PC2 1 &pcfg_pull_none>;
			};

			clkout_32k: clkout-32k {
				rockchip,pins =
					<0 RK_PC2 1 &pcfg_pull_none>;
			};
		};
	};
};
