
&i2c0 {
        status = "okay";
        i2c-scl-rising-time-ns = <168>;
        i2c-scl-falling-time-ns = <4>;
        clock-frequency = <400000>;

        vdd_cpu_b: syr827@40 {
                compatible = "silergy,syr827";
                reg = <0x40>;
                vin-supply = <&vcc5v0_sys>;
                regulator-compatible = "fan53555-reg";
                pinctrl-names = "default";
                pinctrl-0 = <&vsel1_gpio>;
                vsel-gpios = <&gpio1 17 GPIO_ACTIVE_HIGH>;
                regulator-name = "vdd_cpu_b";
                regulator-min-microvolt = <712500>;
                regulator-max-microvolt = <1500000>;
                regulator-ramp-delay = <1000>;
                fcs,suspend-voltage-selector = <1>;
                regulator-always-on;
                regulator-boot-on;
                regulator-initial-state = <3>;
                        regulator-state-mem {
                        regulator-off-in-suspend;
                };
        };

        vdd_gpu: syr828@41 {
                compatible = "silergy,syr828";
                reg = <0x41>;
                vin-supply = <&vcc5v0_sys>;
                regulator-compatible = "fan53555-reg";
                pinctrl-names = "default";
                pinctrl-0 = <&vsel2_gpio>;
                vsel-gpios = <&gpio1 14 GPIO_ACTIVE_HIGH>;
                regulator-name = "vdd_gpu";
                regulator-min-microvolt = <712500>;
                regulator-max-microvolt = <1500000>;
                regulator-ramp-delay = <1000>;
                fcs,suspend-voltage-selector = <1>;
                regulator-always-on;
                regulator-boot-on;
                regulator-initial-state = <3>;
                        regulator-state-mem {
                        regulator-off-in-suspend;
                };
        };

        rk808: pmic@1b {
                compatible = "rockchip,rk808";
                reg = <0x1b>;
                interrupt-parent = <&gpio1>;
                interrupts = <21 IRQ_TYPE_LEVEL_LOW>;
                pinctrl-names = "default";
                pinctrl-0 = <&pmic_int_l &pmic_dvs2>;
                rockchip,system-power-controller;
                wakeup-source;
                #clock-cells = <1>;
              //  clock-output-names = "xin32k", "rk808-clkout2";
               clock-output-names = "rk808-clkout1", "rk808-clkout2";   //wifi 
/*
               vcc1-supply = <&vcc3v3_sys>;
               vcc2-supply = <&vcc3v3_sys>;
               vcc3-supply = <&vcc3v3_sys>;
               vcc4-supply = <&vcc3v3_sys>;
               vcc6-supply = <&vcc3v3_sys>;
               vcc7-supply = <&vcc3v3_sys>;
                vcc8-supply = <&vcc3v3_sys>;
               vcc9-supply = <&vcc3v3_sys>;
               vcc10-supply = <&vcc3v3_sys>;
               vcc11-supply = <&vcc3v3_sys>;
                vcc12-supply = <&vcc3v3_sys>;
               vddio-supply = <&vcc_3v0>;

*/
                vcc1-supply = <&vcc5v0_sys>;
                vcc2-supply = <&vcc5v0_sys>;
                vcc3-supply = <&vcc5v0_sys>;
                vcc4-supply = <&vcc5v0_sys>;
                vcca-supply = <&vcc5v0_sys>;
                vcc6-supply = <&vcc5v0_sys>;
                vcc7-supply = <&vcc5v0_sys>;
                vcc8-supply = <&vcc3v3_sys>;
                vcc9-supply = <&vcc5v0_sys>;
                vcc10-supply = <&vcc5v0_sys>;
                vcc11-supply = <&vcc5v0_sys>;
                vcc12-supply = <&vcc3v3_sys>;
                vddio-supply = <&vcc1v8_pmu>;

                regulators {
                        vdd_center: DCDC_REG1 {
                                regulator-always-on;
                                regulator-boot-on;
                                regulator-min-microvolt = <750000>;
                                regulator-max-microvolt = <1350000>;
                                regulator-ramp-delay = <6001>;
                                regulator-name = "vdd_center";
                                regulator-state-mem {
                                        regulator-off-in-suspend;
                                };
                        };

                        vdd_cpu_l: DCDC_REG2 {
                                regulator-always-on;
                                regulator-boot-on;
                                regulator-min-microvolt = <750000>;
                                regulator-max-microvolt = <1350000>;
                                regulator-ramp-delay = <6001>;
                                regulator-name = "vdd_cpu_l";
                                regulator-state-mem {
                                        regulator-off-in-suspend;
                                };
                        };

                        vcc_ddr: DCDC_REG3 {
                                regulator-always-on;
                                regulator-boot-on;
                                regulator-name = "vcc_ddr";
                                regulator-state-mem {
                                        regulator-on-in-suspend;
                                };
                        };

                        vcc_1v8: DCDC_REG4 {
                                regulator-always-on;
                                regulator-boot-on;
                                regulator-min-microvolt = <1800000>;
                                regulator-max-microvolt = <1800000>;
                                regulator-name = "vcc_1v8";
                                regulator-state-mem {
                                        regulator-on-in-suspend;
                                        regulator-suspend-microvolt = <1800000>;
                                };
                        };

                        vcc1v8_dvp: LDO_REG1 {
                                regulator-always-on;
                                regulator-boot-on;
                                regulator-min-microvolt = <1800000>;
                                regulator-max-microvolt = <1800000>;
                                regulator-name = "vcc1v8_dvp";
                                regulator-state-mem {
                                        regulator-off-in-suspend;
                                };
                        };

                        vcc3v0_tp: LDO_REG2 {
                                regulator-always-on;
                                regulator-boot-on;
                                regulator-min-microvolt = <3000000>;
                                regulator-max-microvolt = <3000000>;
                                regulator-name = "vcc3v0_tp";
                                regulator-state-mem {
                                        //regulator-off-in-suspend;
                                        regulator-on-in-suspend;
                                        regulator-suspend-microvolt = <3000000>;
                                };
                        };

                        vcc1v8_pmu: LDO_REG3 {
                                regulator-always-on;
                                regulator-boot-on;
                                regulator-min-microvolt = <1800000>;
                                regulator-max-microvolt = <1800000>;
                                regulator-name = "vcc1v8_pmu";
                                regulator-state-mem {
                                        regulator-on-in-suspend;
                                        regulator-suspend-microvolt = <1800000>;
                                };
                        };

                        vccio_sd: LDO_REG4 {
                                regulator-always-on;
                                regulator-boot-on;
                                regulator-min-microvolt = <1800000>;
                                regulator-max-microvolt = <3300000>;
                                regulator-name = "vccio_sd";
                                regulator-state-mem {
                                        regulator-on-in-suspend;
                                        regulator-suspend-microvolt = <3300000>;
                                };
                        };

                        vcca3v0_codec: LDO_REG5 {
                                regulator-always-on;
                                regulator-boot-on;
                                regulator-min-microvolt = <3000000>;
                                regulator-max-microvolt = <3000000>;
                                regulator-name = "vcca3v0_codec";
                                regulator-state-mem {
                                        regulator-off-in-suspend;
                                     //   regulator-suspend-microvolt = <3000000>;
                                };
                        };

                        vcc_1v5: LDO_REG6 {
                                regulator-always-on;
                                regulator-boot-on;
                                regulator-min-microvolt = <1500000>;
                                regulator-max-microvolt = <1500000>;
                                regulator-name = "vcc_1v5";
                                regulator-state-mem {
                                        regulator-on-in-suspend;
                                        regulator-suspend-microvolt = <1500000>;
                                };
                        };

                        vcca1v8_codec: LDO_REG7 {
                                regulator-always-on;
                                regulator-boot-on;
                                regulator-min-microvolt = <1800000>;
                                regulator-max-microvolt = <1800000>;
                                regulator-name = "vcca1v8_codec";
                                regulator-state-mem {
                                        regulator-off-in-suspend;
                                    //    regulator-suspend-microvolt = <1800000>;
                                };
                        };

                        vcc_3v0: LDO_REG8 {
                                regulator-always-on;
                                regulator-boot-on;
                                regulator-min-microvolt = <3000000>;
                                regulator-max-microvolt = <3000000>;
                                regulator-name = "vcc_3v0";
                                regulator-state-mem {
                                        regulator-on-in-suspend;
                                        regulator-suspend-microvolt = <3000000>;
                                };
                        };

                        vcc3v3_s3: SWITCH_REG1 {
                                regulator-always-on;
                                regulator-boot-on;
                                regulator-name = "vcc3v3_s3";
                                regulator-state-mem {
                                        regulator-off-in-suspend;
                                };
                        };

                        vcc3v3_s0: SWITCH_REG2 {
                                regulator-always-on;
                                regulator-boot-on;
                                regulator-name = "vcc3v3_s0";
                                regulator-state-mem {
                                        regulator-off-in-suspend;
                                };
                        };
                };
        };
};
