// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Copyright (c) 2020 Rockchip Electronics Co., Ltd.
 *
 */

/dts-v1/;

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/pinctrl/rockchip.h>
#include <dt-bindings/input/rk-input.h>
#include <dt-bindings/sensor-dev.h>
#include <dt-bindings/display/drm_mipi_dsi.h>
#include "rk3566.dtsi"
#include "rk3568-android.dtsi"
#include "rk3566-eink.dtsi"

/ {
	model = "Rockchip RK3566 RK817 EINK LP4X Board";
	compatible = "rockchip,rk3566-rk817-eink", "rockchip,rk3566";

	charge-animation {
		compatible = "rockchip,uboot-charge";
		rockchip,uboot-charge-on = <1>;
		rockchip,android-charge-on = <0>;
		rockchip,uboot-low-power-voltage = <3350>;
		rockchip,screen-on-voltage = <3400>;
		rockchip,auto-wakeup-interval = <60>;
		status = "okay";
	};

	adc_keys: adc-keys {
		status = "disabled";
		compatible = "adc-keys";
		io-channels = <&saradc 0>;
		io-channel-names = "buttons";
		keyup-threshold-microvolt = <1800000>;
		poll-interval = <100>;

		vol-up-key {
			label = "volume up";
			linux,code = <KEY_VOLUMEUP>;
			press-threshold-microvolt = <1750>;
		};

		vol-down-key {
			label = "volume down";
			linux,code = <KEY_VOLUMEDOWN>;
			press-threshold-microvolt = <297500>;
		};
	};

	hdmi_sound: hdmi-sound {
		compatible = "simple-audio-card";
		simple-audio-card,format = "i2s";
		simple-audio-card,mclk-fs = <128>;
		simple-audio-card,name = "rockchip,hdmi";
		status = "disabled";

		simple-audio-card,cpu {
				sound-dai = <&i2s0_8ch>;
		};
		simple-audio-card,codec {
				sound-dai = <&hdmi>;
		};
	};

	vccsys: vccsys {
		compatible = "regulator-fixed";
		regulator-name = "vcc3v8_sys";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <3800000>;
		regulator-max-microvolt = <3800000>;
	};

	rk817-sound {
		compatible = "rockchip,multicodecs-card";
		rockchip,card-name = "rockchip-rk817";
		hp-det-gpio = <&gpio4 RK_PC4 GPIO_ACTIVE_LOW>;
		rockchip,format = "i2s";
		rockchip,mclk-fs = <256>;
		rockchip,cpu = <&i2s1_8ch>;
		rockchip,codec = <&rk817_codec>;
		pinctrl-names = "default";
		pinctrl-0 = <&hp_det>;
	};

	sdio_pwrseq: sdio-pwrseq {
		status = "disabled";
		compatible = "mmc-pwrseq-simple";
		clocks = <&rk817 1>;
		clock-names = "ext_clock";
		pinctrl-names = "default";
		pinctrl-0 = <&wifi_enable_h>;

		/*
		 * On the module itself this is one of these (depending
		 * on the actual card populated):
		 * - SDIO_RESET_L_WL_REG_ON
		 * - PDN (power down when low)
		 */
		post-power-on-delay-ms = <200>;
		reset-gpios = <&gpio2 RK_PB1 GPIO_ACTIVE_LOW>;
	};

	vcc_sd: vcc-sd {
		compatible = "regulator-gpio";
		enable-active-low;
		enable-gpio = <&gpio0 RK_PA5 GPIO_ACTIVE_LOW>;
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		pinctrl-names = "default";
		pinctrl-0 = <&vcc_sd_h>;
		regulator-name = "vcc_sd";
		states = <3300000 0x0
			3300000 0x1>;
	};

	wireless-wlan {
		compatible = "wlan-platdata";
		rockchip,grf = <&grf>;
		wifi_chip_type = "ap6255";
		pinctrl-names = "default";
		pinctrl-0 = <&wifi_host_wake_irq>;
		WIFI,host_wake_irq = <&gpio2 RK_PB2 GPIO_ACTIVE_HIGH>;
		status = "disabled";
	};

	wireless-bluetooth {
		compatible = "bluetooth-platdata";
		clocks = <&rk817 1>;
		clock-names = "ext_clock";
		//wifi-bt-power-toggle;
		uart_rts_gpios = <&gpio2 RK_PB5 GPIO_ACTIVE_LOW>;
		pinctrl-names = "default", "rts_gpio";
		pinctrl-0 = <&uart1m0_rtsn>;
		pinctrl-1 = <&uart1_gpios>;
		BT,reset_gpio    = <&gpio2 RK_PB7 GPIO_ACTIVE_HIGH>;
		BT,wake_gpio     = <&gpio2 RK_PC1 GPIO_ACTIVE_HIGH>;
		BT,wake_host_irq = <&gpio2 RK_PC0 GPIO_ACTIVE_HIGH>;
		status = "disabled";
	};
};

&ebc {
	/* clock rate 1000M/n, (n=1~32) */
	assigned-clocks = <&cru CPLL_333M>, <&cru DCLK_EBC>;
	assigned-clock-rates = <250000000>, <250000000>;
	status = "okay";
};

&ebc_dev {
	pmic = <&tps65185>;
	status = "okay";
#if 0
	/* ED097TC2U1 */
	panel,width = <1200>;
	panel,height = <825>;
	panel,vir_width = <1200>;
	panel,vir_height = <825>;
	panel,sdck = <25000000>;
	panel,lsl = <4>;
	panel,lbl = <4>;
	panel,ldl = <300>;
	panel,lel = <36>;
	panel,gdck-sta = <18>;
	panel,lgonl = <265>;
	panel,fsl = <2>;
	panel,fbl = <4>;
	panel,fdl = <825>;
	panel,fel = <24>;
	panel,mirror = <0>;
	panel,panel_16bit = <0>;
	panel,panel_color = <0>;
	panel,width-mm = <203>;
	panel,height-mm = <140>;
#else
	/* ES103TC1 */
	panel,width = <1872>;
	panel,height = <1404>;
	panel,vir_width = <1872>;
	panel,vir_height = <1404>;
	panel,sdck = <33300000>;
	panel,lsl = <18>;
	panel,lbl = <17>;
	panel,ldl = <234>;
	panel,lel = <7>;
	panel,gdck-sta = <34>;
	panel,lgonl = <192>;
	panel,fsl = <1>;
	panel,fbl = <4>;
	panel,fdl = <1404>;
	panel,fel = <12>;
	panel,mirror = <0>;
	panel,panel_16bit = <1>;
	panel,panel_color = <0>;
	panel,width-mm = <157>;
	panel,height-mm = <210>;
#endif
};

&cpu0 {
	cpu-supply = <&vdd_cpu>;
};

&gpu {
	mali-supply = <&vdd_gpu>;
	status = "okay";
};

&hdmi {
	status = "disabled";
};

&hdmi_in_vp0 {
	status = "disabled";
};

&hdmi_in_vp1 {
	status = "disabled";
};

&hdmi_sound {
	status = "disabled";
};

&i2c0 {
	status = "okay";

	vdd_cpu: tcs4525@1c {
		compatible = "tcs,tcs4525";
		reg = <0x1c>;
		vin-supply = <&vccsys>;
		regulator-compatible = "fan53555-reg";
		regulator-name = "vdd_cpu";
		regulator-min-microvolt = <712500>;
		regulator-max-microvolt = <1390000>;
		regulator-init-microvolt = <900000>;
		regulator-ramp-delay = <2300>;
		fcs,suspend-voltage-selector = <1>;
		regulator-boot-on;
		regulator-always-on;
		regulator-state-mem {
			regulator-off-in-suspend;
		};
	};

	rk817: pmic@20 {
		compatible = "rockchip,rk817";
		reg = <0x20>;
		interrupt-parent = <&gpio0>;
		interrupts = <3 IRQ_TYPE_LEVEL_LOW>;

		pinctrl-names = "default", "pmic-sleep",
				"pmic-power-off", "pmic-reset";
		pinctrl-0 = <&pmic_int>;
		pinctrl-1 = <&soc_slppin_slp>, <&rk817_slppin_slp>;
		pinctrl-2 = <&soc_slppin_gpio>, <&rk817_slppin_pwrdn>;
		pinctrl-3 = <&soc_slppin_gpio>, <&rk817_slppin_rst>;
		rockchip,system-power-controller;
		wakeup-source;
		#clock-cells = <1>;
		clock-output-names = "rk808-clkout1", "rk808-clkout2";
		//fb-inner-reg-idxs = <2>;
		/* 1: rst regs (default in codes), 0: rst the pmic */
		pmic-reset-func = <0>;
		/* not save the PMIC_POWER_EN register in uboot */
		not-save-power-en = <1>;
		vcc1-supply = <&vccsys>;
		vcc2-supply = <&vccsys>;
		vcc3-supply = <&vccsys>;
		vcc4-supply = <&vccsys>;
		vcc5-supply = <&vccsys>;
		vcc6-supply = <&vccsys>;
		vcc7-supply = <&vccsys>;
		vcc8-supply = <&vccsys>;
		vcc9-supply = <&dcdc_boost>;

		pwrkey {
			status = "okay";
		};

		pinctrl_rk8xx: pinctrl_rk8xx {
			gpio-controller;
			#gpio-cells = <2>;

			rk817_slppin_null: rk817_slppin_null {
				pins = "gpio_slp";
				function = "pin_fun0";
			};

			rk817_slppin_slp: rk817_slppin_slp {
				pins = "gpio_slp";
				function = "pin_fun1";
			};

			rk817_slppin_pwrdn: rk817_slppin_pwrdn {
				pins = "gpio_slp";
				function = "pin_fun2";
			};

			rk817_slppin_rst: rk817_slppin_rst {
				pins = "gpio_slp";
				function = "pin_fun3";
			};
		};

		regulators {
			vdd_logic: DCDC_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <500000>;
				regulator-max-microvolt = <1350000>;
				regulator-init-microvolt = <900000>;
				regulator-ramp-delay = <6001>;
				regulator-initial-mode = <0x2>;
				regulator-name = "vdd_logic";
				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <900000>;
				};
			};

			vdd_gpu: DCDC_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <500000>;
				regulator-max-microvolt = <1350000>;
				regulator-init-microvolt = <900000>;
				regulator-ramp-delay = <6001>;
				regulator-initial-mode = <0x2>;
				regulator-name = "vdd_gpu";
					regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_ddr: DCDC_REG3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-initial-mode = <0x2>;
				regulator-name = "vcc_ddr";
				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};

			vcc_3v3: DCDC_REG4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-initial-mode = <0x2>;
				regulator-name = "vcc_3v3";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcca1v8_pmu: LDO_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcca1v8_pmu";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vdda_0v9: LDO_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <900000>;
				regulator-max-microvolt = <900000>;
				regulator-name = "vdda_0v9";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdda0v9_pmu: LDO_REG3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <900000>;
				regulator-max-microvolt = <900000>;
				regulator-name = "vdda0v9_pmu";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <900000>;
				};
			};

			vccio_acodec: LDO_REG4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vccio_acodec";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vccio_sd: LDO_REG5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vccio_sd";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc3v3_pmu: LDO_REG6 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vcc3v3_pmu";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vcc_1v8: LDO_REG7 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc_1v8";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc1v8_dvp: LDO_REG8 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc1v8_dvp";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc2v8_dvp: LDO_REG9 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <2800000>;
				regulator-max-microvolt = <2800000>;
				regulator-name = "vcc2v8_dvp";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			dcdc_boost: BOOST {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <4700000>;
				regulator-max-microvolt = <5400000>;
				regulator-name = "boost";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			otg_switch: OTG_SWITCH {
				regulator-name = "otg_switch";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};
		};

		battery {
			compatible = "rk817,battery";
			ocv_table = <3400 3513 3578 3687 3734 3752 3763
				     3766 3771 3784 3804 3836 3885 3925
				     3962 4005 4063 4114 4169 4227 4303>;
			design_capacity = <5000>;
			design_qmax = <5500>;
			bat_res = <100>;
			sleep_enter_current = <150>;
			sleep_exit_current = <180>;
			sleep_filter_current = <100>;
			power_off_thresd = <3450>;
			zero_algorithm_vol = <3850>;
			max_soc_offset = <60>;
			monitor_sec = <5>;
			sample_res = <10>;
			virtual_power = <0>;
		};

		charger {
			compatible = "rk817,charger";
			min_input_voltage = <4500>;
			max_input_current = <1500>;
			max_chrg_current = <2000>;
			max_chrg_voltage = <4300>;
			chrg_term_mode = <0>;
			chrg_finish_cur = <300>;
			virtual_power = <0>;
			dc_det_adc = <0>;
			extcon = <&usb2phy0>;
			gate_function_disable = <1>;
		};

		rk817_codec: codec {
			#sound-dai-cells = <0>;
			compatible = "rockchip,rk817-codec";
			clocks = <&cru I2S1_MCLKOUT>;
			clock-names = "mclk";
			assigned-clocks = <&cru I2S1_MCLKOUT>, <&cru I2S1_MCLK_TX_IOE>;
			assigned-clock-rates = <12288000>;
			assigned-clock-parents = <&cru I2S1_MCLKOUT_TX>, <&cru I2S1_MCLKOUT_TX>;
			pinctrl-names = "default";
			pinctrl-0 = <&i2s1m0_mclk>;
			hp-volume = <20>;
			spk-volume = <3>;
			out-l2spk-r2hp;
			spk-ctl-gpios = <&gpio0 RK_PA6 GPIO_ACTIVE_HIGH>;
			status = "okay";
		};
	};
};

&i2c1 {
	status = "okay";
	tps65185: tps65185@68 {
		status = "okay";
		compatible = "ti,tps65185";
		reg = <0x68>;
		pinctrl-names = "default";
		pinctrl-0 = <&tps65185_gpio>;
		int-gpios = <&gpio3 RK_PA6 GPIO_ACTIVE_HIGH>;
		wakeup-gpios = <&gpio3 RK_PA5 GPIO_ACTIVE_HIGH>;
		vcomctl-gpios = <&gpio4 RK_PB2 GPIO_ACTIVE_HIGH>;
		powerup-gpios = <&gpio3 RK_PB0 GPIO_ACTIVE_HIGH>;
	};
};

&i2c2 {
	status = "okay";
	wacom: wacom@9 {
		compatible = "wacom,w9013";
		reg = <0x09>;
		pinctrl-names = "default";
		pinctrl-0 = <&wacom_gpio>;
		gpio_detect = <&gpio3 RK_PA3 GPIO_ACTIVE_HIGH>;
		gpio_intr = <&gpio3 RK_PA1 GPIO_ACTIVE_HIGH>;
		gpio_rst = <&gpio3 RK_PA2 GPIO_ACTIVE_HIGH>;
		revert_x = <0>;
		revert_y = <0>;
		xy_exchange = <0>;
	};
};

&i2c3 {
	status = "okay";
	pinctrl-names = "default";
	pinctrl-0 = <&i2c3m1_xfer>;

	ts@40 {
		compatible = "gslX680-pad";
		reg = <0x40>;
		touch-gpio = <&gpio3 RK_PB0 IRQ_TYPE_LEVEL_HIGH>;
		reset-gpio = <&gpio3 RK_PB1 IRQ_TYPE_LEVEL_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&tp_gpio>;
		screen_max_x = <1200>;
		screen_max_y = <1920>;
		revert_x = <0>;
		revert_y = <1>;
		revert_xy = <0>;
		chip_id = <1>;
		status = "disabled";
	};

	tsc@24 {
		status = "okay";
		compatible = "cy,cyttsp5_i2c_adapter";
		reg = <0x24>;
		cy,adapter_id = "cyttsp5_i2c_adapter";
		//cytp-supply = <&vcc_sd>;
		cy,core {
			cy,name = "cyttsp5_core";
			pinctrl-names = "default";
			pinctrl-0 = <&tsc_gpio>;
			cy,irq_gpio =  <&gpio3 RK_PB1 GPIO_ACTIVE_HIGH>;
			cy,rst_gpio =  <&gpio3 RK_PB2 GPIO_ACTIVE_HIGH>;
			cy,1v8_gpio =  <&gpio3 RK_PC4 GPIO_ACTIVE_HIGH>;
			cy,2v8_gpio =  <&gpio3 RK_PC5 GPIO_ACTIVE_HIGH>;
			cy,hid_desc_register = <1>;
			/* CY_CORE_FLAG_RESTORE_PARAMETERS */
			cy,flags = <6>;
			/* CY_CORE_EWG_NONE */
			cy,easy_wakeup_gesture = <0>;
			cy,btn_keys = <172 /* KEY_HOMEPAGE */
						/* previously was KEY_HOME, new Android versions use KEY_HOMEPAGE */
						139 /* KEY_MENU */
						158 /* KEY_BACK */
						217 /* KEY_SEARCH */
						114 /* KEY_VOLUMEDOWN */
						115 /* KEY_VOLUMEUP */
						212 /* KEY_CAMERA */
						116>; /* KEY_POWER */
			cy,btn_keys-tag = <0>;
			cy,mt {
				cy,name = "cyttsp5_mt";
				cy,inp_dev_name = "cyttsp5_mt";
				cy,flags = <0>;
				cy,abs =
					/* ABS_MT_POSITION_X, CY_ABS_MIN_X, CY_ABS_MAX_X, 0, 0 */
					<0x35 0 1872 0 0
					/* ABS_MT_POSITION_Y, CY_ABS_MIN_Y, CY_ABS_MAX_Y, 0, 0 */
					0x36 0 1404 0 0
					/* ABS_MT_PRESSURE, CY_ABS_MIN_P, CY_ABS_MAX_P, 0, 0 */
					0x3a 0 255 0 0
					/* CY_IGNORE_VALUE, CY_ABS_MIN_W, CY_ABS_MAX_W, 0, 0 */
					0xffff 0 255 0 0
					/* ABS_MT_TRACKING_ID, CY_ABS_MIN_T, CY_ABS_MAX_T, 0, 0 */
					0x39 0 15 0 0
					/* ABS_MT_TOUCH_MAJOR, 0, 255, 0, 0 */
					0x30 0 255 0 0
					/* ABS_MT_TOUCH_MINOR, 0, 255, 0, 0 */
					0x31 0 255 0 0
					/* ABS_MT_ORIENTATION, -127, 127, 0, 0 */
					0x34 0xffffff81 127 0 0
					/* ABS_MT_TOOL_TYPE, 0, MT_TOOL_MAX, 0, 0 */
					0x37 0 1 0 0
					/* ABS_DISTANCE, 0, 255, 0, 0 */
					0x19 0 255 0 0>;

					cy,vkeys_x = <1872>;
					cy,vkeys_y = <1404>;
					cy,revert_x = <0>;
					cy,revert_y = <1>;
					cy,xy_exchange = <0>;

					cy,virtual_keys =
						/* KeyCode CenterX CenterY Width Height */
						/* KEY_BACK */
						<158 1360 90 160 180
						/* KEY_MENU */
						139 1360 270 160 180
						/* KEY_HOMEPAGE */
						172 1360 450 160 180
						/* KEY SEARCH */
						217 1360 630 160 180>;
			};

			cy,btn {
				cy,name = "cyttsp5_btn";
				cy,inp_dev_name = "cyttsp5_btn";
			};

			cy,proximity {
				cy,name = "cyttsp5_proximity";
				cy,inp_dev_name = "cyttsp5_proximity";
				cy,abs =
			/* ABS_DISTANCE, CY_PROXIMITY_MIN_VAL, CY_PROXIMITY_MAX_VAL, 0, 0 */
					<0x19 0 1 0 0>;
			};
		};
	};
};

&i2c5 {
	status = "disabled";

	kxtj: kxtj3@e {
		status = "disabled";
		compatible = "gs_kxtj9";
		pinctrl-names = "default";
		pinctrl-0 = <&kxtj3_irq_gpio>;
		reg = <0x0e>;
		irq-gpio = <&gpio4 RK_PC6 IRQ_TYPE_EDGE_RISING>;
		type = <SENSOR_TYPE_ACCEL>;
		irq_enable = <0>;
		poll_delay_ms = <30>;
		power-off-in-suspend = <1>;
		layout = <5>;
	};
};

&i2s0_8ch {
	status = "disabled";
};

&i2s1_8ch {
	status = "okay";
	rockchip,clk-trcm = <1>;
	pinctrl-names = "default";
	pinctrl-0 = <&i2s1m0_sclktx
		     &i2s1m0_lrcktx
		     &i2s1m0_sdi0
		     &i2s1m0_sdo0>;
};

&jpegd {
	status = "okay";
};

&jpegd_mmu {
	status = "okay";
};

&video_phy0 {
	status = "disabled";
};

&mpp_srv {
	status = "okay";
};

&nandc0 {
	status = "disabled";
};

&pinctrl {
	wacom {
		wacom_gpio: wacom-gpio {
			rockchip,pins =
					<3 RK_PA1 RK_FUNC_GPIO &pcfg_pull_up>,
					<3 RK_PA2 RK_FUNC_GPIO &pcfg_pull_up>,
					<3 RK_PA3 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};
	tsc {
		tsc_gpio: tsc-gpio {
			rockchip,pins =
					<3 RK_PB1 RK_FUNC_GPIO &pcfg_pull_up>,
					<3 RK_PB2 RK_FUNC_GPIO &pcfg_pull_up>,
					<3 RK_PC4 RK_FUNC_GPIO &pcfg_pull_up>,
					<3 RK_PC5 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	tps_pmic {
		tps65185_gpio: tps65185-gpio {
			rockchip,pins =
					<4 RK_PB2 RK_FUNC_GPIO &pcfg_pull_up>,
					<3 RK_PA5 RK_FUNC_GPIO &pcfg_pull_up>,
					<3 RK_PA6 RK_FUNC_GPIO &pcfg_pull_up>,
					<3 RK_PB0 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	tp {
		tp_gpio: tp-gpio {
			rockchip,pins =
				<3 RK_PB0 RK_FUNC_GPIO &pcfg_pull_up>,
				<3 RK_PB1 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	headphone {
		hp_det: hp-det {
			rockchip,pins = <4 RK_PC4 RK_FUNC_GPIO &pcfg_pull_down>;
		};
	};

	sensor {
		kxtj3_irq_gpio: kxtj3-irq-gpio {
			rockchip,pins = <4 RK_PC6 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	pmic {
		pmic_int: pmic_int {
			rockchip,pins =
				<0 RK_PA3 RK_FUNC_GPIO &pcfg_pull_up>;
		};

		soc_slppin_gpio: soc_slppin_gpio {
			rockchip,pins =
				<0 RK_PA2 RK_FUNC_GPIO &pcfg_output_low>;
		};

		soc_slppin_slp: soc_slppin_slp {
			rockchip,pins =
				<0 RK_PA2 1 &pcfg_pull_none>;
		};

		soc_slppin_rst: soc_slppin_rst {
			rockchip,pins =
				<0 RK_PA2 2 &pcfg_pull_none>;
		};
	};

	sdio-pwrseq {
		wifi_enable_h: wifi-enable-h {
			rockchip,pins = <2 RK_PB1 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	vcc_sd {
		vcc_sd_h: vcc-sd-h {
			rockchip,pins = <0 RK_PA5 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	wireless-wlan {
		wifi_host_wake_irq: wifi-host-wake-irq {
			rockchip,pins = <2 RK_PB2 RK_FUNC_GPIO &pcfg_pull_down>;
		};
	};

	wireless-bluetooth {
		uart1_gpios: uart1-gpios {
			rockchip,pins = <2 RK_PB5 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};
};

&pmu_io_domains {
	status = "okay";
	pmuio1-supply = <&vcc3v3_pmu>;
	pmuio2-supply = <&vcc3v3_pmu>;
	vccio1-supply = <&vccio_acodec>;
	vccio3-supply = <&vccio_sd>;
	vccio4-supply = <&vcc_3v3>;
	vccio5-supply = <&vcc_3v3>;
	vccio6-supply = <&vcc_3v3>;
	vccio7-supply = <&vcc_3v3>;
};

&pwm4 {
	status = "disabled";
};

&rk_rga {
	status = "okay";
};

&rkvdec {
	status = "okay";
};

&rkvdec_mmu {
	status = "okay";
};

&rkvenc {
	status = "okay";
};

&rkvenc_mmu {
	status = "okay";
};

&saradc {
	status = "disabled";
	vref-supply = <&vcc_1v8>;
};

&sdhci {
	bus-width = <8>;
	no-sdio;
	no-sd;
	non-removable;
	keep-power-in-suspend;
	max-frequency = <200000000>;
	status = "okay";
};

&sdmmc0 {
	max-frequency = <50000000>;
	no-sdio;
	no-mmc;
	bus-width = <4>;
	cap-mmc-highspeed;
	cap-sd-highspeed;
	disable-wp;
	sd-uhs-sdr104;
	vmmc-supply = <&vcc_sd>;
	vqmmc-supply = <&vccio_sd>;
	pinctrl-names = "default";
	pinctrl-0 = <&sdmmc0_bus4 &sdmmc0_clk &sdmmc0_cmd &sdmmc0_det>;
	status = "okay";
};

&sdmmc1 {
	max-frequency = <150000000>;
	no-sd;
	no-mmc;
	bus-width = <4>;
	disable-wp;
	cap-sd-highspeed;
	cap-sdio-irq;
	keep-power-in-suspend;
	mmc-pwrseq = <&sdio_pwrseq>;
	non-removable;
	pinctrl-names = "default";
	pinctrl-0 = <&sdmmc1_bus4 &sdmmc1_cmd &sdmmc1_clk>;
	sd-uhs-sdr104;
	status = "disabled";
};

&tsadc {
	status = "okay";
};

&uart1 {
	status = "disabled";
	pinctrl-names = "default";
	pinctrl-0 = <&uart1m0_xfer &uart1m0_ctsn>;
};

&u2phy0_otg {
	status = "okay";
};

&usb2phy0 {
	status = "okay";
};

&usbdrd_dwc3 {
	status = "okay";
};

&usbdrd30 {
	status = "okay";
};

&vdpu {
	status = "okay";
};

&vdpu_mmu {
	status = "okay";
};

&vepu {
	status = "okay";
};

&vepu_mmu {
	status = "okay";
};

&vop {
	status = "okay";
};

&vop_mmu {
	status = "okay";
};
