// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Copyright (c) 2020 Rockchip Electronics Co., Ltd.
 *
 */

/dts-v1/;

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/pinctrl/rockchip.h>
#include "rk3566.dtsi"
#include "rk3566-evb.dtsi"

/ {
	model = "Rockchip RK3566 EVB3 DDR3 V10 Board";
	compatible = "rockchip,rk3566-evb3-DDR3-v10", "rockchip,rk3566";

	rk_headset: rk-headset {
		compatible = "rockchip_headset";
		headset_gpio = <&gpio4 RK_PB3 GPIO_ACTIVE_LOW>;
		pinctrl-names = "default";
		pinctrl-0 = <&hp_det>;
	};

	vcc3v3_vga: vcc3v3-vga {
		compatible = "regulator-fixed";
		regulator-name = "vcc3v3_vga";
		regulator-always-on;
		regulator-boot-on;
		gpio = <&gpio4 RK_PB2 GPIO_ACTIVE_HIGH>;
		enable-active-high;
		vin-supply = <&vcc3v3_sys>;
	};

	vcc_camera: vcc-camera-regulator {
		compatible = "regulator-fixed";
		gpio = <&gpio0 RK_PC1 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&camera_pwr>;
		regulator-name = "vcc_camera";
		enable-active-high;
		regulator-always-on;
		regulator-boot-on;
	};
};

&bt_sound {
	status = "disabled";
	simple-audio-card,cpu {
		sound-dai = <&i2s2_2ch>;
	};
};

&combphy1_usq {
	status = "okay";
};

&csi2_dphy_hw {
	status = "okay";
};

&csi2_dphy0 {
	status = "okay";

	ports {
		#address-cells = <1>;
		#size-cells = <0>;
		port@0 {
			reg = <0>;
			#address-cells = <1>;
			#size-cells = <0>;

			mipi_in_ucam0: endpoint@1 {
				reg = <1>;
				remote-endpoint = <&ov5695_out>;
				data-lanes = <1 2>;
			};
			mipi_in_ucam1: endpoint@2 {
				reg = <2>;
				remote-endpoint = <&gc8034_out>;
				data-lanes = <1 2 3 4>;
			};
		};
		port@1 {
			reg = <1>;
			#address-cells = <1>;
			#size-cells = <0>;

			csidphy_out: endpoint@0 {
				reg = <0>;
				remote-endpoint = <&isp0_in>;
			};
		};
	};
};

/*
 * video_phy0 needs to be enabled
 * when dsi0 is enabled
 */
&dsi0 {
	status = "okay";
};

&dsi0_in_vp0 {
	status = "disabled";
};

&dsi0_in_vp1 {
	status = "okay";
};

&dsi0_panel {
	power-supply = <&vcc3v3_lcd0_n>;
	reset-gpios = <&gpio1 RK_PA5 GPIO_ACTIVE_LOW>;
	pinctrl-names = "default";
	pinctrl-0 = <&lcd0_rst_gpio>;
};

/*
 * video_phy1 needs to be enabled
 * when dsi1 is enabled
 */
&dsi1 {
	status = "disabled";
};

&dsi1_in_vp0 {
	status = "disabled";
};

&dsi1_in_vp1 {
	status = "disabled";
};

&dsi1_panel {
	power-supply = <&vcc3v3_lcd1_n>;
	reset-gpios = <&gpio4 RK_PC6 GPIO_ACTIVE_LOW>;
	pinctrl-names = "default";
	pinctrl-0 = <&lcd1_rst_gpio>;
};

&edp {
	hpd-gpios = <&gpio1 RK_PA7 GPIO_ACTIVE_HIGH>;
	status = "okay";
};

&edp_phy {
	status = "okay";
};

&edp_in_vp0 {
	status = "okay";
};

&edp_in_vp1 {
	status = "disabled";
};

&gmac1 {
	phy-mode = "rgmii";
	clock_in_out = "output";

	snps,reset-gpio = <&gpio3 RK_PA1 GPIO_ACTIVE_LOW>;
	snps,reset-active-low;
	/* Reset time is 20ms, 100ms for rtl8211f */
	snps,reset-delays-us = <0 20000 100000>;

	assigned-clocks = <&cru SCLK_GMAC1_RX_TX>, <&cru SCLK_GMAC1>;
	assigned-clock-parents = <&cru SCLK_GMAC1_RGMII_SPEED>, <&cru CLK_MAC1_2TOP>;
	assigned-clock-rates = <0>, <125000000>;

	pinctrl-names = "default";
	pinctrl-0 = <&gmac1m0_miim
		     &gmac1m0_tx_bus2_level3
		     &gmac1m0_rx_bus2
		     &gmac1m0_rgmii_clk_level2
		     &gmac1m0_rgmii_bus_level3>;

	tx_delay = <0x41>;
	rx_delay = <0x2e>;

	phy-handle = <&rgmii_phy1>;
	status = "okay";
};

&gt1x {
	power-supply = <&vcc3v3_lcd0_n>;
};

&i2c2 {
	status = "okay";
	pinctrl-0 = <&i2c2m1_xfer>;

	gc2145: gc2145@3c {
		status = "okay";
		compatible = "galaxycore,gc2145";
		reg = <0x3c>;
		clocks = <&cru CLK_CIF_OUT>;
		clock-names = "xvclk";
		power-domains = <&power RK3568_PD_VI>;
		pinctrl-names = "default";
		pinctrl-0 = <&cif_clk &cif_dvp_clk &cif_dvp_bus16>;

		/*avdd-supply = <&vcc2v8_dvp>;*/
		/*dovdd-supply = <&vcc1v8_dvp>;*/
		/*dvdd-supply = <&vcc1v8_dvp>;*/

		power-gpios = <&gpio3 RK_PD4 GPIO_ACTIVE_HIGH>;
		/*reset-gpios = <&gpio3 RK_PB5 GPIO_ACTIVE_LOW>;*/
		pwdn-gpios = <&gpio3 RK_PD2 GPIO_ACTIVE_HIGH>;
		rockchip,camera-module-index = <1>;
		rockchip,camera-module-facing = "front";
		rockchip,camera-module-name = "CameraKing";
		rockchip,camera-module-lens-name = "Largan";
		port {
			gc2145_out: endpoint {
				remote-endpoint = <&dvp_in_bcam>;
			};
		};
	};

	ov5695: ov5695@36 {
		status = "okay";
		compatible = "ovti,ov5695";
		reg = <0x36>;
		clocks = <&cru CLK_CAM0_OUT>;
		clock-names = "xvclk";
		power-domains = <&power RK3568_PD_VI>;
		pinctrl-names = "default";
		pinctrl-0 = <&cam_clkout0>;
		reset-gpios = <&gpio3 RK_PD0 GPIO_ACTIVE_HIGH>;
		pwdn-gpios = <&gpio3 RK_PC6 GPIO_ACTIVE_HIGH>;
		/*power-gpios = <&gpio0 RK_PC1 GPIO_ACTIVE_HIGH>;*/
		rockchip,camera-module-index = <0>;
		rockchip,camera-module-facing = "back";
		rockchip,camera-module-name = "TongJu";
		rockchip,camera-module-lens-name = "CHT842-MD";
		port {
			ov5695_out: endpoint {
				remote-endpoint = <&mipi_in_ucam0>;
				data-lanes = <1 2>;
			};
		};
	};

	gc8034: gc8034@37 {
		compatible = "galaxycore,gc8034";
		status = "okay";
		reg = <0x37>;
		clocks = <&cru CLK_CAM0_OUT>;
		clock-names = "xvclk";
		power-domains = <&power RK3568_PD_VI>;
		pinctrl-names = "default";
		pinctrl-0 = <&cam_clkout0>;
		reset-gpios = <&gpio3 RK_PD0 GPIO_ACTIVE_LOW>;
		pwdn-gpios = <&gpio3 RK_PC6 GPIO_ACTIVE_LOW>;
		rockchip,camera-module-index = <0>;
		rockchip,camera-module-facing = "back";
		rockchip,camera-module-name = "RK-CMK-8M-2-v1";
		rockchip,camera-module-lens-name = "CK8401";
		port {
			gc8034_out: endpoint {
				remote-endpoint = <&mipi_in_ucam1>;
				data-lanes = <1 2 3 4>;
			};
		};
	};

};

&i2s1_8ch {
	status = "disabled";
};

&i2s2_2ch {
	pinctrl-0 = <&i2s2m0_sclktx &i2s2m0_lrcktx &i2s2m0_sdi &i2s2m0_sdo>;
	rockchip,bclk-fs = <32>;
	status = "disabled";
};

&i2s3_2ch {
	status = "okay";
	pinctrl-names = "default";
	rockchip,clk-trcm = <1>;
	pinctrl-0 = <&i2s3m1_sclk
		     &i2s3m1_lrck
		     &i2s3m1_sdi
		     &i2s3m1_sdo>;
};

&mdio1 {
	rgmii_phy1: phy@0 {
		compatible = "ethernet-phy-ieee802.3-c22";
		reg = <0x0>;
	};
};

&video_phy0 {
	status = "okay";
};

&video_phy1 {
	status = "disabled";
};

&pdm {
	status = "disabled";
	pinctrl-names = "default";
	pinctrl-0 = <&pdmm1_clk1
		     &pdmm1_sdi1
		     &pdmm1_sdi2
		     &pdmm1_sdi3>;
};

&pdmics {
	status = "disabled";
};

&pdm_mic_array {
	status = "disabled";
};

&pinctrl {
	cam {
		camera_pwr: camera-pwr {
			rockchip,pins =
				/* camera power en */
				<0 RK_PC1 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	headphone {
		hp_det: hp-det {
			rockchip,pins = <4 RK_PB3 RK_FUNC_GPIO &pcfg_pull_down>;
		};
	};

	lcd0 {
		lcd0_rst_gpio: lcd-rst-gpio {
			rockchip,pins = <1 RK_PA5 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	lcd1 {
		lcd1_rst_gpio: lcd1-rst-gpio {
			rockchip,pins = <4 RK_PC6 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	sdio-pwrseq {
		wifi_enable_h: wifi-enable-h {
			rockchip,pins = <2 RK_PB1 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	wireless-wlan {
		wifi_host_wake_irq: wifi-host-wake-irq {
			rockchip,pins = <2 RK_PB2 RK_FUNC_GPIO &pcfg_pull_down>;
		};
	};

	wireless-bluetooth {
		uart1_gpios: uart1-gpios {
			rockchip,pins = <2 RK_PB5 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};
};

&rkcif {
	status = "okay";
};

&rkcif_dvp {
	status = "okay";

	port {
		/* Parallel bus endpoint */
		dvp_in_bcam: endpoint {
			remote-endpoint = <&gc2145_out>;
			bus-width = <8>;
			vsync-active = <0>;
			hsync-active = <1>;
		};
	};
};

&rkisp {
	status = "okay";
};

&rkisp_mmu {
	status = "okay";
};

&rkisp_vir0 {
	status = "okay";

	port {
		#address-cells = <1>;
		#size-cells = <0>;

		isp0_in: endpoint@0 {
			reg = <0>;
			remote-endpoint = <&csidphy_out>;
		};
	};
};

&rk809_codec {
	compatible = "rockchip,rk809-codec", "rockchip,rk817-codec";
	clocks = <&cru I2S3_MCLKOUT>;
	clock-names = "mclk";
	assigned-clocks = <&cru I2S3_MCLKOUT>, <&cru I2S3_MCLK_IOE>;
	assigned-clock-rates = <12288000>;
	assigned-clock-parents = <&cru I2S3_MCLKOUT_TX>, <&cru I2S3_MCLKOUT>;
	pinctrl-names = "default";
	pinctrl-0 = <&i2s3m1_mclk>;
	hp-volume = <20>;
	spk-volume = <3>;
	mic-in-differential;
	status = "okay";
};

&rk809_sound {
	status = "okay";
	compatible = "simple-audio-card";
	simple-audio-card,format = "i2s";
	simple-audio-card,name = "rockchip,rk809-codec";
	simple-audio-card,mclk-fs = <256>;

	simple-audio-card,cpu {
		sound-dai = <&i2s3_2ch>;
	};
	simple-audio-card,codec {
		sound-dai = <&rk809_codec 0>;
	};
};

&route_dsi0 {
	status = "okay";
	connect = <&vp1_out_dsi0>;
};

&sata1 {
	status = "okay";
};

&sdio_pwrseq {
	reset-gpios = <&gpio2 RK_PB1 GPIO_ACTIVE_LOW>;
};

&sdmmc1 {
	max-frequency = <150000000>;
	no-sd;
	no-mmc;
	bus-width = <4>;
	disable-wp;
	cap-sd-highspeed;
	cap-sdio-irq;
	keep-power-in-suspend;
	mmc-pwrseq = <&sdio_pwrseq>;
	non-removable;
	pinctrl-names = "default";
	pinctrl-0 = <&sdmmc1_bus4 &sdmmc1_cmd &sdmmc1_clk>;
	sd-uhs-sdr104;
	status = "okay";
};

&sdmmc2 {
	status = "disabled";
};

&spdif_8ch {
	status = "disabled";
};

&uart1 {
	status = "okay";
	pinctrl-names = "default";
	pinctrl-0 = <&uart1m0_xfer &uart1m0_ctsn>;
};

&vcc3v3_lcd0_n {
	gpio = <&gpio0 RK_PC0 GPIO_ACTIVE_HIGH>;
	enable-active-high;
};

&wireless_bluetooth {
	compatible = "bluetooth-platdata";
	clocks = <&rk809 1>;
	clock-names = "ext_clock";
	//wifi-bt-power-toggle;
	uart_rts_gpios = <&gpio2 RK_PB5 GPIO_ACTIVE_LOW>;
	pinctrl-names = "default", "rts_gpio";
	pinctrl-0 = <&uart1m0_rtsn>;
	pinctrl-1 = <&uart1_gpios>;
	BT,reset_gpio    = <&gpio2 RK_PB7 GPIO_ACTIVE_HIGH>;
	BT,wake_gpio     = <&gpio2 RK_PC1 GPIO_ACTIVE_HIGH>;
	BT,wake_host_irq = <&gpio2 RK_PC0 GPIO_ACTIVE_HIGH>;
	status = "okay";
};

&wireless_wlan {
	pinctrl-names = "default";
	pinctrl-0 = <&wifi_host_wake_irq>;
	WIFI,host_wake_irq = <&gpio2 RK_PB2 GPIO_ACTIVE_HIGH>;
	WIFI,poweren_gpio = <&gpio2 RK_PB1 GPIO_ACTIVE_HIGH>;
};

&work_led {
	gpios = <&gpio0 RK_PD3 GPIO_ACTIVE_HIGH>;
};
