// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Copyright (c) 2023 Rockchip Electronics Co., Ltd.
 *
 */

#include "dt-bindings/usb/pd.h"
#include "rk3588.dtsi"
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/pwm/pwm.h>
#include <dt-bindings/pinctrl/rockchip.h>
#include <dt-bindings/input/rk-input.h>
#include <dt-bindings/display/drm_mipi_dsi.h>
#include <dt-bindings/display/rockchip_vop.h>
#include "rk3588-rk806-single.dtsi"

/ {
	adc_keys: adc-keys {
		compatible = "adc-keys";
		io-channels = <&saradc 1>;
		io-channel-names = "buttons";
		keyup-threshold-microvolt = <1800000>;
		poll-interval = <100>;

		vol-up-key {
			label = "volume up";
			linux,code = <KEY_VOLUMEUP>;
			press-threshold-microvolt = <17000>;
		};
	};

	dp0_sound: dp0-sound {
		status = "disabled";
		compatible = "rockchip,hdmi";
		rockchip,card-name= "rockchip-dp0";
		rockchip,mclk-fs = <512>;
		rockchip,cpu = <&spdif_tx2>;
		rockchip,codec = <&dp0 1>;
		rockchip,jack-det;
	};

	hdmi1_sound: hdmi1-sound {
		status = "disabled";
		compatible = "rockchip,hdmi";
		rockchip,mclk-fs = <128>;
		rockchip,card-name = "rockchip-hdmi1";
		rockchip,cpu = <&i2s6_8ch>;
		rockchip,codec = <&hdmi1>;
		rockchip,jack-det;
	};

	leds: leds {
		compatible = "gpio-leds";
		work_led: work {
			gpios = <&gpio0 RK_PB7 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "heartbeat";
		};
	};

	pcie30_avdd1v8: pcie30-avdd1v8 {
		compatible = "regulator-fixed";
		regulator-name = "pcie30_avdd1v8";
		regulator-boot-on;
		regulator-always-on;
		regulator-min-microvolt = <1800000>;
		regulator-max-microvolt = <1800000>;
		vin-supply = <&avcc_1v8_s0>;
	};

	pcie30_avdd0v75: pcie30-avdd0v75 {
		compatible = "regulator-fixed";
		regulator-name = "pcie30_avdd0v75";
		regulator-boot-on;
		regulator-always-on;
		regulator-min-microvolt = <750000>;
		regulator-max-microvolt = <750000>;
		vin-supply = <&avdd_0v75_s0>;
	};

	reserved-memory {
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;
		bar0_region: bar0-region@3c000000 {
			reg = <0x0 0x3c000000 0x0 0x00400000>;
		};
		bar2_region: bar2-region@40000000 {
			reg = <0x0 0x40000000 0x0 0x04000000>;
		};
	};

	test-power {
		status = "okay";
	};

	vbus5v0_typec: vbus5v0-typec {
		compatible = "regulator-fixed";
		regulator-name = "vbus5v0_typec";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		enable-active-high;
		gpio = <&gpio4 RK_PA0 GPIO_ACTIVE_HIGH>;
		vin-supply = <&vcc5v0_usb>;
		pinctrl-names = "default";
		pinctrl-0 = <&typec5v_pwren>;
	};

	vcc12v_dcin: vcc12v-dcin {
		compatible = "regulator-fixed";
		regulator-name = "vcc12v_dcin";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <12000000>;
		regulator-max-microvolt = <12000000>;
	};

	vcc5v0_usb: vcc5v0-usb {
		compatible = "regulator-fixed";
		regulator-name = "vcc5v0_usb";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		vin-supply = <&vcc12v_dcin>;
	};

	vcc5v0_sys: vcc5v0-sys {
		compatible = "regulator-fixed";
		regulator-name = "vcc5v0_sys";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		vin-supply = <&vcc12v_dcin>;
	};

	vcc_1v1_nldo_s3: vcc-1v1-nldo-s3 {
		compatible = "regulator-fixed";
		regulator-name = "vcc_1v1_nldo_s3";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <1100000>;
		regulator-max-microvolt = <1100000>;
		vin-supply = <&vcc5v0_sys>;
	};
};

&av1d_mmu {
	status = "okay";
};

&cpu_l0 {
	cpu-supply = <&vdd_cpu_lit_s0>;
	mem-supply = <&vdd_cpu_lit_mem_s0>;
};

&cpu_b0 {
	cpu-supply = <&vdd_cpu_big0_s0>;
	mem-supply = <&vdd_cpu_big0_mem_s0>;
};

&cpu_b2 {
	cpu-supply = <&vdd_cpu_big1_s0>;
	mem-supply = <&vdd_cpu_big1_mem_s0>;
};

&dp0 {
	status = "okay";
};

&dp0_in_vp2 {
	status = "okay";
};

&gpu {
	mali-supply = <&vdd_gpu_s0>;
	mem-supply = <&vdd_gpu_mem_s0>;
	status = "okay";
};

&hdmi1 {
	enable-gpios = <&gpio4 RK_PA1 GPIO_ACTIVE_HIGH>;
	pinctrl-names = "default";
	pinctrl-0 = <&hdmim2_tx1_cec &hdmim1_tx1_hpd &hdmim1_tx1_scl &hdmim1_tx1_sda>;
	status = "okay";
};

&hdmi1_in_vp0 {
	status = "okay";
};

&hdmi1_sound {
	status = "okay";
};

&hdptxphy_hdmi1 {
	status = "okay";
};

&gmac0 {
	/* Use rgmii-rxid mode to disable rx delay inside Soc */
	phy-mode = "rgmii-rxid";
	clock_in_out = "output";

	snps,reset-gpio = <&gpio4 RK_PB2 GPIO_ACTIVE_LOW>;
	snps,reset-active-low;
	/* Reset time is 20ms, 100ms for rtl8211f */
	snps,reset-delays-us = <0 20000 100000>;

	pinctrl-names = "default";
	pinctrl-0 = <&gmac0_miim
		     &gmac0_tx_bus2
		     &gmac0_rx_bus2
		     &gmac0_rgmii_clk
		     &gmac0_rgmii_bus
		     &eth0_pins>;

	tx_delay = <0x44>;
	/* rx_delay = <0x4f>; */

	phy-handle = <&rgmii_phy0>;
	status = "okay";
};

&iep {
	status = "okay";
};

&iep_mmu {
	status = "okay";
};

&i2c0 {
	status = "okay";
	pinctrl-names = "default";
	pinctrl-0 = <&i2c0m2_xfer>;

	vdd_cpu_big0_s0: vdd_cpu_big0_mem_s0: rk8602@42 {
		compatible = "rockchip,rk8602";
		reg = <0x42>;
		vin-supply = <&vcc5v0_sys>;
		regulator-compatible = "rk860x-reg";
		regulator-name = "vdd_cpu_big0_s0";
		regulator-min-microvolt = <550000>;
		regulator-max-microvolt = <1050000>;
		regulator-ramp-delay = <2300>;
		rockchip,suspend-voltage-selector = <1>;
		regulator-boot-on;
		regulator-always-on;
		regulator-state-mem {
			regulator-off-in-suspend;
		};
	};

	vdd_cpu_big1_s0: vdd_cpu_big1_mem_s0: rk8603@43 {
		compatible = "rockchip,rk8603";
		reg = <0x43>;
		vin-supply = <&vcc5v0_sys>;
		regulator-compatible = "rk860x-reg";
		regulator-name = "vdd_cpu_big1_s0";
		regulator-min-microvolt = <550000>;
		regulator-max-microvolt = <1050000>;
		regulator-ramp-delay = <2300>;
		rockchip,suspend-voltage-selector = <1>;
		regulator-boot-on;
		regulator-always-on;
		regulator-state-mem {
			regulator-off-in-suspend;
		};
	};
};

&i2c1 {
	status = "okay";
	pinctrl-names = "default";
	pinctrl-0 = <&i2c1m2_xfer>;

	vdd_npu_s0: vdd_npu_mem_s0: rk8602@42 {
		compatible = "rockchip,rk8602";
		reg = <0x42>;
		vin-supply = <&vcc5v0_sys>;
		regulator-compatible = "rk860x-reg";
		regulator-name = "vdd_npu_s0";
		regulator-min-microvolt = <550000>;
		regulator-max-microvolt = <950000>;
		regulator-ramp-delay = <2300>;
		rockchip,suspend-voltage-selector = <1>;
		regulator-boot-on;
		regulator-always-on;
		regulator-state-mem {
			regulator-off-in-suspend;
		};
	};
};

&i2c4 {
	status = "okay";
	pinctrl-names = "default";
	pinctrl-0 = <&i2c4m2_xfer>;

	usbc0: fusb302@22 {
		compatible = "fcs,fusb302";
		reg = <0x22>;
		interrupt-parent = <&gpio0>;
		interrupts = <RK_PB0 IRQ_TYPE_LEVEL_LOW>;
		pinctrl-names = "default";
		pinctrl-0 = <&usbc0_int>;
		vbus-supply = <&vbus5v0_typec>;
		status = "okay";

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				usbc0_role_sw: endpoint@0 {
					remote-endpoint = <&dwc3_0_role_switch>;
				};
			};
		};

		usb_con: connector {
			compatible = "usb-c-connector";
			label = "USB-C";
			data-role = "dual";
			power-role = "dual";
			try-power-role = "sink";
			op-sink-microwatt = <1000000>;
			sink-pdos =
				<PDO_FIXED(5000, 1000, PDO_FIXED_USB_COMM)>;
			source-pdos =
				<PDO_FIXED(5000, 3000, PDO_FIXED_USB_COMM)>;

			altmodes {
				#address-cells = <1>;
				#size-cells = <0>;

				altmode@0 {
					reg = <0>;
					svid = <0xff01>;
					vdo = <0xffffffff>;
				};
			};

			ports {
				#address-cells = <1>;
				#size-cells = <0>;

				port@0 {
					reg = <0>;
					usbc0_orien_sw: endpoint {
						remote-endpoint = <&usbdp_phy0_orientation_switch>;
					};
				};

				port@1 {
					reg = <1>;
					dp_altmode_mux: endpoint {
						remote-endpoint = <&usbdp_phy0_dp_altmode_mux>;
					};
				};
			};
		};
	};
};

&i2s6_8ch {
	status = "okay";
};

&jpegd {
	status = "okay";
};

&jpegd_mmu {
	status = "okay";
};

&jpege_ccu {
	status = "okay";
};

&jpege0 {
	status = "okay";
};

&jpege0_mmu {
	status = "okay";
};

&jpege1 {
	status = "okay";
};

&jpege1_mmu {
	status = "okay";
};

&jpege2 {
	status = "okay";
};

&jpege2_mmu {
	status = "okay";
};

&jpege3 {
	status = "okay";
};

&jpege3_mmu {
	status = "okay";
};

&mdio0 {
	rgmii_phy0: phy@1 {
		compatible = "ethernet-phy-ieee802.3-c22";
		reg = <0x1>;
		clocks = <&cru REFCLKO25M_ETH0_OUT>;
	};
};

&mpp_srv {
	status = "okay";
};

&pcie30phy {
	status = "okay";
};

&pcie3x4 {
	compatible = "rockchip,rk3588-pcie-std-ep";
	memory-region = <&bar0_region>, <&bar2_region>;
	memory-region-names = "bar0", "bar2";
	status = "okay";
};

&rga3_core0 {
	status = "okay";
};

&rga3_0_mmu {
	status = "okay";
};

&rga3_core1 {
	status = "okay";
};

&rga3_1_mmu {
	status = "okay";
};

&rga2 {
	status = "okay";
};

&rknpu {
	rknpu-supply = <&vdd_npu_s0>;
	mem-supply = <&vdd_npu_mem_s0>;
	status = "okay";
};

&rknpu_mmu {
	status = "okay";
};

&rkvdec_ccu {
	status = "okay";
};

&rkvdec0 {
	status = "okay";
};

&rkvdec0_mmu {
	status = "okay";
};

&rkvdec1 {
	status = "okay";
};

&rkvdec1_mmu {
	status = "okay";
};

&rkvenc_ccu {
	status = "okay";
};

&rkvenc0 {
	status = "okay";
};

&rkvenc0_mmu {
	status = "okay";
};

&rkvenc1 {
	status = "okay";
};

&rkvenc1_mmu {
	status = "okay";
};

&rockchip_suspend {
	status = "okay";
	rockchip,sleep-debug-en = <1>;
};

&route_hdmi1 {
	status = "okay";
};

&saradc {
	status = "okay";
	vref-supply = <&vcc_1v8_s0>;
};

&sdhci {
	bus-width = <8>;
	no-sdio;
	no-sd;
	non-removable;
	max-frequency = <200000000>;
	mmc-hs400-1_8v;
	mmc-hs400-enhanced-strobe;
	status = "okay";
};

&tsadc {
	status = "okay";
};

&u2phy0 {
	status = "okay";
};

&u2phy0_otg {
	status = "okay";
};

&usbdp_phy0_dp {
	status = "okay";
};

&usbdp_phy0_u3 {
	status = "okay";
};

&usbdrd3_0 {
	status = "okay";
};

&usbdp_phy0 {
	status = "okay";
	orientation-switch;
	svid = <0xff01>;
	sbu1-dc-gpios = <&gpio4 RK_PA6 GPIO_ACTIVE_HIGH>;
	sbu2-dc-gpios = <&gpio4 RK_PA7 GPIO_ACTIVE_HIGH>;

	port {
		#address-cells = <1>;
		#size-cells = <0>;
		usbdp_phy0_orientation_switch: endpoint@0 {
			reg = <0>;
			remote-endpoint = <&usbc0_orien_sw>;
		};

		usbdp_phy0_dp_altmode_mux: endpoint@1 {
			reg = <1>;
			remote-endpoint = <&dp_altmode_mux>;
		};
	};
};

&usbdrd_dwc3_0 {
	status = "okay";
	dr_mode = "otg";
	usb-role-switch;
	port {
		#address-cells = <1>;
		#size-cells = <0>;
		dwc3_0_role_switch: endpoint@0 {
			reg = <0>;
			remote-endpoint = <&usbc0_role_sw>;
		};
	};
};

&vdpu {
	status = "okay";
};

&vdpu_mmu {
	status = "okay";
};

&vepu {
	status = "okay";
};

&vop {
	status = "okay";
};

&vop_mmu {
	status = "okay";
};

/* vp0 & vp1 splice for 8K output */
&vp0 {
	rockchip,plane-mask = <(1 << ROCKCHIP_VOP2_CLUSTER0 | 1 << ROCKCHIP_VOP2_ESMART0)>;
	rockchip,primary-plane = <ROCKCHIP_VOP2_ESMART0>;
};

&vp1 {
	rockchip,plane-mask = <(1 << ROCKCHIP_VOP2_CLUSTER1 | 1 << ROCKCHIP_VOP2_ESMART1)>;
	rockchip,primary-plane = <ROCKCHIP_VOP2_ESMART1>;
};

&vp2 {
	rockchip,plane-mask = <(1 << ROCKCHIP_VOP2_CLUSTER2 | 1 << ROCKCHIP_VOP2_ESMART2)>;
	rockchip,primary-plane = <ROCKCHIP_VOP2_ESMART2>;
};

&pinctrl {

	usb-typec {
		usbc0_int: usbc0-int {
			rockchip,pins = <0 RK_PB0 RK_FUNC_GPIO &pcfg_pull_up>;
		};

		typec5v_pwren: typec5v-pwren {
			rockchip,pins = <4 RK_PA0 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};
};
