// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/dts-v1/;
#include <dt-bindings/pwm/pwm.h>
#include <dt-bindings/input/input.h>
#include "rk3399.dtsi"
#include "rk3399-opp.dtsi"

/ {
	model = "Hugsun X99 TV BOX";
	compatible = "hugsun,x99", "rockchip,rk3399";

	chosen {
		stdout-path = "serial2:1500000n8";
	};

	clkin_gmac: external-gmac-clock {
		compatible = "fixed-clock";
		clock-frequency = <125000000>;
		clock-output-names = "clkin_gmac";
		#clock-cells = <0>;
	};

	dc_5v: dc-5v {
		compatible = "regulator-fixed";
		regulator-name = "dc_5v";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
	};

	ir-receiver {
		compatible = "gpio-ir-receiver";
		gpios = <&gpio0 RK_PA6 GPIO_ACTIVE_LOW>;
		pinctrl-names = "default";
		pinctrl-0 = <&ir_rx>;
	};

	leds {
		compatible = "gpio-leds";
		pinctrl-names = "default";
		pinctrl-0 = <&power_led_pin>;

		power_led: led-0 {
			label = "blue:power";
			gpios = <&gpio4 RK_PC2 GPIO_ACTIVE_HIGH>;
			default-state = "on";
			linux,default-trigger = "default-on";
		};
	};

	vcc_sys: vcc-sys {
		compatible = "regulator-fixed";
		regulator-name = "vcc_sys";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		regulator-always-on;
		vin-supply = <&dc_5v>;
	};

	vcc_phy: vcc-phy-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vcc_phy";
		regulator-always-on;
		regulator-boot-on;
	};

	vcc1v8_s0: vcc1v8-s0 {
		compatible = "regulator-fixed";
		regulator-name = "vcc1v8_s0";
		regulator-min-microvolt = <1800000>;
		regulator-max-microvolt = <1800000>;
		regulator-always-on;
	};

	vcc3v3_sys: vcc3v3-sys {
		compatible = "regulator-fixed";
		regulator-name = "vcc3v3_sys";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-always-on;
		vin-supply = <&vcc_sys>;
	};

	vcc5v0_host: vcc5v0-host-regulator {
		compatible = "regulator-fixed";
		enable-active-high;
		gpio = <&gpio4 RK_PD2 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&host_vbus_drv>;
		regulator-name = "vcc5v0_host";
		regulator-always-on;
	};

	vcc5v0_typec: vcc5v0-typec-regulator {
		compatible = "regulator-fixed";
		enable-active-high;
		gpio = <&gpio1 RK_PA3 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&vcc5v0_typec_en>;
		regulator-name = "vcc5v0_typec";
		regulator-always-on;
		vin-supply = <&vcc5v0_usb>;
	};

	vcc5v0_usb: vcc5v0-usb {
		compatible = "regulator-fixed";
		regulator-name = "vcc5v0_usb";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		vin-supply = <&dc_5v>;
	};

	vdd_log: vdd-log {
		compatible = "pwm-regulator";
		pwms = <&pwm2 0 25000 1>;
		pwm-supply = <&vcc_sys>;
		regulator-name = "vdd_log";
		regulator-min-microvolt = <800000>;
		regulator-max-microvolt = <1400000>;
		regulator-always-on;
		regulator-boot-on;
	};

	sdio_pwrseq: sdio-pwrseq {
		compatible = "mmc-pwrseq-simple";
		clocks = <&rk808 1>;
		clock-names = "ext_clock";
		pinctrl-names = "default";
		pinctrl-0 = <&wifi_reg_on_h>;
		reset-gpios = <&gpio0 RK_PB2 GPIO_ACTIVE_LOW>;
	};

};

&cpu_l0 {
	cpu-supply = <&vdd_cpu_l>;
};

&cpu_l1 {
	cpu-supply = <&vdd_cpu_l>;
};

&cpu_l2 {
	cpu-supply = <&vdd_cpu_l>;
};

&cpu_l3 {
	cpu-supply = <&vdd_cpu_l>;
};

&cpu_b0 {
	cpu-supply = <&vdd_cpu_b>;
};

&cpu_b1 {
	cpu-supply = <&vdd_cpu_b>;
};

&emmc_phy {
	status = "okay";
};

&gmac {
	assigned-clocks = <&cru SCLK_RMII_SRC>;
	assigned-clock-parents = <&clkin_gmac>;
	clock_in_out = "input";
	phy-supply = <&vcc_phy>;
	phy-mode = "rgmii";
	pinctrl-names = "default";
	pinctrl-0 = <&rgmii_pins>;
	snps,reset-gpio = <&gpio3 RK_PB7 GPIO_ACTIVE_LOW>;
	snps,reset-active-low;
	snps,reset-delays-us = <0 10000 50000>;
	tx_delay = <0x28>;
	rx_delay = <0x11>;
	status = "okay";
};

&gpu {
	status = "okay";
	mali-supply = <&vdd_gpu>;
};

&hdmi {
	ddc-i2c-bus = <&i2c3>;
	pinctrl-names = "default";
	pinctrl-0 = <&hdmi_cec>;
	status = "okay";
};

&hdmi_sound {
	status = "okay";
};

&i2c0 {
	status = "okay";
	i2c-scl-rising-time-ns = <180>;
	i2c-scl-falling-time-ns = <30>;
	clock-frequency = <400000>;

	vdd_cpu_b: syr827@40 {
		compatible = "silergy,syr827";
		reg = <0x40>;
		regulator-compatible = "fan53555-reg";
		pinctrl-0 = <&vsel1_pin>;
		regulator-name = "vdd_cpu_b";
		regulator-min-microvolt = <712500>;
		regulator-max-microvolt = <1500000>;
		regulator-ramp-delay = <1000>;
		fcs,suspend-voltage-selector = <1>;
		regulator-always-on;
		regulator-boot-on;
		vin-supply = <&vcc_sys>;
		regulator-state-mem {
			regulator-off-in-suspend;
		};
	};

	vdd_gpu: syr828@41 {
		compatible = "silergy,syr828";
		reg = <0x41>;
		regulator-compatible = "fan53555-reg";
		pinctrl-0 = <&vsel2_pin>;
		regulator-name = "vdd_gpu";
		regulator-min-microvolt = <712500>;
		regulator-max-microvolt = <1500000>;
		regulator-ramp-delay = <1000>;
		fcs,suspend-voltage-selector = <1>;
		regulator-always-on;
		regulator-boot-on;
		vin-supply = <&vcc_sys>;
		regulator-initial-mode = <1>;
		regulator-state-mem {
			regulator-off-in-suspend;
		};
	};

	rk808: pmic@1b {
		compatible = "rockchip,rk808";
		reg = <0x1b>;
		interrupt-parent = <&gpio1>;
		interrupts = <21 IRQ_TYPE_LEVEL_LOW>;
		pinctrl-names = "default";
		pinctrl-0 = <&pmic_int_l>;
		rockchip,system-power-controller;
		wakeup-source;
		#clock-cells = <1>;
		clock-output-names = "xin32k", "rtc_clko_wifi";

		vcc1-supply = <&vcc_sys>;
		vcc2-supply = <&vcc_sys>;
		vcc3-supply = <&vcc_sys>;
		vcc4-supply = <&vcc_sys>;
		vcc6-supply = <&vcc_sys>;
		vcc7-supply = <&vcc_sys>;
		vcc8-supply = <&vcc3v3_sys>;
		vcc9-supply = <&vcc_sys>;
		vcc10-supply = <&vcc_sys>;
		vcc11-supply = <&vcc_sys>;
		vcc12-supply = <&vcc3v3_sys>;
		vddio-supply = <&vcc_1v8>;

		regulators {
			vdd_center: DCDC_REG1 {
				regulator-name = "vdd_center";
				regulator-min-microvolt = <900000>;
				regulator-max-microvolt = <900000>;
				regulator-ramp-delay = <6001>;
				regulator-always-on;
				regulator-boot-on;
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd_cpu_l: DCDC_REG2 {
				regulator-name = "vdd_cpu_l";
				regulator-min-microvolt = <750000>;
				regulator-max-microvolt = <1350000>;
				regulator-ramp-delay = <6001>;
				regulator-always-on;
				regulator-boot-on;
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_ddr: DCDC_REG3 {
				regulator-name = "vcc_ddr";
				regulator-always-on;
				regulator-boot-on;
				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};

			vcc_1v8: DCDC_REG4 {
				regulator-name = "vcc_1v8";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-always-on;
				regulator-boot-on;
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vcc1v8_dvp: LDO_REG1 {
				regulator-name = "vcc1v8_dvp";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-always-on;
				regulator-boot-on;
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vcca1v8_hdmi: LDO_REG2 {
				regulator-name = "vcca1v8_hdmi";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-always-on;
				regulator-boot-on;
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vcca_1v8: LDO_REG3 {
				regulator-name = "vcca_1v8";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-always-on;
				regulator-boot-on;
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vcc_sd: LDO_REG4 {
				regulator-name = "vcc_sd";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
				regulator-boot-on;
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vcc3v0_sd: LDO_REG5 {
				regulator-name = "vcc3v0_sd";
				regulator-min-microvolt = <3000000>;
				regulator-max-microvolt = <3000000>;
				regulator-always-on;
				regulator-boot-on;
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3000000>;
				};
			};

			vcc_1v5: LDO_REG6 {
				regulator-name = "vcc_1v5";
				regulator-min-microvolt = <1500000>;
				regulator-max-microvolt = <1500000>;
				regulator-always-on;
				regulator-boot-on;
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1500000>;
				};
			};

			vcca0v9_hdmi: LDO_REG7 {
				regulator-name = "vcca0v9_hdmi";
				regulator-min-microvolt = <900000>;
				regulator-max-microvolt = <900000>;
				regulator-always-on;
				regulator-boot-on;
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <900000>;
				};
			};

			vcc_3v0: LDO_REG8 {
				regulator-name = "vcc_3v0";
				regulator-min-microvolt = <3000000>;
				regulator-max-microvolt = <3000000>;
				regulator-always-on;
				regulator-boot-on;
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3000000>;
				};
			};

			vcc3v3_s3: SWITCH_REG1 {
				regulator-name = "vcc3v3_s3";
				regulator-always-on;
				regulator-boot-on;
				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};

			vcc3v3_s0: SWITCH_REG2 {
				regulator-name = "vcc3v3_s0";
				regulator-always-on;
				regulator-boot-on;
				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};
		};
	};
};

&i2c1 {
	i2c-scl-rising-time-ns = <300>;
	i2c-scl-falling-time-ns = <15>;
	status = "okay";
};

&i2c3 {
	i2c-scl-rising-time-ns = <450>;
	i2c-scl-falling-time-ns = <15>;
	status = "okay";
};

&i2c4 {
	i2c-scl-rising-time-ns = <600>;
	i2c-scl-falling-time-ns = <40>;
	status = "okay";

	fusb0: typec-portc@22 {
		compatible = "fcs,fusb302";
		reg = <0x22>;
		interrupt-parent = <&gpio1>;
		interrupts = <RK_PA2 IRQ_TYPE_LEVEL_LOW>;
		pinctrl-names = "default";
		pinctrl-0 = <&fusb0_int>;
		vbus-supply = <&vcc5v0_typec>;
		status = "okay";
	};
};

&i2c7 {
	status = "okay";
};

&i2s0 {
	rockchip,playback-channels = <8>;
	rockchip,capture-channels = <8>;
	status = "okay";
};

&i2s1 {
	rockchip,playback-channels = <2>;
	rockchip,capture-channels = <2>;
	status = "okay";
};

&i2s2 {
	status = "okay";
};

&io_domains {
	status = "okay";
	audio-supply = <&vcc1v8_s0>;
	bt656-supply = <&vcc1v8_s0>;
	gpio1830-supply = <&vcc_3v0>;
	sdmmc-supply = <&vcc_sd>;
};

&pmu_io_domains {
	status = "okay";
	pmu1830-supply = <&vcc_1v8>;
};

&pinctrl {
	fusb30x {
		fusb0_int: fusb0-int {
			rockchip,pins =
				<1 RK_PA2 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	gmac {
		rgmii_sleep_pins: rgmii-sleep-pins {
			rockchip,pins =
				<3 RK_PB7 RK_FUNC_GPIO &pcfg_output_low>;
		};
	};

	ir {
		ir_rx: ir-rx {
			rockchip,pins = <0 RK_PA6 1 &pcfg_pull_none>;
		};
	};

	leds {
		power_led_pin: power-led-pin {
			rockchip,pins = <4 RK_PC2 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	pmic {
		pmic_int_l: pmic-int-l {
			rockchip,pins =
				<1 RK_PC5 RK_FUNC_GPIO &pcfg_pull_up>;
		};

		vsel1_pin: vsel1-pin {
			rockchip,pins =
				<1 RK_PC1 RK_FUNC_GPIO &pcfg_pull_down>;
		};

		vsel2_pin: vsel2-pin {
			rockchip,pins =
				<1 RK_PB6 RK_FUNC_GPIO &pcfg_pull_down>;
		};
	};

	sdio {
		bt_host_wake_l: bt-host-wake-l {
			rockchip,pins = <0 RK_PA4 RK_FUNC_GPIO &pcfg_pull_none>;
		};

		bt_reg_on_h: bt-reg-on-h {
			/* external pullup to VCC1V8_PMUPLL */
			rockchip,pins = <0 RK_PB1 RK_FUNC_GPIO &pcfg_pull_none>;
		};

		bt_wake_l: bt-wake-l {
			rockchip,pins = <2 RK_PD2 RK_FUNC_GPIO &pcfg_pull_none>;
		};

		wifi_reg_on_h: wifi-reg_on-h {
			rockchip,pins = <0 RK_PB2 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	wifi {
		wifi_host_wake_l: wifi-host-wake-l {
			rockchip,pins = <0 RK_PA3 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	usb-typec {
		vcc5v0_typec_en: vcc5v0_typec_en {
			rockchip,pins = <1 RK_PA3 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	usb2 {
		host_vbus_drv: host-vbus-drv {
			rockchip,pins =
				<4 RK_PD2 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};
};

&pwm2 {
	status = "okay";
	pinctrl-0 = <&pwm2_pin_pull_down>;
};

&saradc {
	vref-supply = <&vcc1v8_s0>;
	status = "okay";
};

&sdmmc {
	clock-frequency = <150000000>;
	max-frequency = <150000000>;
	bus-width = <4>;
	cap-mmc-highspeed;
	cap-sd-highspeed;
	disable-wp;
	vqmmc-supply = <&vcc_sd>;
	pinctrl-names = "default";
	pinctrl-0 = <&sdmmc_clk &sdmmc_cmd &sdmmc_cd &sdmmc_bus4>;
	card-detect-delay = <800>;
	status = "okay";
};

&sdhci {
	bus-width = <8>;
	mmc-hs400-1_8v;
	mmc-hs400-enhanced-strobe;
	non-removable;
	keep-power-in-suspend;
	status = "okay";
};

&sdio0 {
	bus-width = <4>;
	clock-frequency = <50000000>;
	cap-sdio-irq;
	cap-sd-highspeed;
	keep-power-in-suspend;
	mmc-pwrseq = <&sdio_pwrseq>;
	non-removable;
	pinctrl-names = "default";
	pinctrl-0 = <&sdio0_bus4 &sdio0_cmd &sdio0_clk>;
	sd-uhs-sdr104;
	#address-cells = <1>;
	#size-cells = <0>;
	status = "okay";

	brcmf: wifi@1 {
		compatible = "brcm,bcm4329-fmac";
		reg = <1>;
		interrupt-parent = <&gpio0>;
		interrupts = <RK_PA3 GPIO_ACTIVE_HIGH>;
		interrupt-names = "host-wake";
		pinctrl-names = "default";
		pinctrl-0 = <&wifi_host_wake_l>;
	};
};

&spdif {
	status = "okay";
	pinctrl-0 = <&spdif_bus_1>;
};

&spi1 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		#address-cells = <1>;
		#size-cells = <1>;
		reg = <0>;
		spi-max-frequency = <10000000>;
	};
};

&tcphy0 {
	status = "okay";
};

&tcphy1 {
	status = "okay";
};

&tsadc {
	/* tshut mode 0:CRU 1:GPIO */
	rockchip,hw-tshut-mode = <1>;
	/* tshut polarity 0:LOW 1:HIGH */
	rockchip,hw-tshut-polarity = <1>;
	rockchip,hw-tshut-temp = <110000>;
	status = "okay";
};

&u2phy0 {
	status = "okay";

	u2phy0_host: host-port {
		phy-supply = <&vcc5v0_typec>;
		status = "okay";
	};

	u2phy0_otg: otg-port {
		status = "okay";
	};
};

&u2phy1 {
	status = "okay";

	u2phy1_host: host-port {
		phy-supply = <&vcc5v0_host>;
		status = "okay";
	};

	u2phy1_otg: otg-port {
		status = "okay";
	};
};

&uart0 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart0_xfer &uart0_rts &uart0_cts>;
	status = "okay";

	bluetooth {
		compatible = "brcm,bcm43438-bt";
		clocks = <&rk808 1>;
		clock-names = "ext_clock";
		device-wakeup-gpios = <&gpio2 RK_PD2 GPIO_ACTIVE_HIGH>;
		host-wakeup-gpios = <&gpio0 RK_PA4 GPIO_ACTIVE_HIGH>;
		shutdown-gpios = <&gpio0 RK_PB1 GPIO_ACTIVE_HIGH>;
		max-speed = <4000000>;
		pinctrl-names = "default";
		pinctrl-0 = <&bt_reg_on_h &bt_host_wake_l &bt_wake_l>;
		vbat-supply = <&vcc3v3_sys>;
		vddio-supply = <&vcc_1v8>;
	};
};

&uart2 {
	status = "okay";
};

&usb_host0_ehci {
	status = "okay";
};

&usb_host0_ohci {
	status = "okay";
};

&usb_host1_ehci {
	status = "okay";
};

&usb_host1_ohci {
	status = "okay";
};

&usbdrd3_0 {
	status = "okay";
};

&usbdrd_dwc3_0 {
	status = "okay";
	dr_mode = "host";
};

&usbdrd3_1 {
	status = "okay";
};

&usbdrd_dwc3_1 {
	status = "okay";
	dr_mode = "host";
};

&vopb {
	status = "okay";
};

&vopb_mmu {
	status = "okay";
};
