// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Copyright (c) 2017 Fuzhou Rockchip Electronics Co., Ltd
 */

/dts-v1/;
#include <dt-bindings/display/drm_mipi_dsi.h>
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/pinctrl/rockchip.h>
#include <dt-bindings/sensor-dev.h>
#include "rk3326.dtsi"
#include "rk3326-863-cif-sensor.dtsi"
#include "px30-android.dtsi"

/ {
	adc-keys {
		compatible = "adc-keys";
		io-channels = <&saradc 2>;
		io-channel-names = "buttons";
		poll-interval = <100>;
		keyup-threshold-microvolt = <1800000>;

		vol-down-key {
			linux,code = <KEY_VOLUMEDOWN>;
			label = "volume down";
			press-threshold-microvolt = <300000>;
		};

		vol-up-key {
			linux,code = <KEY_VOLUMEUP>;
			label = "volume up";
			press-threshold-microvolt = <17000>;
		};
	};

	backlight: backlight {
		compatible = "pwm-backlight";
		pwms = <&pwm1 0 25000 0>;
		brightness-levels = <
			 0   10  10  11  11  12  12  13
			 13  14  14  15  15  16  16  17
			 17  18  18  19  20  21  22  23
			 24  25  26  27  28  29  30  31
			 32  33  34  35  36  37  38  39
			 40  41  42  43  44  45  46  47
			 48  49  50  51  52  53  54  55
			 56  57  58  59  60  61  62  63
			 64  65  66  67  68  69  70  71
			 72  73  74  75  76  77  78  79
			 80  81  82  83  84  85  86  87
			 88  89  90  91  92  93  94  95
			 96  97  98  99 100 101 102 103
			104 105 106 107 108 109 110 111
			112 113 114 115 116 117 118 119
			120 121 122 123 124 125 126 127
			128 129 130 131 132 133 134 135
			136 137 138 139 140 141 142 143
			144 145 146 147 148 149 150 151
			152 153 154 155 156 157 158 159
			160 161 162 163 164 165 166 167
			168 169 170 171 172 173 174 175
			176 177 178 179 180 181 182 183
			184 185 186 187 188 189 190 191
			192 193 194 195 196 197 198 199
			200 201 202 203 204 205 206 207
			208 209 210 211 212 213 214 215
			216 217 218 219 220 221 222 223
			224 225 226 227 228 229 230 231
			232 233 234 235 236 237 238 239
			240 241 242 243 244 245 246 247
			248 249 250 251 252 253 254 255>;
		default-brightness-level = <200>;
	};

	charge-animation {
		compatible = "rockchip,uboot-charge";
		rockchip,uboot-charge-on = <1>;
		rockchip,android-charge-on = <0>;
		rockchip,uboot-low-power-voltage = <3500>;
		rockchip,screen-on-voltage = <3600>;
		status = "okay";
	};

	rk817-sound {
		compatible = "rockchip,multicodecs-card";
		rockchip,card-name = "rockchip-rk817";
		hp-det-gpio = <&gpio2 RK_PC6 GPIO_ACTIVE_LOW>;
		rockchip,format = "i2s";
		rockchip,mclk-fs = <256>;
		rockchip,cpu = <&i2s1_2ch>;
		rockchip,codec = <&rk817_codec>;
		pinctrl-names = "default";
		pinctrl-0 = <&hp_det>;
	};

	sdio_pwrseq: sdio-pwrseq {
		compatible = "mmc-pwrseq-simple";
		clocks = <&cru SCLK_WIFI_PMU>;
		clock-names = "clk_wifi_pmu";
		pinctrl-names = "default";
		pinctrl-0 = <&wifi_enable_h>;

		/*
		 * On the module itself this is one of these (depending
		 * on the actual card populated):
		 * - SDIO_RESET_L_WL_REG_ON
		 * - PDN (power down when low)
		 */
		reset-gpios = <&gpio0 RK_PA2 GPIO_ACTIVE_LOW>; /* GPIO3_A4 */
	};

	vccsys: vccsys {
		compatible = "regulator-fixed";
		regulator-name = "vcc3v8_sys";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <3800000>;
		regulator-max-microvolt = <3800000>;
	};

	wireless-wlan {
		compatible = "wlan-platdata";
		wifi_chip_type = "rtl8723cs";
		WIFI,host_wake_irq = <&gpio0 RK_PB2 GPIO_ACTIVE_HIGH>;
		WIFI,vbat_gpio = <&gpio3 RK_PB6 GPIO_ACTIVE_LOW>;
		status = "okay";
	};

	wireless-bluetooth {
		compatible = "bluetooth-platdata";
		uart_rts_gpios = <&gpio1 RK_PC3 GPIO_ACTIVE_LOW>;
		pinctrl-names = "default","rts_gpio";
		pinctrl-0 = <&uart1_rts>;
		pinctrl-1 = <&uart1_rts_gpio>;
		BT,reset_gpio = <&gpio0 RK_PC1 GPIO_ACTIVE_HIGH>;
		BT,wake_gpio = <&gpio0 RK_PA1 GPIO_ACTIVE_HIGH>;
		BT,wake_host_irq = <&gpio0 RK_PB3 GPIO_ACTIVE_HIGH>;
		status = "okay";
	};
};


&display_subsystem {
	status = "okay";
};

&dsi {
	status = "okay";

	panel@0 {
		compatible = "aoly,sl008pa21y1285-b00", "simple-panel-dsi";
		reg = <0>;
		backlight = <&backlight>;
		enable-gpios = <&gpio0 RK_PB7 GPIO_ACTIVE_LOW>;
		reset-gpios = <&gpio3 RK_PB7 GPIO_ACTIVE_LOW>;
		prepare-delay-ms = <20>;
		reset-delay-ms = <20>;
		init-delay-ms = <20>;
		enable-delay-ms = <120>;
		disable-delay-ms = <20>;
		unprepare-delay-ms = <20>;

		width-mm = <108>;
		height-mm = <172>;

		dsi,flags = <(MIPI_DSI_MODE_VIDEO | MIPI_DSI_MODE_VIDEO_BURST |
			      MIPI_DSI_MODE_LPM | MIPI_DSI_MODE_EOT_PACKET)>;
		dsi,format = <MIPI_DSI_FMT_RGB888>;
		dsi,lanes = <4>;

		panel-init-sequence = [
			05 78 01 11
			05 14 01 29
		];

		panel-exit-sequence = [
			05 00 01 28
			05 00 01 10
		];

		display-timings {
			native-mode = <&timing0>;

			timing0: timing0 {
				clock-frequency = <66000000>;
				hactive = <800>;
				vactive = <1280>;
				hfront-porch = <2>;
				hsync-len = <18>;
				hback-porch = <18>;
				vfront-porch = <4>;
				vsync-len = <4>;
				vback-porch = <16>;
				hsync-active = <0>;
				vsync-active = <0>;
				de-active = <0>;
				pixelclk-active = <0>;
			};
		};

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				panel_in_dsi: endpoint {
					remote-endpoint = <&dsi_out_panel>;
				};
			};
		};
	};

	ports {
		#address-cells = <1>;
		#size-cells = <0>;

		port@1 {
			reg = <1>;
			dsi_out_panel: endpoint {
				remote-endpoint = <&panel_in_dsi>;
			};
		};
	};
};

&dsi_in_vopb {
	status = "okay";
};

&route_dsi {
	connect = <&vopb_out_dsi>;
	status = "okay";
};

&bus_apll {
	bus-supply = <&vdd_logic>;
	status = "okay";
};

&cpu0 {
	cpu-supply = <&vdd_arm>;
};

&cpu0_opp_table {
	/*
	 * max IR-drop values on different freq condition for this board!
	 */
	rockchip,board-irdrop = <
		/*MHz	MHz	uV */
		0	815	37500
		816	1119	50000
		1200	1512	75000
	>;
};

&dmc_opp_table {
	/*
	 * max IR-drop values on different freq condition for this board!
	 */
	rockchip,board-irdrop = <
		/*MHz	MHz	uV */
		451	800	75000
	>;
};

&dfi {
	status = "okay";
};

&dmc {
	center-supply = <&vdd_logic>;
	status = "okay";
};

&emmc {
	bus-width = <8>;
	cap-mmc-highspeed;
	mmc-hs200-1_8v;
	no-sdio;
	no-sd;
	disable-wp;
	non-removable;
	num-slots = <1>;
	status = "okay";
};

&gpu {
	mali-supply = <&vdd_logic>;
	status = "okay";
};

&i2c0 {
	status = "okay";

	rk817: pmic@20 {
		compatible = "rockchip,rk817";
		reg = <0x20>;
		interrupt-parent = <&gpio0>;
		interrupts = <7 IRQ_TYPE_LEVEL_LOW>;
		pinctrl-names = "default", "pmic-sleep",
				"pmic-power-off", "pmic-reset";
		pinctrl-0 = <&pmic_int>;
		pinctrl-1 = <&soc_slppin_slp>, <&rk817_slppin_slp>;
		pinctrl-2 = <&soc_slppin_gpio>, <&rk817_slppin_pwrdn>;
		pinctrl-3 = <&soc_slppin_rst>, <&rk817_slppin_rst>;
		rockchip,system-power-controller;
		wakeup-source;
		#clock-cells = <1>;
		clock-output-names = "rk808-clkout1", "rk808-clkout2";
		//fb-inner-reg-idxs = <2>;
		/* 1: rst regs (default in codes), 0: rst the pmic */
		pmic-reset-func = <1>;

		vcc1-supply = <&vccsys>;
		vcc2-supply = <&vccsys>;
		vcc3-supply = <&vccsys>;
		vcc4-supply = <&vccsys>;
		vcc5-supply = <&vccsys>;
		vcc6-supply = <&vccsys>;
		vcc7-supply = <&vcc_3v0>;
		vcc8-supply = <&vccsys>;
		vcc9-supply = <&dcdc_boost>;

		pwrkey {
			status = "okay";
		};

		pinctrl_rk8xx: pinctrl_rk8xx {
			gpio-controller;
			#gpio-cells = <2>;

			rk817_ts_gpio1: rk817_ts_gpio1 {
				pins = "gpio_ts";
				function = "pin_fun1";
				/* output-low; */
				/* input-enable; */
			};

			rk817_gt_gpio2: rk817_gt_gpio2 {
				pins = "gpio_gt";
				function = "pin_fun1";
			};

			rk817_pin_ts: rk817_pin_ts {
				pins = "gpio_ts";
				function = "pin_fun0";
			};

			rk817_pin_gt: rk817_pin_gt {
				pins = "gpio_gt";
				function = "pin_fun0";
			};

			rk817_slppin_null: rk817_slppin_null {
				pins = "gpio_slp";
				function = "pin_fun0";
			};

			rk817_slppin_slp: rk817_slppin_slp {
				pins = "gpio_slp";
				function = "pin_fun1";
			};

			rk817_slppin_pwrdn: rk817_slppin_pwrdn {
				pins = "gpio_slp";
				function = "pin_fun2";
			};

			rk817_slppin_rst: rk817_slppin_rst {
				pins = "gpio_slp";
				function = "pin_fun3";
			};
		};

		regulators {
			vdd_logic: DCDC_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <850000>;
				regulator-max-microvolt = <1350000>;
				regulator-ramp-delay = <6001>;
				regulator-initial-mode = <0x2>;
				regulator-name = "vdd_logic";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <950000>;
				};
			};

			vdd_arm: DCDC_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <850000>;
				regulator-max-microvolt = <1350000>;
				regulator-ramp-delay = <6001>;
				regulator-initial-mode = <0x2>;
				regulator-name = "vdd_arm";
				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <950000>;
				};
			};

			vcc_ddr: DCDC_REG3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-initial-mode = <0x2>;
				regulator-name = "vcc_ddr";
				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};

			vcc_3v0: DCDC_REG4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3000000>;
				regulator-max-microvolt = <3000000>;
				regulator-initial-mode = <0x2>;
				regulator-name = "vcc_3v0";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3000000>;
				};
			};

			vcc_1v0: LDO_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <1000000>;
				regulator-name = "vcc_1v0";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1000000>;
				};
			};

			vcc1v8_soc: LDO_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;

				regulator-name = "vcc1v8_soc";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vdd1v0_soc: LDO_REG3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <1000000>;

				regulator-name = "vcc1v0_soc";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1000000>;
				};
			};

			vcc3v0_pmu: LDO_REG4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3000000>;
				regulator-max-microvolt = <3000000>;

				regulator-name = "vcc3v0_pmu";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3000000>;

				};
			};

			vccio_sd: LDO_REG5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;

				regulator-name = "vccio_sd";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vcc_sd: LDO_REG6 {
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;

				regulator-name = "vcc_sd";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;

				};
			};

			vcc2v8_dvp: LDO_REG7 {
				regulator-boot-on;
				regulator-min-microvolt = <2800000>;
				regulator-max-microvolt = <2800000>;

				regulator-name = "vcc2v8_dvp";
				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <2800000>;
				};
			};

			vcc1v8_dvp: LDO_REG8 {
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;

				regulator-name = "vcc1v8_dvp";
				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vdd1v5_dvp: LDO_REG9 {
				regulator-boot-on;
				regulator-min-microvolt = <1500000>;
				regulator-max-microvolt = <1500000>;

				regulator-name = "vdd1v5_dvp";
				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <1500000>;
				};
			};

			dcdc_boost: BOOST {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <4700000>;
				regulator-max-microvolt = <5400000>;
				regulator-name = "boost";
			};

			otg_switch: OTG_SWITCH {
				regulator-name = "otg_switch";
			};
		};

		battery {
			compatible = "rk817,battery";
			ocv_table = <3500 3548 3592 3636 3687 3740 3780
				3806 3827 3846 3864 3889 3929 3964
				3993 4015 4030 4041 4056 4076 4148>;
			design_capacity = <4000>;
			design_qmax = <4200>;
			bat_res = <100>;
			sleep_enter_current = <150>;
			sleep_exit_current = <180>;
			sleep_filter_current = <100>;
			power_off_thresd = <3500>;
			zero_algorithm_vol = <3850>;
			max_soc_offset = <60>;
			monitor_sec = <5>;
			sample_res = <10>;
			virtual_power = <0>;
		};

		charger {
			compatible = "rk817,charger";
			min_input_voltage = <4500>;
			max_input_current = <1500>;
			max_chrg_current = <2000>;
			max_chrg_voltage = <4200>;
			chrg_term_mode = <0>;
			chrg_finish_cur = <300>;
			virtual_power = <0>;
			dc_det_adc = <0>;
			extcon = <&u2phy>;
		};

		rk817_codec: codec {
			#sound-dai-cells = <0>;
			compatible = "rockchip,rk817-codec";
			clocks = <&cru SCLK_I2S1_OUT>;
			clock-names = "mclk";
			pinctrl-names = "default";
			pinctrl-0 = <&i2s1_2ch_mclk>;
			hp-volume = <20>;
			spk-volume = <3>;
			mic-in-differential;
			status = "okay";
		};
	};
};

&i2c1 {
	status = "okay";

	ts@40 {
		status = "okay";
		compatible = "GSL,GSL3673_800X1280";
		reg = <0x40>;
		irq_gpio_number = <&gpio0 RK_PA5 IRQ_TYPE_LEVEL_LOW>;
		rst_gpio_number = <&gpio0 RK_PB4 GPIO_ACTIVE_HIGH>;
	};

	sensor@19 {
		status = "okay";
		compatible = "gs_lis3dh";
		reg = <0x19>;
		type = <SENSOR_TYPE_ACCEL>;
		irq-gpio = <&gpio0 RK_PB5 IRQ_TYPE_LEVEL_LOW>;
		irq_enable = <0>;
		poll_delay_ms = <30>;
		layout = <7>;
		reprobe_en = <1>;
	};
};

&i2c2 {
	status = "okay";
};

&i2s1_2ch {
	status = "okay";
	#sound-dai-cells = <0>;
};

&io_domains {
	status = "okay";

	vccio1-supply = <&vcc_3v0>;
	vccio2-supply = <&vccio_sd>;
	vccio3-supply = <&vcc2v8_dvp>;
	vccio4-supply = <&vcc_3v0>;
	vccio5-supply = <&vcc_3v0>;
};

&nandc0 {
	status = "okay";
};

&pinctrl {
	headphone {
		hp_det: hp-det {
			rockchip,pins = <2 RK_PC6 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	pmic {
		pmic_int: pmic_int {
			rockchip,pins =
				<0 RK_PA7 RK_FUNC_GPIO &pcfg_pull_up>;
		};

		soc_slppin_gpio: soc_slppin_gpio {
			rockchip,pins =
				<0 RK_PA4 RK_FUNC_GPIO &pcfg_output_low>;
		};

		soc_slppin_slp: soc_slppin_slp {
			rockchip,pins =
				<0 RK_PA4 1 &pcfg_pull_none>;
		};

		soc_slppin_rst: soc_slppin_rst {
			rockchip,pins =
				<0 RK_PA4 2 &pcfg_pull_none>;
		};
	};

	sdio-pwrseq {
		wifi_enable_h: wifi-enable-h {
			rockchip,pins = <0 RK_PA2 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};
};

&pmu_io_domains {
	status = "okay";

	pmuio1-supply = <&vcc3v0_pmu>;
	pmuio2-supply = <&vcc3v0_pmu>;
};

&pwm1 {
	status = "okay";
};

&rk_rga {
	status = "okay";
};

&rockchip_suspend {
	status = "okay";
	rockchip,sleep-debug-en = <1>;
};

&saradc {
	status = "okay";
	vref-supply = <&vcc1v8_soc>;
};

&sdmmc {
	bus-width = <4>;
	cap-mmc-highspeed;
	cap-sd-highspeed;
	no-sdio;
	no-mmc;
	card-detect-delay = <800>;
	ignore-pm-notify;
	sd-uhs-sdr12;
	sd-uhs-sdr25;
	sd-uhs-sdr50;
	sd-uhs-sdr104;
	vqmmc-supply = <&vccio_sd>;
	vmmc-supply = <&vcc_sd>;
	status = "disabled";
};

&sdio {
	bus-width = <4>;
	cap-sd-highspeed;
	no-sd;
	no-mmc;
	ignore-pm-notify;
	keep-power-in-suspend;
	non-removable;
	mmc-pwrseq = <&sdio_pwrseq>;
	sd-uhs-sdr104;
	status = "okay";
};

&tsadc {
	pinctrl-names = "gpio", "otpout";
	pinctrl-0 = <&tsadc_otp_gpio>;
	pinctrl-1 = <&tsadc_otp_out>;
	status = "okay";
};

&u2phy {
	status = "okay";

	u2phy_host: host-port {
		rockchip,low-power-mode;
		status = "okay";
	};

	u2phy_otg: otg-port {
		rockchip,low-power-mode;
		status = "okay";
	};
};

&usb20_otg {
	status = "okay";
};

&uart1 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart1_xfer &uart1_cts>;
	status = "okay";
};

&vip_mmu {
	status = "okay";
};

&vopb {
	status = "okay";
};

&vopb_mmu {
	status = "okay";
};

&mpp_srv {
	status = "okay";
};

&vdpu {
	status = "okay";
};

&vepu {
	status = "okay";
};

&vpu_mmu {
	status = "okay";
};

&hevc {
	status = "okay";
};

&hevc_mmu {
	status = "okay";
};
