// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Copyright (c) 2022 Rockchip Electronics Co., Ltd
 *
 */

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/pinctrl/rockchip.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/display/drm_mipi_dsi.h>
#include "rk3358.dtsi"

/ {
	adc-keys {
		compatible = "adc-keys";
		io-channels = <&saradc 2>;
		io-channel-names = "buttons";
		poll-interval = <100>;
		keyup-threshold-microvolt = <1800000>;

		vol-down-key {
			linux,code = <KEY_VOLUMEDOWN>;
			label = "volume down";
			press-threshold-microvolt = <300000>;
		};

		vol-up-key {
			linux,code = <KEY_VOLUMEUP>;
			label = "volume up";
			press-threshold-microvolt = <17000>;
		};
	};

	backlight: backlight {
		compatible = "pwm-backlight";
		pwms = <&pwm1 0 25000 0>;
		brightness-levels = <
			  0   1   2   3   4   5   6   7
			  8   9  10  11  12  13  14  15
			 16  17  18  19  20  21  22  23
			 24  25  26  27  28  29  30  31
			 32  33  34  35  36  37  38  39
			 40  41  42  43  44  45  46  47
			 48  49  50  51  52  53  54  55
			 56  57  58  59  60  61  62  63
			 64  65  66  67  68  69  70  71
			 72  73  74  75  76  77  78  79
			 80  81  82  83  84  85  86  87
			 88  89  90  91  92  93  94  95
			 96  97  98  99 100 101 102 103
			104 105 106 107 108 109 110 111
			112 113 114 115 116 117 118 119
			120 121 122 123 124 125 126 127
			128 129 130 131 132 133 134 135
			136 137 138 139 140 141 142 143
			144 145 146 147 148 149 150 151
			152 153 154 155 156 157 158 159
			160 161 162 163 164 165 166 167
			168 169 170 171 172 173 174 175
			176 177 178 179 180 181 182 183
			184 185 186 187 188 189 190 191
			192 193 194 195 196 197 198 199
			200 201 202 203 204 205 206 207
			208 209 210 211 212 213 214 215
			216 217 218 219 220 221 222 223
			224 225 226 227 228 229 230 231
			232 233 234 235 236 237 238 239
			240 241 242 243 244 245 246 247
			248 249 250 251 252 253 254 255>;
		default-brightness-level = <200>;
	};

	backlight_2: backlight-2 {
		compatible = "pwm-backlight";
		pwms = <&pwm3 0 10000000 0>;
		pinctrl-names = "default";
		pinctrl-0 = <&lcd0_pwren &lcd0_rst>;
		enable-gpios = <&gpio1 RK_PD6 GPIO_ACTIVE_HIGH>;
		brightness-levels = <
			  0   1   2   3   4   5   6   7
			  8   9  10  11  12  13  14  15
			 16  17  18  19  20  21  22  23
			 24  25  26  27  28  29  30  31
			 32  33  34  35  36  37  38  39
			 40  41  42  43  44  45  46  47
			 48  49  50  51  52  53  54  55
			 56  57  58  59  60  61  62  63
			 64  65  66  67  68  69  70  71
			 72  73  74  75  76  77  78  79
			 80  81  82  83  84  85  86  87
			 88  89  90  91  92  93  94  95
			 96  97  98  99 100 101 102 103
			104 105 106 107 108 109 110 111
			112 113 114 115 116 117 118 119
			120 121 122 123 124 125 126 127
			128 129 130 131 132 133 134 135
			136 137 138 139 140 141 142 143
			144 145 146 147 148 149 150 151
			152 153 154 155 156 157 158 159
			160 161 162 163 164 165 166 167
			168 169 170 171 172 173 174 175
			176 177 178 179 180 181 182 183
			184 185 186 187 188 189 190 191
			192 193 194 195 196 197 198 199
			200 201 202 203 204 205 206 207
			208 209 210 211 212 213 214 215
			216 217 218 219 220 221 222 223
			224 225 226 227 228 229 230 231
			232 233 234 235 236 237 238 239
			240 241 242 243 244 245 246 247
			248 249 250 251 252 253 254 255>;
		default-brightness-level = <60>;
	};

	/* The THine 827-Q (rgb to dual lvds) don't need driver */
	panel-rgb {
		compatible = "simple-panel";
		#address-cells = <1>;
		#size-cells = <0>;

		pinctrl-names = "default";
		pinctrl-0 = <&pwdn_rgb>; /* This the pwdn of THine-827-Q */
		power-supply = <&vcc3v3_lcd>;
		backlight = <&backlight_2>;
		enable-gpios = <&gpio1 RK_PD4 GPIO_ACTIVE_HIGH>;
		reset-gpios = <&gpio1 RK_PD7 GPIO_ACTIVE_LOW>;
		prepare-delay-ms = <0>;
		reset-delay-ms = <0>;
		init-delay-ms = <0>;
		enable-delay-ms = <5>;
		disable-delay-ms = <10>;
		unprepare-delay-ms = <0>;

		width-mm = <292>;
		height-mm = <109>;

		bus-format = <MEDIA_BUS_FMT_RGB888_1X24>;

		display-timings {
			native-mode = <&timing1>;

			timing1: timing1 {
				clock-frequency = <88200000>;
				hactive = <1920>;
				vactive = <720>;
				hfront-porch = <40>;
				hsync-len = <20>;
				hback-porch = <24>;
				vfront-porch = <5>;
				vsync-len = <4>;
				vback-porch = <4>;
				hsync-active = <0>;
				vsync-active = <0>;
				de-active = <0>;
				pixelclk-active = <0>;
			};
		};

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				panel_in_rgb: endpoint {
					remote-endpoint = <&rgb_out_panel>;
				};
			};
		};
	};


	rk809-sound {
		compatible = "simple-audio-card";
		simple-audio-card,format = "i2s";
		simple-audio-card,name = "rockchip,rk809-codec";
		simple-audio-card,mclk-fs = <256>;
		simple-audio-card,widgets =
			"Microphone", "Mic Jack",
			"Headphone", "Headphone Jack";
		simple-audio-card,routing =
			"Mic Jack", "MICBIAS1",
			"IN1P", "Mic Jack",
			"Headphone Jack", "HPOL",
			"Headphone Jack", "HPOR";
		simple-audio-card,cpu {
			sound-dai = <&i2s1_2ch>;
		};
		simple-audio-card,codec {
			sound-dai = <&rk809_codec>;
		};
	};

	sdio_pwrseq: sdio-pwrseq {
		compatible = "mmc-pwrseq-simple";
		pinctrl-names = "default";
		pinctrl-0 = <&wifi_enable_h>;

		/*
		 * On the module itself this is one of these (depending
		 * on the actual card populated):
		 * - SDIO_RESET_L_WL_REG_ON
		 * - PDN (power down when low)
		 */
		reset-gpios = <&gpio0 RK_PA3 GPIO_ACTIVE_LOW>;
	};

	vcc5v0_sys: vccsys {
		compatible = "regulator-fixed";
		regulator-name = "vcc5v0_sys";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
	};

	wireless-wlan {
		compatible = "wlan-platdata";
		wifi_chip_type = "AP6212";
		WIFI,host_wake_irq = <&gpio0 RK_PB2 GPIO_ACTIVE_HIGH>;
		status = "okay";
	};

	wireless-bluetooth {
		compatible = "bluetooth-platdata";
		clocks = <&rk809 1>;
		clock-names = "ext_clock";
		uart_rts_gpios = <&gpio1 RK_PC3 GPIO_ACTIVE_LOW>;
		pinctrl-names = "default","rts_gpio";
		pinctrl-0 = <&uart1_rts>;
		pinctrl-1 = <&uart1_rts_gpio>;
		BT,reset_gpio = <&gpio0 RK_PA2 GPIO_ACTIVE_HIGH>;
		BT,wake_gpio = <&gpio0 RK_PA1 GPIO_ACTIVE_HIGH>;
		BT,wake_host_irq = <&gpio0 RK_PB3 GPIO_ACTIVE_HIGH>;
		status = "okay";
	};
};

&display_subsystem {
	status = "okay";
};

&dsi {
	status = "disabled";

	panel@0 {
		compatible = "sitronix,st7703", "simple-panel-dsi";
		reg = <0>;

		pinctrl-names = "default";
		pinctrl-0 = <&mipi_en>;
		enable-gpios = <&gpio1 RK_PB4 GPIO_ACTIVE_HIGH>;

		backlight = <&backlight>;
		prepare-delay-ms = <0>;
		reset-delay-ms = <0>;
		init-delay-ms = <80>;
		enable-delay-ms = <0>;
		disable-delay-ms = <10>;
		unprepare-delay-ms = <60>;

		width-mm = <68>;
		height-mm = <121>;

		dsi,flags = <(MIPI_DSI_MODE_VIDEO | MIPI_DSI_MODE_VIDEO_BURST |
			      MIPI_DSI_MODE_LPM | MIPI_DSI_MODE_EOT_PACKET)>;
		dsi,format = <MIPI_DSI_FMT_RGB888>;
		dsi,lanes = <4>;

		panel-init-sequence = [
			39 00 04 ff 98 81 03
			15 00 02 01 00
			15 00 02 02 00
			15 00 02 03 53
			15 00 02 04 53
			15 00 02 05 13
			15 00 02 06 04
			15 00 02 07 02
			15 00 02 08 02
			15 00 02 09 00
			15 00 02 0a 00
			15 00 02 0b 00
			15 00 02 0c 00
			15 00 02 0d 00
			15 00 02 0e 00
			15 00 02 0f 00

			15 00 02 10 00
			15 00 02 11 00
			15 00 02 12 00
			15 00 02 13 00
			15 00 02 14 00
			15 00 02 15 08
			15 00 02 16 10
			15 00 02 17 00
			15 00 02 18 08
			15 00 02 19 00
			15 00 02 1a 00
			15 00 02 1b 00
			15 00 02 1c 00
			15 00 02 1d 00
			15 00 02 1e c0
			15 00 02 1f 80

			15 00 02 20 02
			15 00 02 21 09
			15 00 02 22 00
			15 00 02 23 00
			15 00 02 24 00
			15 00 02 25 00
			15 00 02 26 00
			15 00 02 27 00
			15 00 02 28 55
			15 00 02 29 03
			15 00 02 2a 00
			15 00 02 2b 00
			15 00 02 2c 00
			15 00 02 2d 00
			15 00 02 2e 00
			15 00 02 2f 00

			15 00 02 30 00
			15 00 02 31 00
			15 00 02 32 00
			15 00 02 33 00
			15 00 02 34 04
			15 00 02 35 05
			15 00 02 36 05
			15 00 02 37 00
			15 00 02 38 3c
			15 00 02 39 35
			15 00 02 3a 00
			15 00 02 3b 40
			15 00 02 3c 00
			15 00 02 3d 00
			15 00 02 3e 00
			15 00 02 3f 00

			15 00 02 40 00
			15 00 02 41 88
			15 00 02 42 00
			15 00 02 43 00
			15 00 02 44 1f

			15 00 02 50 01
			15 00 02 51 23
			15 00 02 52 45
			15 00 02 53 67
			15 00 02 54 89
			15 00 02 55 ab
			15 00 02 56 01
			15 00 02 57 23
			15 00 02 58 45
			15 00 02 59 67
			15 00 02 5a 89
			15 00 02 5b ab
			15 00 02 5c cd
			15 00 02 5d ef
			15 00 02 5e 03
			15 00 02 5f 14

			15 00 02 60 15
			15 00 02 61 0c
			15 00 02 62 0d
			15 00 02 63 0e
			15 00 02 64 0f
			15 00 02 65 10
			15 00 02 66 11
			15 00 02 67 08
			15 00 02 68 02
			15 00 02 69 0a
			15 00 02 6a 02
			15 00 02 6b 02
			15 00 02 6c 02
			15 00 02 6d 02
			15 00 02 6e 02
			15 00 02 6f 02

			15 00 02 70 02
			15 00 02 71 02
			15 00 02 72 06
			15 00 02 73 02
			15 00 02 74 02
			15 00 02 75 14
			15 00 02 76 15
			15 00 02 77 0f
			15 00 02 78 0e
			15 00 02 79 0d
			15 00 02 7a 0c
			15 00 02 7b 11
			15 00 02 7c 10
			15 00 02 7d 06
			15 00 02 7e 02
			15 00 02 7f 0a

			15 00 02 80 02
			15 00 02 81 02
			15 00 02 82 02
			15 00 02 83 02
			15 00 02 84 02
			15 00 02 85 02
			15 00 02 86 02
			15 00 02 87 02
			15 00 02 88 08
			15 00 02 89 02
			15 00 02 8a 02

			39 00 04 ff 98 81 04
			15 00 02 00 80
			15 00 02 70 00
			15 00 02 71 00
			15 00 02 66 fe
			15 00 02 82 15
			15 00 02 84 15
			15 00 02 85 15
			15 00 02 3a 24
			15 00 02 32 ac
			15 00 02 8c 80
			15 00 02 3c f5
			15 00 02 88 33

			39 00 04 ff 98 81 01
			15 00 02 22 0a
			15 00 02 31 00
			15 00 02 53 78
			15 00 02 50 5b
			15 00 02 51 5b
			15 00 02 60 20
			15 00 02 61 00
			15 00 02 62 0d
			15 00 02 63 00

			15 00 02 a0 00
			15 00 02 a1 10
			15 00 02 a2 1c
			15 00 02 a3 13
			15 00 02 a4 15
			15 00 02 a5 26
			15 00 02 a6 1a
			15 00 02 a7 1d
			15 00 02 a8 67
			15 00 02 a9 1c
			15 00 02 aa 29
			15 00 02 ab 5b
			15 00 02 ac 26
			15 00 02 ad 28
			15 00 02 ae 5c
			15 00 02 af 30
			15 00 02 b0 31
			15 00 02 b1 2e
			15 00 02 b2 32
			15 00 02 b3 00

			15 00 02 c0 00
			15 00 02 c1 10
			15 00 02 c2 1c
			15 00 02 c3 13
			15 00 02 c4 15
			15 00 02 c5 26
			15 00 02 c6 1a
			15 00 02 c7 1d
			15 00 02 c8 67
			15 00 02 c9 1c
			15 00 02 ca 29
			15 00 02 cb 5b
			15 00 02 cc 26
			15 00 02 cd 28
			15 00 02 ce 5c
			15 00 02 cf 30
			15 00 02 d0 31
			15 00 02 d1 2e
			15 00 02 d2 32
			15 00 02 d3 00
			39 00 04 ff 98 81 00
			05 00 01 11
			05 01 01 29
		];

		panel-exit-sequence = [
			05 00 01 28
			05 00 01 10
		];

		display-timings {
			native-mode = <&timing0>;

			timing0: timing0 {
				clock-frequency = <64000000>;
				hactive = <720>;
				vactive = <1280>;
				hfront-porch = <40>;
				hsync-len = <10>;
				hback-porch = <40>;
				vfront-porch = <22>;
				vsync-len = <4>;
				vback-porch = <11>;
				hsync-active = <0>;
				vsync-active = <0>;
				de-active = <0>;
				pixelclk-active = <0>;
			};
		};

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				panel_in_dsi: endpoint {
					remote-endpoint = <&dsi_out_panel>;
				};
			};
		};
	};

	ports {
		#address-cells = <1>;
		#size-cells = <0>;

		port@1 {
			reg = <1>;
			dsi_out_panel: endpoint {
				remote-endpoint = <&panel_in_dsi>;
			};
		};
	};
};

&dsi_in_vopb {
	status = "disabled";
};

&dsi_in_vopl {
	status = "disabled";
};

&route_dsi {
	connect = <&vopb_out_dsi>;
	status = "disabled";
};

&rgb {
	status = "okay";
	#address-cells = <1>;
	#size-cells = <0>;

	/delete-property/ phys;
	/delete-property/ phy-names;

	pinctrl-0 = <&lcdc_m0_rgb_pins>;
	pinctrl-1 = <&lcdc_m0_sleep_pins>;

	ports {
		port@1 {
			reg = <1>;

			rgb_out_panel: endpoint {
				remote-endpoint = <&panel_in_rgb>;
			};
		};
	};
};

&rgb_in_vopb {
	status = "okay";
};

&rgb_in_vopl {
	status = "disabled";
};

&route_rgb {
	connect = <&vopb_out_rgb>;
	status = "okay";
};

&cpu0 {
	cpu-supply = <&vdd_arm>;
};

&dfi {
	status = "okay";
};

&dmc {
	center-supply = <&vdd_logic>;
	status = "okay";
};

&emmc {
	bus-width = <8>;
	cap-mmc-highspeed;
	mmc-hs200-1_8v;
	supports-emmc;
	disable-wp;
	non-removable;
	num-slots = <1>;
	status = "okay";
};

&gpu {
	mali-supply = <&vdd_logic>;
	status = "okay";
};

&i2c0 {
	status = "okay";
	clock-frequency = <400000>;

	rk809: pmic@20 {
		compatible = "rockchip,rk809";
		reg = <0x20>;
		interrupt-parent = <&gpio0>;
		interrupts = <7 IRQ_TYPE_LEVEL_LOW>;
		pinctrl-names = "default", "pmic-sleep",
				"pmic-power-off", "pmic-reset";
		pinctrl-0 = <&pmic_int>;
		pinctrl-1 = <&soc_slppin_slp>, <&rk817_slppin_slp>;
		pinctrl-2 = <&soc_slppin_gpio>, <&rk817_slppin_pwrdn>;
		pinctrl-3 = <&soc_slppin_rst>, <&rk817_slppin_rst>;
		rockchip,system-power-controller;
		wakeup-source;
		#clock-cells = <1>;
		clock-output-names = "rk808-clkout1", "rk808-clkout2";
		//fb-inner-reg-idxs = <2>;
		/* 1: rst regs (default in codes), 0: rst the pmic */
		pmic-reset-func = <1>;

		vcc1-supply = <&vcc5v0_sys>;
		vcc2-supply = <&vcc5v0_sys>;
		vcc3-supply = <&vcc5v0_sys>;
		vcc4-supply = <&vcc5v0_sys>;
		vcc5-supply = <&vcc3v3_sys>;
		vcc6-supply = <&vcc3v3_sys>;
		vcc7-supply = <&vcc3v3_sys>;
		vcc8-supply = <&vcc3v3_sys>;
		vcc9-supply = <&vcc5v0_sys>;

		pwrkey {
			status = "okay";
		};

		pinctrl_rk8xx: pinctrl_rk8xx {
			gpio-controller;
			#gpio-cells = <2>;

			rk817_slppin_null: rk817_slppin_null {
				pins = "gpio_slp";
				function = "pin_fun0";
			};

			rk817_slppin_slp: rk817_slppin_slp {
				pins = "gpio_slp";
				function = "pin_fun1";
			};

			rk817_slppin_pwrdn: rk817_slppin_pwrdn {
				pins = "gpio_slp";
				function = "pin_fun2";
			};

			rk817_slppin_rst: rk817_slppin_rst {
				pins = "gpio_slp";
				function = "pin_fun3";
			};
		};

		regulators {
			vdd_logic: DCDC_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <950000>;
				regulator-max-microvolt = <1350000>;
				regulator-ramp-delay = <6001>;
				regulator-initial-mode = <0x2>;
				regulator-name = "vdd_logic";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <950000>;
				};
			};

			vdd_arm: DCDC_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <950000>;
				regulator-max-microvolt = <1350000>;
				regulator-ramp-delay = <6001>;
				regulator-initial-mode = <0x2>;
				regulator-name = "vdd_arm";
				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <950000>;
				};
			};

			vcc_ddr: DCDC_REG3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vcc_ddr";
				regulator-initial-mode = <0x2>;
				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};

			vcc_3v3: DCDC_REG4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-initial-mode = <0x2>;
				regulator-name = "vcc_3v3";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vcc_1v0: LDO_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <1000000>;
				regulator-name = "vcc_1v0";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1000000>;
				};
			};

			vcc_1v8: LDO_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;

				regulator-name = "vcc_1v8";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vdd_1v0: LDO_REG3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <1000000>;

				regulator-name = "vdd_1v0";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1000000>;
				};
			};

			vcc3v3_pmu: LDO_REG4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;

				regulator-name = "vcc3v3_pmu";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3000000>;

				};
			};

			vccio_sd: LDO_REG5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;

				regulator-name = "vccio_sd";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vcc_sd: LDO_REG6 {
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-boot-off;

				regulator-name = "vcc_sd";
				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <3300000>;

				};
			};

			vcc2v8_dvp: LDO_REG7 {
				regulator-boot-on;
				regulator-min-microvolt = <2800000>;
				regulator-max-microvolt = <2800000>;

				regulator-name = "vcc2v8_dvp";
				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <2800000>;
				};
			};

			vcc1v8_dvp: LDO_REG8 {
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;

				regulator-name = "vcc1v8_dvp";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vdd1v5_dvp: LDO_REG9 {
				regulator-boot-on;
				regulator-min-microvolt = <1500000>;
				regulator-max-microvolt = <1500000>;

				regulator-name = "vdd1v5_dvp";
				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <1500000>;
				};
			};

			vcc3v3_sys: DCDC_REG5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vcc3v3_sys";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vcc5v0_host: SWITCH_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vcc5v0_host";
			};

			vcc3v3_lcd: SWITCH_REG2 {
				regulator-boot-on;
				regulator-name = "vcc3v3_lcd";
			};
		};

		rk809_codec: codec {
			#sound-dai-cells = <0>;
			compatible = "rockchip,rk809-codec", "rockchip,rk817-codec";
			clocks = <&cru SCLK_I2S1_OUT>;
			clock-names = "mclk";
			pinctrl-names = "default";
			pinctrl-0 = <&i2s1_2ch_mclk>;
			hp-volume = <20>;
			spk-volume = <3>;
			status = "okay";
		};
	};
};

&i2c1 {
	status = "okay";

	clock-frequency = <400000>;

	/* These are relatively safe rise/fall times; TODO: measure */
	i2c-scl-falling-time-ns = <50>;
	i2c-scl-rising-time-ns = <300>;
};

&i2s1_2ch {
	status = "okay";
	#sound-dai-cells = <0>;
};

&io_domains {
	status = "okay";

	vccio1-supply = <&vcc_3v3>;
	vccio2-supply = <&vcc_3v3>;
	vccio3-supply = <&vcc_3v3>;
	vccio4-supply = <&vcc3v3_pmu>;
	vccio5-supply = <&vcc_1v8>;
};

&isp_mmu {
	status = "okay";
};

&mipi_dphy_rx0 {
	status = "okay";

	ports {
		#address-cells = <1>;
		#size-cells = <0>;

		port@0 {
			reg = <0>;
			#address-cells = <1>;
			#size-cells = <0>;

			mipi_in_ucam: endpoint@1 {
				reg = <1>;
			//	remote-endpoint = <&ucam_out>;
				data-lanes = <1 2>;
			};
		};

		port@1 {
			reg = <1>;
			#address-cells = <1>;
			#size-cells = <0>;

			dphy_rx0_out: endpoint@0 {
				reg = <0>;
				remote-endpoint = <&isp0_mipi_in>;
			};
		};
	};
};

&pmu_io_domains {
	status = "okay";

	pmuio1-supply = <&vcc3v3_pmu>;
	pmuio2-supply = <&vcc3v3_pmu>;
};

&pwm1 {
	status = "okay";
};

&pwm3 {
	status = "okay";
};

&rk_rga {
	status = "okay";
};

&rkisp1 {
	status = "okay";

	port {
		#address-cells = <1>;
		#size-cells = <0>;

		isp0_mipi_in: endpoint@0 {
			reg = <0>;
			remote-endpoint = <&dphy_rx0_out>;
		};
	};
};

&saradc {
	status = "okay";
	vref-supply = <&vcc_1v8>;
};

&sdio {
	bus-width = <4>;
	cap-sd-highspeed;
	supports-sdio;
	ignore-pm-notify;
	keep-power-in-suspend;
	non-removable;
	mmc-pwrseq = <&sdio_pwrseq>;
	sd-uhs-sdr104;
	status = "okay";
};

&tsadc {
	pinctrl-names = "gpio", "otpout";
	pinctrl-0 = <&tsadc_otp_gpio>;
	pinctrl-1 = <&tsadc_otp_out>;
	status = "okay";
};

&uart1 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart1_xfer &uart1_cts>;
	status = "okay";
};

&u2phy {
	status = "okay";

	u2phy_host: host-port {
		status = "okay";
		phy-supply = <&vcc5v0_host>;
	};

	u2phy_otg: otg-port {
		status = "okay";
	};
};

&usb20_otg {
	status = "okay";
};

&usb_host0_ehci {
	status = "okay";
};

&usb_host0_ohci {
	status = "okay";
};

&vopb {
	status = "okay";
};

&vopb_mmu {
	status = "okay";
};

&vopl {
	status = "okay";
};

&vopl_mmu {
	status = "okay";
};

&mpp_srv {
	status = "okay";
};

&vdpu {
	status = "okay";
};

&vepu {
	status = "okay";
};

&vpu_mmu {
	status = "okay";
};

&hevc {
	status = "okay";
};

&hevc_mmu {
	status = "okay";
};

&pinctrl {
	lcd {
		lcd0_pwren: lcd0-pwren {
			rockchip,pins = <1 RK_PD6 RK_FUNC_GPIO &pcfg_output_high>;
		};
		lcd0_rst: lcd0-rst {
			rockchip,pins = <1 RK_PD7 RK_FUNC_GPIO &pcfg_output_high>;
		};
		mipi_en: mipi-en {
			rockchip,pins = <2 RK_PB4 RK_FUNC_GPIO &pcfg_output_high>;
		};
		pwdn_rgb: pwdn-rgb {
			rockchip,pins = <1 RK_PD4 RK_FUNC_GPIO &pcfg_output_high>;
		};
	};

	pmic {
		pmic_int: pmic_int {
			rockchip,pins =
				<0 RK_PA7 RK_FUNC_GPIO &pcfg_pull_up>;
		};

		soc_slppin_gpio: soc_slppin_gpio {
			rockchip,pins =
				<0 RK_PA4 RK_FUNC_GPIO &pcfg_output_low>;
		};

		soc_slppin_slp: soc_slppin_slp {
			rockchip,pins =
				<0 RK_PA4 1 &pcfg_pull_none>;
		};

		soc_slppin_rst: soc_slppin_rst {
			rockchip,pins =
				<0 RK_PA4 2 &pcfg_pull_none>;
		};
	};

	sdio-pwrseq {
		wifi_enable_h: wifi-enable-h {
			rockchip,pins = <0 RK_PA3 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};
};
