// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Copyright (c) 2022 Rockchip Electronics Co., Ltd.
 *
 */

#include "dt-bindings/usb/pd.h"
#include "rk3588.dtsi"
#include "rk3588-evb.dtsi"
#include "rk3588-rk806-single.dtsi"

/ {
	/* If hdmirx node is disabled, delete the reserved-memory node here. */
	reserved-memory {
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;

		/* Reserve 128MB memory for hdmirx-controller@fdee0000 */
		cma {
			compatible = "shared-dma-pool";
			reusable;
			reg = <0x0 (256 * 0x100000) 0x0 (128 * 0x100000)>;
			linux,cma-default;
		};
	};

	es8388_sound: es8388-sound {
		status = "okay";
		compatible = "rockchip,multicodecs-card";
		rockchip,card-name = "rockchip-es8388";
		hp-det-gpio = <&gpio1 RK_PC4 GPIO_ACTIVE_LOW>;
		io-channels = <&saradc 3>;
		io-channel-names = "adc-detect";
		keyup-threshold-microvolt = <1800000>;
		poll-interval = <100>;
		spk-con-gpio = <&gpio4 RK_PA2 GPIO_ACTIVE_HIGH>;
		hp-con-gpio = <&gpio4 RK_PA7 GPIO_ACTIVE_HIGH>;
		rockchip,format = "i2s";
		rockchip,mclk-fs = <256>;
		rockchip,cpu = <&i2s0_8ch>;
		rockchip,codec = <&es8388>;
		rockchip,audio-routing =
			"Headphone", "LOUT1",
			"Headphone", "ROUT1",
			"Speaker", "LOUT2",
			"Speaker", "ROUT2",
			"Headphone", "Headphone Power",
			"Headphone", "Headphone Power",
			"Speaker", "Speaker Power",
			"Speaker", "Speaker Power",
			"LINPUT1", "Main Mic",
			"LINPUT2", "Main Mic",
			"RINPUT1", "Headset Mic",
			"RINPUT2", "Headset Mic";
		pinctrl-names = "default";
		pinctrl-0 = <&hp_det>;
		play-pause-key {
			label = "playpause";
			linux,code = <KEY_PLAYPAUSE>;
			press-threshold-microvolt = <2000>;
		};
	};

	fan: pwm-fan {
		compatible = "pwm-fan";
		#cooling-cells = <2>;
		pwms = <&pwm3 0 50000 0>;
		cooling-levels = <0 50 100 150 200 255>;
		rockchip,temp-trips = <
			50000	1
			55000	2
			60000	3
			65000	4
			70000	5
		>;
	};

	hdmiin-sound {
		compatible = "rockchip,hdmi";
		rockchip,mclk-fs = <128>;
		rockchip,format = "i2s";
		rockchip,bitclock-master = <&hdmirx_ctrler>;
		rockchip,frame-master = <&hdmirx_ctrler>;
		rockchip,card-name = "rockchip,hdmiin";
		rockchip,cpu = <&i2s7_8ch>;
		rockchip,codec = <&hdmirx_ctrler 0>;
		rockchip,jack-det;
	};

	pcie20_avdd0v85: pcie20-avdd0v85 {
		compatible = "regulator-fixed";
		regulator-name = "pcie20_avdd0v85";
		regulator-boot-on;
		regulator-always-on;
		regulator-min-microvolt = <850000>;
		regulator-max-microvolt = <850000>;
		vin-supply = <&vdd_0v85_s0>;
	};

	pcie20_avdd1v8: pcie20-avdd1v8 {
		compatible = "regulator-fixed";
		regulator-name = "pcie20_avdd1v8";
		regulator-boot-on;
		regulator-always-on;
		regulator-min-microvolt = <1800000>;
		regulator-max-microvolt = <1800000>;
		vin-supply = <&avcc_1v8_s0>;
	};

	pcie30_avdd0v75: pcie30-avdd0v75 {
		compatible = "regulator-fixed";
		regulator-name = "pcie30_avdd0v75";
		regulator-boot-on;
		regulator-always-on;
		regulator-min-microvolt = <750000>;
		regulator-max-microvolt = <750000>;
		vin-supply = <&avdd_0v75_s0>;
	};

	pcie30_avdd1v8: pcie30-avdd1v8 {
		compatible = "regulator-fixed";
		regulator-name = "pcie30_avdd1v8";
		regulator-boot-on;
		regulator-always-on;
		regulator-min-microvolt = <1800000>;
		regulator-max-microvolt = <1800000>;
		vin-supply = <&avcc_1v8_s0>;
	};

	sdio_pwrseq: sdio-pwrseq {
		compatible = "mmc-pwrseq-simple";
		clocks = <&hym8563>;
		clock-names = "ext_clock";
		pinctrl-names = "default";
		pinctrl-0 = <&wifi_enable_h>;
		/*
		 * On the module itself this is one of these (depending
		 * on the actual card populated):
		 * - SDIO_RESET_L_WL_REG_ON
		 * - PDN (power down when low)
		 */
		post-power-on-delay-ms = <200>;
		reset-gpios = <&gpio0 RK_PC4 GPIO_ACTIVE_LOW>;
	};

	rk_headset: rk-headset {
		status = "disabled";
		compatible = "rockchip_headset";
		headset_gpio = <&gpio1 RK_PD5 GPIO_ACTIVE_LOW>;
		pinctrl-names = "default";
		pinctrl-0 = <&hp_det>;
		io-channels = <&saradc 3>;
	};


	vcc_1v1_nldo_s3: vcc-1v1-nldo-s3 {
		compatible = "regulator-fixed";
		regulator-name = "vcc_1v1_nldo_s3";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <1100000>;
		regulator-max-microvolt = <1100000>;
		vin-supply = <&vcc5v0_sys>;
	};

	vbus5v0_typec: vbus5v0-typec {
		compatible = "regulator-fixed";
		regulator-name = "vbus5v0_typec";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		enable-active-high;
		gpio = <&gpio3 RK_PA6 GPIO_ACTIVE_HIGH>;
		vin-supply = <&vcc5v0_usb>;
		pinctrl-names = "default";
		pinctrl-0 = <&typec5v_pwren>;
	};

	vcc3v3_lcd_n: vcc3v3-lcd0-n {
		compatible = "regulator-fixed";
		regulator-name = "vcc3v3_lcd0_n";
		regulator-boot-on;
		enable-active-high;
		gpio = <&gpio2 RK_PC1 GPIO_ACTIVE_HIGH>;
		vin-supply = <&vcc_1v8_s0>;
	};

	vcc3v3_pcie30: vcc3v3-pcie30 {
		compatible = "regulator-fixed";
		regulator-name = "vcc3v3_pcie30";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		enable-active-high;
		gpios = <&gpio2 RK_PC5 GPIO_ACTIVE_HIGH>;
		startup-delay-us = <5000>;
		vin-supply = <&vcc12v_dcin>;
	};

	vcc5v0_host: vcc5v0-host {
		compatible = "regulator-fixed";
		regulator-name = "vcc5v0_host";
		regulator-boot-on;
		regulator-always-on;
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		enable-active-high;
		gpio = <&gpio4 RK_PB0 GPIO_ACTIVE_HIGH>;
		vin-supply = <&vcc5v0_usb>;
		pinctrl-names = "default";
		pinctrl-0 = <&vcc5v0_host_en>;
	};

	vcc_mipicsi0: vcc-mipicsi0-regulator {
		compatible = "regulator-fixed";
		gpio = <&gpio1 RK_PD2 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&mipicsi0_pwr>;
		regulator-name = "vcc_mipicsi0";
		enable-active-high;
	};

	vcc_mipicsi1: vcc-mipicsi1-regulator {
		compatible = "regulator-fixed";
		gpio = <&gpio1 RK_PD3 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&mipicsi1_pwr>;
		regulator-name = "vcc_mipicsi1";
		enable-active-high;
	};

	vcc_mipidcphy0: vcc-mipidcphy0-regulator {
		compatible = "regulator-fixed";
		gpio = <&gpio2 RK_PC4 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&mipidcphy0_pwr>;
		regulator-name = "vcc_mipidcphy0";
		enable-active-high;
	};

	vcc_3v3_sd_s0: vcc-3v3-sd-s0-regulator {
		compatible = "regulator-fixed";
		gpio = <&gpio0 RK_PB7 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&sd_s0_pwr>;
		regulator-name = "vcc_3v3_sd_s0";
		enable-active-high;
	};

	wireless_bluetooth: wireless-bluetooth {
		compatible = "bluetooth-platdata";
		clocks = <&hym8563>;
		clock-names = "ext_clock";
		uart_rts_gpios = <&gpio4 RK_PC4 GPIO_ACTIVE_LOW>;
		pinctrl-names = "default", "rts_gpio";
		pinctrl-0 = <&uart9m0_rtsn>, <&bt_reset_gpio>, <&bt_wake_gpio>, <&bt_irq_gpio>;
		pinctrl-1 = <&uart9_gpios>;
		BT,reset_gpio    = <&gpio0 RK_PC6 GPIO_ACTIVE_HIGH>;
		BT,wake_gpio     = <&gpio0 RK_PC5 GPIO_ACTIVE_HIGH>;
		BT,wake_host_irq = <&gpio0 RK_PA0 GPIO_ACTIVE_HIGH>;
		status = "okay";
	};

	wireless_wlan: wireless-wlan {
		compatible = "wlan-platdata";
		wifi_chip_type = "ap6398s";
		pinctrl-names = "default";
		pinctrl-0 = <&wifi_host_wake_irq>;
		WIFI,host_wake_irq = <&gpio0 RK_PB2 GPIO_ACTIVE_HIGH>;
		WIFI,poweren_gpio = <&gpio0 RK_PC4 GPIO_ACTIVE_HIGH>;
		status = "okay";
	};
};

&backlight {
	pwms = <&pwm1 0 25000 0>;
	status = "okay";
};

&combphy0_ps {
	status = "okay";
};

&combphy1_ps {
	status = "okay";
};

&combphy2_psu {
	status = "okay";
};

&dp0 {
	status = "okay";
};
&dp0_in_vp2 {
	status = "okay";
};

&dp0_sound{
	status = "okay";
};
&dp1 {
	pinctrl-names = "default";
	pinctrl-0 = <&dp1m0_pins>;
	status = "okay";
};

&dp1_in_vp2 {
	status = "okay";
};

/*
 * mipi_dcphy0 needs to be enabled
 * when dsi0 is enabled
 */
&dsi0 {
	status = "okay";
};

&dsi0_in_vp2 {
	status = "disabled";
};

&dsi0_in_vp3 {
	status = "okay";
};

&dsi0_panel {
	power-supply = <&vcc3v3_lcd_n>;
	reset-gpios = <&gpio0 RK_PD3 GPIO_ACTIVE_LOW>;
	pinctrl-names = "default";
	pinctrl-0 = <&lcd_rst_gpio>;
};

/*
 * mipi_dcphy1 needs to be enabled
 * when dsi1 is enabled
 */
&dsi1 {
	status = "disabled";
};

&dsi1_in_vp2 {
	status = "disabled";
};

&dsi1_in_vp3 {
	status = "disabled";
};

&dsi1_panel {
	power-supply = <&vcc3v3_lcd_n>;

	/*
	 * because in hardware, the two screens share the reset pin,
	 * so reset-gpios need only in dsi1 enable and dsi0 disabled
	 * case.
	 */

	//reset-gpios = <&gpio0 RK_PD3 GPIO_ACTIVE_LOW>;
	//pinctrl-names = "default";
	//pinctrl-0 = <&lcd_rst_gpio>;
};

&gmac1 {
	/* Use rgmii-rxid mode to disable rx delay inside Soc */
	phy-mode = "rgmii-rxid";
	clock_in_out = "output";

	snps,reset-gpio = <&gpio3 RK_PB7 GPIO_ACTIVE_LOW>;
	snps,reset-active-low;
	/* Reset time is 20ms, 100ms for rtl8211f */
	snps,reset-delays-us = <0 20000 100000>;

	pinctrl-names = "default";
	pinctrl-0 = <&gmac1_miim
		     &gmac1_tx_bus2
		     &gmac1_rx_bus2
		     &gmac1_rgmii_clk
		     &gmac1_rgmii_bus>;

	tx_delay = <0x43>;
	/* rx_delay = <0x3f>; */

	phy-handle = <&rgmii_phy>;
	status = "okay";
};

&hdmi0 {
	enable-gpios = <&gpio4 RK_PB1 GPIO_ACTIVE_HIGH>;
	status = "okay";
};

&hdmi0_in_vp0 {
	status = "okay";
};

&hdmi0_sound {
	status = "okay";
};

&hdmi1 {
	enable-gpios = <&gpio4 RK_PB2 GPIO_ACTIVE_HIGH>;
	status = "okay";
};

&hdmi1_in_vp1 {
	status = "okay";
};

&hdmi1_sound {
	status = "okay";
};

/* Should work with at least 128MB cma reserved above. */
&hdmirx_ctrler {
	status = "okay";

	#sound-dai-cells = <1>;
	/* Effective level used to trigger HPD: 0-low, 1-high */
	hpd-trigger-level = <1>;
	hdmirx-det-gpios = <&gpio1 RK_PD5 GPIO_ACTIVE_LOW>;
	pinctrl-names = "default";
	pinctrl-0 = <&hdmim1_rx &hdmirx_det>;
};

&hdptxphy_hdmi0 {
	status = "okay";
};

&hdptxphy_hdmi1 {
	status = "okay";
};

&i2c0 {
	status = "okay";
	pinctrl-names = "default";
	pinctrl-0 = <&i2c0m2_xfer>;

	vdd_cpu_big0_s0: vdd_cpu_big0_mem_s0: rk8602@42 {
		compatible = "rockchip,rk8602";
		reg = <0x42>;
		vin-supply = <&vcc5v0_sys>;
		regulator-compatible = "rk860x-reg";
		regulator-name = "vdd_cpu_big0_s0";
		regulator-min-microvolt = <550000>;
		regulator-max-microvolt = <1050000>;
		regulator-ramp-delay = <2300>;
		rockchip,suspend-voltage-selector = <1>;
		regulator-boot-on;
		regulator-always-on;
		regulator-state-mem {
			regulator-off-in-suspend;
		};
	};

	vdd_cpu_big1_s0: vdd_cpu_big1_mem_s0: rk8603@43 {
		compatible = "rockchip,rk8603";
		reg = <0x43>;
		vin-supply = <&vcc5v0_sys>;
		regulator-compatible = "rk860x-reg";
		regulator-name = "vdd_cpu_big1_s0";
		regulator-min-microvolt = <550000>;
		regulator-max-microvolt = <1050000>;
		regulator-ramp-delay = <2300>;
		rockchip,suspend-voltage-selector = <1>;
		regulator-boot-on;
		regulator-always-on;
		regulator-state-mem {
			regulator-off-in-suspend;
		};
	};
};

&i2c1 {
	status = "okay";
	pinctrl-names = "default";
	pinctrl-0 = <&i2c1m2_xfer>;

	vdd_npu_s0: vdd_npu_mem_s0: rk8602@42 {
		compatible = "rockchip,rk8602";
		reg = <0x42>;
		vin-supply = <&vcc5v0_sys>;
		regulator-compatible = "rk860x-reg";
		regulator-name = "vdd_npu_s0";
		regulator-min-microvolt = <550000>;
		regulator-max-microvolt = <950000>;
		regulator-ramp-delay = <2300>;
		rockchip,suspend-voltage-selector = <1>;
		regulator-boot-on;
		regulator-always-on;
		regulator-state-mem {
			regulator-off-in-suspend;
		};
	};
};

&i2c4 {
	status = "okay";
	pinctrl-0 = <&i2c4m1_xfer>;

	ls_stk3332: light@47 {
		compatible = "ls_stk3332";
		status = "disabled";
		reg = <0x47>;
		type = <SENSOR_TYPE_LIGHT>;
		irq_enable = <0>;
		als_threshold_high = <100>;
		als_threshold_low = <10>;
		als_ctrl_gain = <2>; /* 0:x1 1:x4 2:x16 3:x64 */
		poll_delay_ms = <100>;
	};

	ps_stk3332: proximity@47 {
		compatible = "ps_stk3332";
		status = "disabled";
		reg = <0x47>;
		type = <SENSOR_TYPE_PROXIMITY>;
		//pinctrl-names = "default";
		//pinctrl-0 = <&gpio3_c6>;
		//irq-gpio = <&gpio3 RK_PC6 IRQ_TYPE_LEVEL_LOW>;
		//irq_enable = <1>;
		ps_threshold_high = <0x200>;
		ps_threshold_low = <0x100>;
		ps_ctrl_gain = <3>; /* 0:x1 1:x2 2:x5 3:x8 */
		ps_led_current = <4>; /* 0:3.125mA 1:6.25mA 2:12.5mA 3:25mA 4:50mA 5:100mA*/
		poll_delay_ms = <100>;
	};

	icm42607_acc: icm_acc@68 {
		status = "okay";
		compatible = "icm42607_acc";
		reg = <0x68>;
		irq-gpio = <&gpio4 RK_PC2 IRQ_TYPE_EDGE_RISING>;
		irq_enable = <0>;
		poll_delay_ms = <30>;
		type = <SENSOR_TYPE_ACCEL>;
		layout = <0>;
	};

	icm42607_gyro: icm_gyro@68 {
		status = "okay";
		compatible = "icm42607_gyro";
		reg = <0x68>;
		poll_delay_ms = <30>;
		type = <SENSOR_TYPE_GYROSCOPE>;
		layout = <0>;
	};
};

&i2c5 {
	status = "okay";
	gt1x: gt1x@14 {
		compatible = "goodix,gt1x";
		reg = <0x14>;
		pinctrl-names = "default";
		pinctrl-0 = <&touch_gpio>;
		goodix,rst-gpio = <&gpio3 RK_PC1 GPIO_ACTIVE_HIGH>;
		goodix,irq-gpio = <&gpio3 RK_PC0 IRQ_TYPE_LEVEL_LOW>;
		power-supply = <&vcc3v3_lcd_n>;
	};
};

&i2c6 {
	status = "okay";

	usbc0: husb311@4e {
		compatible = "hynetek,husb311";
		reg = <0x4e>;
		interrupt-parent = <&gpio3>;
		interrupts = <RK_PB6 IRQ_TYPE_LEVEL_LOW>;
		pinctrl-names = "default";
		pinctrl-0 = <&usbc0_int>;
		vbus-supply = <&vbus5v0_typec>;
		status = "okay";

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				usbc0_role_sw: endpoint@0 {
					remote-endpoint = <&dwc3_0_role_switch>;
				};
			};
		};

		usb_con: connector {
			compatible = "usb-c-connector";
			label = "USB-C";
			data-role = "dual";
			power-role = "dual";
			try-power-role = "sink";
			op-sink-microwatt = <1000000>;
			sink-pdos =
				<PDO_FIXED(5000, 1000, PDO_FIXED_USB_COMM)>;
			source-pdos =
				<PDO_FIXED(5000, 3000, PDO_FIXED_USB_COMM)>;

			altmodes {
				#address-cells = <1>;
				#size-cells = <0>;

				altmode@0 {
					reg = <0>;
					svid = <0xff01>;
					vdo = <0xffffffff>;
				};
			};

			ports {
				#address-cells = <1>;
				#size-cells = <0>;

				port@0 {
					reg = <0>;
					usbc0_orien_sw: endpoint {
						remote-endpoint = <&usbdp_phy0_orientation_switch>;
					};
				};

				port@1 {
					reg = <1>;
					dp_altmode_mux: endpoint {
						remote-endpoint = <&usbdp_phy0_dp_altmode_mux>;
					};
				};
			};
		};
	};

	hym8563: hym8563@51 {
		compatible = "haoyu,hym8563";
		reg = <0x51>;
		#clock-cells = <0>;
		clock-frequency = <32768>;
		clock-output-names = "hym8563";
		pinctrl-names = "default";
		pinctrl-0 = <&hym8563_int>;
		interrupt-parent = <&gpio0>;
		interrupts = <RK_PB0 IRQ_TYPE_LEVEL_LOW>;
		wakeup-source;
	};
};

&i2c7 {
	status = "okay";
	es8388: es8388@11 {
		status = "okay";
		#sound-dai-cells = <0>;
		compatible = "everest,es8388", "everest,es8323";
		reg = <0x11>;
		clocks = <&mclkout_i2s0>;
		clock-names = "mclk";
		assigned-clocks = <&mclkout_i2s0>;
		assigned-clock-rates = <12288000>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2s0_mclk>;
	};
};

&i2s5_8ch {
	status = "okay";
};

&i2s6_8ch {
	status = "okay";
};

&i2s7_8ch {
	status = "okay";
};

&mdio1 {
	rgmii_phy: phy@1 {
		compatible = "ethernet-phy-ieee802.3-c22";
		reg = <0x1>;
	};
};

&mipi_dcphy0 {
	status = "okay";
};

&mipi_dcphy1 {
	status = "disabled";
};

&pcie2x1l0 {
	reset-gpios = <&gpio1 RK_PB4 GPIO_ACTIVE_HIGH>;
	status = "okay";
};

&pcie30phy {
	rockchip,pcie30-phymode = <PHY_MODE_PCIE_AGGREGATION>;
	status = "okay";
};

&pcie3x4 {
	reset-gpios = <&gpio4 RK_PB6 GPIO_ACTIVE_HIGH>;
	vpcie3v3-supply = <&vcc3v3_pcie30>;
	pinctrl-names = "default";
	pinctrl-0 = <&pcie20x1_0_clkreqn_m1>;
	status = "okay";
};

&pinctrl {
	cam {
		mipicsi0_pwr: mipicsi0-pwr {
			rockchip,pins =
				/* camera power en */
				<1 RK_PD2 RK_FUNC_GPIO &pcfg_pull_none>;
		};
		mipicsi1_pwr: mipicsi1-pwr {
			rockchip,pins =
				/* camera power en */
				<1 RK_PD3 RK_FUNC_GPIO &pcfg_pull_none>;
		};
		mipidcphy0_pwr: mipidcphy0-pwr {
			rockchip,pins =
				/* camera power en */
				<2 RK_PC4 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};


	hdmi {
		hdmirx_det: hdmirx-det {
			rockchip,pins = <1 RK_PD5 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	headphone {
		hp_det: hp-det {
			rockchip,pins = <1 RK_PC4 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	hym8563 {
		hym8563_int: hym8563-int {
			rockchip,pins = <0 RK_PB0 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	lcd {
		lcd_rst_gpio: lcd-rst-gpio {
			rockchip,pins = <0 RK_PD3 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	leds {
		work_leds_gpio: work-leds-gpio {
			rockchip,pins = <1 RK_PC6 RK_FUNC_GPIO &pcfg_pull_down>;
		};
	};

	sdio-pwrseq {
		wifi_enable_h: wifi-enable-h {
			rockchip,pins = <0 RK_PC4 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	sdmmc {
		sd_s0_pwr: sd-s0-pwr {
			rockchip,pins = <0 RK_PB7 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	touch {
		touch_gpio: touch-gpio {
			rockchip,pins =
				<3 RK_PC1 RK_FUNC_GPIO &pcfg_pull_down>,
				<3 RK_PC0 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	usb {
		vcc5v0_host_en: vcc5v0-host-en {
			rockchip,pins = <4 RK_PB0 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	usb-typec {
		usbc0_int: usbc0-int {
			rockchip,pins = <3 RK_PB6 RK_FUNC_GPIO &pcfg_pull_up>;
		};

		typec5v_pwren: typec5v-pwren {
			rockchip,pins = <3 RK_PA6 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	wireless-bluetooth {
		uart9_gpios: uart9-gpios {
			rockchip,pins = <4 RK_PC4 RK_FUNC_GPIO &pcfg_pull_none>;
		};

		bt_reset_gpio: bt-reset-gpio {
			rockchip,pins = <0 RK_PC6 RK_FUNC_GPIO &pcfg_pull_none>;
		};

		bt_wake_gpio: bt-wake-gpio {
			rockchip,pins = <0 RK_PC5 RK_FUNC_GPIO &pcfg_pull_none>;
		};

		bt_irq_gpio: bt-irq-gpio {
			rockchip,pins = <0 RK_PA0 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	wireless-wlan {
		wifi_host_wake_irq: wifi-host-wake-irq {
			rockchip,pins = <0 RK_PB2 RK_FUNC_GPIO &pcfg_pull_down>;
		};
	};

	pcie {
		pcie20x1_0_clkreqn_m1: pcie20x1-0-clkreqn-m1 {
			rockchip,pins = <4 RK_PB4 RK_FUNC_GPIO &pcfg_output_low>;
		};
	};
};

&pwm1 {
	status = "okay";
};

&pwm3 {
	pinctrl-0 = <&pwm3m1_pins>;
	status = "okay";
};

&route_dsi0 {
	status = "okay";
	connect = <&vp3_out_dsi0>;
};

&route_dsi1 {
	status = "disabled";
	connect = <&vp3_out_dsi1>;
};

&route_hdmi0 {
	status = "okay";
};

&route_hdmi1 {
	status = "okay";
};

&sata0 {
	status = "okay";
};

&sdio {
	max-frequency = <150000000>;
	no-sd;
	no-mmc;
	bus-width = <4>;
	disable-wp;
	cap-sd-highspeed;
	cap-sdio-irq;
	keep-power-in-suspend;
	mmc-pwrseq = <&sdio_pwrseq>;
	non-removable;
	pinctrl-names = "default";
	pinctrl-0 = <&sdiom0_pins>;
	sd-uhs-sdr104;
	status = "okay";
};

&sdmmc {
	status = "okay";
	vmmc-supply = <&vcc_3v3_sd_s0>;
};

&uart9 {
	status = "okay";
	pinctrl-names = "default";
	pinctrl-0 = <&uart9m0_xfer &uart9m0_ctsn>;
};

&u2phy0_otg {
	rockchip,typec-vbus-det;
};

&u2phy1_otg {
	phy-supply = <&vcc5v0_host>;
};

&u2phy2_host {
	phy-supply = <&vcc5v0_host>;
};

&u2phy3_host {
	phy-supply = <&vcc5v0_host>;
};

&usbdp_phy0 {
	orientation-switch;
	svid = <0xff01>;
	sbu1-dc-gpios = <&gpio4 RK_PA0 GPIO_ACTIVE_HIGH>;
	sbu2-dc-gpios = <&gpio4 RK_PA1 GPIO_ACTIVE_HIGH>;

	port {
		#address-cells = <1>;
		#size-cells = <0>;
		usbdp_phy0_orientation_switch: endpoint@0 {
			reg = <0>;
			remote-endpoint = <&usbc0_orien_sw>;
		};

		usbdp_phy0_dp_altmode_mux: endpoint@1 {
			reg = <1>;
			remote-endpoint = <&dp_altmode_mux>;
		};
	};
};

&usbdp_phy1 {
	rockchip,dp-lane-mux = <0 1 2 3>;
};

&usbdrd_dwc3_0 {
	dr_mode = "otg";
	usb-role-switch;
	port {
		#address-cells = <1>;
		#size-cells = <0>;
		dwc3_0_role_switch: endpoint@0 {
			reg = <0>;
			remote-endpoint = <&usbc0_role_sw>;
		};
	};
};

&usbhost3_0 {
	status = "disabled";
};

&usbhost_dwc3_0 {
	status = "disabled";
};

&work_led {
	gpios = <&gpio1 RK_PC6 GPIO_ACTIVE_HIGH>;
	pinctrl-names = "default";
	pinctrl-0 = <&work_leds_gpio>;
};
