// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Copyright (c) 2022 Rockchip Electronics Co., Ltd.
 *
 */

#include "rk3588.dtsi"

&cluster0_opp_table {
	/*
	 * The Max frequency is 1296MHz in default normal mode.
	 * The Max frequency is 1704MHz in overdrive mode,
	 * but under the overdrive mode for a long time,
	 * the chipset may shorten the lifetime,
	 * especially in high temperature condition.
	 */
	/delete-node/ opp-j-m-1416000000;
	/delete-node/ opp-j-m-1608000000;
	/delete-node/ opp-j-m-1704000000;
};

&cluster1_opp_table {
	/*
	 * The Max frequency is 1608MHz in default normal mode.
	 * The Max frequency is 2016MHz in overdrive mode,
	 * but under the overdrive mode for a long time,
	 * the chipset may shorten the lifetime,
	 * especially in high temperature condition.
	 */
	/delete-node/ opp-j-m-1800000000;
	/delete-node/ opp-j-m-2016000000;
};

&cluster2_opp_table {
	/*
	 * The Max frequency is 1608MHz in default normal mode.
	 * The Max frequency is 2016MHz in overdrive mode,
	 * but under the overdrive mode for a long time,
	 * the chipset may shorten the lifetime,
	 * especially in high temperature condition.
	 */
	/delete-node/ opp-j-m-1800000000;
	/delete-node/ opp-j-m-2016000000;
};

&gpu_opp_table {
	/*
	 * The Max frequency is 700MHz in default normal mode.
	 * The Max frequency is 850MHz in overdrive mode,
	 * but under the overdrive mode for a long time,
	 * the chipset may shorten the lifetime,
	 * especially in high temperature condition.
	 */
	/delete-node/ opp-j-850000000;
};

&npu_opp_table {
	/*
	 * The Max frequency is 800MHz in default normal mode.
	 * The Max frequency is 950MHz in overdrive mode,
	 * but under the overdrive mode for a long time,
	 * the chipset may shorten the lifetime,
	 * especially in high temperature condition.
	 */
	/delete-node/ opp-j-m-950000000;
};
