// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Copyright (c) 2020 Rockchip Electronics Co., Ltd.
 *
 */

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/pwm/pwm.h>
#include <dt-bindings/pinctrl/rockchip.h>
#include <dt-bindings/input/rk-input.h>
#include <dt-bindings/display/drm_mipi_dsi.h>
#include <dt-bindings/sensor-dev.h>
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/pinctrl/rockchip.h>


#include "../rk3568.dtsi"

/ {
    
  rpdzkj:rpdzkj_config {
          compatible = "rp_config";
          user_version = "rpdzkj";
          system_rotate = "0";
                    csi_camera_rotate = "0"; //all csi camera rotation //0 90 180 270 //no effect
                    csi_camera_facing = "0"; //0:auto  1:all front   2:all back //no effect
                    usb_camera_rotate = "0"; //all usb camera rotation //0 90 180 270 
                    usb_camera_facing = "0"; //0:auto  1:all front   2:all back
          lcd_density = "160";
          language = "zh-CN";   //zh-CN //en-US
          time_zone = "Asia/Shanghai"; //Asia/Shanghai = +8   //Europe/London  = +1       //Africa/Casablanca     = +0;
          not_navigation_bar = "false";
          not_status_bar = "false";
          default_launcher = "true";
          has_root = "true";
          usb_not_permission = "true";
          gps_use = "false";
          gps_serial_port = "/dev/ttyS4";
          primary_device = "DSI";
          extend_device = "HDMI-A";
          extend_rotate = "0";
          rotation_efull = "false";
	        extend_rotate_2 = "0";//0 0//1 90 //2 180 //3 270
	        rotation_efull_2 = "true";
	        extend_rotate_3 = "0";//0 0//1 90 //2 180 //3 270
	        rotation_efull_3 = "true";
          home_apk = "null";
          status = "okay";
  };
  
  
        vdd_cpu: vdd-cpu {
                compatible = "pwm-regulator";
                pwms = <&pwm0 0 5000 1>;
                regulator-name = "vdd_cpu";
                regulator-min-microvolt = <675000>;
                regulator-max-microvolt = <1250000>;
                regulator-init-microvolt = <1000000>;
                regulator-ramp-delay = <6001>;       
                regulator-always-on;
                regulator-boot-on;
                regulator-settling-time-up-us = <250>;
                pwm-supply = <&vcc5v0_sys>;
                status = "okay";
        };

    edp_panel:panel {
        status = "disabled";
    };

    lvds_panel: panel@0 {
        status = "disabled";
    };



    audiopwmout_diff: audiopwmout-diff {
        status = "disabled";
        compatible = "simple-audio-card";
        simple-audio-card,format = "i2s";
        simple-audio-card,name = "rockchip,audiopwmout-diff";
        simple-audio-card,mclk-fs = <256>;
        simple-audio-card,bitclock-master = <&master>;
        simple-audio-card,frame-master = <&master>;
        simple-audio-card,cpu {
            sound-dai = <&i2s3_2ch>;
        };
        master: simple-audio-card,codec {
            sound-dai = <&dig_acodec>;
        };
    };
        
        
        
    rk_headset: rk-headset {
        compatible = "rockchip_headset";
//        headset_gpio = <&gpio1 RK_PB0 GPIO_ACTIVE_HIGH>;
    };
    

    dc_12v: dc-12v {
        compatible = "regulator-fixed";
        regulator-name = "dc_12v";
        regulator-always-on;
        regulator-boot-on;
        regulator-min-microvolt = <12000000>;
        regulator-max-microvolt = <12000000>;
    };

    hdmi_sound: hdmi-sound {
        status = "disabled";
        compatible = "rockchip,hdmi";
        rockchip,mclk-fs = <128>;
        rockchip,card-name = "rockchip,hdmi";
        rockchip,cpu = <&i2s0_8ch>;
        rockchip,codec = <&hdmi>;
    };
/*
    leds: leds {
        compatible = "gpio-leds";
        work_led: work {
            gpios = <&gpio0 RK_PC0 GPIO_ACTIVE_HIGH>;
            linux,default-trigger = "heartbeat";
        };
    };
*/
    pdmics: dummy-codec {
        status = "disabled";
        compatible = "rockchip,dummy-codec";
        #sound-dai-cells = <0>;
    };

    pdm_mic_array: pdm-mic-array {
        status = "disabled";
        compatible = "simple-audio-card";
        simple-audio-card,name = "rockchip,pdm-mic-array";
        simple-audio-card,cpu {
            sound-dai = <&pdm>;
        };
        simple-audio-card,codec {
            sound-dai = <&pdmics>;
        };
    };

    rk809_sound: rk809-sound {
        status = "okay";
        compatible = "simple-audio-card";
        simple-audio-card,format = "i2s";
        simple-audio-card,name = "rockchip,rk809-codec";
        simple-audio-card,mclk-fs = <256>;

        simple-audio-card,cpu {
            sound-dai = <&i2s1_8ch>;
        };
        simple-audio-card,codec {
            sound-dai = <&rk809_codec>;
        };
    };

    spdif-sound {
        status = "disabled";
        compatible = "simple-audio-card";
        simple-audio-card,name = "ROCKCHIP,SPDIF";
        simple-audio-card,cpu {
                sound-dai = <&spdif_8ch>;
        };
        simple-audio-card,codec {
                sound-dai = <&spdif_out>;
        };
    };

    spdif_out: spdif-out {
            status = "disabled";
            compatible = "linux,spdif-dit";
            #sound-dai-cells = <0>;
    };

    vad_sound: vad-sound {
        status = "disabled";
        compatible = "rockchip,multicodecs-card";
        rockchip,card-name = "rockchip,rk3568-vad";
        rockchip,cpu = <&i2s1_8ch>;
        rockchip,codec = <&rk809_codec>, <&vad>;
    };

    vcc3v3_sys: vcc3v3-sys {
        compatible = "regulator-fixed";
        regulator-name = "vcc3v3_sys";
        regulator-always-on;
        regulator-boot-on;
        regulator-min-microvolt = <3300000>;
        regulator-max-microvolt = <3300000>;
        vin-supply = <&dc_12v>;
    };

    vcc5v0_sys: vcc5v0-sys {
        compatible = "regulator-fixed";
        regulator-name = "vcc5v0_sys";
        regulator-always-on;
        regulator-boot-on;
        regulator-min-microvolt = <5000000>;
        regulator-max-microvolt = <5000000>;
        vin-supply = <&dc_12v>;
    };


    vcc3v3_lcd0_n: vcc3v3-lcd0-n {
        compatible = "regulator-fixed";
        regulator-name = "vcc3v3_lcd0_n";
        regulator-boot-on;
        regulator-min-microvolt = <3300000>;
        regulator-max-microvolt = <3300000>;
        enable-active-high;
//        gpio = <&gpio0 RK_PC7 GPIO_ACTIVE_HIGH>;
        vin-supply = <&vcc3v3_sys>;

        regulator-state-mem {
            regulator-off-in-suspend;
        };
    };

    vcc3v3_lcd1_n: vcc3v3-lcd1-n {
        compatible = "regulator-fixed";
        regulator-name = "vcc3v3_lcd1_n";
        regulator-boot-on;
        regulator-min-microvolt = <3300000>;
        regulator-max-microvolt = <3300000>;
        enable-active-high;
//        gpio = <&gpio0 RK_PC5 GPIO_ACTIVE_HIGH>;
        vin-supply = <&vcc3v3_sys>;

        regulator-state-mem {
            regulator-off-in-suspend;
        };
    };
    
    
    vcc2v5_sys: vcc2v5-ddr {
        compatible = "regulator-fixed";
        regulator-name = "vcc2v5-sys";
        regulator-always-on;
        regulator-boot-on;
        regulator-min-microvolt = <2500000>;
        regulator-max-microvolt = <2500000>;
        vin-supply = <&vcc3v3_sys>;
    };


/*
    sdio_pwrseq: sdio-pwrseq {
        compatible = "mmc-pwrseq-simple";
        clocks = <&rk809 1>;
        clock-names = "ext_clock";
        pinctrl-names = "default";
        pinctrl-0 = <&wifi_enable_h>;

//        
//         * On the module itself this is one of these (depending
//         * on the actual card populated):
//         * - SDIO_RESET_L_WL_REG_ON
//         * - PDN (power down when low)
//        
        post-power-on-delay-ms = <200>;
        reset-gpios = <&gpio3 RK_PD5 GPIO_ACTIVE_LOW>;
    };

    wireless_wlan: wireless-wlan {
        compatible = "wlan-platdata";
        rockchip,grf = <&grf>;
        wifi_chip_type = "ap6398s";
        status = "okay";
    };

    wireless_bluetooth: wireless-bluetooth {
        compatible = "bluetooth-platdata";
        clocks = <&rk809 1>;
        clock-names = "ext_clock";
        //wifi-bt-power-toggle;
        uart_rts_gpios = <&gpio2 RK_PB1 GPIO_ACTIVE_LOW>;
        pinctrl-names = "default", "rts_gpio";
        pinctrl-0 = <&uart8m0_rtsn>;
        pinctrl-1 = <&uart8_gpios>;
        BT,reset_gpio    = <&gpio3 RK_PA0 GPIO_ACTIVE_HIGH>;
        BT,wake_gpio     = <&gpio3 RK_PA1 GPIO_ACTIVE_HIGH>;
        BT,wake_host_irq = <&gpio3 RK_PA2 GPIO_ACTIVE_HIGH>;
        status = "okay";
    };
*/
    test-power {
        status = "okay";
    };
};

&bus_npu {
    bus-supply = <&vdd_logic>;
    pvtm-supply = <&vdd_cpu>;
    status = "okay";
};

&pwm0 {
        status = "okay";
        pinctrl-names = "active";
};

&cpu0 {
    cpu-supply = <&vdd_cpu>;
};

&dfi {
    status = "disabled";
};

&dmc {
    center-supply = <&vdd_logic>;
    status = "disabled";
};


&gpu {
    mali-supply = <&vdd_gpu>;
    status = "okay";
};


&i2c0 {
    status = "okay";
    rk809: pmic@20 {
        compatible = "rockchip,rk809";
        reg = <0x20>;
        interrupt-parent = <&gpio0>;
        interrupts = <3 IRQ_TYPE_LEVEL_LOW>;

        pinctrl-names = "default", "pmic-sleep",
                "pmic-power-off", "pmic-reset";
        pinctrl-0 = <&pmic_int>;
        pinctrl-1 = <&soc_slppin_slp>, <&rk817_slppin_slp>;
        pinctrl-2 = <&soc_slppin_gpio>, <&rk817_slppin_pwrdn>;
        pinctrl-3 = <&soc_slppin_gpio>, <&rk817_slppin_rst>;

        rockchip,system-power-controller;
        wakeup-source;
        #clock-cells = <1>;
        clock-output-names = "rk808-clkout1", "rk808-clkout2";
        //fb-inner-reg-idxs = <2>;
        /* 1: rst regs (default in codes), 0: rst the pmic */
        pmic-reset-func = <0>;
        /* not save the PMIC_POWER_EN register in uboot */
        not-save-power-en = <1>;

        vcc1-supply = <&vcc3v3_sys>;
        vcc2-supply = <&vcc3v3_sys>;
        vcc3-supply = <&vcc3v3_sys>;
        vcc4-supply = <&vcc3v3_sys>;
        vcc5-supply = <&vcc3v3_sys>;
        vcc6-supply = <&vcc3v3_sys>;
        vcc7-supply = <&vcc3v3_sys>;
        vcc8-supply = <&vcc3v3_sys>;
        vcc9-supply = <&vcc3v3_sys>;

        pwrkey {
            status = "okay";
        };

        pinctrl_rk8xx: pinctrl_rk8xx {
            gpio-controller;
            #gpio-cells = <2>;

            rk817_slppin_null: rk817_slppin_null {
                pins = "gpio_slp";
                function = "pin_fun0";
            };

            rk817_slppin_slp: rk817_slppin_slp {
                pins = "gpio_slp";
                function = "pin_fun1";
            };

            rk817_slppin_pwrdn: rk817_slppin_pwrdn {
                pins = "gpio_slp";
                function = "pin_fun2";
            };

            rk817_slppin_rst: rk817_slppin_rst {
                pins = "gpio_slp";
                function = "pin_fun3";
            };
        };

        regulators {
            vdd_logic: DCDC_REG1 {
                regulator-always-on;
                regulator-boot-on;
                regulator-min-microvolt = <950000>;
                regulator-max-microvolt = <1350000>;
                regulator-init-microvolt = <950000>;
                regulator-ramp-delay = <6001>;
                regulator-initial-mode = <0x2>;
                regulator-name = "vdd_logic";
                regulator-state-mem {
                    regulator-off-in-suspend;
                };
            };

            vdd_gpu: DCDC_REG2 {
                regulator-always-on;
                regulator-boot-on;
                regulator-min-microvolt = <500000>;
                regulator-max-microvolt = <1350000>;
                regulator-init-microvolt = <900000>;
                regulator-ramp-delay = <6001>;
                regulator-initial-mode = <0x2>;
                regulator-name = "vdd_gpu";
                regulator-state-mem {
                    regulator-off-in-suspend;
                };
            };

            vcc_ddr: DCDC_REG3 {
                regulator-always-on;
                regulator-boot-on;
                regulator-initial-mode = <0x2>;
                regulator-name = "vcc_ddr";
                regulator-state-mem {
                    regulator-on-in-suspend;
                };
            };

            vdd_npu: DCDC_REG4 {
                regulator-always-on;
                regulator-boot-on;
                regulator-min-microvolt = <500000>;
                regulator-max-microvolt = <1350000>;
                regulator-init-microvolt = <900000>;
                regulator-ramp-delay = <6001>;
                regulator-initial-mode = <0x2>;
                regulator-name = "vdd_npu";
                regulator-state-mem {
                    regulator-off-in-suspend;
                };
            };

            vdda0v9_image: LDO_REG1 {
                regulator-boot-on;
                regulator-always-on;
                regulator-min-microvolt = <900000>;
                regulator-max-microvolt = <900000>;
                regulator-name = "vdda0v9_image";
                regulator-state-mem {
                    regulator-off-in-suspend;
                };
            };

            vdda_0v9: LDO_REG2 {
                regulator-always-on;
                regulator-boot-on;
                regulator-min-microvolt = <900000>;
                regulator-max-microvolt = <900000>;
                regulator-name = "vdda_0v9";
                regulator-state-mem {
                    regulator-off-in-suspend;
                };
            };

            vdda0v9_pmu: LDO_REG3 {
                regulator-always-on;
                regulator-boot-on;
                regulator-min-microvolt = <900000>;
                regulator-max-microvolt = <900000>;
                regulator-name = "vdda0v9_pmu";
                regulator-state-mem {
                    regulator-on-in-suspend;
                    regulator-suspend-microvolt = <900000>;
                };
            };

            vccio_acodec: LDO_REG4 {
                regulator-always-on;
                regulator-boot-on;
                regulator-min-microvolt = <3000000>;
                regulator-max-microvolt = <3000000>;
                regulator-name = "vccio_acodec";
                regulator-state-mem {
                    regulator-off-in-suspend;
                };
            };

            vccio_sd: LDO_REG5 {
                regulator-always-on;
                regulator-boot-on;
                regulator-min-microvolt = <1800000>;
                regulator-max-microvolt = <3300000>;
                regulator-name = "vccio_sd";
                regulator-state-mem {
                    regulator-off-in-suspend;
                };
            };

            vcc3v3_pmu: LDO_REG6 {
                regulator-always-on;
                regulator-boot-on;
                regulator-min-microvolt = <3300000>;
                regulator-max-microvolt = <3300000>;
                regulator-name = "vcc3v3_pmu";
                regulator-state-mem {
                    regulator-on-in-suspend;
                    regulator-suspend-microvolt = <3300000>;
                };
            };

            vcca_1v8: LDO_REG7 {
                regulator-always-on;
                regulator-boot-on;
                regulator-min-microvolt = <1800000>;
                regulator-max-microvolt = <1800000>;
                regulator-name = "vcca_1v8";
                regulator-state-mem {
                    regulator-off-in-suspend;
                };
            };

            vcca1v8_pmu: LDO_REG8 {
                regulator-always-on;
                regulator-boot-on;
                regulator-min-microvolt = <1800000>;
                regulator-max-microvolt = <1800000>;
                regulator-name = "vcca1v8_pmu";
                regulator-state-mem {
                    regulator-on-in-suspend;
                    regulator-suspend-microvolt = <1800000>;
                };
            };

            vcca1v8_image: LDO_REG9 {
                regulator-always-on;
                regulator-boot-on;
                regulator-min-microvolt = <1800000>;
                regulator-max-microvolt = <1800000>;
                regulator-name = "vcca1v8_image";
                regulator-state-mem {
                    regulator-off-in-suspend;
                };
            };

            vcc_1v8: DCDC_REG5 {
                regulator-always-on;
                regulator-boot-on;
                regulator-min-microvolt = <1800000>;
                regulator-max-microvolt = <1800000>;
                regulator-name = "vcc_1v8";
                regulator-state-mem {
                    regulator-off-in-suspend;
                };
            };

            vcc_3v3: SWITCH_REG1 {
                regulator-always-on;
                regulator-boot-on;
                regulator-name = "vcc_3v3";
                regulator-state-mem {
                    regulator-off-in-suspend;
                };
            };

            vcc3v3_sd: SWITCH_REG2 {
                regulator-always-on;
                regulator-boot-on;
                regulator-name = "vcc3v3_sd";
                regulator-state-mem {
                    regulator-off-in-suspend;
                };
            };
        };

        rk809_codec: codec {
            #sound-dai-cells = <0>;
            compatible = "rockchip,rk809-codec", "rockchip,rk817-codec";
            clocks = <&cru I2S1_MCLKOUT>;
            clock-names = "mclk";
            assigned-clocks = <&cru I2S1_MCLKOUT>, <&cru I2S1_MCLK_TX_IOE>;
            assigned-clock-rates = <12288000>;
            assigned-clock-parents = <&cru I2S1_MCLKOUT_TX>, <&cru I2S1_MCLKOUT_TX>;
            pinctrl-names = "default";
            pinctrl-0 = <&i2s1m0_mclk>;
            hp-volume = <3>;    //3(max)-255(min)
            spk-volume = <30>;    //3(max)-255(min)
            capture_volume = <255>;
            //mic-in-differential;
            status = "okay";
        };
    };
};

&i2s0_8ch {
    status = "okay";
};

&i2s1_8ch {
    status = "okay";
    rockchip,clk-trcm = <1>;
    pinctrl-names = "default";
    pinctrl-0 = <&i2s1m0_sclktx
             &i2s1m0_lrcktx
             &i2s1m0_sdi0
             &i2s1m0_sdo0>;
};

&iep {
    status = "okay";
};

&iep_mmu {
    status = "okay";
};

&jpegd {
    status = "okay";
};

&jpegd_mmu {
    status = "okay";
};

&mpp_srv {
    status = "okay";
};

&nandc0 {
    #address-cells = <1>;
    #size-cells = <0>;
    status = "okay";

    nand@0 {
        reg = <0>;
        nand-bus-width = <8>;
        nand-ecc-mode = "hw";
        nand-ecc-strength = <16>;
        nand-ecc-step-size = <1024>;
    };
};

&pinctrl {
    pmic {
        pmic_int: pmic_int {
            rockchip,pins =
                <0 RK_PA3 RK_FUNC_GPIO &pcfg_pull_up>;
        };

        soc_slppin_gpio: soc_slppin_gpio {
            rockchip,pins =
                <0 RK_PA2 RK_FUNC_GPIO &pcfg_output_low_pull_down>;
        };

        soc_slppin_slp: soc_slppin_slp {
            rockchip,pins =
                <0 RK_PA2 1 &pcfg_pull_up>;
        };

        soc_slppin_rst: soc_slppin_rst {
            rockchip,pins =
                <0 RK_PA2 2 &pcfg_pull_none>;
        };
    };
/*
    sdio-pwrseq {
        wifi_enable_h: wifi-enable-h {
            rockchip,pins = <3 RK_PD5 RK_FUNC_GPIO &pcfg_pull_none>;
        };
    };

    usb {
        vcc5v0_host_en: vcc5v0-host-en {
            rockchip,pins = <0 RK_PA6 RK_FUNC_GPIO &pcfg_pull_none>;
        };

        vcc5v0_otg_en: vcc5v0-otg-en {
            rockchip,pins = <0 RK_PA5 RK_FUNC_GPIO &pcfg_pull_none>;
        };
    };

    wireless-bluetooth {
        uart8_gpios: uart8-gpios {
            rockchip,pins = <2 RK_PB1 RK_FUNC_GPIO &pcfg_pull_none>;
        };
    };
*/
};

 /*
  * There are 10 independent IO domains in RK3566/RK3568, including PMUIO[0:2] and VCCIO[1:7].
  * 1/ PMUIO0 and PMUIO1 are fixed-level power domains which cannot be configured;
  * 2/ PMUIO2 and VCCIO1,VCCIO[3:7] domains require that their hardware power supply voltages
  *    must be consistent with the software configuration correspondingly
  *    a/ When the hardware IO level is connected to 1.8V, the software voltage configuration
  *       should also be configured to 1.8V accordingly;
  *    b/ When the hardware IO level is connected to 3.3V, the software voltage configuration
  *       should also be configured to 3.3V accordingly;
  * 3/ VCCIO2 voltage control selection (0xFDC20140)
  *    BIT[0]: 0x0: from GPIO_0A7 (default)
  *    BIT[0]: 0x1: from GRF
  *    Default is determined by Pin FLASH_VOL_SEL/GPIO0_A7:
  *    L:VCCIO2 must supply 3.3V
  *    H:VCCIO2 must supply 1.8V
  */
&pmu_io_domains {
    status = "okay";
    pmuio2-supply = <&vcc3v3_pmu>;
    vccio1-supply = <&vccio_acodec>;
    vccio3-supply = <&vccio_sd>;
    vccio4-supply = <&vcc_3v3>;
    vccio5-supply = <&vcc_3v3>;
    vccio6-supply = <&vcc_3v3>;
    vccio7-supply = <&vcc_3v3>;
};


&rk_rga {
    status = "okay";
};

&rkvdec {
    status = "okay";
};

&rkvdec_mmu {
    status = "okay";
};

&rkvenc {
    venc-supply = <&vdd_logic>;
    status = "okay";
};

&rkvenc_mmu {
    status = "okay";
};

&rknpu {
    rknpu-supply = <&vdd_npu>;
    status = "okay";
};

&rknpu_mmu {
    status = "okay";
};

&route_hdmi {
    status = "okay";
    connect = <&vp0_out_hdmi>;
};

&saradc {
    status = "okay";
    vref-supply = <&vcca_1v8>;
};

&sdhci {
    bus-width = <8>;
    supports-emmc;
    non-removable;
    max-frequency = <200000000>;
    status = "okay";
};

&sdmmc0 {
    max-frequency = <150000000>;
    supports-sd;
    bus-width = <4>;
    cap-mmc-highspeed;
    cap-sd-highspeed;
    disable-wp;
    sd-uhs-sdr104;
    vmmc-supply = <&vcc3v3_sd>;
    vqmmc-supply = <&vccio_sd>;
    pinctrl-names = "default";
    pinctrl-0 = <&sdmmc0_bus4 &sdmmc0_clk &sdmmc0_cmd &sdmmc0_det>;
    status = "okay";
};
/*
&sdmmc2 {
    max-frequency = <150000000>;
    supports-sdio;
    bus-width = <4>;
    disable-wp;
    cap-sd-highspeed;
    cap-sdio-irq;
    keep-power-in-suspend;
    mmc-pwrseq = <&sdio_pwrseq>;
    non-removable;
    pinctrl-names = "default";
    pinctrl-0 = <&sdmmc2m0_bus4 &sdmmc2m0_cmd &sdmmc2m0_clk>;
    sd-uhs-sdr104;
    status = "okay";
};
*/
&sfc {
    status = "okay";
};

&spdif_8ch {
    status = "disabled";
};

&tsadc {
    status = "okay";
};

&u2phy0_host {
//    phy-supply = <&vcc5v0_host>;
    status = "okay";
};

&u2phy0_otg {
//    vbus-supply = <&vcc5v0_otg>;
    status = "okay";
};

&u2phy1_host {
//    phy-supply = <&vcc5v0_host>;
    status = "okay";
};

&u2phy1_otg {
//    phy-supply = <&vcc5v0_host>;
    status = "okay";
};

&usb2phy0 {
    status = "okay";
};

&usb2phy1 {
    status = "okay";
};

&usb_host0_ehci {
    status = "okay";
};

&usb_host0_ohci {
    status = "okay";
};

&usb_host1_ehci {
    status = "okay";
};

&usb_host1_ohci {
    status = "okay";
};

&usbdrd_dwc3 {
    dr_mode = "otg";
    extcon = <&usb2phy0>;
    status = "okay";
};

&usbdrd30 {
    status = "okay";
};

&usbhost_dwc3 {
    status = "okay";
};

&usbhost30 {
    status = "okay";
};

&vad {
    rockchip,audio-src = <&i2s1_8ch>;
    rockchip,buffer-time-ms = <128>;
    rockchip,det-channel = <0>;
    rockchip,mode = <0>;
};

&vdpu {
    status = "okay";
};

&vdpu_mmu {
    status = "okay";
};

&vepu {
    status = "okay";
};

&vepu_mmu {
    status = "okay";
};

&vop {
    status = "okay";
    assigned-clocks = <&cru DCLK_VOP0>, <&cru DCLK_VOP1>;
    assigned-clock-parents = <&pmucru PLL_HPLL>, <&cru PLL_VPLL>;
};

&vop_mmu {
    status = "okay";
};

&dsi0 {
dsi0_panel: panel@0 {
            status = "disabled";
        };
};

&dsi1 {
dsi1_panel: panel@0 {
            status = "disabled";
        };
};

// sata usb30 pcie phys
&combphy0_us {
    status = "okay";
};

&combphy1_usq {
    status = "okay";
};

&combphy2_psq {
    status = "okay";
};

    

//gpio0_b0 for hub reset pin
/delete-node/ &xin32k;
