// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Copyright (c) 2021 Rockchip Electronics Co., Ltd.
 *
 */

/dts-v1/;

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/pinctrl/rockchip.h>
#include <dt-bindings/input/rk-input.h>
#include <dt-bindings/sensor-dev.h>
#include <dt-bindings/display/drm_mipi_dsi.h>
#include "rk3566.dtsi"
#include "rk3568-android.dtsi"
#include "rk3566-eink.dtsi"

/ {
	model = "Rockchip RK3566 RK817 EINK W6 LP4X Board";
	compatible = "rockchip,rk3566-rk817-eink-W6", "rockchip,rk3566";

	charge-animation {
		compatible = "rockchip,uboot-charge";
		rockchip,uboot-charge-on = <1>;
		rockchip,android-charge-on = <0>;
		rockchip,uboot-low-power-voltage = <3350>;
		rockchip,screen-on-voltage = <3400>;
		rockchip,auto-wakeup-interval = <60>;
		status = "okay";
	};

	adc_keys: adc-keys {
		status = "disabled";
		compatible = "adc-keys";
		io-channels = <&saradc 0>;
		io-channel-names = "buttons";
		keyup-threshold-microvolt = <1800000>;
		poll-interval = <100>;

		vol-up-key {
			label = "volume up";
			linux,code = <KEY_VOLUMEUP>;
			press-threshold-microvolt = <1750>;
		};
	};

	hdmi_sound: hdmi-sound {
		compatible = "simple-audio-card";
		simple-audio-card,format = "i2s";
		simple-audio-card,mclk-fs = <128>;
		simple-audio-card,name = "rockchip,hdmi";
		status = "disabled";

		simple-audio-card,cpu {
			sound-dai = <&i2s0_8ch>;
		};
		simple-audio-card,codec {
			sound-dai = <&hdmi>;
		};
	};

	leds: gpio-leds {
		compatible = "gpio-leds";
		pinctrl-names = "default";
		pinctrl-0 =<&leds_gpio>;

		led@1 {
			gpios = <&gpio3 RK_PC4 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "battery-full";
			label = "battery_full";
			retain-state-suspended;
		};

		led@2 {
			gpios = <&gpio3 RK_PC5 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "battery-charging";
			label = "battery_charging";
			retain-state-suspended;
		};
	};

	vccsys: vccsys {
		compatible = "regulator-fixed";
		regulator-name = "vcc3v8_sys";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <3800000>;
		regulator-max-microvolt = <3800000>;
	};

	vcc_camera: vcc-camera-regulator {
		compatible = "regulator-fixed";
		gpio = <&gpio4 RK_PC3 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&camera_rst>;
		regulator-name = "vcc_camera";
		enable-active-high;
		regulator-always-on;
		regulator-boot-on;
	};

	vcc_tp: vcc-tp-regulator {
		compatible = "regulator-fixed";
		enable-active-high;
		gpio = <&gpio0 RK_PC0 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&vcc_tp_en>;
		regulator-name = "vcc_tp";
	};

	dummy_codec: dummy-codec {
		compatible = "rockchip,dummy-codec";
		#sound-dai-cells = <0>;
	};

	mic_sound: mic-sound {
		compatible = "simple-audio-card";
		simple-audio-card,name = "rockchip,rk-mic-sound";
		simple-audio-card,cpu {
			sound-dai = <&i2s1_8ch>;
		};
		simple-audio-card,codec {
			sound-dai = <&dummy_codec>;
		};
	};

	sdio_pwrseq: sdio-pwrseq {
		compatible = "mmc-pwrseq-simple";
		clocks = <&rk817 1>;
		clock-names = "ext_clock";
		pinctrl-names = "default";
		pinctrl-0 = <&wifi_enable_h>;

		/*
		 * On the module itself this is one of these (depending
		 * on the actual card populated):
		 * - SDIO_RESET_L_WL_REG_ON
		 * - PDN (power down when low)
		 */
		post-power-on-delay-ms = <200>;
		reset-gpios = <&gpio0 RK_PC6 GPIO_ACTIVE_LOW>;
	};

	wireless-wlan {
		compatible = "wlan-platdata";
		rockchip,grf = <&grf>;
		wifi_chip_type = "ap6255";
		pinctrl-names = "default";
		pinctrl-0 = <&wifi_vbat &wifi_host_wake_irq>;
		WIFI,vbat_gpio = <&gpio0 RK_PA0 GPIO_ACTIVE_HIGH>;
		WIFI,host_wake_irq = <&gpio0 RK_PC5 GPIO_ACTIVE_HIGH>;
		status = "okay";
	};

	wireless-bluetooth {
		compatible = "bluetooth-platdata";
		clocks = <&rk817 1>;
		clock-names = "ext_clock";
		wifi-bt-power-toggle;
		uart_rts_gpios = <&gpio2 RK_PB5 GPIO_ACTIVE_LOW>;
		pinctrl-names = "default", "rts_gpio";
		pinctrl-0 = <&uart1m0_rtsn>;
		pinctrl-1 = <&uart1_gpios>;
		BT,reset_gpio    = <&gpio0 RK_PC4 GPIO_ACTIVE_HIGH>;
		BT,wake_gpio     = <&gpio0 RK_PC2 GPIO_ACTIVE_HIGH>;
		BT,wake_host_irq = <&gpio0 RK_PC3 GPIO_ACTIVE_HIGH>;
		status = "okay";
	};
};

&ebc {
	/* clock rate 1000M/n, (n=1~32) */
	assigned-clocks = <&cru CPLL_333M>, <&cru DCLK_EBC>;
	assigned-clock-rates = <85000000>, <85000000>;
	status = "okay";
};

&ebc_dev {
	pmic = <&tps65185>;
	status = "okay";

	/* ED060XCD */
	panel,width = <1024>;
	panel,height = <758>;
	panel,vir_width = <1024>;
	panel,vir_height = <758>;
	panel,sdck = <20000000>;
	panel,lsl = <6>;
	panel,lbl = <6>;
	panel,ldl = <256>;
	panel,lel = <38>;
	panel,gdck-sta = <4>;
	panel,lgonl = <262>;
	panel,fsl = <2>;
	panel,fbl = <4>;
	panel,fdl = <758>;
	panel,fel = <5>;
	panel,mirror = <0>;
	panel,panel_16bit = <0>;
	panel,panel_color = <0>;
	panel,width-mm = <90>;
	panel,height-mm = <122>;
};

&cpu0 {
	cpu-supply = <&vdd_cpu>;
};

&csi2_dphy_hw {
	status = "okay";
};

&csi2_dphy0 {
	status = "okay";

	ports {
		#address-cells = <1>;
		#size-cells = <0>;
		port@0 {
			reg = <0>;
			#address-cells = <1>;
			#size-cells = <0>;

			mipi_in_ucam0: endpoint@0 {
				reg = <0>;
				remote-endpoint = <&ov5648_out>;
				data-lanes = <1 2>;
			};
		};
		port@1 {
			reg = <1>;
			#address-cells = <1>;
			#size-cells = <0>;

			csidphy0_out: endpoint@0 {
				reg = <0>;
				remote-endpoint = <&isp0_in>;
			};
		};
	};
};

&gpu {
	mali-supply = <&vdd_gpu>;
	status = "okay";
};

&hdmi {
	status = "disabled";
};

&hdmi_in_vp0 {
	status = "disabled";
};

&hdmi_in_vp1 {
	status = "disabled";
};

&hdmi_sound {
	status = "disabled";
};

&i2c0 {
	status = "okay";

	vdd_cpu: tcs4525@1c {
		compatible = "tcs,tcs4525";
		reg = <0x1c>;
		vin-supply = <&vccsys>;
		regulator-compatible = "fan53555-reg";
		regulator-name = "vdd_cpu";
		regulator-min-microvolt = <712500>;
		regulator-max-microvolt = <1390000>;
		regulator-init-microvolt = <900000>;
		regulator-ramp-delay = <2300>;
		fcs,suspend-voltage-selector = <0>;
		regulator-boot-on;
		regulator-always-on;
		regulator-initial-mode = <0x2>;
		regulator-state-mem {
			regulator-on-in-suspend;
			regulator-suspend-microvolt = <1100000>;
			regulator-changeable-in-suspend;
		};
	};

	rk817: pmic@20 {
		compatible = "rockchip,rk817";
		reg = <0x20>;
		interrupt-parent = <&gpio0>;
		interrupts = <3 IRQ_TYPE_LEVEL_LOW>;
		pinctrl-names = "default";
//		pinctrl-names = "default", "pmic-sleep",
//				"pmic-power-off", "pmic-reset";
		pinctrl-0 = <&pmic_int>;
//		pinctrl-1 = <&soc_slppin_slp>, <&rk817_slppin_slp>;
//		pinctrl-2 = <&soc_slppin_gpio>, <&rk817_slppin_pwrdn>;
//		pinctrl-3 = <&soc_slppin_gpio>, <&rk817_slppin_rst>;
		rockchip,system-power-controller;
		wakeup-source;
		#clock-cells = <1>;
		clock-output-names = "rk808-clkout1", "rk808-clkout2";
		//fb-inner-reg-idxs = <2>;
		/* 1: rst regs (default in codes), 0: rst the pmic */
		pmic-reset-func = <0>;
		/* not save the PMIC_POWER_EN register in uboot */
		not-save-power-en = <1>;
		vcc1-supply = <&vccsys>;
		vcc2-supply = <&vccsys>;
		vcc3-supply = <&vccsys>;
		vcc4-supply = <&vccsys>;
		vcc5-supply = <&vccsys>;
		vcc6-supply = <&vccsys>;
		vcc7-supply = <&vccsys>;
		vcc8-supply = <&vccsys>;
		vcc9-supply = <&dcdc_boost>;

		pwrkey {
			status = "okay";
		};

		pinctrl_rk8xx: pinctrl_rk8xx {
			gpio-controller;
			#gpio-cells = <2>;

			rk817_slppin_null: rk817_slppin_null {
				pins = "gpio_slp";
				function = "pin_fun0";
			};

			rk817_slppin_slp: rk817_slppin_slp {
				pins = "gpio_slp";
				function = "pin_fun1";
			};

			rk817_slppin_pwrdn: rk817_slppin_pwrdn {
				pins = "gpio_slp";
				function = "pin_fun2";
			};

			rk817_slppin_rst: rk817_slppin_rst {
				pins = "gpio_slp";
				function = "pin_fun3";
			};
		};

		regulators {
			vdd_logic: DCDC_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <500000>;
				regulator-max-microvolt = <1350000>;
				regulator-init-microvolt = <900000>;
				regulator-ramp-delay = <6001>;
				regulator-initial-mode = <0x2>;
				regulator-name = "vdd_logic";
				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <900000>;
					regulator-changeable-in-suspend;
				};
			};

			vdd_gpu: DCDC_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <500000>;
				regulator-max-microvolt = <1350000>;
				regulator-init-microvolt = <900000>;
				regulator-ramp-delay = <6001>;
				regulator-initial-mode = <0x2>;
				regulator-name = "vdd_gpu";
					regulator-state-mem {
					regulator-off-in-suspend;
					regulator-changeable-in-suspend;
				};
			};

			vcc_ddr: DCDC_REG3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-initial-mode = <0x2>;
				regulator-name = "vcc_ddr";
				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};

			vcc_3v3: DCDC_REG4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-initial-mode = <0x2>;
				regulator-name = "vcc_3v3";
				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-changeable-in-suspend;
				};
			};

			vcca1v8_pmu: LDO_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcca1v8_pmu";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
					regulator-changeable-in-suspend;
				};
			};

			vdda_0v9: LDO_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <900000>;
				regulator-max-microvolt = <900000>;
				regulator-name = "vdda_0v9";
				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-changeable-in-suspend;
				};
			};

			vdda0v9_pmu: LDO_REG3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <900000>;
				regulator-max-microvolt = <900000>;
				regulator-name = "vdda0v9_pmu";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <900000>;
					regulator-changeable-in-suspend;
				};
			};

			vccio_acodec: LDO_REG4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vccio_acodec";
				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-changeable-in-suspend;
				};
			};

			vccio_sd: LDO_REG5 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vccio_sd";
				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-changeable-in-suspend;
				};
			};

			vcc3v3_pmu: LDO_REG6 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vcc3v3_pmu";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3000000>;
					regulator-changeable-in-suspend;
				};
			};

			vcc_1v8: LDO_REG7 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc_1v8";
				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-changeable-in-suspend;
				};
			};

			vcc1v8_dvp: LDO_REG8 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc1v8_dvp";
				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-changeable-in-suspend;
				};
			};

			sleep_sta_ctl: LDO_REG9 {
				regulator-name = "sleep_sta_ctl";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
					regulator-changeable-in-suspend;
				};
			};

			dcdc_boost: BOOST {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <4700000>;
				regulator-max-microvolt = <5400000>;
				regulator-name = "boost";
				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-changeable-in-suspend;
				};
			};

			otg_switch: OTG_SWITCH {
				regulator-name = "otg_switch";
				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-changeable-in-suspend;
				};
			};
		};

		battery {
			compatible = "rk817,battery";
			ocv_table = <3400 3513 3578 3687 3734 3752 3763
				     3766 3771 3784 3804 3836 3885 3925
				     3962 4005 4063 4114 4169 4227 4303>;
			design_capacity = <2250>;
			design_qmax = <2750>;
			bat_res = <100>;
			sleep_enter_current = <150>;
			sleep_exit_current = <180>;
			sleep_filter_current = <100>;
			power_off_thresd = <3450>;
			zero_algorithm_vol = <3850>;
			max_soc_offset = <60>;
			monitor_sec = <5>;
			sample_res = <10>;
			virtual_power = <0>;
			low_power_sleep = <1>;
		};

		charger {
			compatible = "rk817,charger";
			min_input_voltage = <4500>;
			max_input_current = <1500>;
			max_chrg_current = <2000>;
			max_chrg_voltage = <4300>;
			chrg_term_mode = <0>;
			chrg_finish_cur = <300>;
			virtual_power = <0>;
			dc_det_adc = <0>;
			extcon = <&usb2phy0>;
			gate_function_disable = <1>;
		};
	};
};

&i2c1 {
	status = "okay";

	ov5648: ov5648@36 {
		status = "okay";
		compatible = "ovti,ov5648";
		reg = <0x36>;
		clocks = <&cru CLK_CAM0_OUT>;
		clock-names = "xvclk";
		/* avdd-supply = <&vcc2v8_dvp>; */
		dovdd-supply = <&vcc1v8_dvp>;
		/* dvdd-supply = <&vcc1v8_dvp>; */

		power-domains = <&power RK3568_PD_VI>;
		pinctrl-names = "default";
		pinctrl-0 = <&cam_clkout0>;
		//reset pin control by hardware,used this pin switch to mipi input
		//1->2LANE(LANE 0&1) FRONT camera, 0->4LANE REAR camera
		//reset-gpios = <&gpio4 RK_PC3 GPIO_ACTIVE_LOW>;
		pwdn-gpios = <&gpio4 RK_PC2 GPIO_ACTIVE_HIGH>;
		rockchip,camera-module-index = <0>;
		rockchip,camera-module-facing = "back";
		rockchip,camera-module-name = "HS5885-BNSM1018-V01";
		rockchip,camera-module-lens-name = "default";
		port {
			ov5648_out: endpoint {
				remote-endpoint = <&mipi_in_ucam0>;
				data-lanes = <1 2>;
			};
		};
	};
};

&i2c3 {
	status = "okay";
	pinctrl-names = "default";
	pinctrl-0 = <&i2c3m1_xfer>;

	tps65185: tps65185@68 {
		compatible = "ti,tps65185";
		reg = <0x68>;
		pinctrl-names = "default";
		pinctrl-0 = <&tps65185_gpio>;
		int-gpios = <&gpio3 RK_PA6 GPIO_ACTIVE_HIGH>;
		wakeup-gpios = <&gpio3 RK_PA5 GPIO_ACTIVE_HIGH>;
		vcomctl-gpios = <&gpio4 RK_PB2 GPIO_ACTIVE_HIGH>;
		powerup-gpios = <&gpio3 RK_PB0 GPIO_ACTIVE_HIGH>;
		poweren-gpios = <&gpio0 RK_PC1 GPIO_ACTIVE_HIGH>;
	};

};

&i2c5 {
	status = "okay";

	sensor@4c {
		status = "okay";
		compatible = "gs_mma7660";
		reg = <0x4c>;
		type = <SENSOR_TYPE_ACCEL>;
		irq_enable = <0>;
		poll_delay_ms = <30>;
		layout = <6>;
		reprobe_en = <1>;
	};

	gt9xx: gt9xx@14 {
		compatible = "goodix,gt9xx";
		reg = <0x14>;
		pinctrl-names = "default";
		pinctrl-0 = <&tp_gpio>;
		touch-gpio = <&gpio0 RK_PA6 GPIO_ACTIVE_HIGH>;
		reset-gpio = <&gpio0 RK_PA5 GPIO_ACTIVE_HIGH>;
		touchscreen-size-x = <1024>;
		touchscreen-size-y = <758>;
		max-x = <1024>;
		max-y = <758>;
		tp-size = <9111>;
		tp-supply = <&vcc_tp>;
		wakeup-source;
		touchscreen-key-map = <158>; //KEY_HOMEPAGE=172,KEY_BACK=158,KEY_MENU=139
		goodix,driver-send-cfg = <0>;
		goodix,cfg-group0 =[
			42 00 03 00 04 0A 45 03 22 1F 28 0F 64 3C 03 0F 00 00 00 00 11 00
			08 00 00 00 00 8B 29 0E 71 6F B2 04 00 00 00 39 02 10 00 21 00 00
			00 03 64 32 00 00 00 3C 78 94 D5 02 07 00 00 04 C8 40 00 B1 4A 00
			9E 55 00 8E 61 00 7F 70 00 7F 70 00 00 00 F0 90 3C FF FF 07 00 00
			00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
			00 00 1C 1A 18 16 14 12 10 0E 0C 0A 08 06 04 02 FF FF FF FF FF FF
			FF FF FF FF FF FF FF FF FF FF 00 02 04 06 08 0A 0C 0F 10 12 13 16
			18 1C 1D 1E 1F 20 21 22 FF FF FF FF FF FF FF FF FF FF FF FF FF FF
			FF FF FF FF FF FF FF FF F6 01
		];
	};

	ft5436: focaltech@38 {
		status = "okay";
		compatible = "focaltech,ft5436";
		reg = <0x38>;
		pinctrl-names = "default";
		pinctrl-0 = <&tp_gpio>;
		vdd-supply = <&vcc_tp>;
		focaltech,reset-gpio = <&gpio0 RK_PA5 GPIO_ACTIVE_HIGH>;
		focaltech,irq-gpio = <&gpio0 RK_PA6 IRQ_TYPE_EDGE_FALLING>;
		focaltech,max-touch-number = <5>;
		focaltech,display-coords =  <0 0 1024 758>;
		focaltech,have-key = <1>;
		focaltech,key-number = <1>;

		focaltech,key-x-coords = <300>;
		focaltech,key-y-coords = <1200>;
		wakeup-source;
	};
};

&i2s0_8ch {
	status = "disabled";
};

&i2s1_8ch {
	status = "okay";
	rockchip,clk-trcm = <1>;
	pinctrl-names = "default";
	pinctrl-0 = <&i2s1m0_sclktx
		     &i2s1m0_lrcktx
		     &i2s1m0_sdi0
		     &i2s1m0_sdo0>;
};

&jpegd {
	status = "okay";
};

&jpegd_mmu {
	status = "okay";
};

&video_phy0 {
	status = "disabled";
};

&mpp_srv {
	status = "okay";
};

&nandc0 {
	status = "disabled";
};

&pinctrl {
	cam {
		cam_clkout0: cam-clkout0 {
			rockchip,pins =
				/* cam_clkout0 */
				<4 RK_PA7 1 &pcfg_pull_none>;
		};

		camera_rst: camera-rst {
			rockchip,pins =
				<4 RK_PC3 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	leds {
		leds_gpio: leds-gpio {
			rockchip,pins =
				<3 RK_PC4 RK_FUNC_GPIO &pcfg_pull_none>,
				<3 RK_PC5 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	tps_pmic {
		tps65185_gpio: tps65185-gpio {
			rockchip,pins =
				<4 RK_PB2 RK_FUNC_GPIO &pcfg_pull_up>,
				<3 RK_PA5 RK_FUNC_GPIO &pcfg_pull_up>,
				<3 RK_PA6 RK_FUNC_GPIO &pcfg_pull_up>,
				<3 RK_PB0 RK_FUNC_GPIO &pcfg_pull_up>,
				<0 RK_PC1 RK_FUNC_GPIO &pcfg_output_high>;
		};
	};

	tp {
		tp_gpio: tp-gpio {
			rockchip,pins =
				<0 RK_PA5 RK_FUNC_GPIO &pcfg_pull_up>,
				<0 RK_PA6 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	pmic {
		pmic_int: pmic_int {
			rockchip,pins =
				<0 RK_PA3 RK_FUNC_GPIO &pcfg_pull_up>;
		};

		soc_slppin_gpio: soc_slppin_gpio {
			rockchip,pins =
				<0 RK_PA2 RK_FUNC_GPIO &pcfg_output_low>;
		};

		soc_slppin_slp: soc_slppin_slp {
			rockchip,pins =
				<0 RK_PA2 1 &pcfg_pull_none>;
		};

		soc_slppin_rst: soc_slppin_rst {
			rockchip,pins =
				<0 RK_PA2 2 &pcfg_pull_none>;
		};
	};

	sdio-pwrseq {
		wifi_enable_h: wifi-enable-h {
			rockchip,pins = <0 RK_PC6 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	vcc-tp {
		vcc_tp_en: vcc-tp-en {
			rockchip,pins = <0 RK_PC0 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	wireless-wlan {
		wifi_vbat: wifi-vbat {
			rockchip,pins = <0 RK_PA0 RK_FUNC_GPIO &pcfg_pull_none>;
		};

		wifi_host_wake_irq: wifi-host-wake-irq {
			rockchip,pins = <0 RK_PC5 RK_FUNC_GPIO &pcfg_pull_down>;
		};
	};

	wireless-bluetooth {
		uart1_gpios: uart1-gpios {
			rockchip,pins = <2 RK_PB5 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};
};

&pmu_io_domains {
	status = "okay";
	pmuio1-supply = <&vcc3v3_pmu>;
	pmuio2-supply = <&vcca1v8_pmu>;
	vccio1-supply = <&vccio_acodec>;
	vccio3-supply = <&vcc_3v3>;
	vccio4-supply = <&vcca1v8_pmu>;
	vccio5-supply = <&vcc_3v3>;
	vccio6-supply = <&vcc_3v3>;
	vccio7-supply = <&vcc1v8_dvp>;
};

&pwm4 {
	status = "disabled";
};

&rk_rga {
	status = "okay";
};

&rkisp {
	status = "okay";
};

&rkisp_mmu {
	status = "okay";
};

&rkisp_vir0 {
	status = "okay";

	port {
		#address-cells = <1>;
		#size-cells = <0>;

		isp0_in: endpoint@0 {
			reg = <0>;
			remote-endpoint = <&csidphy0_out>;
		};
	};
};

&rkvdec {
	status = "okay";
};

&rkvdec_mmu {
	status = "okay";
};

&rkvenc {
	status = "okay";
};

&rkvenc_mmu {
	status = "okay";
};

&rockchip_suspend {
	status = "okay";

	rockchip,regulator-off-in-mem-lite =
		<&vdd_cpu>, <&vdd_logic>, <&vdd_gpu>, <&vcc_3v3>, <&vdda_0v9>, <&vcc_1v8>,
		<&vccio_acodec>, <&vccio_sd>, <&vcc1v8_dvp>, <&dcdc_boost>, <&otg_switch>,
		<&sleep_sta_ctl>;
	rockchip,regulator-on-in-mem-lite =
		<&vcc_ddr>, <&vdda0v9_pmu>, <&vcca1v8_pmu>, <&vcc3v3_pmu>;

	rockchip,regulator-off-in-mem =
		<&vdd_cpu>, <&vdd_logic>, <&vdd_gpu>, <&vcc_3v3>, <&vdda_0v9>, <&vcc_1v8>,
		<&vccio_acodec>, <&vccio_sd>, <&vcc1v8_dvp>, <&dcdc_boost>, <&otg_switch>,
		<&sleep_sta_ctl>;
	rockchip,regulator-on-in-mem =
		<&vcc_ddr>, <&vdda0v9_pmu>, <&vcca1v8_pmu>, <&vcc3v3_pmu>;

	rockchip,regulator-off-in-mem-ultra =
		<&vdd_logic>, <&vdd_gpu>, <&vcc_ddr>, <&vcc_3v3>, <&vdda_0v9>, <&vcc_1v8>,
		<&vdda0v9_pmu>, <&vcca1v8_pmu>, <&vcc3v3_pmu>, <&vccio_acodec>, <&vccio_sd>,
		<&vcc1v8_dvp>, <&dcdc_boost>, <&otg_switch>;
	rockchip,regulator-on-in-mem-ultra = <&vdd_cpu>, <&sleep_sta_ctl>;
};

&saradc {
	status = "disabled";
	vref-supply = <&vcc_1v8>;
};

&sdhci {
	bus-width = <8>;
	no-sdio;
	no-sd;
	non-removable;
	keep-power-in-suspend;
	max-frequency = <200000000>;
	status = "okay";
};

&sdmmc1 {
	max-frequency = <150000000>;
	no-sd;
	no-mmc;
	bus-width = <4>;
	disable-wp;
	cap-sd-highspeed;
	cap-sdio-irq;
	keep-power-in-suspend;
	mmc-pwrseq = <&sdio_pwrseq>;
	non-removable;
	pinctrl-names = "default";
	pinctrl-0 = <&sdmmc1_bus4 &sdmmc1_cmd &sdmmc1_clk>;
	sd-uhs-sdr104;
	rockchip,default-sample-phase = <90>;
	status = "okay";
};

&tsadc {
	status = "okay";
};

&uart1 {
	status = "okay";
	pinctrl-names = "default";
	pinctrl-0 = <&uart1m0_xfer &uart1m0_ctsn>;
};

&u2phy0_otg {
	status = "okay";
};

&usb2phy0 {
	status = "okay";
};

&usbdrd_dwc3 {
	status = "okay";
};

&usbdrd30 {
	status = "okay";
};

&vdpu {
	status = "okay";
};

&vdpu_mmu {
	status = "okay";
};

&vepu {
	status = "okay";
};

&vepu_mmu {
	status = "okay";
};

&vop {
	status = "okay";
};

&vop_mmu {
	status = "okay";
};
