// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Copyright (c) 2022 Rockchip Electronics Co., Ltd.
 */

#include <dt-bindings/display/media-bus-format.h>

/ {
	aliases {
		pinctrl0 = &pinctrl;
	};

	backlight {
		compatible = "simple-bus";
		#address-cells = <1>;
		#size-cells = <0>;

		i2c2_max96755f_backlight: backlight@0 {
			compatible = "pwm-backlight";
			reg = <0>;
			pwms = <&pwm0 0 1000000 0>;
			brightness-levels = <0 4 8 16 32 64 128 255>;
			default-brightness-level = <6>;
		};

		i2c4_max96745_backlight: backlight@1 {
			compatible = "pwm-backlight";
			reg = <1>;
			pwms = <&pwm10 0 1000000 0>;
			brightness-levels = <0 4 8 16 32 64 128 255>;
			default-brightness-level = <6>;
		};

		i2c5_max96745_backlight: backlight@2 {
			compatible = "pwm-backlight";
			reg = <2>;
			pwms = <&pwm7 0 1000000 0>;
			brightness-levels = <0 4 8 16 32 64 128 255>;
			default-brightness-level = <6>;
		};

		i2c6_max96755f_backlight: backlight@3 {
			compatible = "pwm-backlight";
			reg = <3>;
			pwms = <&pwm13 0 1000000 0>;
			brightness-levels = <0 4 8 16 32 64 128 255>;
			default-brightness-level = <6>;
		};

		i2c7_max96745_backlight: backlight@4 {
			compatible = "pwm-backlight";
			reg = <4>;
			pwms = <&pwm11 0 1000000 0>;
			brightness-levels = <0 4 8 16 32 64 128 255>;
			default-brightness-level = <6>;
		};

		i2c8_max96745_backlight: backlight@5 {
			compatible = "pwm-backlight";
			reg = <5>;
			pwms = <&pwm14 0 1000000 0>;
			brightness-levels = <0 4 8 16 32 64 128 255>;
			default-brightness-level = <6>;
		};
	};
};

&dp0 {
	//split-mode;
	force-hpd;
	status = "okay";
};

&dp0_in_vp0 {
	status = "okay";
};

&dp0_out {
	link-frequencies = /bits/ 64 <2700000000>;
	remote-endpoint = <&i2c4_max96745_in>;
};

&usbdp_phy0 {
	rockchip,dp-lane-mux = <0 1 2 3>;
	status = "okay";
};

&usbdp_phy0_dp {
	status = "okay";
};

&route_dp0 {
	connect = <&vp0_out_dp0>;
	status = "okay";
};

&dp1 {
	force-hpd;
	status = "disabled";
};

&dp1_out {
	link-frequencies = /bits/ 64 <2700000000>;
	remote-endpoint = <&i2c8_max96745_in>;
};

&usbdp_phy1 {
	rockchip,dp-lane-mux = <0 1 2 3>;
	status = "okay";
};

&usbdp_phy1_dp {
	status = "okay";
};

&dsi0 {
	status = "okay";

	ports {
		#address-cells = <1>;
		#size-cells = <0>;

		port@1 {
			reg = <1>;

			dsi0_out: endpoint {
				remote-endpoint = <&i2c2_max96755f_in>;
			};
		};
	};
};

&mipi_dcphy0 {
	status = "okay";
};

&dsi0_in_vp2 {
	status = "okay";
};

&route_dsi0 {
	connect = <&vp2_out_dsi0>;
	status = "disabled";
};

&dsi1 {
	status = "disabled";

	ports {
		#address-cells = <1>;
		#size-cells = <0>;

		port@1 {
			reg = <1>;

			dsi1_out: endpoint {
				remote-endpoint = <&i2c6_max96755f_in>;
			};
		};
	};
};

&mipi_dcphy1 {
	status = "okay";
};

&dsi1_in_vp3 {
	status = "okay";
};

&route_dsi1 {
	connect = <&vp3_out_dsi1>;
	status = "disabled";
};

&edp0 {
	//split-mode;
	force-hpd;
	status = "okay";
};

&edp0_out {
	link-frequencies = /bits/ 64 <2700000000>;
	remote-endpoint = <&i2c5_max96745_in>;
};

&hdptxphy0 {
	status = "okay";
};

&edp0_in_vp1 {
	status = "okay";
};

&route_edp0 {
	connect = <&vp1_out_edp0>;
	status = "okay";
};

&edp1 {
	force-hpd;
	status = "disabled";
};

&edp1_out {
	link-frequencies = /bits/ 64 <2700000000>;
	remote-endpoint = <&i2c7_max96745_in>;
};

&hdptxphy1 {
	status = "okay";
};

&hdmi0 {
	status = "disabled";
};

&hdmi1 {
	status = "disabled";
};

&hdptxphy_hdmi0 {
	status = "disabled";
};

&hdptxphy_hdmi1 {
	status = "disabled";
};

&i2c2 {
	pinctrl-0 = <&i2c2m4_xfer>;
	clock-frequency = <400000>;
	status = "okay";

	max96755@40 {
		compatible = "maxim,max96755";
		reg = <0x40>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2c2_serdes_pins>;
		lock-gpios = <&gpio1 RK_PA4 GPIO_ACTIVE_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		sel-mipi;
		status = "okay";

		serdes-init-sequence = [
			0001 0008
			0002 0053
			0003 0040
			0010 0031
			0013 00ca
			0010 0000
			02be 001c
			02bf 0040
			02c0 0020
			0311 0057
			0331 0033
			0332 004e
			03a4 0000
			0385 0000
			0386 0000
			0387 0000
			005b 0012
			0053 0010
		];

		i2c2_max96755f_pinctrl: i2c2-max96755f-pinctrl {
			compatible = "maxim,max96755-pinctrl";
			status = "okay";

			i2c2_max96755f_pinctrl_hog: hog {
				i2c {
					groups = "MAX96755_I2C";
					function = "MAX96755_I2C";
				};
			};

			i2c2_max96755f_panel_pins: panel-pins {
				bl-pwm {
					pins = "MAX96755_MFP0";
					function = "DES_GPIO0_OUTPUT";
				};
			};

			i2c2_max96755f_gpio: i2c2-max96755f-gpio {
				compatible = "maxim,max96755-gpio";
				status = "okay";

				gpio-controller;
				#gpio-cells = <2>;
				gpio-ranges = <&i2c2_max96755f_pinctrl 0 160 24>;
			};
		};

		i2c2_max96755f_bridge: i2c2-max96755f-bridge  {
			compatible = "maxim,max96755-bridge";
			pinctrl-names = "default";
			pinctrl-0 = <&i2c2_max96755f_pinctrl_hog>;
			status = "okay";
		};

		ports {
				#address-cells = <1>;
				#size-cells = <0>;

				port@0 {
					reg = <0>;

					i2c2_max96755f_in: endpoint {
						remote-endpoint = <&dsi0_out>;
					};
				};

				port@1 {
					reg = <1>;

					i2c2_max96755f_out: endpoint {
						remote-endpoint = <&i2c2_max96755f_panel_in>;
					};
				};
			};
	};


	max96772@48 {
		compatible = "maxim,max96772";
		reg = <0x48>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "okay";

		serdes-init-sequence = [
			0001 0002
			0010 0011
			0050 0000
			07f0 0001
			e791 0000
			e793 0000
			e794 0000
			e795 000a
			e796 007a
			e797 0000
			e798 003c
			e799 0000
			e79a 003c
			e79b 0000
			e79c 00a0
			e79d 0005
			e79e 0054
			e79f 0001
			e7a0 0002
			e7a1 0000
			e7a2 0014
			e7a3 0000
			e7a4 00fc
			e7a5 000e
			e7a6 0055
			e7a7 0055
			e7a8 0000
			e7a9 0080
			e7aa 0040
			e7ab 0000
			e7ac 0003
			e7ad 0000
			e7b0 0000
			e7b1 0000
			e7b2 0050
			e7b3 0000
			e7b4 0000
			e7b5 0040
			e7b6 006c
			e7b7 0020
			e7b8 0007
			e7b9 0000
			e7ba 0001
			e7bb 0000
			e7bc 0000
			e7bd 0000
			e7be 0052
			e7bf 0000
		];

		i2c2_max96772_pinctrl: i2c2-max96772-pinctrl {
			compatible = "maxim,max96772-pinctrl";
			status = "okay";

			i2c2_max96772_gpio: i2c2-max96772-gpio {
				compatible = "maxim,max96772-gpio";
				status = "okay";

				gpio-controller;
				#gpio-cells = <2>;
				gpio-ranges = <&i2c2_max96772_pinctrl 0 185 24>;
			};
		};

		i2c2_max96772_panel: i2c2-max96772-panel {
			compatible = "maxim,max96772-panel";
			backlight = <&i2c2_max96755f_backlight>;

			panel-timing {
				clock-frequency = <180000000>;
				hactive = <2560>;
				vactive = <1440>;
				hfront-porch = <122>;
				hsync-len = <60>;
				hback-porch = <60>;
				vfront-porch = <340>;
				vsync-len = <2>;
				vback-porch = <20>;
				hsync-active = <0>;
				vsync-active = <0>;
				de-active = <0>;
				pixelclk-active = <0>;
			};

			port {
				i2c2_max96755f_panel_in: endpoint {
					remote-endpoint = <&i2c2_max96755f_out>;
				};
			};

		};

	};

	ts@30 {
		compatible = "gac,gac_ts";
		reg = <0x30>;
		gac,max_x = <2560>;
		gac,max_y = <1440>;
	};
};

&i2c4 {
	pinctrl-0 = <&i2c4m2_xfer>;
	clock-frequency = <400000>;
	status = "okay";

	max96745@42 {
		compatible = "maxim,max96745";
		reg = <0x42>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2c4_serdes_pins>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";

		serdes-init-sequence = [
			0070 0016
			0005 00c0
			0107 0042
			0027 0022
			0026 0022
			002a 0007
			641a 00f0
		];


		i2c4_max96745_pinctrl: i2c4-max96745-pinctrl {
			compatible = "maxim,max96745-pinctrl";
			status = "okay";

			i2c4_max96745_gpio: i2c4-max96745-gpio {
				compatible = "maxim,max96745-gpio";
				status = "okay";

				gpio-controller;
				#gpio-cells = <2>;
				gpio-ranges = <&i2c4_max96745_pinctrl 0 210 25>;
			};
		};

		i2c4_max96745_bridge: i2c4-max96745-bridge {
			compatible = "maxim,max96745-bridge";
			lock-gpios = <&gpio3 RK_PD4 GPIO_ACTIVE_HIGH>;
			status = "okay";
		};

		ports {
				#address-cells = <1>;
				#size-cells = <0>;

				port@0 {
					reg = <0>;

					i2c4_max96745_in: endpoint {
						remote-endpoint = <&dp0_out>;
					};
				};

				port@1 {
					reg = <1>;

					i2c4_max96745_out: endpoint {
						remote-endpoint = <&i2c4_max96745_panel_in>;
					};
				};
			};

	};


	max96752@48 {
		compatible = "maxim,max96752";
		reg = <0x48>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";

		serdes-init-sequence = [
			0001 0002
			0002 0043
			0140 0020
			01ce 005e
			0200 0084
			020e 0040
			020c 0084
			0207 00a1
			0206 0083
			0215 0090
			0227 0090
			020f 0090
			0221 0090
			0212 0090
			0209 0090
		];

		i2c4_max96752_pinctrl: i2c4-max96752-pinctrl {
			compatible = "maxim,max96752-pinctrl";
			status = "okay";

			i2c4_max96752_gpio: i2c4-max96752-gpio {
				compatible = "maxim,max96752-gpio";
				status = "okay";

				gpio-controller;
				#gpio-cells = <2>;
				gpio-ranges = <&i2c4_max96752_pinctrl 0 236 25>;
			};
		};

		i2c4_max96752_panel: i2c4-max96752-panel {
			compatible = "maxim,max96752-panel";
			reg = <0x48>;
			backlight = <&i2c4_max96745_backlight>;

			panel-timing {
				clock-frequency = <148500000>;
				hactive = <1920>;
				vactive = <1080>;
				hfront-porch = <20>;
				hsync-len = <20>;
				hback-porch = <20>;
				vfront-porch = <250>;
				vsync-len = <2>;
				vback-porch = <8>;
				hsync-active = <0>;
				vsync-active = <0>;
				de-active = <0>;
				pixelclk-active = <0>;
			};

			port {
				i2c4_max96745_panel_in: endpoint {
					remote-endpoint = <&i2c4_max96745_out>;
				};
			};
		};

	};
};

&i2c5 {
	clock-frequency = <400000>;
	status = "okay";

	max96745@42 {
		compatible = "maxim,max96745";
		reg = <0x42>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2c5_serdes_pins>;
		lock-gpios = <&gpio0 RK_PD2 GPIO_ACTIVE_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "okay";

		serdes-init-sequence = [
			0070 0016
			0005 00c0
			0107 0042
			0027 0022
			0026 0022
			002a 0007
			641a 00f0
		];


		i2c5_max96745_pinctrl: i2c5-max96745-pinctrl {
			compatible = "maxim,max96745-pinctrl";
			pinctrl-names = "default";
			pinctrl-0 = <&i2c5_max96745_pinctrl_hog>, <&i2c5_max96745_panel_pins>;
			status = "okay";

			i2c5_max96745_pinctrl_hog: hog {
				i2c {
					groups = "MAX96745_I2C";
					function = "MAX96745_I2C";
				};
			};

			i2c5_max96745_panel_pins: panel-pins {
				bl-pwm {
					pins = "MAX96745_MFP0";
					function = "DES_GPIO0_OUTPUT_A";
				};
			};

			i2c5_max96745_gpio: i2c5-max96745-gpio {
				compatible = "maxim,max96745-gpio";
				status = "okay";

				gpio-controller;
				#gpio-cells = <2>;
				gpio-ranges = <&i2c5_max96745_pinctrl 0 262 25>;
			};
		};

		i2c5_max96745_bridge: i2c5-max96745-bridge {
			compatible = "maxim,max96745-bridge";
			status = "okay";
		};

		ports {
				#address-cells = <1>;
				#size-cells = <0>;

				port@0 {
					reg = <0>;

					i2c5_max96745_in: endpoint {
						remote-endpoint = <&edp0_out>;
					};
				};

				port@1 {
					reg = <1>;

					i2c5_max96745_out: endpoint {
						remote-endpoint = <&i2c5_max96745_panel_in>;
					};
				};
			};

	};


	max96752@48 {
		compatible = "maxim,max96752";
		reg = <0x48>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "okay";

		serdes-init-sequence = [
			0001 0002
			0002 0043
			0140 0020
			01ce 005e
			0200 0084
			020e 0040
			020c 0084
			0207 00a1
			0206 0083
			0215 0090
			0227 0090
			020f 0090
			0221 0090
			0212 0090
			0209 0090
		];

		i2c5_max96752_pinctrl: i2c5-max96752-pinctrl {
			compatible = "maxim,max96752-pinctrl";
			status = "okay";

			i2c5_max96752_gpio: i2c5-max96752-gpio {
				compatible = "maxim,max96752-gpio";
				status = "okay";

				gpio-controller;
				#gpio-cells = <2>;
				gpio-ranges = <&i2c5_max96752_pinctrl 0 288 25>;
			};
		};

		i2c5_max96752_panel: i2c5-max96752-panel {
			compatible = "maxim,max96752-panel";
			reg = <0x48>;
			backlight = <&i2c5_max96745_backlight>;
			panel-size= <346 194>;

			panel-timing {
				clock-frequency = <148500000>;
				hactive = <1920>;
				vactive = <1080>;
				hfront-porch = <20>;
				hsync-len = <20>;
				hback-porch = <20>;
				vfront-porch = <250>;
				vsync-len = <2>;
				vback-porch = <8>;
				hsync-active = <0>;
				vsync-active = <0>;
				de-active = <0>;
				pixelclk-active = <0>;
			};

			port {
				i2c5_max96745_panel_in: endpoint {
					remote-endpoint = <&i2c5_max96745_out>;
				};
			};

		};
	};
};

&i2c6 {
	pinctrl-0 = <&i2c6m3_xfer>;
	clock-frequency = <400000>;
	status = "okay";

	max96755f@40 {
		compatible = "maxim,max96755f";
		reg = <0x40>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2c6_serdes_pins>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";


		pinctrl {
			compatible = "maxim,max96755f-pinctrl";
			pinctrl-names = "default";
			pinctrl-0 = <&i2c6_max96755f_pinctrl_hog>;

			i2c6_max96755f_pinctrl_hog: hog {
				i2c {
					groups = "I2C";
					function = "I2C";
				};
			};


			i2c6_max96755f_panel_pins: panel-pins {
				bl-pwm {
					pins = "MFP18";
					function = "GPIO_TX_0";
				};
			};
		};

		bridge {
			compatible = "maxim,max96755f-bridge";
			lock-gpios = <&gpio1 RK_PA5 GPIO_ACTIVE_HIGH>;

			ports {
				#address-cells = <1>;
				#size-cells = <0>;

				port@0 {
					reg = <0>;

					i2c6_max96755f_in: endpoint {
						remote-endpoint = <&dsi1_out>;
					};
				};

				port@1 {
					reg = <1>;

					i2c6_max96755f_out: endpoint {
						remote-endpoint = <&i2c6_max96755f_panel_in>;
					};
				};
			};
		};

		gmsl@0 {
			reg = <0>;
			clock-frequency = <400000>;
			#address-cells = <1>;
			#size-cells = <0>;

			panel@48 {
				compatible = "boe,av156fht-l83";
				reg = <0x48>;
				backlight = <&i2c6_max96755f_backlight>;
				pinctrl-names = "default";
				pinctrl-0 = <&i2c6_max96755f_panel_pins>;

				panel-timing {
					clock-frequency = <148500000>;
					hactive = <1920>;
					vactive = <1080>;
					hfront-porch = <20>;
					hsync-len = <20>;
					hback-porch = <20>;
					vfront-porch = <250>;
					vsync-len = <2>;
					vback-porch = <8>;
					hsync-active = <0>;
					vsync-active = <0>;
					de-active = <0>;
					pixelclk-active = <0>;
				};

				port {
					i2c6_max96755f_panel_in: endpoint {
						remote-endpoint = <&i2c6_max96755f_out>;
					};
				};
			};
		};
	};
};

&i2c7 {
	pinctrl-0 = <&i2c7m3_xfer>;
	clock-frequency = <400000>;
	status = "disabled";

	max96745@42 {
		compatible = "maxim,max96745";
		reg = <0x42>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2c7_serdes_pins>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";


		pinctrl {
			compatible = "maxim,max96745-pinctrl";
			pinctrl-names = "default";
			pinctrl-0 = <&i2c7_max96745_pinctrl_hog>;

			i2c7_max96745_pinctrl_hog: hog {
				i2c {
					groups = "I2C";
					function = "I2C";
				};
			};

			i2c7_max96745_panel_pins: panel-pins {
				bl-pwm {
					pins = "MFP0";
					function = "GPIO_TX_A_0";
				};
			};
		};

		bridge {
			compatible = "maxim,max96745-bridge";
			lock-gpios = <&gpio4 RK_PA7 GPIO_ACTIVE_HIGH>;

			ports {
				#address-cells = <1>;
				#size-cells = <0>;

				port@0 {
					reg = <0>;

					i2c7_max96745_in: endpoint {
						remote-endpoint = <&edp1_out>;
					};
				};

				port@1 {
					reg = <1>;

					i2c7_max96745_out: endpoint {
						remote-endpoint = <&i2c7_max96745_panel_in>;
					};
				};
			};
		};

		gmsl@0 {
			reg = <0>;
			clock-frequency = <400000>;
			#address-cells = <1>;
			#size-cells = <0>;

			panel@48 {
				compatible = "boe,av156fht-l83";
				reg = <0x48>;
				backlight = <&i2c7_max96745_backlight>;
				pinctrl-names = "default";
				pinctrl-0 = <&i2c7_max96745_panel_pins>;

				panel-timing {
					clock-frequency = <148500000>;
					hactive = <1920>;
					vactive = <1080>;
					hfront-porch = <20>;
					hsync-len = <20>;
					hback-porch = <20>;
					vfront-porch = <250>;
					vsync-len = <2>;
					vback-porch = <8>;
					hsync-active = <0>;
					vsync-active = <0>;
					de-active = <0>;
					pixelclk-active = <0>;
				};

				port {
					i2c7_max96745_panel_in: endpoint {
						remote-endpoint = <&i2c7_max96745_out>;
					};
				};
			};
		};
	};
};

&i2c8 {
	pinctrl-0 = <&i2c8m2_xfer>;
	clock-frequency = <400000>;
	status = "disabled";

	max96745@42 {
		compatible = "maxim,max96745";
		reg = <0x42>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2c8_serdes_pins>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";


		pinctrl {
			compatible = "maxim,max96745-pinctrl";
			pinctrl-names = "default";
			pinctrl-0 = <&i2c8_max96745_pinctrl_hog>;

			i2c8_max96745_pinctrl_hog: hog {
				i2c {
					groups = "I2C";
					function = "I2C";
				};
			};

			i2c8_max96745_panel_pins: panel-pins {
				bl-pwm {
					pins = "MFP0";
					function = "GPIO_TX_A_0";
				};
			};
		};

		bridge {
			compatible = "maxim,max96745-bridge";
			lock-gpios = <&gpio3 RK_PD2 GPIO_ACTIVE_HIGH>;

			ports {
				#address-cells = <1>;
				#size-cells = <0>;

				port@0 {
					reg = <0>;

					i2c8_max96745_in: endpoint {
						remote-endpoint = <&dp1_out>;
					};
				};

				port@1 {
					reg = <1>;

					i2c8_max96745_out: endpoint {
						remote-endpoint = <&i2c8_max96745_panel_in>;
					};
				};
			};
		};

		gmsl@0 {
			reg = <0>;
			clock-frequency = <400000>;
			#address-cells = <1>;
			#size-cells = <0>;

			panel@48 {
				compatible = "boe,av156fht-l83";
				reg = <0x48>;
				backlight = <&i2c8_max96745_backlight>;
				pinctrl-names = "default";
				pinctrl-0 = <&i2c8_max96745_panel_pins>;

				panel-timing {
					clock-frequency = <148500000>;
					hactive = <1920>;
					vactive = <1080>;
					hfront-porch = <20>;
					hsync-len = <20>;
					hback-porch = <20>;
					vfront-porch = <250>;
					vsync-len = <2>;
					vback-porch = <8>;
					hsync-active = <0>;
					vsync-active = <0>;
					de-active = <0>;
					pixelclk-active = <0>;
				};

				port {
					i2c8_max96745_panel_in: endpoint {
						remote-endpoint = <&i2c8_max96745_out>;
					};
				};
			};
		};
	};
};

&pinctrl {
	serdes {
		i2c2_serdes_pins: i2c2-serdes-pins {
			rockchip,pins =
				<1 RK_PA4 RK_FUNC_GPIO &pcfg_pull_up>;
		};

		i2c4_serdes_pins: i2c4-serdes-pins {
			rockchip,pins =
				<3 RK_PD4 RK_FUNC_GPIO &pcfg_pull_up>;
		};

		i2c5_serdes_pins: i2c5-serdes-pins {
			rockchip,pins =
				<0 RK_PD2 RK_FUNC_GPIO &pcfg_pull_up>;
		};

		i2c6_serdes_pins: i2c6-serdes-pins {
			rockchip,pins =
				<1 RK_PA5 RK_FUNC_GPIO &pcfg_pull_up>;
		};

		i2c7_serdes_pins: i2c7-serdes-pins {
			rockchip,pins =
				<4 RK_PA7 RK_FUNC_GPIO &pcfg_pull_up>;
		};

		i2c8_serdes_pins: i2c8-serdes-pins {
			rockchip,pins =
				<3 RK_PD2 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};
};

&pwm0 {
	pinctrl-0 = <&pwm0m2_pins>;
	status = "okay";
};

&pwm10 {
	pinctrl-0 = <&pwm10m2_pins>;
	status = "okay";
};

&pwm11 {
	pinctrl-0 = <&pwm11m3_pins>;
	status = "okay";
};

&pwm7 {
	pinctrl-0 = <&pwm7m0_pins>;
	status = "okay";
};

&pwm13 {
	pinctrl-0 = <&pwm13m1_pins>;
	status = "okay";
};

&pwm14 {
	pinctrl-0 = <&pwm14m0_pins>;
	status = "okay";
};
