#include "rp-lcd-hdmi.dtsi"
#define RP_SINGLE_LCD
#define RP_EDP_USED

&edp_panel {
    status = "okay";
        compatible = "simple-panel";
        prepare-delay-ms = <20>;
        enable-delay-ms = <20>;
        disable-delay-ms = <20>;
        unprepare-delay-ms = <20>;
    
        /**
         * power-supply = <>;
         * reset-gpios = <>;
         *
         * lcd reset pin and power supply
         * please refer to ***-lcd-gpio.dtsi
         * that included in main dts.
         */
         
        display-timings {
                native-mode = <&timing0>;

                timing0: timing0 {//EDP 15.6 1366x768
                        clock-frequency = <72300000>;
                        hactive = <1366>;
                        vactive = <768>;
                        hfront-porch = <48>;
                        hsync-len = <32>;
                        hback-porch = <80>;
                        vfront-porch = <3>;
                        vsync-len = <5>;
                        vback-porch = <14>;
                        hsync-active = <0>;
                        vsync-active = <0>;
                        de-active = <0>;
                        pixelclk-active = <0>;
                };

                timing1: timing1 {// EDP 13.3 
                        clock-frequency = <138000000>;
                        hactive = <1920>;
                        vactive = <1080>;
                        hfront-porch = <48>;
                        hsync-len = <32>;
                        hback-porch = <80>;
                        vfront-porch = <3>;
                        vsync-len = <5>;
                        vback-porch = <23>;
                        hsync-active = <0>;
                        vsync-active = <0>;
                        de-active = <0>;
                        pixelclk-active = <0>;
                };
        };

        ports {
                    panel_in_edp: endpoint {
                            remote-endpoint = <&edp_out_panel>;
            };
    };
};



&edp {
    status = "okay";
    force-hpd;
        ports {
                port@1 {
                        reg = <1>;

                        edp_out_panel: endpoint {
                                remote-endpoint = <&panel_in_edp>;
                        };
                };
        };
};

&edp_phy {
    status = "okay";
};

&edp_in_vp0 {
    status = "okay";
};

&edp_in_vp1 {
    status = "disabled";
};

&hdmi_in_vp0 {
    status = "disabled";
};
&hdmi_in_vp1 {
    status = "okay";
};

&route_edp {
    status = "okay";
    connect = <&vp0_out_edp>;
};





&gt9xx {
        status = "okay";

                compatible = "goodix,gt9xx";
                reg = <0x5d>;
                gtp_resolution_x = <1366>;
                gtp_resolution_y = <768>;
                gtp_int_tarigger = <1>;
                gtp_change_x2y = <0>;
                gtp_overturn_x = <0>;
                gtp_overturn_y = <0>;
                gtp_send_cfg = <1>;
                gtp_touch_wakeup = <1>;

        /**
         * goodix_rst_gpio = <>;
         * goodix_irq_gpio = <>;
         *
         * touch panel interrupt and reset pin
         * please refer to ***-lcd-gpio.dtsi
         * that included in main dts.
         */

                goodix,cfg-group0 = [
            41 80 07 38 04 0A 2D 00 01 06
            28 08 55 32 03 05 00 00 00 00
            00 00 04 17 19 1D 14 95 35 FF
            4C 4E B5 06 00 00 00 00 03 2D
            00 00 00 00 00 00 00 00 00 00
            00 2D 5A 94 D0 42 00 08 00 04
            61 30 00 57 37 00 4D 3F 00 45
            49 00 3E 54 00 3E 00 00 00 00
            00 00 00 00 00 00 00 00 00 00
            00 00 00 00 00 00 00 00 00 00
            00 00 00 00 00 00 00 00 00 00
            00 00 1D 1C 1B 1A 19 18 17 16
            15 14 13 12 11 10 0F 0E 0D 0C
            0B 0A 09 08 07 06 05 04 03 02
            01 00 00 01 02 03 04 05 06 07
            08 09 0A 0B 0C 0D 0E 0F 10 11
            12 13 14 15 16 17 18 19 1B 1C
            1D 1E 1F 20 21 22 23 24 25 26
            27 28 29 2A EA 01
                ];
};


