#define RP_SINGLE_LCD

&rpdzkj {
        compatible = "rp_config";
        user_version = "rpdzkj";
        system_rotate = "0";
        csi_camera_rotate = "0"; //all csi camera rotation //0 90 180 270 //no effect
        csi_camera_facing = "0"; //0:auto  1:all front   2:all back //no effect
        usb_camera_rotate = "0"; //all usb camera rotation //0 90 180 270 
        usb_camera_facing = "0"; //0:auto  1:all front   2:all back
        lcd_density = "160";
        language = "zh-CN";   //zh-CN //en-US
        time_zone = "Asia/Shanghai"; //Asia/Shanghai = +8   //Europe/London  = +1       //Africa/Casablanca     = +0;
        not_navigation_bar = "false";
        not_status_bar = "false";
        default_launcher = "true";
        has_root = "true";
        usb_not_permission = "true";
        gps_use = "false";
        gps_serial_port = "/dev/ttyS4";
        primary_device = "DSI";
        extend_device = "HDMI-A";
        extend_rotate = "0";//0 0//1 90 //2 180 //3 270
        rotation_efull = "false";
        extend_rotate_2 = "0";//0 0//1 90 //2 180 //3 270
        rotation_efull_2 = "true";
        extend_rotate_3 = "0";//0 0//1 90 //2 180 //3 270
        rotation_efull_3 = "true";
        home_apk = "null";
        status = "okay";
};



&dsi {
    status = "okay";
    //rockchip,lane-rate = <480>;
    
    dsi_panel: panel@0 {
        status = "okay";
        compatible = "aoly,sl008pa21y1285-b00","simple-panel-dsi";
        reg = <0>;

        init-delay-ms = <120>;
        reset-delay-ms = <120>;
        enable-delay-ms = <120>;
        prepare-delay-ms = <120>;
        unprepare-delay-ms = <60>;
        disable-delay-ms = <60>;
//        dsi,flags = <(MIPI_DSI_MODE_VIDEO | MIPI_DSI_MODE_VIDEO_BURST |
//                        MIPI_DSI_MODE_LPM | MIPI_DSI_MODE_EOT_PACKET)>;

//        dsi,flags = <(MIPI_DSI_MODE_VIDEO | MIPI_DSI_MODE_VIDEO_BURST |
//            MIPI_DSI_MODE_LPM | MIPI_DSI_MODE_EOT_PACKET)>;
                        
        dsi,flags = <(MIPI_DSI_MODE_VIDEO | MIPI_DSI_MODE_VIDEO_BURST |
              MIPI_DSI_MODE_VIDEO_HBP | MIPI_DSI_MODE_LPM |
              MIPI_DSI_MODE_EOT_PACKET)>;
              
        dsi,format = <MIPI_DSI_FMT_RGB888>;
        dsi,lanes  = <4>;

        /**
         * power-supply = <>;
         * reset-gpios = <>;
         *
         * lcd reset pin and power supply
         * please refer to ***-lcd-gpio.dtsi
         * that included in main dts.
         */

        panel-init-sequence = [
            05 78 01 11
            05 05 01 29
        ];

        panel-exit-sequence = [
            05 00 01 28
            05 78 01 10
        ];

        disp_timings0: display-timings {
            native-mode = <&dsi_timing0>;
            dsi_timing0: timing0 {
                clock-frequency = <148500000>;//140000000
                hactive = <1920>;
                vactive = <1080>;
                hback-porch = <148>;//60
                hfront-porch = <88>;
                vback-porch = <36>;//23
                vfront-porch = <4>;//12
                hsync-len = <44>;
                vsync-len = <5>;
                hsync-active = <0>;
                vsync-active = <0>;
                de-active = <0>;
                pixelclk-active = <0>;
            };
        };

        ports {
            #address-cells = <1>;
            #size-cells = <0>;

            port@0 {
                reg = <0>;
                panel_in_dsi: endpoint {
                    remote-endpoint = <&dsi_out_panel>;
                };
            };
        };
    };

    ports {
        #address-cells = <1>;
        #size-cells = <0>;

        port@1 {
            reg = <1>;
            dsi_out_panel: endpoint {
                remote-endpoint = <&panel_in_dsi>;
            };
        };
    };

};


&dsi_in_vp0 {
    status = "okay";
};

&video_phy {
 status = "okay";
};

&route_dsi {
    status = "okay";
    connect = <&vp0_out_dsi>;
};


&i2c2 {
        status = "okay";
        clock-frequency = <100000>;

    /delete-node/ gt1x@14;
        lt89121: lt89121@48 {
                status = "okay";
                compatible = "lt8912_i2c";
                reg = <0x48>;
            //  reset-gpios = <&gpio3 23 GPIO_ACTIVE_HIGH>;
        };


};


