// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Copyright (c) 2015 Caesar Wang <wxt@rock-chips.com>
 */

/dts-v1/;
#include "rk3368-evb.dtsi"

/ {
	model = "Rockchip RK3368 EVB with ACT8846 pmic";
	compatible = "rockchip,rk3368-evb-act8846", "rockchip,rk3368";
};

&i2c0 {
	clock-frequency = <400000>;

	vdd_cpu: syr827@40 {
		compatible = "silergy,syr827";
		reg = <0x40>;
		fcs,suspend-voltage-selector = <1>;
		regulator-name = "vdd_cpu";
		regulator-min-microvolt = <850000>;
		regulator-max-microvolt = <1350000>;
		regulator-always-on;
		regulator-boot-on;
		vin-supply = <&vcc_sys>;
	};

	vdd_gpu: syr828@41 {
		compatible = "silergy,syr828";
		reg = <0x41>;
		fcs,suspend-voltage-selector = <1>;
		regulator-name = "vdd_gpu";
		regulator-min-microvolt = <850000>;
		regulator-max-microvolt = <1350000>;
		regulator-always-on;
		vin-supply = <&vcc_sys>;
	};

	act8846: act8846@5a {
		compatible = "active-semi,act8846";
		reg = <0x5a>;
		status = "okay";

		vp1-supply = <&vcc_sys>;
		vp2-supply = <&vcc_sys>;
		vp3-supply = <&vcc_sys>;
		vp4-supply = <&vcc_sys>;
		inl1-supply = <&vcc_io>;
		inl2-supply = <&vcc_sys>;
		inl3-supply = <&vcc_20>;

		regulators {
			vcc_ddr: REG1 {
				regulator-name = "VCC_DDR";
				regulator-min-microvolt = <1200000>;
				regulator-max-microvolt = <1200000>;
				regulator-always-on;
			};

			vcc_io: REG2 {
				regulator-name = "VCC_IO";
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};

			vdd_log: REG3 {
				regulator-name = "VDD_LOG";
				regulator-min-microvolt = <700000>;
				regulator-max-microvolt = <1500000>;
				regulator-always-on;
			};

			vcc_20: REG4 {
				regulator-name = "VCC_20";
				regulator-min-microvolt = <2000000>;
				regulator-max-microvolt = <2000000>;
				regulator-always-on;
			};

			vccio_sd: REG5 {
				regulator-name = "VCCIO_SD";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};

			vdd10_lcd: REG6 {
				regulator-name = "VDD10_LCD";
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <1000000>;
				regulator-always-on;
			};

			vcca_codec: REG7 {
				regulator-name = "VCCA_CODEC";
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};

			vcca_tp: REG8 {
				regulator-name = "VCCA_TP";
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};

			vccio_pmu: REG9 {
				regulator-name = "VCCIO_PMU";
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};

			vdd_10: REG10 {
				regulator-name = "VDD_10";
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <1000000>;
				regulator-always-on;
			};

			vcc_18: REG11 {
				regulator-name = "VCC_18";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-always-on;
			};

			vcc18_lcd: REG12 {
				regulator-name = "VCC18_LCD";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-always-on;
			};
		};
	};
};
