// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Copyright (c) 2021 Rockchip Electronics Co., Ltd.
 */

#include <dt-bindings/pinctrl/rockchip.h>
#include "rockchip-pinconf.dtsi"

/*
 * This file is auto generated by pin2dts tool, please keep these code
 * by adding changes at end of this file.
 */
&pinctrl {
	clk32k {
		/omit-if-no-ref/
		clk32k_out1: clk32k-out1 {
			rockchip,pins =
				/* clk32k_out1 */
				<2 RK_PC5 1 &pcfg_pull_none>;
		};

	};

	eth0 {
		/omit-if-no-ref/
		eth0_pins: eth0-pins {
			rockchip,pins =
				/* eth0_refclko_25m */
				<2 RK_PC3 1 &pcfg_pull_none>;
		};

	};

	fspi {
		/omit-if-no-ref/
		fspim1_pins: fspim1-pins {
			rockchip,pins =
				/* fspi_clk_m1 */
				<2 RK_PB3 3 &pcfg_pull_up_drv_level_2>,
				/* fspi_cs0n_m1 */
				<2 RK_PB4 3 &pcfg_pull_up_drv_level_2>,
				/* fspi_d0_m1 */
				<2 RK_PA6 3 &pcfg_pull_up_drv_level_2>,
				/* fspi_d1_m1 */
				<2 RK_PA7 3 &pcfg_pull_up_drv_level_2>,
				/* fspi_d2_m1 */
				<2 RK_PB0 3 &pcfg_pull_up_drv_level_2>,
				/* fspi_d3_m1 */
				<2 RK_PB1 3 &pcfg_pull_up_drv_level_2>;
		};

		/omit-if-no-ref/
		fspim1_cs1: fspim1-cs1 {
			rockchip,pins =
				/* fspi_cs1n_m1 */
				<2 RK_PB5 3 &pcfg_pull_up_drv_level_2>;
		};
	};

	gmac0 {
		/omit-if-no-ref/
		gmac0_miim: gmac0-miim {
			rockchip,pins =
				/* gmac0_mdc */
				<4 RK_PC4 1 &pcfg_pull_none>,
				/* gmac0_mdio */
				<4 RK_PC5 1 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		gmac0_clkinout: gmac0-clkinout {
			rockchip,pins =
				/* gmac0_mclkinout */
				<4 RK_PC3 1 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		gmac0_rx_bus2: gmac0-rx-bus2 {
			rockchip,pins =
				/* gmac0_rxd0 */
				<2 RK_PC1 1 &pcfg_pull_none>,
				/* gmac0_rxd1 */
				<2 RK_PC2 1 &pcfg_pull_none>,
				/* gmac0_rxdv_crs */
				<4 RK_PC2 1 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		gmac0_tx_bus2: gmac0-tx-bus2 {
			rockchip,pins =
				/* gmac0_txd0 */
				<2 RK_PB6 1 &pcfg_pull_none>,
				/* gmac0_txd1 */
				<2 RK_PB7 1 &pcfg_pull_none>,
				/* gmac0_txen */
				<2 RK_PC0 1 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		gmac0_rgmii_clk: gmac0-rgmii-clk {
			rockchip,pins =
				/* gmac0_rxclk */
				<2 RK_PB0 1 &pcfg_pull_none>,
				/* gmac0_txclk */
				<2 RK_PB3 1 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		gmac0_rgmii_bus: gmac0-rgmii-bus {
			rockchip,pins =
				/* gmac0_rxd2 */
				<2 RK_PA6 1 &pcfg_pull_none>,
				/* gmac0_rxd3 */
				<2 RK_PA7 1 &pcfg_pull_none>,
				/* gmac0_txd2 */
				<2 RK_PB1 1 &pcfg_pull_none>,
				/* gmac0_txd3 */
				<2 RK_PB2 1 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		gmac0_ppsclk: gmac0-ppsclk {
			rockchip,pins =
				/* gmac0_ppsclk */
				<2 RK_PC4 1 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		gmac0_ppstring: gmac0-ppstring {
			rockchip,pins =
				/* gmac0_ppstring */
				<2 RK_PB5 1 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		gmac0_ptp_refclk: gmac0-ptp-refclk {
			rockchip,pins =
				/* gmac0_ptp_refclk */
				<2 RK_PB4 1 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		gmac0_txer: gmac0-txer {
			rockchip,pins =
				/* gmac0_txer */
				<4 RK_PC6 1 &pcfg_pull_none>;
		};

	};

	hdmi {
		/omit-if-no-ref/
		hdmim0_tx1_cec: hdmim0-tx1-cec {
			rockchip,pins =
				/* hdmim0_tx1_cec */
				<2 RK_PC4 4 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		hdmim0_tx1_scl: hdmim0-tx1-scl {
			rockchip,pins =
				/* hdmim0_tx1_scl */
				<2 RK_PB5 4 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		hdmim0_tx1_sda: hdmim0-tx1-sda {
			rockchip,pins =
				/* hdmim0_tx1_sda */
				<2 RK_PB4 4 &pcfg_pull_none>;
		};
	};

	i2c0 {
		/omit-if-no-ref/
		i2c0m1_xfer: i2c0m1-xfer {
			rockchip,pins =
				/* i2c0_scl_m1 */
				<4 RK_PC5 9 &pcfg_pull_none_smt>,
				/* i2c0_sda_m1 */
				<4 RK_PC6 9 &pcfg_pull_none_smt>;
		};
	};

	i2c2 {
		/omit-if-no-ref/
		i2c2m1_xfer: i2c2m1-xfer {
			rockchip,pins =
				/* i2c2_scl_m1 */
				<2 RK_PC1 9 &pcfg_pull_none_smt>,
				/* i2c2_sda_m1 */
				<2 RK_PC0 9 &pcfg_pull_none_smt>;
		};
	};

	i2c3 {
		/omit-if-no-ref/
		i2c3m3_xfer: i2c3m3-xfer {
			rockchip,pins =
				/* i2c3_scl_m3 */
				<2 RK_PB2 9 &pcfg_pull_none_smt>,
				/* i2c3_sda_m3 */
				<2 RK_PB3 9 &pcfg_pull_none_smt>;
		};
	};

	i2c4 {
		/omit-if-no-ref/
		i2c4m1_xfer: i2c4m1-xfer {
			rockchip,pins =
				/* i2c4_scl_m1 */
				<2 RK_PB5 9 &pcfg_pull_none_smt>,
				/* i2c4_sda_m1 */
				<2 RK_PB4 9 &pcfg_pull_none_smt>;
		};
	};

	i2c5 {
		/omit-if-no-ref/
		i2c5m4_xfer: i2c5m4-xfer {
			rockchip,pins =
				/* i2c5_scl_m4 */
				<2 RK_PB6 9 &pcfg_pull_none_smt>,
				/* i2c5_sda_m4 */
				<2 RK_PB7 9 &pcfg_pull_none_smt>;
		};
	};

	i2c6 {
		/omit-if-no-ref/
		i2c6m2_xfer: i2c6m2-xfer {
			rockchip,pins =
				/* i2c6_scl_m2 */
				<2 RK_PC3 9 &pcfg_pull_none_smt>,
				/* i2c6_sda_m2 */
				<2 RK_PC2 9 &pcfg_pull_none_smt>;
		};
	};

	i2c7 {
		/omit-if-no-ref/
		i2c7m1_xfer: i2c7m1-xfer {
			rockchip,pins =
				/* i2c7_scl_m1 */
				<4 RK_PC3 9 &pcfg_pull_none_smt>,
				/* i2c7_sda_m1 */
				<4 RK_PC4 9 &pcfg_pull_none_smt>;
		};
	};

	i2c8 {
		/omit-if-no-ref/
		i2c8m1_xfer: i2c8m1-xfer {
			rockchip,pins =
				/* i2c8_scl_m1 */
				<2 RK_PB0 9 &pcfg_pull_none_smt>,
				/* i2c8_sda_m1 */
				<2 RK_PB1 9 &pcfg_pull_none_smt>;
		};
	};

	i2s2 {
		/omit-if-no-ref/
		i2s2m0_idle: i2s2m0-idle {
			rockchip,pins =
				/* i2s2m0_lrck_gpio */
				<2 RK_PC0 0 &pcfg_pull_none>,
				/* i2s2m0_sclk_gpio */
				<2 RK_PB7 0 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		i2s2m0_lrck: i2s2m0-lrck {
			rockchip,pins =
				/* i2s2m0_lrck */
				<2 RK_PC0 2 &pcfg_pull_none_smt>;
		};

		/omit-if-no-ref/
		i2s2m0_mclk: i2s2m0-mclk {
			rockchip,pins =
				/* i2s2m0_mclk */
				<2 RK_PB6 2 &pcfg_pull_none_smt>;
		};

		/omit-if-no-ref/
		i2s2m0_sclk: i2s2m0-sclk {
			rockchip,pins =
				/* i2s2m0_sclk */
				<2 RK_PB7 2 &pcfg_pull_none_smt>;
		};

		/omit-if-no-ref/
		i2s2m0_sdi: i2s2m0-sdi {
			rockchip,pins =
				/* i2s2m0_sdi */
				<2 RK_PC3 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		i2s2m0_sdo: i2s2m0-sdo {
			rockchip,pins =
				/* i2s2m0_sdo */
				<4 RK_PC3 2 &pcfg_pull_none>;
		};
	};

	pwm2 {
		/omit-if-no-ref/
		pwm2m2_pins: pwm2m2-pins {
			rockchip,pins =
				/* pwm2_m2 */
				<4 RK_PC2 11 &pcfg_pull_none>;
		};
	};

	pwm4 {
		/omit-if-no-ref/
		pwm4m1_pins: pwm4m1-pins {
			rockchip,pins =
				/* pwm4_m1 */
				<4 RK_PC3 11 &pcfg_pull_none>;
		};
	};

	pwm5 {
		/omit-if-no-ref/
		pwm5m2_pins: pwm5m2-pins {
			rockchip,pins =
				/* pwm5_m2 */
				<4 RK_PC4 11 &pcfg_pull_none>;
		};
	};

	pwm6 {
		/omit-if-no-ref/
		pwm6m2_pins: pwm6m2-pins {
			rockchip,pins =
				/* pwm6_m2 */
				<4 RK_PC5 11 &pcfg_pull_none>;
		};
	};

	pwm7 {
		/omit-if-no-ref/
		pwm7m3_pins: pwm7m3-pins {
			rockchip,pins =
				/* pwm7_ir_m3 */
				<4 RK_PC6 11 &pcfg_pull_none>;
		};
	};

	sdio {
		/omit-if-no-ref/
		sdiom0_pins: sdiom0-pins {
			rockchip,pins =
				/* sdio_clk_m0 */
				<2 RK_PB3 2 &pcfg_pull_none>,
				/* sdio_cmd_m0 */
				<2 RK_PB2 2 &pcfg_pull_up>,
				/* sdio_d0_m0 */
				<2 RK_PA6 2 &pcfg_pull_up>,
				/* sdio_d1_m0 */
				<2 RK_PA7 2 &pcfg_pull_up>,
				/* sdio_d2_m0 */
				<2 RK_PB0 2 &pcfg_pull_up>,
				/* sdio_d3_m0 */
				<2 RK_PB1 2 &pcfg_pull_up>;
		};
	};

	spi1 {
		/omit-if-no-ref/
		spi1m0_pins: spi1m0-pins {
			rockchip,pins =
				/* spi1_clk_m0 */
				<2 RK_PC0 8 &pcfg_pull_up_drv_level_1>,
				/* spi1_miso_m0 */
				<2 RK_PC1 8 &pcfg_pull_up_drv_level_1>,
				/* spi1_mosi_m0 */
				<2 RK_PC2 8 &pcfg_pull_up_drv_level_1>;
		};

		/omit-if-no-ref/
		spi1m0_cs0: spi1m0-cs0 {
			rockchip,pins =
				/* spi1_cs0_m0 */
				<2 RK_PC3 8 &pcfg_pull_up_drv_level_1>;
		};

		/omit-if-no-ref/
		spi1m0_cs1: spi1m0-cs1 {
			rockchip,pins =
				/* spi1_cs1_m0 */
				<2 RK_PC4 8 &pcfg_pull_up_drv_level_1>;
		};
	};

	spi3 {
		/omit-if-no-ref/
		spi3m0_pins: spi3m0-pins {
			rockchip,pins =
				/* spi3_clk_m0 */
				<4 RK_PC6 8 &pcfg_pull_up_drv_level_1>,
				/* spi3_miso_m0 */
				<4 RK_PC4 8 &pcfg_pull_up_drv_level_1>,
				/* spi3_mosi_m0 */
				<4 RK_PC5 8 &pcfg_pull_up_drv_level_1>;
		};

		/omit-if-no-ref/
		spi3m0_cs0: spi3m0-cs0 {
			rockchip,pins =
				/* spi3_cs0_m0 */
				<4 RK_PC2 8 &pcfg_pull_up_drv_level_1>;
		};

		/omit-if-no-ref/
		spi3m0_cs1: spi3m0-cs1 {
			rockchip,pins =
				/* spi3_cs1_m0 */
				<4 RK_PC3 8 &pcfg_pull_up_drv_level_1>;
		};
	};

	uart1 {
		/omit-if-no-ref/
		uart1m0_xfer: uart1m0-xfer {
			rockchip,pins =
				/* uart1_rx_m0 */
				<2 RK_PB6 10 &pcfg_pull_up>,
				/* uart1_tx_m0 */
				<2 RK_PB7 10 &pcfg_pull_up>;
		};

		/omit-if-no-ref/
		uart1m0_ctsn: uart1m0-ctsn {
			rockchip,pins =
				/* uart1m0_ctsn */
				<2 RK_PC1 10 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		uart1m0_rtsn: uart1m0-rtsn {
			rockchip,pins =
				/* uart1m0_rtsn */
				<2 RK_PC0 10 &pcfg_pull_none>;
		};
	};

	uart6 {
		/omit-if-no-ref/
		uart6m0_xfer: uart6m0-xfer {
			rockchip,pins =
				/* uart6_rx_m0 */
				<2 RK_PA6 10 &pcfg_pull_up>,
				/* uart6_tx_m0 */
				<2 RK_PA7 10 &pcfg_pull_up>;
		};

		/omit-if-no-ref/
		uart6m0_ctsn: uart6m0-ctsn {
			rockchip,pins =
				/* uart6m0_ctsn */
				<2 RK_PB1 10 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		uart6m0_rtsn: uart6m0-rtsn {
			rockchip,pins =
				/* uart6m0_rtsn */
				<2 RK_PB0 10 &pcfg_pull_none>;
		};
	};

	uart7 {
		/omit-if-no-ref/
		uart7m0_xfer: uart7m0-xfer {
			rockchip,pins =
				/* uart7_rx_m0 */
				<2 RK_PB4 10 &pcfg_pull_up>,
				/* uart7_tx_m0 */
				<2 RK_PB5 10 &pcfg_pull_up>;
		};

		/omit-if-no-ref/
		uart7m0_ctsn: uart7m0-ctsn {
			rockchip,pins =
				/* uart7m0_ctsn */
				<4 RK_PC6 10 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		uart7m0_rtsn: uart7m0-rtsn {
			rockchip,pins =
				/* uart7m0_rtsn */
				<4 RK_PC2 10 &pcfg_pull_none>;
		};
	};

	uart9 {
		/omit-if-no-ref/
		uart9m0_xfer: uart9m0-xfer {
			rockchip,pins =
				/* uart9_rx_m0 */
				<2 RK_PC4 10 &pcfg_pull_up>,
				/* uart9_tx_m0 */
				<2 RK_PC2 10 &pcfg_pull_up>;
		};

		/omit-if-no-ref/
		uart9m0_ctsn: uart9m0-ctsn {
			rockchip,pins =
				/* uart9m0_ctsn */
				<4 RK_PC5 10 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		uart9m0_rtsn: uart9m0-rtsn {
			rockchip,pins =
				/* uart9m0_rtsn */
				<4 RK_PC4 10 &pcfg_pull_none>;
		};
	};
};
