// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Copyright (c) 2022 Rockchip Electronics Co., Ltd.
 */

#include <dt-bindings/pinctrl/rockchip.h>
#include "rockchip-pinconf.dtsi"

/*
 * This file is auto generated by pin2dts tool, please keep these code
 * by adding changes at end of this file.
 */
&pinctrl {
	cam {
		/omit-if-no-ref/
		camm0_clk0_out: camm0-clk0-out {
			rockchip,pins =
				/* camm0_clk0_out */
				<3 RK_PB2 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		camm0_clk1_out: camm0-clk1-out {
			rockchip,pins =
				/* camm0_clk1_out */
				<3 RK_PB3 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		camm1_clk0_out: camm1-clk0-out {
			rockchip,pins =
				/* camm1_clk0_out */
				<4 RK_PB1 3 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		camm1_clk1_out: camm1-clk1-out {
			rockchip,pins =
				/* camm1_clk1_out */
				<4 RK_PB7 3 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		cam_clk2_out: cam-clk2-out {
			rockchip,pins =
				/* cam_clk2_out */
				<3 RK_PB4 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		cam_clk3_out: cam-clk3-out {
			rockchip,pins =
				/* cam_clk3_out */
				<3 RK_PB5 2 &pcfg_pull_none>;
		};
	};

	can0 {
		/omit-if-no-ref/
		can0m0_pins: can0m0-pins {
			rockchip,pins =
				/* can0_rx_m0 */
				<3 RK_PA1 4 &pcfg_pull_none>,
				/* can0_tx_m0 */
				<3 RK_PA0 4 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		can0m1_pins: can0m1-pins {
			rockchip,pins =
				/* can0_rx_m1 */
				<3 RK_PB7 6 &pcfg_pull_none>,
				/* can0_tx_m1 */
				<3 RK_PB6 6 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		can0m2_pins: can0m2-pins {
			rockchip,pins =
				/* can0_rx_m2 */
				<0 RK_PC7 2 &pcfg_pull_none>,
				/* can0_tx_m2 */
				<0 RK_PC6 2 &pcfg_pull_none>;
		};
	};

	can1 {
		/omit-if-no-ref/
		can1m0_pins: can1m0-pins {
			rockchip,pins =
				/* can1_rx_m0 */
				<1 RK_PB7 4 &pcfg_pull_none>,
				/* can1_tx_m0 */
				<1 RK_PC0 5 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		can1m1_pins: can1m1-pins {
			rockchip,pins =
				/* can1_rx_m1 */
				<0 RK_PC1 4 &pcfg_pull_none>,
				/* can1_tx_m1 */
				<0 RK_PC0 4 &pcfg_pull_none>;
		};
	};

	clk {
		/omit-if-no-ref/
		clk_32k_in: clk-32k-in {
			rockchip,pins =
				/* clk_32k_in */
				<0 RK_PB0 1 &pcfg_pull_none>;
		};
	};

	clk0 {
		/omit-if-no-ref/
		clk0_32k_out: clk0-32k-out {
			rockchip,pins =
				/* clk0_32k_out */
				<0 RK_PB0 2 &pcfg_pull_none>;
		};
	};

	clk1 {
		/omit-if-no-ref/
		clk1_32k_out: clk1-32k-out {
			rockchip,pins =
				/* clk1_32k_out */
				<2 RK_PA1 3 &pcfg_pull_none>;
		};
	};

	cpu {
		/omit-if-no-ref/
		cpu_pins: cpu-pins {
			rockchip,pins =
				/* cpu_avs */
				<0 RK_PB7 3 &pcfg_pull_none>;
		};
	};

	dsm {
		/omit-if-no-ref/
		dsm_pins: dsm-pins {
			rockchip,pins =
				/* dsm_aud_ln */
				<1 RK_PB4 5 &pcfg_pull_none>,
				/* dsm_aud_lp */
				<1 RK_PB3 5 &pcfg_pull_none>,
				/* dsm_aud_rn */
				<1 RK_PB6 6 &pcfg_pull_none>,
				/* dsm_aud_rp */
				<1 RK_PB5 6 &pcfg_pull_none>;
		};
	};

	emmc {
		/omit-if-no-ref/
		emmc_bus8: emmc-bus8 {
			rockchip,pins =
				/* emmc_d0 */
				<1 RK_PA0 1 &pcfg_pull_up_drv_level_2>,
				/* emmc_d1 */
				<1 RK_PA1 1 &pcfg_pull_up_drv_level_2>,
				/* emmc_d2 */
				<1 RK_PA2 1 &pcfg_pull_up_drv_level_2>,
				/* emmc_d3 */
				<1 RK_PA3 1 &pcfg_pull_up_drv_level_2>,
				/* emmc_d4 */
				<1 RK_PA4 1 &pcfg_pull_up_drv_level_2>,
				/* emmc_d5 */
				<1 RK_PA5 1 &pcfg_pull_up_drv_level_2>,
				/* emmc_d6 */
				<1 RK_PA6 1 &pcfg_pull_up_drv_level_2>,
				/* emmc_d7 */
				<1 RK_PA7 1 &pcfg_pull_up_drv_level_2>;
		};

		/omit-if-no-ref/
		emmc_clk: emmc-clk {
			rockchip,pins =
				/* emmc_clk */
				<1 RK_PB1 1 &pcfg_pull_up_drv_level_2>;
		};

		/omit-if-no-ref/
		emmc_cmd: emmc-cmd {
			rockchip,pins =
				/* emmc_cmd */
				<1 RK_PB0 1 &pcfg_pull_up_drv_level_2>;
		};

		/omit-if-no-ref/
		emmc_strb: emmc-strb {
			rockchip,pins =
				/* emmc_strb */
				<1 RK_PB2 1 &pcfg_pull_none>;
		};
	};

	eth {
		/omit-if-no-ref/
		ethm0_pins: ethm0-pins {
			rockchip,pins =
				/* eth_clk_25m_out_m0 */
				<4 RK_PB1 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		ethm1_pins: ethm1-pins {
			rockchip,pins =
				/* eth_clk_25m_out_m1 */
				<2 RK_PA1 2 &pcfg_pull_none>;
		};
	};

	fspi {
		/omit-if-no-ref/
		fspi_pins: fspi-pins {
			rockchip,pins =
				/* fspi_clk */
				<1 RK_PB1 2 &pcfg_pull_none>,
				/* fspi_d0 */
				<1 RK_PA0 2 &pcfg_pull_none>,
				/* fspi_d1 */
				<1 RK_PA1 2 &pcfg_pull_none>,
				/* fspi_d2 */
				<1 RK_PA2 2 &pcfg_pull_none>,
				/* fspi_d3 */
				<1 RK_PA3 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		fspi_csn0: fspi-csn0 {
			rockchip,pins =
				/* fspi_csn0 */
				<1 RK_PB0 2 &pcfg_pull_none>;
		};
		/omit-if-no-ref/
		fspi_csn1: fspi-csn1 {
			rockchip,pins =
				/* fspi_csn1 */
				<1 RK_PB2 2 &pcfg_pull_none>;
		};
	};

	gpu {
		/omit-if-no-ref/
		gpu_pins: gpu-pins {
			rockchip,pins =
				/* gpu_avs */
				<0 RK_PC0 3 &pcfg_pull_none>;
		};
	};

	i2c0 {
		/omit-if-no-ref/
		i2c0_xfer: i2c0-xfer {
			rockchip,pins =
				/* i2c0_scl */
				<0 RK_PB1 1 &pcfg_pull_none_smt>,
				/* i2c0_sda */
				<0 RK_PB2 1 &pcfg_pull_none_smt>;
		};
	};

	i2c1 {
		/omit-if-no-ref/
		i2c1m0_xfer: i2c1m0-xfer {
			rockchip,pins =
				/* i2c1_scl_m0 */
				<0 RK_PB3 1 &pcfg_pull_none_smt>,
				/* i2c1_sda_m0 */
				<0 RK_PB4 1 &pcfg_pull_none_smt>;
		};

		/omit-if-no-ref/
		i2c1m1_xfer: i2c1m1-xfer {
			rockchip,pins =
				/* i2c1_scl_m1 */
				<4 RK_PB4 5 &pcfg_pull_none_smt>,
				/* i2c1_sda_m1 */
				<4 RK_PB5 5 &pcfg_pull_none_smt>;
		};
	};

	i2c2 {
		/omit-if-no-ref/
		i2c2m0_xfer: i2c2m0-xfer {
			rockchip,pins =
				/* i2c2_scl_m0 */
				<0 RK_PB5 1 &pcfg_pull_none_smt>,
				/* i2c2_sda_m0 */
				<0 RK_PB6 1 &pcfg_pull_none_smt>;
		};

		/omit-if-no-ref/
		i2c2m1_xfer: i2c2m1-xfer {
			rockchip,pins =
				/* i2c2_scl_m1 */
				<3 RK_PD2 5 &pcfg_pull_none_smt>,
				/* i2c2_sda_m1 */
				<3 RK_PD3 5 &pcfg_pull_none_smt>;
		};
	};

	i2c3 {
		/omit-if-no-ref/
		i2c3m0_xfer: i2c3m0-xfer {
			rockchip,pins =
				/* i2c3_scl_m0 */
				<3 RK_PA0 1 &pcfg_pull_none_smt>,
				/* i2c3_sda_m0 */
				<3 RK_PA1 1 &pcfg_pull_none_smt>;
		};

		/omit-if-no-ref/
		i2c3m1_xfer: i2c3m1-xfer {
			rockchip,pins =
				/* i2c3_scl_m1 */
				<4 RK_PA5 5 &pcfg_pull_none_smt>,
				/* i2c3_sda_m1 */
				<4 RK_PA6 5 &pcfg_pull_none_smt>;
		};
	};

	i2c4 {
		/omit-if-no-ref/
		i2c4m0_xfer: i2c4m0-xfer {
			rockchip,pins =
				/* i2c4_scl_m0 */
				<3 RK_PB6 5 &pcfg_pull_none_smt>,
				/* i2c4_sda_m0 */
				<3 RK_PB7 5 &pcfg_pull_none_smt>;
		};

		/omit-if-no-ref/
		i2c4m1_xfer: i2c4m1-xfer {
			rockchip,pins =
				/* i2c4_scl_m1 */
				<0 RK_PA5 2 &pcfg_pull_none_smt>,
				/* i2c4_sda_m1 */
				<0 RK_PA4 2 &pcfg_pull_none_smt>;
		};
	};

	i2c5 {
		/omit-if-no-ref/
		i2c5m0_xfer: i2c5m0-xfer {
			rockchip,pins =
				/* i2c5_scl_m0 */
				<3 RK_PC2 1 &pcfg_pull_none_smt>,
				/* i2c5_sda_m0 */
				<3 RK_PC3 1 &pcfg_pull_none_smt>;
		};

		/omit-if-no-ref/
		i2c5m1_xfer: i2c5m1-xfer {
			rockchip,pins =
				/* i2c5_scl_m1 */
				<1 RK_PC7 4 &pcfg_pull_none_smt>,
				/* i2c5_sda_m1 */
				<1 RK_PD0 4 &pcfg_pull_none_smt>;
		};
	};

	i2s0 {
		/omit-if-no-ref/
		i2s0m0_lrck: i2s0m0-lrck {
			rockchip,pins =
				/* i2s0_lrck_m0 */
				<3 RK_PA4 1 &pcfg_pull_none_smt>;
		};

		/omit-if-no-ref/
		i2s0m0_mclk: i2s0m0-mclk {
			rockchip,pins =
				/* i2s0_mclk_m0 */
				<3 RK_PA2 1 &pcfg_pull_none_smt>;
		};

		/omit-if-no-ref/
		i2s0m0_sclk: i2s0m0-sclk {
			rockchip,pins =
				/* i2s0_sclk_m0 */
				<3 RK_PA3 1 &pcfg_pull_none_smt>;
		};

		/omit-if-no-ref/
		i2s0m0_sdi0: i2s0m0-sdi0 {
			rockchip,pins =
				/* i2s0_sdi0_m0 */
				<3 RK_PB1 1 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		i2s0m0_sdi1: i2s0m0-sdi1 {
			rockchip,pins =
				/* i2s0_sdi1_m0 */
				<3 RK_PB0 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		i2s0m0_sdi2: i2s0m0-sdi2 {
			rockchip,pins =
				/* i2s0_sdi2_m0 */
				<3 RK_PA7 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		i2s0m0_sdi3: i2s0m0-sdi3 {
			rockchip,pins =
				/* i2s0_sdi3_m0 */
				<3 RK_PA6 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		i2s0m0_sdo0: i2s0m0-sdo0 {
			rockchip,pins =
				/* i2s0_sdo0_m0 */
				<3 RK_PA5 1 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		i2s0m0_sdo1: i2s0m0-sdo1 {
			rockchip,pins =
				/* i2s0_sdo1_m0 */
				<3 RK_PA6 1 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		i2s0m0_sdo2: i2s0m0-sdo2 {
			rockchip,pins =
				/* i2s0_sdo2_m0 */
				<3 RK_PA7 1 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		i2s0m0_sdo3: i2s0m0-sdo3 {
			rockchip,pins =
				/* i2s0_sdo3_m0 */
				<3 RK_PB0 1 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		i2s0m1_lrck: i2s0m1-lrck {
			rockchip,pins =
				/* i2s0_lrck_m1 */
				<1 RK_PC4 3 &pcfg_pull_none_smt>;
		};

		/omit-if-no-ref/
		i2s0m1_mclk: i2s0m1-mclk {
			rockchip,pins =
				/* i2s0_mclk_m1 */
				<1 RK_PC6 3 &pcfg_pull_none_smt>;
		};

		/omit-if-no-ref/
		i2s0m1_sclk: i2s0m1-sclk {
			rockchip,pins =
				/* i2s0_sclk_m1 */
				<1 RK_PC5 3 &pcfg_pull_none_smt>;
		};

		/omit-if-no-ref/
		i2s0m1_sdi0: i2s0m1-sdi0 {
			rockchip,pins =
				/* i2s0_sdi0_m1 */
				<1 RK_PC1 3 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		i2s0m1_sdi1: i2s0m1-sdi1 {
			rockchip,pins =
				/* i2s0_sdi1_m1 */
				<1 RK_PC2 3 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		i2s0m1_sdi2: i2s0m1-sdi2 {
			rockchip,pins =
				/* i2s0_sdi2_m1 */
				<1 RK_PD3 3 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		i2s0m1_sdi3: i2s0m1-sdi3 {
			rockchip,pins =
				/* i2s0_sdi3_m1 */
				<1 RK_PD4 3 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		i2s0m1_sdo0: i2s0m1-sdo0 {
			rockchip,pins =
				/* i2s0_sdo0_m1 */
				<1 RK_PC3 3 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		i2s0m1_sdo1: i2s0m1-sdo1 {
			rockchip,pins =
				/* i2s0_sdo1_m1 */
				<1 RK_PD1 3 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		i2s0m1_sdo2: i2s0m1-sdo2 {
			rockchip,pins =
				/* i2s0_sdo2_m1 */
				<1 RK_PD2 3 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		i2s0m1_sdo3: i2s0m1-sdo3 {
			rockchip,pins =
				/* i2s0_sdo3_m1 */
				<2 RK_PA1 5 &pcfg_pull_none>;
		};
	};

	i2s1 {
		/omit-if-no-ref/
		i2s1m0_lrck: i2s1m0-lrck {
			rockchip,pins =
				/* i2s1_lrck_m0 */
				<3 RK_PC6 2 &pcfg_pull_none_smt>;
		};

		/omit-if-no-ref/
		i2s1m0_mclk: i2s1m0-mclk {
			rockchip,pins =
				/* i2s1_mclk_m0 */
				<3 RK_PC4 2 &pcfg_pull_none_smt>;
		};

		/omit-if-no-ref/
		i2s1m0_sclk: i2s1m0-sclk {
			rockchip,pins =
				/* i2s1_sclk_m0 */
				<3 RK_PC5 2 &pcfg_pull_none_smt>;
		};

		/omit-if-no-ref/
		i2s1m0_sdi0: i2s1m0-sdi0 {
			rockchip,pins =
				/* i2s1_sdi0_m0 */
				<3 RK_PD0 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		i2s1m0_sdi1: i2s1m0-sdi1 {
			rockchip,pins =
				/* i2s1_sdi1_m0 */
				<3 RK_PD1 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		i2s1m0_sdi2: i2s1m0-sdi2 {
			rockchip,pins =
				/* i2s1_sdi2_m0 */
				<3 RK_PD2 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		i2s1m0_sdi3: i2s1m0-sdi3 {
			rockchip,pins =
				/* i2s1_sdi3_m0 */
				<3 RK_PD3 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		i2s1m0_sdo0: i2s1m0-sdo0 {
			rockchip,pins =
				/* i2s1_sdo0_m0 */
				<3 RK_PC7 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		i2s1m0_sdo1: i2s1m0-sdo1 {
			rockchip,pins =
				/* i2s1_sdo1_m0 */
				<4 RK_PB4 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		i2s1m0_sdo2: i2s1m0-sdo2 {
			rockchip,pins =
				/* i2s1_sdo2_m0 */
				<4 RK_PB5 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		i2s1m0_sdo3: i2s1m0-sdo3 {
			rockchip,pins =
				/* i2s1_sdo3_m0 */
				<4 RK_PB6 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		i2s1m1_lrck: i2s1m1-lrck {
			rockchip,pins =
				/* i2s1_lrck_m1 */
				<3 RK_PB4 1 &pcfg_pull_none_smt>;
		};

		/omit-if-no-ref/
		i2s1m1_mclk: i2s1m1-mclk {
			rockchip,pins =
				/* i2s1_mclk_m1 */
				<3 RK_PB2 1 &pcfg_pull_none_smt>;
		};

		/omit-if-no-ref/
		i2s1m1_sclk: i2s1m1-sclk {
			rockchip,pins =
				/* i2s1_sclk_m1 */
				<3 RK_PB3 1 &pcfg_pull_none_smt>;
		};

		/omit-if-no-ref/
		i2s1m1_sdi0: i2s1m1-sdi0 {
			rockchip,pins =
				/* i2s1_sdi0_m1 */
				<3 RK_PC1 1 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		i2s1m1_sdi1: i2s1m1-sdi1 {
			rockchip,pins =
				/* i2s1_sdi1_m1 */
				<3 RK_PC0 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		i2s1m1_sdi2: i2s1m1-sdi2 {
			rockchip,pins =
				/* i2s1_sdi2_m1 */
				<3 RK_PB7 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		i2s1m1_sdi3: i2s1m1-sdi3 {
			rockchip,pins =
				/* i2s1_sdi3_m1 */
				<3 RK_PB6 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		i2s1m1_sdo0: i2s1m1-sdo0 {
			rockchip,pins =
				/* i2s1_sdo0_m1 */
				<3 RK_PB5 1 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		i2s1m1_sdo1: i2s1m1-sdo1 {
			rockchip,pins =
				/* i2s1_sdo1_m1 */
				<3 RK_PB6 1 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		i2s1m1_sdo2: i2s1m1-sdo2 {
			rockchip,pins =
				/* i2s1_sdo2_m1 */
				<3 RK_PB7 1 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		i2s1m1_sdo3: i2s1m1-sdo3 {
			rockchip,pins =
				/* i2s1_sdo3_m1 */
				<3 RK_PC0 1 &pcfg_pull_none>;
		};
	};

	i2s2 {
		/omit-if-no-ref/
		i2s2m0_lrck: i2s2m0-lrck {
			rockchip,pins =
				/* i2s2_lrck_m0 */
				<1 RK_PD6 1 &pcfg_pull_none_smt>;
		};

		/omit-if-no-ref/
		i2s2m0_mclk: i2s2m0-mclk {
			rockchip,pins =
				/* i2s2_mclk_m0 */
				<2 RK_PA1 1 &pcfg_pull_none_smt>;
		};

		/omit-if-no-ref/
		i2s2m0_sclk: i2s2m0-sclk {
			rockchip,pins =
				/* i2s2_sclk_m0 */
				<1 RK_PD5 1 &pcfg_pull_none_smt>;
		};

		/omit-if-no-ref/
		i2s2m0_sdi: i2s2m0-sdi {
			rockchip,pins =
				/* i2s2_sdi_m0 */
				<2 RK_PA0 1 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		i2s2m0_sdo: i2s2m0-sdo {
			rockchip,pins =
				/* i2s2_sdo_m0 */
				<1 RK_PD7 1 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		i2s2m1_lrck: i2s2m1-lrck {
			rockchip,pins =
				/* i2s2_lrck_m1 */
				<4 RK_PA1 3 &pcfg_pull_none_smt>;
		};

		/omit-if-no-ref/
		i2s2m1_mclk: i2s2m1-mclk {
			rockchip,pins =
				/* i2s2_mclk_m1 */
				<3 RK_PD6 3 &pcfg_pull_none_smt>;
		};

		/omit-if-no-ref/
		i2s2m1_sclk: i2s2m1-sclk {
			rockchip,pins =
				/* i2s2_sclk_m1 */
				<4 RK_PB1 4 &pcfg_pull_none_smt>;
		};

		/omit-if-no-ref/
		i2s2m1_sdi: i2s2m1-sdi {
			rockchip,pins =
				/* i2s2_sdi_m1 */
				<3 RK_PD4 4 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		i2s2m1_sdo: i2s2m1-sdo {
			rockchip,pins =
				/* i2s2_sdo_m1 */
				<3 RK_PD5 4 &pcfg_pull_none>;
		};
	};

	isp {
		/omit-if-no-ref/
		isp_pins: isp-pins {
			rockchip,pins =
				/* isp_flash_trigin */
				<3 RK_PC1 2 &pcfg_pull_none>,
				/* isp_flash_trigout */
				<3 RK_PC3 2 &pcfg_pull_none>,
				/* isp_prelight_trigout */
				<3 RK_PC2 2 &pcfg_pull_none>;
		};
	};

	jtag {
		/omit-if-no-ref/
		jtagm0_pins: jtagm0-pins {
			rockchip,pins =
				/* jtag_cpu_mcu_tck_m0 */
				<0 RK_PD1 2 &pcfg_pull_none>,
				/* jtag_cpu_mcu_tms_m0 */
				<0 RK_PD0 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		jtagm1_pins: jtagm1-pins {
			rockchip,pins =
				/* jtag_cpu_mcu_tck_m1 */
				<1 RK_PB5 2 &pcfg_pull_none>,
				/* jtag_cpu_mcu_tms_m1 */
				<1 RK_PB6 2 &pcfg_pull_none>;
		};
	};

	npu {
		/omit-if-no-ref/
		npu_pins: npu-pins {
			rockchip,pins =
				/* npu_avs */
				<0 RK_PC1 3 &pcfg_pull_none>;
		};
	};

	pcie20 {
		/omit-if-no-ref/
		pcie20m0_pins: pcie20m0-pins {
			rockchip,pins =
				/* pcie20_clkreqn_m0 */
				<0 RK_PA6 1 &pcfg_pull_none>,
				/* pcie20_perstn_m0 */
				<0 RK_PB5 2 &pcfg_pull_none>,
				/* pcie20_waken_m0 */
				<0 RK_PB6 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		pcie20m1_pins: pcie20m1-pins {
			rockchip,pins =
				/* pcie20_clkreqn_m1 */
				<3 RK_PA6 4 &pcfg_pull_none>,
				/* pcie20_perstn_m1 */
				<3 RK_PB0 4 &pcfg_pull_none>,
				/* pcie20_waken_m1 */
				<3 RK_PA7 4 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		pcie20_buttonrstn: pcie20-buttonrstn {
			rockchip,pins =
				/* pcie20_buttonrstn */
				<0 RK_PB0 3 &pcfg_pull_none>;
		};
	};

	pdm {
		/omit-if-no-ref/
		pdmm0_clk0: pdmm0-clk0 {
			rockchip,pins =
				/* pdm_clk0_m0 */
				<3 RK_PA6 3 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		pdmm0_clk1: pdmm0-clk1 {
			rockchip,pins =
				/* pdm_clk1_m0 */
				<3 RK_PA2 3 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		pdmm0_sdi0: pdmm0-sdi0 {
			rockchip,pins =
				/* pdm_sdi0_m0 */
				<3 RK_PB1 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		pdmm0_sdi1: pdmm0-sdi1 {
			rockchip,pins =
				/* pdm_sdi1_m0 */
				<3 RK_PB0 3 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		pdmm0_sdi2: pdmm0-sdi2 {
			rockchip,pins =
				/* pdm_sdi2_m0 */
				<3 RK_PA7 3 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		pdmm0_sdi3: pdmm0-sdi3 {
			rockchip,pins =
				/* pdm_sdi3_m0 */
				<3 RK_PA0 3 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		pdmm1_clk0: pdmm1-clk0 {
			rockchip,pins =
				/* pdm_clk0_m1 */
				<4 RK_PB7 4 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		pdmm1_clk1: pdmm1-clk1 {
			rockchip,pins =
				/* pdm_clk1_m1 */
				<4 RK_PB1 5 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		pdmm1_sdi0: pdmm1-sdi0 {
			rockchip,pins =
				/* pdm_sdi0_m1 */
				<4 RK_PA7 4 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		pdmm1_sdi1: pdmm1-sdi1 {
			rockchip,pins =
				/* pdm_sdi1_m1 */
				<4 RK_PB0 4 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		pdmm1_sdi2: pdmm1-sdi2 {
			rockchip,pins =
				/* pdm_sdi2_m1 */
				<4 RK_PA5 4 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		pdmm1_sdi3: pdmm1-sdi3 {
			rockchip,pins =
				/* pdm_sdi3_m1 */
				<4 RK_PA6 4 &pcfg_pull_none>;
		};
	};

	pmic {
		/omit-if-no-ref/
		pmic_int: pmic-int {
			rockchip,pins =
				<0 RK_PA3 0 &pcfg_pull_up>;
		};

		/omit-if-no-ref/
		soc_slppin_gpio: soc-slppin-gpio {
			rockchip,pins =
				<0 RK_PA2 0 &pcfg_output_low>;
		};

		/omit-if-no-ref/
		soc_slppin_slp: soc-slppin-slp {
			rockchip,pins =
				<0 RK_PA2 1 &pcfg_pull_none>;
		};
	};

	pmu {
		/omit-if-no-ref/
		pmu_pins: pmu-pins {
			rockchip,pins =
				/* pmu_debug */
				<0 RK_PA5 3 &pcfg_pull_none>;
		};
	};

	pwm0 {
		/omit-if-no-ref/
		pwm0m0_pins: pwm0m0-pins {
			rockchip,pins =
				/* pwm0_m0 */
				<0 RK_PC3 2 &pcfg_pull_none_drv_level_1>;
		};

		/omit-if-no-ref/
		pwm0m1_pins: pwm0m1-pins {
			rockchip,pins =
				/* pwm0_m1 */
				<1 RK_PC5 4 &pcfg_pull_none_drv_level_1>;
		};
	};

	pwm1 {
		/omit-if-no-ref/
		pwm1m0_pins: pwm1m0-pins {
			rockchip,pins =
				/* pwm1_m0 */
				<0 RK_PC4 2 &pcfg_pull_none_drv_level_1>;
		};

		/omit-if-no-ref/
		pwm1m1_pins: pwm1m1-pins {
			rockchip,pins =
				/* pwm1_m1 */
				<1 RK_PC6 4 &pcfg_pull_none_drv_level_1>;
		};
	};

	pwm2 {
		/omit-if-no-ref/
		pwm2m0_pins: pwm2m0-pins {
			rockchip,pins =
				/* pwm2_m0 */
				<0 RK_PC5 2 &pcfg_pull_none_drv_level_1>;
		};

		/omit-if-no-ref/
		pwm2m1_pins: pwm2m1-pins {
			rockchip,pins =
				/* pwm2_m1 */
				<1 RK_PC7 3 &pcfg_pull_none_drv_level_1>;
		};
	};

	pwm3 {
		/omit-if-no-ref/
		pwm3m0_pins: pwm3m0-pins {
			rockchip,pins =
				/* pwm3_m0 */
				<0 RK_PA7 1 &pcfg_pull_none_drv_level_1>;
		};

		/omit-if-no-ref/
		pwm3m1_pins: pwm3m1-pins {
			rockchip,pins =
				/* pwm3_m1 */
				<1 RK_PD0 3 &pcfg_pull_none_drv_level_1>;
		};
	};

	pwm4 {
		/omit-if-no-ref/
		pwm4m0_pins: pwm4m0-pins {
			rockchip,pins =
				/* pwm4_m0 */
				<0 RK_PB7 2 &pcfg_pull_none_drv_level_1>;
		};

		/omit-if-no-ref/
		pwm4m1_pins: pwm4m1-pins {
			rockchip,pins =
				/* pwm4_m1 */
				<1 RK_PD1 4 &pcfg_pull_none_drv_level_1>;
		};
	};

	pwm5 {
		/omit-if-no-ref/
		pwm5m0_pins: pwm5m0-pins {
			rockchip,pins =
				/* pwm5_m0 */
				<0 RK_PC2 2 &pcfg_pull_none_drv_level_1>;
		};

		/omit-if-no-ref/
		pwm5m1_pins: pwm5m1-pins {
			rockchip,pins =
				/* pwm5_m1 */
				<1 RK_PD2 4 &pcfg_pull_none_drv_level_1>;
		};
	};

	pwm6 {
		/omit-if-no-ref/
		pwm6m0_pins: pwm6m0-pins {
			rockchip,pins =
				/* pwm6_m0 */
				<0 RK_PC1 2 &pcfg_pull_none_drv_level_1>;
		};

		/omit-if-no-ref/
		pwm6m1_pins: pwm6m1-pins {
			rockchip,pins =
				/* pwm6_m1 */
				<1 RK_PD3 4 &pcfg_pull_none_drv_level_1>;
		};
	};

	pwm7 {
		/omit-if-no-ref/
		pwm7m0_pins: pwm7m0-pins {
			rockchip,pins =
				/* pwm7_m0 */
				<0 RK_PC0 2 &pcfg_pull_none_drv_level_1>;
		};

		/omit-if-no-ref/
		pwm7m1_pins: pwm7m1-pins {
			rockchip,pins =
				/* pwm7_m1 */
				<1 RK_PD4 4 &pcfg_pull_none_drv_level_1>;
		};
	};

	pwm8 {
		/omit-if-no-ref/
		pwm8m0_pins: pwm8m0-pins {
			rockchip,pins =
				/* pwm8_m0 */
				<3 RK_PA4 2 &pcfg_pull_none_drv_level_1>;
		};

		/omit-if-no-ref/
		pwm8m1_pins: pwm8m1-pins {
			rockchip,pins =
				/* pwm8_m1 */
				<1 RK_PC1 4 &pcfg_pull_none_drv_level_1>;
		};
	};

	pwm9 {
		/omit-if-no-ref/
		pwm9m0_pins: pwm9m0-pins {
			rockchip,pins =
				/* pwm9_m0 */
				<3 RK_PA5 2 &pcfg_pull_none_drv_level_1>;
		};

		/omit-if-no-ref/
		pwm9m1_pins: pwm9m1-pins {
			rockchip,pins =
				/* pwm9_m1 */
				<1 RK_PC2 4 &pcfg_pull_none_drv_level_1>;
		};
	};

	pwm10 {
		/omit-if-no-ref/
		pwm10m0_pins: pwm10m0-pins {
			rockchip,pins =
				/* pwm10_m0 */
				<1 RK_PB5 5 &pcfg_pull_none_drv_level_1>;
		};

		/omit-if-no-ref/
		pwm10m1_pins: pwm10m1-pins {
			rockchip,pins =
				/* pwm10_m1 */
				<1 RK_PC3 4 &pcfg_pull_none_drv_level_1>;
		};
	};

	pwm11 {
		/omit-if-no-ref/
		pwm11m0_pins: pwm11m0-pins {
			rockchip,pins =
				/* pwm11_m0 */
				<1 RK_PB6 5 &pcfg_pull_none_drv_level_1>;
		};

		/omit-if-no-ref/
		pwm11m1_pins: pwm11m1-pins {
			rockchip,pins =
				/* pwm11_m1 */
				<1 RK_PC4 4 &pcfg_pull_none_drv_level_1>;
		};
	};

	pwm12 {
		/omit-if-no-ref/
		pwm12m0_pins: pwm12m0-pins {
			rockchip,pins =
				/* pwm12_m0 */
				<4 RK_PA1 4 &pcfg_pull_none_drv_level_1>;
		};

		/omit-if-no-ref/
		pwm12m1_pins: pwm12m1-pins {
			rockchip,pins =
				/* pwm12_m1 */
				<3 RK_PB4 5 &pcfg_pull_none_drv_level_1>;
		};
	};

	pwm13 {
		/omit-if-no-ref/
		pwm13m0_pins: pwm13m0-pins {
			rockchip,pins =
				/* pwm13_m0 */
				<4 RK_PA4 3 &pcfg_pull_none_drv_level_1>;
		};

		/omit-if-no-ref/
		pwm13m1_pins: pwm13m1-pins {
			rockchip,pins =
				/* pwm13_m1 */
				<3 RK_PB5 5 &pcfg_pull_none_drv_level_1>;
		};
	};

	pwm14 {
		/omit-if-no-ref/
		pwm14m0_pins: pwm14m0-pins {
			rockchip,pins =
				/* pwm14_m0 */
				<3 RK_PC5 4 &pcfg_pull_none_drv_level_1>;
		};

		/omit-if-no-ref/
		pwm14m1_pins: pwm14m1-pins {
			rockchip,pins =
				/* pwm14_m1 */
				<1 RK_PD7 5 &pcfg_pull_none_drv_level_1>;
		};
	};

	pwm15 {
		/omit-if-no-ref/
		pwm15m0_pins: pwm15m0-pins {
			rockchip,pins =
				/* pwm15_m0 */
				<3 RK_PC6 4 &pcfg_pull_none_drv_level_1>;
		};

		/omit-if-no-ref/
		pwm15m1_pins: pwm15m1-pins {
			rockchip,pins =
				/* pwm15_m1 */
				<2 RK_PA0 5 &pcfg_pull_none_drv_level_1>;
		};
	};

	pwr {
		/omit-if-no-ref/
		pwr_pins: pwr-pins {
			rockchip,pins =
				/* pwr_ctrl0 */
				<0 RK_PA2 1 &pcfg_pull_none>,
				/* pwr_ctrl1 */
				<0 RK_PA3 1 &pcfg_pull_none>;
		};
	};

	ref {
		/omit-if-no-ref/
		ref_pins: ref-pins {
			rockchip,pins =
				/* ref_clk_out */
				<0 RK_PA0 1 &pcfg_pull_none>;
		};
	};

	rgmii {
		/omit-if-no-ref/
		rgmiim0_miim: rgmiim0-miim {
			rockchip,pins =
				/* rgmii_mdc_m0 */
				<4 RK_PB2 2 &pcfg_pull_none>,
				/* rgmii_mdio_m0 */
				<4 RK_PB3 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		rgmiim0_rx_er: rgmiim0-rx_er {
			rockchip,pins =
				/* rgmii_rxer_m0 */
				<4 RK_PB0 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		rgmiim0_rx_bus2: rgmiim0-rx_bus2 {
			rockchip,pins =
				/* rgmii_rxd0_m0 */
				<4 RK_PA5 2 &pcfg_pull_none>,
				/* rgmii_rxd1_m0 */
				<4 RK_PA6 2 &pcfg_pull_none>,
				/* rgmii_rxdv_m0 */
				<4 RK_PA7 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		rgmiim0_tx_bus2: rgmiim0-tx_bus2 {
			rockchip,pins =
				/* rgmii_txd0_m0 */
				<4 RK_PA2 2 &pcfg_pull_none>,
				/* rgmii_txd1_m0 */
				<4 RK_PA3 2 &pcfg_pull_none>,
				/* rgmii_txen_m0 */
				<4 RK_PA4 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		rgmiim0_rgmii_clk: rgmiim0-rgmii_clk {
			rockchip,pins =
				/* rgmii_rxclk_m0 */
				<4 RK_PA1 2 &pcfg_pull_none>,
				/* rgmii_txclk_m0 */
				<3 RK_PD6 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		rgmiim0_rgmii_bus: rgmiim0-rgmii_bus {
			rockchip,pins =
				/* rgmii_rxd2_m0 */
				<3 RK_PD7 2 &pcfg_pull_none>,
				/* rgmii_rxd3_m0 */
				<4 RK_PA0 2 &pcfg_pull_none>,
				/* rgmii_txd2_m0 */
				<3 RK_PD4 2 &pcfg_pull_none>,
				/* rgmii_txd3_m0 */
				<3 RK_PD5 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		rgmiim0_clk: rgmiim0-clk {
			rockchip,pins =
				/* rgmiim0_clk */
				<4 RK_PB7 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		rgmiim1_miim: rgmiim1-miim {
			rockchip,pins =
				/* rgmii_mdc_m1 */
				<1 RK_PC7 2 &pcfg_pull_none>,
				/* rgmii_mdio_m1 */
				<1 RK_PD0 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		rgmiim1_rx_er: rgmiim1-rx_er {
			rockchip,pins =
				/* rgmii_rxer_m1 */
				<2 RK_PA0 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		rgmiim1_rx_bus2: rgmiim1-rx_bus2 {
			rockchip,pins =
				/* rgmii_rxd0_m1 */
				<1 RK_PD4 2 &pcfg_pull_none>,
				/* rgmii_rxd1_m1 */
				<1 RK_PD7 2 &pcfg_pull_none>,
				/* rgmii_rxdv_m1 */
				<1 RK_PD6 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		rgmiim1_tx_bus2: rgmiim1-tx_bus2 {
			rockchip,pins =
				/* rgmii_txd0_m1 */
				<1 RK_PD1 2 &pcfg_pull_none>,
				/* rgmii_txd1_m1 */
				<1 RK_PD2 2 &pcfg_pull_none>,
				/* rgmii_txen_m1 */
				<1 RK_PD3 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		rgmiim1_rgmii_clk: rgmiim1-rgmii_clk {
			rockchip,pins =
				/* rgmii_rxclk_m1 */
				<1 RK_PC6 2 &pcfg_pull_none>,
				/* rgmii_txclk_m1 */
				<1 RK_PC3 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		rgmiim1_rgmii_bus: rgmiim1-rgmii_bus {
			rockchip,pins =
				/* rgmii_rxd2_m1 */
				<1 RK_PC4 2 &pcfg_pull_none>,
				/* rgmii_rxd3_m1 */
				<1 RK_PC5 2 &pcfg_pull_none>,
				/* rgmii_txd2_m1 */
				<1 RK_PC1 2 &pcfg_pull_none>,
				/* rgmii_txd3_m1 */
				<1 RK_PC2 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		rgmiim1_clk: rgmiim1-clk {
			rockchip,pins =
				/* rgmiim1_clk */
				<1 RK_PD5 2 &pcfg_pull_none>;
		};
	};

	rmii {
		/omit-if-no-ref/
		rmii_pins: rmii-pins {
			rockchip,pins =
				/* rmii_clk */
				<1 RK_PD5 5 &pcfg_pull_none>,
				/* rmii_mdc */
				<1 RK_PC7 5 &pcfg_pull_none>,
				/* rmii_mdio */
				<1 RK_PD0 5 &pcfg_pull_none>,
				/* rmii_rxd0 */
				<1 RK_PD4 5 &pcfg_pull_none>,
				/* rmii_rxd1 */
				<1 RK_PD7 6 &pcfg_pull_none>,
				/* rmii_rxdv_crs */
				<1 RK_PD6 5 &pcfg_pull_none>,
				/* rmii_rxer */
				<2 RK_PA0 6 &pcfg_pull_none>,
				/* rmii_txd0 */
				<1 RK_PD1 5 &pcfg_pull_none>,
				/* rmii_txd1 */
				<1 RK_PD2 5 &pcfg_pull_none>,
				/* rmii_txen */
				<1 RK_PD3 5 &pcfg_pull_none>;
		};
	};

	sdmmc0 {
		/omit-if-no-ref/
		sdmmc0_bus4: sdmmc0-bus4 {
			rockchip,pins =
				/* sdmmc0_d0 */
				<1 RK_PB3 1 &pcfg_pull_up_drv_level_2>,
				/* sdmmc0_d1 */
				<1 RK_PB4 1 &pcfg_pull_up_drv_level_2>,
				/* sdmmc0_d2 */
				<1 RK_PB5 1 &pcfg_pull_up_drv_level_2>,
				/* sdmmc0_d3 */
				<1 RK_PB6 1 &pcfg_pull_up_drv_level_2>;
		};

		/omit-if-no-ref/
		sdmmc0_clk: sdmmc0-clk {
			rockchip,pins =
				/* sdmmc0_clk */
				<1 RK_PC0 1 &pcfg_pull_up_drv_level_2>;
		};

		/omit-if-no-ref/
		sdmmc0_cmd: sdmmc0-cmd {
			rockchip,pins =
				/* sdmmc0_cmd */
				<1 RK_PB7 1 &pcfg_pull_up_drv_level_2>;
		};

		/omit-if-no-ref/
		sdmmc0_det: sdmmc0-det {
			rockchip,pins =
				/* sdmmc0_detn */
				<0 RK_PA4 1 &pcfg_pull_up>;
		};

		/omit-if-no-ref/
		sdmmc0_pwren: sdmmc0-pwren {
			rockchip,pins =
				/* sdmmc0_pwren */
				<0 RK_PA5 1 &pcfg_pull_none>;
		};
	};

	sdmmc1 {
		/omit-if-no-ref/
		sdmmc1_bus4: sdmmc1-bus4 {
			rockchip,pins =
				/* sdmmc1_d0 */
				<1 RK_PC1 1 &pcfg_pull_up_drv_level_2>,
				/* sdmmc1_d1 */
				<1 RK_PC2 1 &pcfg_pull_up_drv_level_2>,
				/* sdmmc1_d2 */
				<1 RK_PC3 1 &pcfg_pull_up_drv_level_2>,
				/* sdmmc1_d3 */
				<1 RK_PC4 1 &pcfg_pull_up_drv_level_2>;
		};

		/omit-if-no-ref/
		sdmmc1_clk: sdmmc1-clk {
			rockchip,pins =
				/* sdmmc1_clk */
				<1 RK_PC6 1 &pcfg_pull_up_drv_level_2>;
		};

		/omit-if-no-ref/
		sdmmc1_cmd: sdmmc1-cmd {
			rockchip,pins =
				/* sdmmc1_cmd */
				<1 RK_PC5 1 &pcfg_pull_up_drv_level_2>;
		};

		/omit-if-no-ref/
		sdmmc1_det: sdmmc1-det {
			rockchip,pins =
				/* sdmmc1_detn */
				<1 RK_PD0 1 &pcfg_pull_up>;
		};

		/omit-if-no-ref/
		sdmmc1_pwren: sdmmc1-pwren {
			rockchip,pins =
				/* sdmmc1_pwren */
				<1 RK_PC7 1 &pcfg_pull_none>;
		};
	};

	spdif {
		/omit-if-no-ref/
		spdifm0_pins: spdifm0-pins {
			rockchip,pins =
				/* spdif_tx_m0 */
				<3 RK_PA1 3 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		spdifm1_pins: spdifm1-pins {
			rockchip,pins =
				/* spdif_tx_m1 */
				<0 RK_PB7 4 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		spdifm2_pins: spdifm2-pins {
			rockchip,pins =
				/* spdif_tx_m2 */
				<1 RK_PB7 2 &pcfg_pull_none>;
		};
	};

	spi0 {
		/omit-if-no-ref/
		spi0m0_pins: spi0m0-pins {
			rockchip,pins =
				/* spi0_clk_m0 */
				<0 RK_PC3 3 &pcfg_pull_none_drv_level_3>,
				/* spi0_miso_m0 */
				<0 RK_PC5 3 &pcfg_pull_none_drv_level_3>,
				/* spi0_mosi_m0 */
				<0 RK_PC4 3 &pcfg_pull_none_drv_level_3>;
		};

		/omit-if-no-ref/
		spi0m0_csn0: spi0m0-csn0 {
			rockchip,pins =
				/* spi0m0_csn0 */
				<0 RK_PC2 3 &pcfg_pull_none_drv_level_3>;
		};
		/omit-if-no-ref/
		spi0m0_csn1: spi0m0-csn1 {
			rockchip,pins =
				/* spi0m0_csn1 */
				<0 RK_PB7 1 &pcfg_pull_none_drv_level_3>;
		};

		/omit-if-no-ref/
		spi0m1_pins: spi0m1-pins {
			rockchip,pins =
				/* spi0_clk_m1 */
				<3 RK_PB5 4 &pcfg_pull_none_drv_level_3>,
				/* spi0_miso_m1 */
				<3 RK_PC0 4 &pcfg_pull_none_drv_level_3>,
				/* spi0_mosi_m1 */
				<3 RK_PB4 4 &pcfg_pull_none_drv_level_3>;
		};

		/omit-if-no-ref/
		spi0m1_csn0: spi0m1-csn0 {
			rockchip,pins =
				/* spi0m1_csn0 */
				<3 RK_PB7 4 &pcfg_pull_none_drv_level_3>;
		};
		/omit-if-no-ref/
		spi0m1_csn1: spi0m1-csn1 {
			rockchip,pins =
				/* spi0m1_csn1 */
				<3 RK_PB6 4 &pcfg_pull_none_drv_level_3>;
		};
	};

	spi1 {
		/omit-if-no-ref/
		spi1m0_pins: spi1m0-pins {
			rockchip,pins =
				/* spi1_clk_m0 */
				<3 RK_PD6 4 &pcfg_pull_none_drv_level_3>,
				/* spi1_miso_m0 */
				<4 RK_PA3 4 &pcfg_pull_none_drv_level_3>,
				/* spi1_mosi_m0 */
				<4 RK_PA2 4 &pcfg_pull_none_drv_level_3>;
		};

		/omit-if-no-ref/
		spi1m0_csn0: spi1m0-csn0 {
			rockchip,pins =
				/* spi1m0_csn0 */
				<3 RK_PD7 4 &pcfg_pull_none_drv_level_3>;
		};
		/omit-if-no-ref/
		spi1m0_csn1: spi1m0-csn1 {
			rockchip,pins =
				/* spi1m0_csn1 */
				<4 RK_PA0 4 &pcfg_pull_none_drv_level_3>;
		};

		/omit-if-no-ref/
		spi1m1_pins: spi1m1-pins {
			rockchip,pins =
				/* spi1_clk_m1 */
				<1 RK_PC0 4 &pcfg_pull_none_drv_level_3>,
				/* spi1_miso_m1 */
				<1 RK_PB4 4 &pcfg_pull_none_drv_level_3>,
				/* spi1_mosi_m1 */
				<1 RK_PB3 4 &pcfg_pull_none_drv_level_3>;
		};

		/omit-if-no-ref/
		spi1m1_csn0: spi1m1-csn0 {
			rockchip,pins =
				/* spi1m1_csn0 */
				<1 RK_PB6 4 &pcfg_pull_none_drv_level_3>;
		};
		/omit-if-no-ref/
		spi1m1_csn1: spi1m1-csn1 {
			rockchip,pins =
				/* spi1m1_csn1 */
				<1 RK_PB5 4 &pcfg_pull_none_drv_level_3>;
		};
	};

	spi2 {
		/omit-if-no-ref/
		spi2m0_pins: spi2m0-pins {
			rockchip,pins =
				/* spi2_clk_m0 */
				<4 RK_PB6 4 &pcfg_pull_none_drv_level_3>,
				/* spi2_miso_m0 */
				<3 RK_PD2 4 &pcfg_pull_none_drv_level_3>,
				/* spi2_mosi_m0 */
				<3 RK_PD3 4 &pcfg_pull_none_drv_level_3>;
		};

		/omit-if-no-ref/
		spi2m0_csn0: spi2m0-csn0 {
			rockchip,pins =
				/* spi2m0_csn0 */
				<4 RK_PB5 4 &pcfg_pull_none_drv_level_3>;
		};
		/omit-if-no-ref/
		spi2m0_csn1: spi2m0-csn1 {
			rockchip,pins =
				/* spi2m0_csn1 */
				<4 RK_PB4 4 &pcfg_pull_none_drv_level_3>;
		};

		/omit-if-no-ref/
		spi2m1_pins: spi2m1-pins {
			rockchip,pins =
				/* spi2_clk_m1 */
				<2 RK_PA1 4 &pcfg_pull_none_drv_level_3>,
				/* spi2_miso_m1 */
				<2 RK_PA0 4 &pcfg_pull_none_drv_level_3>,
				/* spi2_mosi_m1 */
				<1 RK_PD7 4 &pcfg_pull_none_drv_level_3>;
		};

		/omit-if-no-ref/
		spi2m1_csn0: spi2m1-csn0 {
			rockchip,pins =
				/* spi2m1_csn0 */
				<1 RK_PD6 4 &pcfg_pull_none_drv_level_3>;
		};
		/omit-if-no-ref/
		spi2m1_csn1: spi2m1-csn1 {
			rockchip,pins =
				/* spi2m1_csn1 */
				<1 RK_PD5 4 &pcfg_pull_none_drv_level_3>;
		};
	};

	tsadc {
		/omit-if-no-ref/
		tsadcm0_pins: tsadcm0-pins {
			rockchip,pins =
				/* tsadc_shut_m0 */
				<0 RK_PA1 1 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		tsadcm1_pins: tsadcm1-pins {
			rockchip,pins =
				/* tsadc_shut_m1 */
				<0 RK_PA2 2 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		tsadc_shut_org: tsadc-shut-org {
			rockchip,pins =
				/* tsadc_shut_org */
				<0 RK_PA1 2 &pcfg_pull_none>;
		};
	};

	uart0 {
		/omit-if-no-ref/
		uart0m0_xfer: uart0m0-xfer {
			rockchip,pins =
				/* uart0_rx_m0 */
				<0 RK_PD0 1 &pcfg_pull_up>,
				/* uart0_tx_m0 */
				<0 RK_PD1 1 &pcfg_pull_up>;
		};

		/omit-if-no-ref/
		uart0m1_xfer: uart0m1-xfer {
			rockchip,pins =
				/* uart0_rx_m1 */
				<1 RK_PB3 2 &pcfg_pull_up>,
				/* uart0_tx_m1 */
				<1 RK_PB4 2 &pcfg_pull_up>;
		};
	};

	uart1 {
		/omit-if-no-ref/
		uart1m0_xfer: uart1m0-xfer {
			rockchip,pins =
				/* uart1_rx_m0 */
				<1 RK_PD1 1 &pcfg_pull_up>,
				/* uart1_tx_m0 */
				<1 RK_PD2 1 &pcfg_pull_up>;
		};

		/omit-if-no-ref/
		uart1m0_ctsn: uart1m0-ctsn {
			rockchip,pins =
				/* uart1m0_ctsn */
				<1 RK_PD4 1 &pcfg_pull_none>;
		};
		/omit-if-no-ref/
		uart1m0_rtsn: uart1m0-rtsn {
			rockchip,pins =
				/* uart1m0_rtsn */
				<1 RK_PD3 1 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		uart1m1_xfer: uart1m1-xfer {
			rockchip,pins =
				/* uart1_rx_m1 */
				<4 RK_PA6 3 &pcfg_pull_up>,
				/* uart1_tx_m1 */
				<4 RK_PA5 3 &pcfg_pull_up>;
		};

		/omit-if-no-ref/
		uart1m1_ctsn: uart1m1-ctsn {
			rockchip,pins =
				/* uart1m1_ctsn */
				<4 RK_PB0 3 &pcfg_pull_none>;
		};
		/omit-if-no-ref/
		uart1m1_rtsn: uart1m1-rtsn {
			rockchip,pins =
				/* uart1m1_rtsn */
				<4 RK_PA7 3 &pcfg_pull_none>;
		};
	};

	uart2 {
		/omit-if-no-ref/
		uart2m0_xfer: uart2m0-xfer {
			rockchip,pins =
				/* uart2_rx_m0 */
				<0 RK_PC1 1 &pcfg_pull_up>,
				/* uart2_tx_m0 */
				<0 RK_PC0 1 &pcfg_pull_up>;
		};

		/omit-if-no-ref/
		uart2m0_ctsn: uart2m0-ctsn {
			rockchip,pins =
				/* uart2m0_ctsn */
				<0 RK_PC2 1 &pcfg_pull_none>;
		};
		/omit-if-no-ref/
		uart2m0_rtsn: uart2m0-rtsn {
			rockchip,pins =
				/* uart2m0_rtsn */
				<0 RK_PC3 1 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		uart2m1_xfer: uart2m1-xfer {
			rockchip,pins =
				/* uart2_rx_m1 */
				<3 RK_PA1 2 &pcfg_pull_up>,
				/* uart2_tx_m1 */
				<3 RK_PA0 2 &pcfg_pull_up>;
		};

		/omit-if-no-ref/
		uart2m1_ctsn: uart2m1-ctsn {
			rockchip,pins =
				/* uart2m1_ctsn */
				<3 RK_PA2 2 &pcfg_pull_none>;
		};
		/omit-if-no-ref/
		uart2m1_rtsn: uart2m1-rtsn {
			rockchip,pins =
				/* uart2m1_rtsn */
				<3 RK_PA3 2 &pcfg_pull_none>;
		};
	};

	uart3 {
		/omit-if-no-ref/
		uart3m0_xfer: uart3m0-xfer {
			rockchip,pins =
				/* uart3_rx_m0 */
				<4 RK_PB5 6 &pcfg_pull_up>,
				/* uart3_tx_m0 */
				<4 RK_PB4 6 &pcfg_pull_up>;
		};

		/omit-if-no-ref/
		uart3m0_ctsn: uart3m0-ctsn {
			rockchip,pins =
				/* uart3m0_ctsn */
				<4 RK_PB6 3 &pcfg_pull_none>;
		};
		/omit-if-no-ref/
		uart3m0_rtsn: uart3m0-rtsn {
			rockchip,pins =
				/* uart3m0_rtsn */
				<3 RK_PD1 4 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		uart3m1_xfer: uart3m1-xfer {
			rockchip,pins =
				/* uart3_rx_m1 */
				<3 RK_PC0 3 &pcfg_pull_up>,
				/* uart3_tx_m1 */
				<3 RK_PB7 3 &pcfg_pull_up>;
		};

		/omit-if-no-ref/
		uart3m1_ctsn: uart3m1-ctsn {
			rockchip,pins =
				/* uart3m1_ctsn */
				<3 RK_PB6 3 &pcfg_pull_none>;
		};
		/omit-if-no-ref/
		uart3m1_rtsn: uart3m1-rtsn {
			rockchip,pins =
				/* uart3m1_rtsn */
				<3 RK_PC1 3 &pcfg_pull_none>;
		};
	};

	uart4 {
		/omit-if-no-ref/
		uart4m0_xfer: uart4m0-xfer {
			rockchip,pins =
				/* uart4_rx_m0 */
				<3 RK_PD1 3 &pcfg_pull_up>,
				/* uart4_tx_m0 */
				<3 RK_PD0 3 &pcfg_pull_up>;
		};

		/omit-if-no-ref/
		uart4m0_ctsn: uart4m0-ctsn {
			rockchip,pins =
				/* uart4m0_ctsn */
				<3 RK_PC5 3 &pcfg_pull_none>;
		};
		/omit-if-no-ref/
		uart4m0_rtsn: uart4m0-rtsn {
			rockchip,pins =
				/* uart4m0_rtsn */
				<3 RK_PC6 3 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		uart4m1_xfer: uart4m1-xfer {
			rockchip,pins =
				/* uart4_rx_m1 */
				<1 RK_PD5 3 &pcfg_pull_up>,
				/* uart4_tx_m1 */
				<1 RK_PD6 3 &pcfg_pull_up>;
		};

		/omit-if-no-ref/
		uart4m1_ctsn: uart4m1-ctsn {
			rockchip,pins =
				/* uart4m1_ctsn */
				<2 RK_PA0 3 &pcfg_pull_none>;
		};
		/omit-if-no-ref/
		uart4m1_rtsn: uart4m1-rtsn {
			rockchip,pins =
				/* uart4m1_rtsn */
				<1 RK_PD7 3 &pcfg_pull_none>;
		};
	};

	uart5 {
		/omit-if-no-ref/
		uart5m0_xfer: uart5m0-xfer {
			rockchip,pins =
				/* uart5_rx_m0 */
				<1 RK_PB7 3 &pcfg_pull_up>,
				/* uart5_tx_m0 */
				<1 RK_PC0 3 &pcfg_pull_up>;
		};

		/omit-if-no-ref/
		uart5m0_ctsn: uart5m0-ctsn {
			rockchip,pins =
				/* uart5m0_ctsn */
				<1 RK_PB5 3 &pcfg_pull_none>;
		};
		/omit-if-no-ref/
		uart5m0_rtsn: uart5m0-rtsn {
			rockchip,pins =
				/* uart5m0_rtsn */
				<1 RK_PB6 3 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		uart5m1_xfer: uart5m1-xfer {
			rockchip,pins =
				/* uart5_rx_m1 */
				<3 RK_PA7 5 &pcfg_pull_up>,
				/* uart5_tx_m1 */
				<3 RK_PA6 5 &pcfg_pull_up>;
		};

		/omit-if-no-ref/
		uart5m1_ctsn: uart5m1-ctsn {
			rockchip,pins =
				/* uart5m1_ctsn */
				<3 RK_PA0 5 &pcfg_pull_none>;
		};
		/omit-if-no-ref/
		uart5m1_rtsn: uart5m1-rtsn {
			rockchip,pins =
				/* uart5m1_rtsn */
				<3 RK_PA1 5 &pcfg_pull_none>;
		};
	};

	uart6 {
		/omit-if-no-ref/
		uart6m0_xfer: uart6m0-xfer {
			rockchip,pins =
				/* uart6_rx_m0 */
				<0 RK_PC7 1 &pcfg_pull_up>,
				/* uart6_tx_m0 */
				<0 RK_PC6 1 &pcfg_pull_up>;
		};

		/omit-if-no-ref/
		uart6m0_ctsn: uart6m0-ctsn {
			rockchip,pins =
				/* uart6m0_ctsn */
				<0 RK_PC4 1 &pcfg_pull_none>;
		};
		/omit-if-no-ref/
		uart6m0_rtsn: uart6m0-rtsn {
			rockchip,pins =
				/* uart6m0_rtsn */
				<0 RK_PC5 1 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		uart6m1_xfer: uart6m1-xfer {
			rockchip,pins =
				/* uart6_rx_m1 */
				<4 RK_PB0 5 &pcfg_pull_up>,
				/* uart6_tx_m1 */
				<4 RK_PA7 5 &pcfg_pull_up>;
		};

		/omit-if-no-ref/
		uart6m1_ctsn: uart6m1-ctsn {
			rockchip,pins =
				/* uart6m1_ctsn */
				<4 RK_PA2 3 &pcfg_pull_none>;
		};
		/omit-if-no-ref/
		uart6m1_rtsn: uart6m1-rtsn {
			rockchip,pins =
				/* uart6m1_rtsn */
				<4 RK_PA3 3 &pcfg_pull_none>;
		};
	};

	uart7 {
		/omit-if-no-ref/
		uart7m0_xfer: uart7m0-xfer {
			rockchip,pins =
				/* uart7_rx_m0 */
				<3 RK_PC7 3 &pcfg_pull_up>,
				/* uart7_tx_m0 */
				<3 RK_PC4 3 &pcfg_pull_up>;
		};

		/omit-if-no-ref/
		uart7m0_ctsn: uart7m0-ctsn {
			rockchip,pins =
				/* uart7m0_ctsn */
				<3 RK_PD2 3 &pcfg_pull_none>;
		};
		/omit-if-no-ref/
		uart7m0_rtsn: uart7m0-rtsn {
			rockchip,pins =
				/* uart7m0_rtsn */
				<3 RK_PD3 3 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		uart7m1_xfer: uart7m1-xfer {
			rockchip,pins =
				/* uart7_rx_m1 */
				<1 RK_PB3 3 &pcfg_pull_up>,
				/* uart7_tx_m1 */
				<1 RK_PB4 3 &pcfg_pull_up>;
		};
	};

	uart8 {
		/omit-if-no-ref/
		uart8m0_xfer: uart8m0-xfer {
			rockchip,pins =
				/* uart8_rx_m0 */
				<3 RK_PB3 3 &pcfg_pull_up>,
				/* uart8_tx_m0 */
				<3 RK_PB2 3 &pcfg_pull_up>;
		};

		/omit-if-no-ref/
		uart8m0_ctsn: uart8m0-ctsn {
			rockchip,pins =
				/* uart8m0_ctsn */
				<3 RK_PB4 3 &pcfg_pull_none>;
		};
		/omit-if-no-ref/
		uart8m0_rtsn: uart8m0-rtsn {
			rockchip,pins =
				/* uart8m0_rtsn */
				<3 RK_PB5 3 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		uart8m1_xfer: uart8m1-xfer {
			rockchip,pins =
				/* uart8_rx_m1 */
				<3 RK_PD5 3 &pcfg_pull_up>,
				/* uart8_tx_m1 */
				<3 RK_PD4 3 &pcfg_pull_up>;
		};

		/omit-if-no-ref/
		uart8m1_ctsn: uart8m1-ctsn {
			rockchip,pins =
				/* uart8m1_ctsn */
				<3 RK_PD7 3 &pcfg_pull_none>;
		};
		/omit-if-no-ref/
		uart8m1_rtsn: uart8m1-rtsn {
			rockchip,pins =
				/* uart8m1_rtsn */
				<4 RK_PA0 3 &pcfg_pull_none>;
		};
	};

	uart9 {
		/omit-if-no-ref/
		uart9m0_xfer: uart9m0-xfer {
			rockchip,pins =
				/* uart9_rx_m0 */
				<4 RK_PB3 3 &pcfg_pull_up>,
				/* uart9_tx_m0 */
				<4 RK_PB2 3 &pcfg_pull_up>;
		};

		/omit-if-no-ref/
		uart9m0_ctsn: uart9m0-ctsn {
			rockchip,pins =
				/* uart9m0_ctsn */
				<4 RK_PB4 3 &pcfg_pull_none>;
		};
		/omit-if-no-ref/
		uart9m0_rtsn: uart9m0-rtsn {
			rockchip,pins =
				/* uart9m0_rtsn */
				<4 RK_PB5 3 &pcfg_pull_none>;
		};

		/omit-if-no-ref/
		uart9m1_xfer: uart9m1-xfer {
			rockchip,pins =
				/* uart9_rx_m1 */
				<3 RK_PC3 3 &pcfg_pull_up>,
				/* uart9_tx_m1 */
				<3 RK_PC2 3 &pcfg_pull_up>;
		};
	};

	vo {
		/omit-if-no-ref/
		vo_pins: vo-pins {
			rockchip,pins =
				/* vo_lcdc_clk */
				<4 RK_PB7 1 &pcfg_pull_none_drv_level_4>,
				/* vo_lcdc_d0 */
				<4 RK_PA4 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d1 */
				<4 RK_PA5 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d2 */
				<4 RK_PB2 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d3 */
				<3 RK_PC4 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d4 */
				<3 RK_PC5 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d5 */
				<3 RK_PC6 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d6 */
				<3 RK_PC7 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d7 */
				<3 RK_PD0 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d8 */
				<4 RK_PA6 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d9 */
				<4 RK_PA7 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d10 */
				<3 RK_PD1 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d11 */
				<3 RK_PD2 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d12 */
				<3 RK_PD3 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d13 */
				<3 RK_PD4 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d14 */
				<3 RK_PD5 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d15 */
				<3 RK_PD6 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d16 */
				<4 RK_PB0 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d17 */
				<4 RK_PB1 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d18 */
				<4 RK_PB3 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d19 */
				<3 RK_PD7 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d20 */
				<4 RK_PA0 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d21 */
				<4 RK_PA1 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d22 */
				<4 RK_PA2 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d23 */
				<4 RK_PA3 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_den */
				<4 RK_PB6 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_hsync */
				<4 RK_PB4 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_vsync */
				<4 RK_PB5 1 &pcfg_pull_none_drv_level_3>;
		};
	};
};

/*
 * This part is edited handly.
 */
&pinctrl {
	vo {
		/omit-if-no-ref/
		bt1120_pins: bt1120-pins {
			rockchip,pins =
				/* vo_lcdc_clk */
				<4 RK_PB7 1 &pcfg_pull_none_drv_level_4>,
				/* vo_lcdc_d3 */
				<3 RK_PC4 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d4 */
				<3 RK_PC5 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d5 */
				<3 RK_PC6 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d6 */
				<3 RK_PC7 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d7 */
				<3 RK_PD0 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d10 */
				<3 RK_PD1 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d11 */
				<3 RK_PD2 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d12 */
				<3 RK_PD3 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d13 */
				<3 RK_PD4 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d14 */
				<3 RK_PD5 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d15 */
				<3 RK_PD6 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d19 */
				<3 RK_PD7 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d20 */
				<4 RK_PA0 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d21 */
				<4 RK_PA1 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d22 */
				<4 RK_PA2 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d23 */
				<4 RK_PA3 1 &pcfg_pull_none_drv_level_3>;
		};

		/omit-if-no-ref/
		bt656_pins: bt656-pins {
			rockchip,pins =
				/* vo_lcdc_clk */
				<4 RK_PB7 1 &pcfg_pull_none_drv_level_4>,
				/* vo_lcdc_d3 */
				<3 RK_PC4 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d4 */
				<3 RK_PC5 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d5 */
				<3 RK_PC6 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d6 */
				<3 RK_PC7 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d7 */
				<3 RK_PD0 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d10 */
				<3 RK_PD1 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d11 */
				<3 RK_PD2 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d12 */
				<3 RK_PD3 1 &pcfg_pull_none_drv_level_3>;
		};

		/omit-if-no-ref/
		rgb3x8_pins_m0: rgb3x8-pins-m0 {
			rockchip,pins =
				/* vo_lcdc_clk */
				<4 RK_PB7 1 &pcfg_pull_none_drv_level_4>,
				/* vo_lcdc_d3 */
				<3 RK_PC4 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d4 */
				<3 RK_PC5 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d5 */
				<3 RK_PC6 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d6 */
				<3 RK_PC7 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d7 */
				<3 RK_PD0 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d10 */
				<3 RK_PD1 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d11 */
				<3 RK_PD2 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d12 */
				<3 RK_PD3 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_den */
				<4 RK_PB6 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_hsync */
				<4 RK_PB4 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_vsync */
				<4 RK_PB5 1 &pcfg_pull_none_drv_level_3>;
		};

		/omit-if-no-ref/
		rgb3x8_pins_m1: rgb3x8-pins-m1 {
			rockchip,pins =
				/* vo_lcdc_clk */
				<4 RK_PB7 1 &pcfg_pull_none_drv_level_4>,
				/* vo_lcdc_d13 */
				<3 RK_PD4 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d14 */
				<3 RK_PD5 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d15 */
				<3 RK_PD6 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d19 */
				<3 RK_PD7 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d20 */
				<4 RK_PA0 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d21 */
				<4 RK_PA1 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d22 */
				<4 RK_PA2 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d23 */
				<4 RK_PA3 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_den */
				<4 RK_PB6 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_hsync */
				<4 RK_PB4 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_vsync */
				<4 RK_PB5 1 &pcfg_pull_none_drv_level_3>;
		};

		/omit-if-no-ref/
		rgb565_pins: rgb565-pins {
			rockchip,pins =
				/* vo_lcdc_clk */
				<4 RK_PB7 1 &pcfg_pull_none_drv_level_4>,
				/* vo_lcdc_d3 */
				<3 RK_PC4 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d4 */
				<3 RK_PC5 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d5 */
				<3 RK_PC6 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d6 */
				<3 RK_PC7 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d7 */
				<3 RK_PD0 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d10 */
				<3 RK_PD1 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d11 */
				<3 RK_PD2 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d12 */
				<3 RK_PD3 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d13 */
				<3 RK_PD4 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d14 */
				<3 RK_PD5 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d15 */
				<3 RK_PD6 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d19 */
				<3 RK_PD7 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d20 */
				<4 RK_PA0 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d21 */
				<4 RK_PA1 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d22 */
				<4 RK_PA2 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d23 */
				<4 RK_PA3 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_den */
				<4 RK_PB6 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_hsync */
				<4 RK_PB4 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_vsync */
				<4 RK_PB5 1 &pcfg_pull_none_drv_level_3>;
		};

		/omit-if-no-ref/
		rgb666_pins: rgb666-pins {
			rockchip,pins =
				/* vo_lcdc_clk */
				<4 RK_PB7 1 &pcfg_pull_none_drv_level_4>,
				/* vo_lcdc_d2 */
				<4 RK_PB2 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d3 */
				<3 RK_PC4 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d4 */
				<3 RK_PC5 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d5 */
				<3 RK_PC6 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d6 */
				<3 RK_PC7 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d7 */
				<3 RK_PD0 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d10 */
				<3 RK_PD1 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d11 */
				<3 RK_PD2 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d12 */
				<3 RK_PD3 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d13 */
				<3 RK_PD4 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d14 */
				<3 RK_PD5 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d15 */
				<3 RK_PD6 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d18 */
				<4 RK_PB3 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d19 */
				<3 RK_PD7 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d20 */
				<4 RK_PA0 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d21 */
				<4 RK_PA1 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d22 */
				<4 RK_PA2 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_d23 */
				<4 RK_PA3 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_den */
				<4 RK_PB6 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_hsync */
				<4 RK_PB4 1 &pcfg_pull_none_drv_level_3>,
				/* vo_lcdc_vsync */
				<4 RK_PB5 1 &pcfg_pull_none_drv_level_3>;
		};
	};
};
