// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Copyright (c) 2020 Rockchip Electronics Co., Ltd.
 */

#include <dt-bindings/pinctrl/rockchip.h>
#include "rockchip-pinconf.dtsi"

/*
 * This file is auto generated by pin2dts tool, please keep these code
 * by adding changes at end of this file.
 */
&pinctrl {
    acodec {
        /omit-if-no-ref/
        acodec_pins: acodec-pins {
            rockchip,pins =
                /* acodec_adc_sync */
                <1 RK_PB1 5 &pcfg_pull_none>,
                /* acodec_adcclk */
                <1 RK_PA1 5 &pcfg_pull_none>,
                /* acodec_adcdata */
                <1 RK_PA0 5 &pcfg_pull_none>,
                /* acodec_dac_datal */
                <1 RK_PA7 5 &pcfg_pull_none>,
                /* acodec_dac_datar */
                <1 RK_PB0 5 &pcfg_pull_none>,
                /* acodec_dacclk */
                <1 RK_PA3 5 &pcfg_pull_none>,
                /* acodec_dacsync */
                <1 RK_PA5 5 &pcfg_pull_none>;
        };
    };

    audiopwm {
        /omit-if-no-ref/
        audiopwm_lout: audiopwm-lout {
            rockchip,pins =
                /* audiopwm_lout */
                <1 RK_PA0 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        audiopwm_loutn: audiopwm-loutn {
            rockchip,pins =
                /* audiopwm_loutn */
                <1 RK_PA1 6 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        audiopwm_loutp: audiopwm-loutp {
            rockchip,pins =
                /* audiopwm_loutp */
                <1 RK_PA0 6 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        audiopwm_rout: audiopwm-rout {
            rockchip,pins =
                /* audiopwm_rout */
                <1 RK_PA1 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        audiopwm_routn: audiopwm-routn {
            rockchip,pins =
                /* audiopwm_routn */
                <1 RK_PA7 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        audiopwm_routp: audiopwm-routp {
            rockchip,pins =
                /* audiopwm_routp */
                <1 RK_PA6 4 &pcfg_pull_none>;
        };
    };

    bt656 {
        /omit-if-no-ref/
        bt656m0_pins: bt656m0-pins {
            rockchip,pins =
                /* bt656_clkm0 */
                <3 RK_PA0 2 &pcfg_pull_none>,
                /* bt656_d0m0 */
                <2 RK_PD0 2 &pcfg_pull_none>,
                /* bt656_d1m0 */
                <2 RK_PD1 2 &pcfg_pull_none>,
                /* bt656_d2m0 */
                <2 RK_PD2 2 &pcfg_pull_none>,
                /* bt656_d3m0 */
                <2 RK_PD3 2 &pcfg_pull_none>,
                /* bt656_d4m0 */
                <2 RK_PD4 2 &pcfg_pull_none>,
                /* bt656_d5m0 */
                <2 RK_PD5 2 &pcfg_pull_none>,
                /* bt656_d6m0 */
                <2 RK_PD6 2 &pcfg_pull_none>,
                /* bt656_d7m0 */
                <2 RK_PD7 2 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        bt656m1_pins: bt656m1-pins {
            rockchip,pins =
                /* bt656_clkm1 */
                <4 RK_PB4 5 &pcfg_pull_none>,
                /* bt656_d0m1 */
                <3 RK_PC6 5 &pcfg_pull_none>,
                /* bt656_d1m1 */
                <3 RK_PC7 5 &pcfg_pull_none>,
                /* bt656_d2m1 */
                <3 RK_PD0 5 &pcfg_pull_none>,
                /* bt656_d3m1 */
                <3 RK_PD1 5 &pcfg_pull_none>,
                /* bt656_d4m1 */
                <3 RK_PD2 5 &pcfg_pull_none>,
                /* bt656_d5m1 */
                <3 RK_PD3 5 &pcfg_pull_none>,
                /* bt656_d6m1 */
                <3 RK_PD4 5 &pcfg_pull_none>,
                /* bt656_d7m1 */
                <3 RK_PD5 5 &pcfg_pull_none>;
        };
    };

    bt1120 {
        /omit-if-no-ref/
        bt1120_pins: bt1120-pins {
            rockchip,pins =
                /* bt1120_clk */
                <3 RK_PA6 2 &pcfg_pull_none>,
                /* bt1120_d0 */
                <3 RK_PA1 2 &pcfg_pull_none>,
                /* bt1120_d1 */
                <3 RK_PA2 2 &pcfg_pull_none>,
                /* bt1120_d2 */
                <3 RK_PA3 2 &pcfg_pull_none>,
                /* bt1120_d3 */
                <3 RK_PA4 2 &pcfg_pull_none>,
                /* bt1120_d4 */
                <3 RK_PA5 2 &pcfg_pull_none>,
                /* bt1120_d5 */
                <3 RK_PA7 2 &pcfg_pull_none>,
                /* bt1120_d6 */
                <3 RK_PB0 2 &pcfg_pull_none>,
                /* bt1120_d7 */
                <3 RK_PB1 2 &pcfg_pull_none>,
                /* bt1120_d8 */
                <3 RK_PB2 2 &pcfg_pull_none>,
                /* bt1120_d9 */
                <3 RK_PB3 2 &pcfg_pull_none>,
                /* bt1120_d10 */
                <3 RK_PB4 2 &pcfg_pull_none>,
                /* bt1120_d11 */
                <3 RK_PB5 2 &pcfg_pull_none>,
                /* bt1120_d12 */
                <3 RK_PB6 2 &pcfg_pull_none>,
                /* bt1120_d13 */
                <3 RK_PC1 2 &pcfg_pull_none>,
                /* bt1120_d14 */
                <3 RK_PC2 2 &pcfg_pull_none>,
                /* bt1120_d15 */
                <3 RK_PC3 2 &pcfg_pull_none>;
        };
    };

    cam {
        /omit-if-no-ref/
        cam_clkout0: cam-clkout0 {
            rockchip,pins =
                /* cam_clkout0 */
                <4 RK_PA7 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        cam_clkout1: cam-clkout1 {
            rockchip,pins =
                /* cam_clkout1 */
                <4 RK_PB0 1 &pcfg_pull_none>;
        };
    };

    can0 {
        /omit-if-no-ref/
        can0m0_pins: can0m0-pins {
            rockchip,pins =
                /* can0_rxm0 */
                <0 RK_PB4 2 &pcfg_pull_none>,
                /* can0_txm0 */
                <0 RK_PB3 2 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        can0m1_pins: can0m1-pins {
            rockchip,pins =
                /* can0_rxm1 */
                <2 RK_PA2 4 &pcfg_pull_none>,
                /* can0_txm1 */
                <2 RK_PA1 4 &pcfg_pull_none>;
        };
    };

    can1 {
        /omit-if-no-ref/
        can1m0_pins: can1m0-pins {
            rockchip,pins =
                /* can1_rxm0 */
                <1 RK_PA0 3 &pcfg_pull_none>,
                /* can1_txm0 */
                <1 RK_PA1 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        can1m1_pins: can1m1-pins {
            rockchip,pins =
                /* can1_rxm1 */
                <4 RK_PC2 3 &pcfg_pull_none>,
                /* can1_txm1 */
                <4 RK_PC3 3 &pcfg_pull_none>;
        };
    };

    can2 {
        /omit-if-no-ref/
        can2m0_pins: can2m0-pins {
            rockchip,pins =
                /* can2_rxm0 */
                <4 RK_PB4 3 &pcfg_pull_none>,
                /* can2_txm0 */
                <4 RK_PB5 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        can2m1_pins: can2m1-pins {
            rockchip,pins =
                /* can2_rxm1 */
                <2 RK_PB1 4 &pcfg_pull_none>,
                /* can2_txm1 */
                <2 RK_PB2 4 &pcfg_pull_none>;
        };
    };

    cif {
        /omit-if-no-ref/
        cif_clk: cif-clk {
            rockchip,pins =
                /* cif_clkout */
                <4 RK_PC0 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        cif_dvp_clk: cif-dvp-clk {
            rockchip,pins =
                /* cif_clkin */
                <4 RK_PC1 1 &pcfg_pull_none>,
                /* cif_href */
                <4 RK_PB6 1 &pcfg_pull_none>,
                /* cif_vsync */
                <4 RK_PB7 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        cif_dvp_bus16: cif-dvp-bus16 {
            rockchip,pins =
                /* cif_d8 */
                <3 RK_PD6 1 &pcfg_pull_none>,
                /* cif_d9 */
                <3 RK_PD7 1 &pcfg_pull_none>,
                /* cif_d10 */
                <4 RK_PA0 1 &pcfg_pull_none>,
                /* cif_d11 */
                <4 RK_PA1 1 &pcfg_pull_none>,
                /* cif_d12 */
                <4 RK_PA2 1 &pcfg_pull_none>,
                /* cif_d13 */
                <4 RK_PA3 1 &pcfg_pull_none>,
                /* cif_d14 */
                <4 RK_PA4 1 &pcfg_pull_none>,
                /* cif_d15 */
                <4 RK_PA5 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        cif_dvp_bus8: cif-dvp-bus8 {
            rockchip,pins =
                /* cif_d0 */
                <3 RK_PC6 1 &pcfg_pull_none>,
                /* cif_d1 */
                <3 RK_PC7 1 &pcfg_pull_none>,
                /* cif_d2 */
                <3 RK_PD0 1 &pcfg_pull_none>,
                /* cif_d3 */
                <3 RK_PD1 1 &pcfg_pull_none>,
                /* cif_d4 */
                <3 RK_PD2 1 &pcfg_pull_none>,
                /* cif_d5 */
                <3 RK_PD3 1 &pcfg_pull_none>,
                /* cif_d6 */
                <3 RK_PD4 1 &pcfg_pull_none>,
                /* cif_d7 */
                <3 RK_PD5 1 &pcfg_pull_none>;
        };
    };

    clk32k {
        /omit-if-no-ref/
        clk32k_in: clk32k-in {
            rockchip,pins =
                /* clk32k_in */
                <0 RK_PB0 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        clk32k_out0: clk32k-out0 {
            rockchip,pins =
                /* clk32k_out0 */
                <0 RK_PB0 2 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        clk32k_out1: clk32k-out1 {
            rockchip,pins =
                /* clk32k_out1 */
                <2 RK_PC6 1 &pcfg_pull_none>;
        };
    };

    cpu {
        /omit-if-no-ref/
        cpu_pins: cpu-pins {
            rockchip,pins =
                /* cpu_avs */
                <0 RK_PB7 2 &pcfg_pull_none>;
        };
    };

    ebc {
        /omit-if-no-ref/
        ebc_extern: ebc-extern {
            rockchip,pins =
                /* ebc_sdce1 */
                <4 RK_PA7 2 &pcfg_pull_none>,
                /* ebc_sdce2 */
                <4 RK_PB0 2 &pcfg_pull_none>,
                /* ebc_sdce3 */
                <4 RK_PB1 2 &pcfg_pull_none>,
                /* ebc_sdshr */
                <4 RK_PB5 2 &pcfg_pull_none>,
                /* ebc_vcom */
                <4 RK_PB2 2 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        ebc_pins: ebc-pins {
            rockchip,pins =
                /* ebc_gdclk */
                <4 RK_PC0 2 &pcfg_pull_none>,
                /* ebc_gdoe */
                <4 RK_PB3 2 &pcfg_pull_none>,
                /* ebc_gdsp */
                <4 RK_PB4 2 &pcfg_pull_none>,
                /* ebc_sdce0 */
                <4 RK_PA6 2 &pcfg_pull_none>,
                /* ebc_sdclk */
                <4 RK_PC1 2 &pcfg_pull_none>,
                /* ebc_sddo0 */
                <3 RK_PC6 2 &pcfg_pull_none>,
                /* ebc_sddo1 */
                <3 RK_PC7 2 &pcfg_pull_none>,
                /* ebc_sddo2 */
                <3 RK_PD0 2 &pcfg_pull_none>,
                /* ebc_sddo3 */
                <3 RK_PD1 2 &pcfg_pull_none>,
                /* ebc_sddo4 */
                <3 RK_PD2 2 &pcfg_pull_none>,
                /* ebc_sddo5 */
                <3 RK_PD3 2 &pcfg_pull_none>,
                /* ebc_sddo6 */
                <3 RK_PD4 2 &pcfg_pull_none>,
                /* ebc_sddo7 */
                <3 RK_PD5 2 &pcfg_pull_none>,
                /* ebc_sddo8 */
                <3 RK_PD6 2 &pcfg_pull_none>,
                /* ebc_sddo9 */
                <3 RK_PD7 2 &pcfg_pull_none>,
                /* ebc_sddo10 */
                <4 RK_PA0 2 &pcfg_pull_none>,
                /* ebc_sddo11 */
                <4 RK_PA1 2 &pcfg_pull_none>,
                /* ebc_sddo12 */
                <4 RK_PA2 2 &pcfg_pull_none>,
                /* ebc_sddo13 */
                <4 RK_PA3 2 &pcfg_pull_none>,
                /* ebc_sddo14 */
                <4 RK_PA4 2 &pcfg_pull_none>,
                /* ebc_sddo15 */
                <4 RK_PA5 2 &pcfg_pull_none>,
                /* ebc_sdle */
                <4 RK_PB6 2 &pcfg_pull_none>,
                /* ebc_sdoe */
                <4 RK_PB7 2 &pcfg_pull_none>;
        };
    };

    edpdp {
        /omit-if-no-ref/
        edpdpm0_pins: edpdpm0-pins {
            rockchip,pins =
                /* edpdp_hpdinm0 */
                <4 RK_PC4 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        edpdpm1_pins: edpdpm1-pins {
            rockchip,pins =
                /* edpdp_hpdinm1 */
                <0 RK_PC2 2 &pcfg_pull_none>;
        };
    };

    emmc {
        /omit-if-no-ref/
        emmc_rstnout: emmc-rstnout {
            rockchip,pins =
                /* emmc_rstn */
                <1 RK_PC7 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        emmc_bus8: emmc-bus8 {
            rockchip,pins =
                /* emmc_d0 */
                <1 RK_PB4 1 &pcfg_pull_up_drv_level_2>,
                /* emmc_d1 */
                <1 RK_PB5 1 &pcfg_pull_up_drv_level_2>,
                /* emmc_d2 */
                <1 RK_PB6 1 &pcfg_pull_up_drv_level_2>,
                /* emmc_d3 */
                <1 RK_PB7 1 &pcfg_pull_up_drv_level_2>,
                /* emmc_d4 */
                <1 RK_PC0 1 &pcfg_pull_up_drv_level_2>,
                /* emmc_d5 */
                <1 RK_PC1 1 &pcfg_pull_up_drv_level_2>,
                /* emmc_d6 */
                <1 RK_PC2 1 &pcfg_pull_up_drv_level_2>,
                /* emmc_d7 */
                <1 RK_PC3 1 &pcfg_pull_up_drv_level_2>;
        };

        /omit-if-no-ref/
        emmc_clk: emmc-clk {
            rockchip,pins =
                /* emmc_clkout */
                <1 RK_PC5 1 &pcfg_pull_up_drv_level_2>;
        };

        /omit-if-no-ref/
        emmc_cmd: emmc-cmd {
            rockchip,pins =
                /* emmc_cmd */
                <1 RK_PC4 1 &pcfg_pull_up_drv_level_2>;
        };

        /omit-if-no-ref/
        emmc_datastrobe: emmc-datastrobe {
            rockchip,pins =
                /* emmc_datastrobe */
                <1 RK_PC6 1 &pcfg_pull_none>;
        };
    };

    eth0 {
        /omit-if-no-ref/
        eth0_pins: eth0-pins {
            rockchip,pins =
                /* eth0_refclko25m */
                <2 RK_PC1 2 &pcfg_pull_none>;
        };
    };

    eth1 {
        /omit-if-no-ref/
        eth1m0_pins: eth1m0-pins {
            rockchip,pins =
                /* eth1_refclko25mm0 */
                <3 RK_PB0 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        eth1m1_pins: eth1m1-pins {
            rockchip,pins =
                /* eth1_refclko25mm1 */
                <4 RK_PB3 3 &pcfg_pull_none>;
        };
    };

    flash {
        /omit-if-no-ref/
        flash_pins: flash-pins {
            rockchip,pins =
                /* flash_ale */
                <1 RK_PD0 2 &pcfg_pull_none>,
                /* flash_cle */
                <1 RK_PC6 3 &pcfg_pull_none>,
                /* flash_cs0n */
                <1 RK_PD3 2 &pcfg_pull_none>,
                /* flash_cs1n */
                <1 RK_PD4 2 &pcfg_pull_none>,
                /* flash_d0 */
                <1 RK_PB4 2 &pcfg_pull_none>,
                /* flash_d1 */
                <1 RK_PB5 2 &pcfg_pull_none>,
                /* flash_d2 */
                <1 RK_PB6 2 &pcfg_pull_none>,
                /* flash_d3 */
                <1 RK_PB7 2 &pcfg_pull_none>,
                /* flash_d4 */
                <1 RK_PC0 2 &pcfg_pull_none>,
                /* flash_d5 */
                <1 RK_PC1 2 &pcfg_pull_none>,
                /* flash_d6 */
                <1 RK_PC2 2 &pcfg_pull_none>,
                /* flash_d7 */
                <1 RK_PC3 2 &pcfg_pull_none>,
                /* flash_dqs */
                <1 RK_PC5 2 &pcfg_pull_none>,
                /* flash_rdn */
                <1 RK_PD2 2 &pcfg_pull_none>,
                /* flash_rdy */
                <1 RK_PD1 2 &pcfg_pull_none>,
                /* flash_wpn */
                <1 RK_PC7 3 &pcfg_pull_none>,
                /* flash_wrn */
                <1 RK_PC4 2 &pcfg_pull_none>;
        };
    };

    fspi {
        /omit-if-no-ref/
        fspi_pins: fspi-pins {
            rockchip,pins =
                /* fspi_clk */
                <1 RK_PD0 1 &pcfg_pull_none>,
                /* fspi_cs0n */
                <1 RK_PD3 1 &pcfg_pull_none>,
                /* fspi_d0 */
                <1 RK_PD1 1 &pcfg_pull_none>,
                /* fspi_d1 */
                <1 RK_PD2 1 &pcfg_pull_none>,
                /* fspi_d2 */
                <1 RK_PC7 2 &pcfg_pull_none>,
                /* fspi_d3 */
                <1 RK_PD4 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        fspi_cs1: fspi-cs1 {
            rockchip,pins =
                /* fspi_cs1n */
                <1 RK_PC6 2 &pcfg_pull_up>;
        };
    };

    gmac0 {
        /omit-if-no-ref/
        gmac0_miim: gmac0-miim {
            rockchip,pins =
                /* gmac0_mdc */
                <2 RK_PC3 2 &pcfg_pull_none>,
                /* gmac0_mdio */
                <2 RK_PC4 2 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        gmac0_clkinout: gmac0-clkinout {
            rockchip,pins =
                /* gmac0_mclkinout */
                <2 RK_PC2 2 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        gmac0_rx_er: gmac0-rx-er {
            rockchip,pins =
                /* gmac0_rxer */
                <2 RK_PC5 2 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        gmac0_rx_bus2: gmac0-rx-bus2 {
            rockchip,pins =
                /* gmac0_rxd0 */
                <2 RK_PB6 1 &pcfg_pull_none>,
                /* gmac0_rxd1 */
                <2 RK_PB7 2 &pcfg_pull_none>,
                /* gmac0_rxdvcrs */
                <2 RK_PC0 2 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        gmac0_tx_bus2: gmac0-tx-bus2 {
            rockchip,pins =
                /* gmac0_txd0 */
                <2 RK_PB3 1 &pcfg_pull_none_drv_level_2>,
                /* gmac0_txd1 */
                <2 RK_PB4 1 &pcfg_pull_none_drv_level_2>,
                /* gmac0_txen */
                <2 RK_PB5 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        gmac0_rgmii_clk: gmac0-rgmii-clk {
            rockchip,pins =
                /* gmac0_rxclk */
                <2 RK_PA5 2 &pcfg_pull_none>,
                /* gmac0_txclk */
                <2 RK_PB0 2 &pcfg_pull_none_drv_level_1>;
        };

        /omit-if-no-ref/
        gmac0_rgmii_bus: gmac0-rgmii-bus {
            rockchip,pins =
                /* gmac0_rxd2 */
                <2 RK_PA3 2 &pcfg_pull_none>,
                /* gmac0_rxd3 */
                <2 RK_PA4 2 &pcfg_pull_none>,
                /* gmac0_txd2 */
                <2 RK_PA6 2 &pcfg_pull_none_drv_level_2>,
                /* gmac0_txd3 */
                <2 RK_PA7 2 &pcfg_pull_none_drv_level_2>;
        };
    };

    gmac1 {
        /omit-if-no-ref/
        gmac1m0_miim: gmac1m0-miim {
            rockchip,pins =
                /* gmac1_mdcm0 */
                <3 RK_PC4 3 &pcfg_pull_none>,
                /* gmac1_mdiom0 */
                <3 RK_PC5 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        gmac1m0_clkinout: gmac1m0-clkinout {
            rockchip,pins =
                /* gmac1_mclkinoutm0 */
                <3 RK_PC0 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        gmac1m0_rx_er: gmac1m0-rx-er {
            rockchip,pins =
                /* gmac1_rxerm0 */
                <3 RK_PB4 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        gmac1m0_rx_bus2: gmac1m0-rx-bus2 {
            rockchip,pins =
                /* gmac1_rxd0m0 */
                <3 RK_PB1 3 &pcfg_pull_none>,
                /* gmac1_rxd1m0 */
                <3 RK_PB2 3 &pcfg_pull_none>,
                /* gmac1_rxdvcrsm0 */
                <3 RK_PB3 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        gmac1m0_tx_bus2: gmac1m0-tx-bus2 {
            rockchip,pins =
                /* gmac1_txd0m0 */
                <3 RK_PB5 3 &pcfg_pull_none_drv_level_2>,
                /* gmac1_txd1m0 */
                <3 RK_PB6 3 &pcfg_pull_none_drv_level_2>,
                /* gmac1_txenm0 */
                <3 RK_PB7 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        gmac1m0_rgmii_clk: gmac1m0-rgmii-clk {
            rockchip,pins =
                /* gmac1_rxclkm0 */
                <3 RK_PA7 3 &pcfg_pull_none>,
                /* gmac1_txclkm0 */
                <3 RK_PA6 3 &pcfg_pull_none_drv_level_1>;
        };

        /omit-if-no-ref/
        gmac1m0_rgmii_bus: gmac1m0-rgmii-bus {
            rockchip,pins =
                /* gmac1_rxd2m0 */
                <3 RK_PA4 3 &pcfg_pull_none>,
                /* gmac1_rxd3m0 */
                <3 RK_PA5 3 &pcfg_pull_none>,
                /* gmac1_txd2m0 */
                <3 RK_PA2 3 &pcfg_pull_none_drv_level_2>,
                /* gmac1_txd3m0 */
                <3 RK_PA3 3 &pcfg_pull_none_drv_level_2>;
        };

        /omit-if-no-ref/
        gmac1m1_miim: gmac1m1-miim {
            rockchip,pins =
                /* gmac1_mdcm1 */
                <4 RK_PB6 3 &pcfg_pull_none>,
                /* gmac1_mdiom1 */
                <4 RK_PB7 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        gmac1m1_clkinout: gmac1m1-clkinout {
            rockchip,pins =
                /* gmac1_mclkinoutm1 */
                <4 RK_PC1 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        gmac1m1_rx_er: gmac1m1-rx-er {
            rockchip,pins =
                /* gmac1_rxerm1 */
                <4 RK_PB2 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        gmac1m1_rx_bus2: gmac1m1-rx-bus2 {
            rockchip,pins =
                /* gmac1_rxd0m1 */
                <4 RK_PA7 3 &pcfg_pull_none>,
                /* gmac1_rxd1m1 */
                <4 RK_PB0 3 &pcfg_pull_none>,
                /* gmac1_rxdvcrsm1 */
                <4 RK_PB1 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        gmac1m1_tx_bus2: gmac1m1-tx-bus2 {
            rockchip,pins =
                /* gmac1_txd0m1 */
                <4 RK_PA4 3 &pcfg_pull_none_drv_level_2>,
                /* gmac1_txd1m1 */
                <4 RK_PA5 3 &pcfg_pull_none_drv_level_2>,
                /* gmac1_txenm1 */
                <4 RK_PA6 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        gmac1m1_rgmii_clk: gmac1m1-rgmii-clk {
            rockchip,pins =
                /* gmac1_rxclkm1 */
                <4 RK_PA3 3 &pcfg_pull_none>,
                /* gmac1_txclkm1 */
                <4 RK_PA0 3 &pcfg_pull_none_drv_level_1>;
        };

        /omit-if-no-ref/
        gmac1m1_rgmii_bus: gmac1m1-rgmii-bus {
            rockchip,pins =
                /* gmac1_rxd2m1 */
                <4 RK_PA1 3 &pcfg_pull_none>,
                /* gmac1_rxd3m1 */
                <4 RK_PA2 3 &pcfg_pull_none>,
                /* gmac1_txd2m1 */
                <3 RK_PD6 3 &pcfg_pull_none_drv_level_2>,
                /* gmac1_txd3m1 */
                <3 RK_PD7 3 &pcfg_pull_none_drv_level_2>;
        };
    };

    gpu {
        /omit-if-no-ref/
        gpu_pins: gpu-pins {
            rockchip,pins =
                /* gpu_avs */
                <0 RK_PC0 2 &pcfg_pull_none>,
                /* gpu_pwren */
                <0 RK_PA6 4 &pcfg_pull_none>;
        };
    };

    hdmitx {
        /omit-if-no-ref/
        hdmitxm0_cec: hdmitxm0-cec {
            rockchip,pins =
                /* hdmitxm0_cec */
                <4 RK_PD1 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        hdmitxm1_cec: hdmitxm1-cec {
            rockchip,pins =
                /* hdmitxm1_cec */
                <0 RK_PC7 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        hdmitx_scl: hdmitx-scl {
            rockchip,pins =
                /* hdmitx_scl */
                <4 RK_PC7 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        hdmitx_sda: hdmitx-sda {
            rockchip,pins =
                /* hdmitx_sda */
                <4 RK_PD0 1 &pcfg_pull_none>;
        };
    };

    i2c0 {
        /omit-if-no-ref/
        i2c0_xfer: i2c0-xfer {
            rockchip,pins =
                /* i2c0_scl */
                <0 RK_PB1 1 &pcfg_pull_none_smt>,
                /* i2c0_sda */
                <0 RK_PB2 1 &pcfg_pull_none_smt>;
        };
    };

    i2c1 {
        /omit-if-no-ref/
        i2c1_xfer: i2c1-xfer {
            rockchip,pins =
                /* i2c1_scl */
                <0 RK_PB3 1 &pcfg_pull_none_smt>,
                /* i2c1_sda */
                <0 RK_PB4 1 &pcfg_pull_none_smt>;
        };
    };

    i2c2 {
        /omit-if-no-ref/
        i2c2m0_xfer: i2c2m0-xfer {
            rockchip,pins =
                /* i2c2_sclm0 */
                <0 RK_PB5 1 &pcfg_pull_none_smt>,
                /* i2c2_sdam0 */
                <0 RK_PB6 1 &pcfg_pull_none_smt>;
        };

        /omit-if-no-ref/
        i2c2m1_xfer: i2c2m1-xfer {
            rockchip,pins =
                /* i2c2_sclm1 */
                <4 RK_PB5 1 &pcfg_pull_none_smt>,
                /* i2c2_sdam1 */
                <4 RK_PB4 1 &pcfg_pull_none_smt>;
        };
    };

    i2c3 {
        /omit-if-no-ref/
        i2c3m0_xfer: i2c3m0-xfer {
            rockchip,pins =
                /* i2c3_sclm0 */
                <1 RK_PA1 1 &pcfg_pull_none_smt>,
                /* i2c3_sdam0 */
                <1 RK_PA0 1 &pcfg_pull_none_smt>;
        };

        /omit-if-no-ref/
        i2c3m1_xfer: i2c3m1-xfer {
            rockchip,pins =
                /* i2c3_sclm1 */
                <3 RK_PB5 4 &pcfg_pull_none_smt>,
                /* i2c3_sdam1 */
                <3 RK_PB6 4 &pcfg_pull_none_smt>;
        };
    };

    i2c4 {
        /omit-if-no-ref/
        i2c4m0_xfer: i2c4m0-xfer {
            rockchip,pins =
                /* i2c4_sclm0 */
                <4 RK_PB3 1 &pcfg_pull_none_smt>,
                /* i2c4_sdam0 */
                <4 RK_PB2 1 &pcfg_pull_none_smt>;
        };

        /omit-if-no-ref/
        i2c4m1_xfer: i2c4m1-xfer {
            rockchip,pins =
                /* i2c4_sclm1 */
                <2 RK_PB2 2 &pcfg_pull_none_smt>,
                /* i2c4_sdam1 */
                <2 RK_PB1 2 &pcfg_pull_none_smt>;
        };
    };

    i2c5 {
        /omit-if-no-ref/
        i2c5m0_xfer: i2c5m0-xfer {
            rockchip,pins =
                /* i2c5_sclm0 */
                <3 RK_PB3 4 &pcfg_pull_none_smt>,
                /* i2c5_sdam0 */
                <3 RK_PB4 4 &pcfg_pull_none_smt>;
        };

        /omit-if-no-ref/
        i2c5m1_xfer: i2c5m1-xfer {
            rockchip,pins =
                /* i2c5_sclm1 */
                <4 RK_PC7 2 &pcfg_pull_none_smt>,
                /* i2c5_sdam1 */
                <4 RK_PD0 2 &pcfg_pull_none_smt>;
        };
    };

    i2s1 {
        /omit-if-no-ref/
        i2s1m0_lrckrx: i2s1m0-lrckrx {
            rockchip,pins =
                /* i2s1m0_lrckrx */
                <1 RK_PA6 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m0_lrcktx: i2s1m0-lrcktx {
            rockchip,pins =
                /* i2s1m0_lrcktx */
                <1 RK_PA5 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m0_mclk: i2s1m0-mclk {
            rockchip,pins =
                /* i2s1m0_mclk */
                <1 RK_PA2 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m0_sclkrx: i2s1m0-sclkrx {
            rockchip,pins =
                /* i2s1m0_sclkrx */
                <1 RK_PA4 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m0_sclktx: i2s1m0-sclktx {
            rockchip,pins =
                /* i2s1m0_sclktx */
                <1 RK_PA3 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m0_sdi0: i2s1m0-sdi0 {
            rockchip,pins =
                /* i2s1m0_sdi0 */
                <1 RK_PB3 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m0_sdi1: i2s1m0-sdi1 {
            rockchip,pins =
                /* i2s1m0_sdi1 */
                <1 RK_PB2 2 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m0_sdi2: i2s1m0-sdi2 {
            rockchip,pins =
                /* i2s1m0_sdi2 */
                <1 RK_PB1 2 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m0_sdi3: i2s1m0-sdi3 {
            rockchip,pins =
                /* i2s1m0_sdi3 */
                <1 RK_PB0 2 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m0_sdo0: i2s1m0-sdo0 {
            rockchip,pins =
                /* i2s1m0_sdo0 */
                <1 RK_PA7 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m0_sdo1: i2s1m0-sdo1 {
            rockchip,pins =
                /* i2s1m0_sdo1 */
                <1 RK_PB0 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m0_sdo2: i2s1m0-sdo2 {
            rockchip,pins =
                /* i2s1m0_sdo2 */
                <1 RK_PB1 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m0_sdo3: i2s1m0-sdo3 {
            rockchip,pins =
                /* i2s1m0_sdo3 */
                <1 RK_PB2 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m1_lrckrx: i2s1m1-lrckrx {
            rockchip,pins =
                /* i2s1m1_lrckrx */
                <4 RK_PA7 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m1_lrcktx: i2s1m1-lrcktx {
            rockchip,pins =
                /* i2s1m1_lrcktx */
                <3 RK_PD0 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m1_mclk: i2s1m1-mclk {
            rockchip,pins =
                /* i2s1m1_mclk */
                <3 RK_PC6 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m1_sclkrx: i2s1m1-sclkrx {
            rockchip,pins =
                /* i2s1m1_sclkrx */
                <4 RK_PA6 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m1_sclktx: i2s1m1-sclktx {
            rockchip,pins =
                /* i2s1m1_sclktx */
                <3 RK_PC7 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m1_sdi0: i2s1m1-sdi0 {
            rockchip,pins =
                /* i2s1m1_sdi0 */
                <3 RK_PD2 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m1_sdi1: i2s1m1-sdi1 {
            rockchip,pins =
                /* i2s1m1_sdi1 */
                <3 RK_PD3 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m1_sdi2: i2s1m1-sdi2 {
            rockchip,pins =
                /* i2s1m1_sdi2 */
                <3 RK_PD4 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m1_sdi3: i2s1m1-sdi3 {
            rockchip,pins =
                /* i2s1m1_sdi3 */
                <3 RK_PD5 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m1_sdo0: i2s1m1-sdo0 {
            rockchip,pins =
                /* i2s1m1_sdo0 */
                <3 RK_PD1 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m1_sdo1: i2s1m1-sdo1 {
            rockchip,pins =
                /* i2s1m1_sdo1 */
                <4 RK_PB0 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m1_sdo2: i2s1m1-sdo2 {
            rockchip,pins =
                /* i2s1m1_sdo2 */
                <4 RK_PB1 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m1_sdo3: i2s1m1-sdo3 {
            rockchip,pins =
                /* i2s1m1_sdo3 */
                <4 RK_PB5 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m2_lrckrx: i2s1m2-lrckrx {
            rockchip,pins =
                /* i2s1m2_lrckrx */
                <3 RK_PC5 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m2_lrcktx: i2s1m2-lrcktx {
            rockchip,pins =
                /* i2s1m2_lrcktx */
                <2 RK_PD2 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m2_mclk: i2s1m2-mclk {
            rockchip,pins =
                /* i2s1m2_mclk */
                <2 RK_PD0 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m2_sclkrx: i2s1m2-sclkrx {
            rockchip,pins =
                /* i2s1m2_sclkrx */
                <3 RK_PC3 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m2_sclktx: i2s1m2-sclktx {
            rockchip,pins =
                /* i2s1m2_sclktx */
                <2 RK_PD1 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m2_sdi0: i2s1m2-sdi0 {
            rockchip,pins =
                /* i2s1m2_sdi0 */
                <2 RK_PD3 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m2_sdi1: i2s1m2-sdi1 {
            rockchip,pins =
                /* i2s1m2_sdi1 */
                <2 RK_PD4 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m2_sdi2: i2s1m2-sdi2 {
            rockchip,pins =
                /* i2s1m2_sdi2 */
                <2 RK_PD5 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m2_sdi3: i2s1m2-sdi3 {
            rockchip,pins =
                /* i2s1m2_sdi3 */
                <2 RK_PD6 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m2_sdo0: i2s1m2-sdo0 {
            rockchip,pins =
                /* i2s1m2_sdo0 */
                <2 RK_PD7 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m2_sdo1: i2s1m2-sdo1 {
            rockchip,pins =
                /* i2s1m2_sdo1 */
                <3 RK_PA0 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m2_sdo2: i2s1m2-sdo2 {
            rockchip,pins =
                /* i2s1m2_sdo2 */
                <3 RK_PC1 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s1m2_sdo3: i2s1m2-sdo3 {
            rockchip,pins =
                /* i2s1m2_sdo3 */
                <3 RK_PC2 5 &pcfg_pull_none>;
        };
    };

    i2s2 {
        /omit-if-no-ref/
        i2s2m0_lrckrx: i2s2m0-lrckrx {
            rockchip,pins =
                /* i2s2m0_lrckrx */
                <2 RK_PC0 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s2m0_lrcktx: i2s2m0-lrcktx {
            rockchip,pins =
                /* i2s2m0_lrcktx */
                <2 RK_PC3 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s2m0_mclk: i2s2m0-mclk {
            rockchip,pins =
                /* i2s2m0_mclk */
                <2 RK_PC1 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s2m0_sclkrx: i2s2m0-sclkrx {
            rockchip,pins =
                /* i2s2m0_sclkrx */
                <2 RK_PB7 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s2m0_sclktx: i2s2m0-sclktx {
            rockchip,pins =
                /* i2s2m0_sclktx */
                <2 RK_PC2 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s2m0_sdi: i2s2m0-sdi {
            rockchip,pins =
                /* i2s2m0_sdi */
                <2 RK_PC5 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s2m0_sdo: i2s2m0-sdo {
            rockchip,pins =
                /* i2s2m0_sdo */
                <2 RK_PC4 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s2m1_lrckrx: i2s2m1-lrckrx {
            rockchip,pins =
                /* i2s2m1_lrckrx */
                <4 RK_PA5 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s2m1_lrcktx: i2s2m1-lrcktx {
            rockchip,pins =
                /* i2s2m1_lrcktx */
                <4 RK_PA4 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s2m1_mclk: i2s2m1-mclk {
            rockchip,pins =
                /* i2s2m1_mclk */
                <4 RK_PB6 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s2m1_sclkrx: i2s2m1-sclkrx {
            rockchip,pins =
                /* i2s2m1_sclkrx */
                <4 RK_PC1 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s2m1_sclktx: i2s2m1-sclktx {
            rockchip,pins =
                /* i2s2m1_sclktx */
                <4 RK_PB7 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s2m1_sdi: i2s2m1-sdi {
            rockchip,pins =
                /* i2s2m1_sdi */
                <4 RK_PB2 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s2m1_sdo: i2s2m1-sdo {
            rockchip,pins =
                /* i2s2m1_sdo */
                <4 RK_PB3 5 &pcfg_pull_none>;
        };
    };

    i2s3 {
        /omit-if-no-ref/
        i2s3m0_lrck: i2s3m0-lrck {
            rockchip,pins =
                /* i2s3m0_lrck */
                <3 RK_PA4 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s3m0_mclk: i2s3m0-mclk {
            rockchip,pins =
                /* i2s3m0_mclk */
                <3 RK_PA2 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s3m0_sclk: i2s3m0-sclk {
            rockchip,pins =
                /* i2s3m0_sclk */
                <3 RK_PA3 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s3m0_sdi: i2s3m0-sdi {
            rockchip,pins =
                /* i2s3m0_sdi */
                <3 RK_PA6 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s3m0_sdo: i2s3m0-sdo {
            rockchip,pins =
                /* i2s3m0_sdo */
                <3 RK_PA5 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s3m1_lrck: i2s3m1-lrck {
            rockchip,pins =
                /* i2s3m1_lrck */
                <4 RK_PC4 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s3m1_mclk: i2s3m1-mclk {
            rockchip,pins =
                /* i2s3m1_mclk */
                <4 RK_PC2 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s3m1_sclk: i2s3m1-sclk {
            rockchip,pins =
                /* i2s3m1_sclk */
                <4 RK_PC3 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s3m1_sdi: i2s3m1-sdi {
            rockchip,pins =
                /* i2s3m1_sdi */
                <4 RK_PC6 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        i2s3m1_sdo: i2s3m1-sdo {
            rockchip,pins =
                /* i2s3m1_sdo */
                <4 RK_PC5 5 &pcfg_pull_none>;
        };
    };

    isp {
        /omit-if-no-ref/
        isp_pins: isp-pins {
            rockchip,pins =
                /* isp_flashtrigin */
                <4 RK_PB4 4 &pcfg_pull_none>,
                /* isp_flashtrigout */
                <4 RK_PA6 1 &pcfg_pull_none>,
                /* isp_prelighttrig */
                <4 RK_PB1 1 &pcfg_pull_none>;
        };
    };

    jtag {
        /omit-if-no-ref/
        jtag_pins: jtag-pins {
            rockchip,pins =
                /* jtag_tck */
                <1 RK_PD7 2 &pcfg_pull_none>,
                /* jtag_tms */
                <2 RK_PA0 2 &pcfg_pull_none>;
        };
    };

    lcdc {
        /omit-if-no-ref/
        lcdc_ctl: lcdc-ctl {
            rockchip,pins =
                /* lcdc_clk */
                <3 RK_PA0 1 &pcfg_pull_none>,
                /* lcdc_d0 */
                <2 RK_PD0 1 &pcfg_pull_none>,
                /* lcdc_d1 */
                <2 RK_PD1 1 &pcfg_pull_none>,
                /* lcdc_d2 */
                <2 RK_PD2 1 &pcfg_pull_none>,
                /* lcdc_d3 */
                <2 RK_PD3 1 &pcfg_pull_none>,
                /* lcdc_d4 */
                <2 RK_PD4 1 &pcfg_pull_none>,
                /* lcdc_d5 */
                <2 RK_PD5 1 &pcfg_pull_none>,
                /* lcdc_d6 */
                <2 RK_PD6 1 &pcfg_pull_none>,
                /* lcdc_d7 */
                <2 RK_PD7 1 &pcfg_pull_none>,
                /* lcdc_d8 */
                <3 RK_PA1 1 &pcfg_pull_none>,
                /* lcdc_d9 */
                <3 RK_PA2 1 &pcfg_pull_none>,
                /* lcdc_d10 */
                <3 RK_PA3 1 &pcfg_pull_none>,
                /* lcdc_d11 */
                <3 RK_PA4 1 &pcfg_pull_none>,
                /* lcdc_d12 */
                <3 RK_PA5 1 &pcfg_pull_none>,
                /* lcdc_d13 */
                <3 RK_PA6 1 &pcfg_pull_none>,
                /* lcdc_d14 */
                <3 RK_PA7 1 &pcfg_pull_none>,
                /* lcdc_d15 */
                <3 RK_PB0 1 &pcfg_pull_none>,
                /* lcdc_d16 */
                <3 RK_PB1 1 &pcfg_pull_none>,
                /* lcdc_d17 */
                <3 RK_PB2 1 &pcfg_pull_none>,
                /* lcdc_d18 */
                <3 RK_PB3 1 &pcfg_pull_none>,
                /* lcdc_d19 */
                <3 RK_PB4 1 &pcfg_pull_none>,
                /* lcdc_d20 */
                <3 RK_PB5 1 &pcfg_pull_none>,
                /* lcdc_d21 */
                <3 RK_PB6 1 &pcfg_pull_none>,
                /* lcdc_d22 */
                <3 RK_PB7 1 &pcfg_pull_none>,
                /* lcdc_d23 */
                <3 RK_PC0 1 &pcfg_pull_none>,
                /* lcdc_den */
                <3 RK_PC3 1 &pcfg_pull_none>,
                /* lcdc_hsync */
                <3 RK_PC1 1 &pcfg_pull_none>,
                /* lcdc_vsync */
                <3 RK_PC2 1 &pcfg_pull_none>;
        };
    };

    mcu {
        /omit-if-no-ref/
        mcu_pins: mcu-pins {
            rockchip,pins =
                /* mcu_jtagtck */
                <0 RK_PB4 4 &pcfg_pull_none>,
                /* mcu_jtagtdi */
                <0 RK_PC1 4 &pcfg_pull_none>,
                /* mcu_jtagtdo */
                <0 RK_PB3 4 &pcfg_pull_none>,
                /* mcu_jtagtms */
                <0 RK_PC2 4 &pcfg_pull_none>,
                /* mcu_jtagtrstn */
                <0 RK_PC3 4 &pcfg_pull_none>;
        };
    };

    npu {
        /omit-if-no-ref/
        npu_pins: npu-pins {
            rockchip,pins =
                /* npu_avs */
                <0 RK_PC1 2 &pcfg_pull_none>;
        };
    };

    pcie20 {
        /omit-if-no-ref/
        pcie20m0_pins: pcie20m0-pins {
            rockchip,pins =
                /* pcie20_clkreqnm0 */
                <0 RK_PA5 3 &pcfg_pull_none>,
                /* pcie20_perstnm0 */
                <0 RK_PB6 3 &pcfg_pull_none>,
                /* pcie20_wakenm0 */
                <0 RK_PB5 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pcie20m1_pins: pcie20m1-pins {
            rockchip,pins =
                /* pcie20_clkreqnm1 */
                <2 RK_PD0 4 &pcfg_pull_none>,
                /* pcie20_perstnm1 */
                <3 RK_PC1 4 &pcfg_pull_none>,
                /* pcie20_wakenm1 */
                <2 RK_PD1 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pcie20m2_pins: pcie20m2-pins {
            rockchip,pins =
                /* pcie20_clkreqnm2 */
                <1 RK_PB0 4 &pcfg_pull_none>,
                /* pcie20_perstnm2 */
                <1 RK_PB2 4 &pcfg_pull_none>,
                /* pcie20_wakenm2 */
                <1 RK_PB1 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pcie20_buttonrstn: pcie20-buttonrstn {
            rockchip,pins =
                /* pcie20_buttonrstn */
                <0 RK_PB4 3 &pcfg_pull_none>;
        };
    };

    pcie30x1 {
        /omit-if-no-ref/
        pcie30x1m0_pins: pcie30x1m0-pins {
            rockchip,pins =
                /* pcie30x1_clkreqnm0 */
                <0 RK_PA4 3 &pcfg_pull_none>,
                /* pcie30x1_perstnm0 */
                <0 RK_PC3 3 &pcfg_pull_none>,
                /* pcie30x1_wakenm0 */
                <0 RK_PC2 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pcie30x1m1_pins: pcie30x1m1-pins {
            rockchip,pins =
                /* pcie30x1_clkreqnm1 */
                <2 RK_PD2 4 &pcfg_pull_none>,
                /* pcie30x1_perstnm1 */
                <3 RK_PA1 4 &pcfg_pull_none>,
                /* pcie30x1_wakenm1 */
                <2 RK_PD3 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pcie30x1m2_pins: pcie30x1m2-pins {
            rockchip,pins =
                /* pcie30x1_clkreqnm2 */
                <1 RK_PA5 4 &pcfg_pull_none>,
                /* pcie30x1_perstnm2 */
                <1 RK_PA2 4 &pcfg_pull_none>,
                /* pcie30x1_wakenm2 */
                <1 RK_PA3 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pcie30x1_buttonrstn: pcie30x1-buttonrstn {
            rockchip,pins =
                /* pcie30x1_buttonrstn */
                <0 RK_PB3 3 &pcfg_pull_none>;
        };
    };

    pcie30x2 {
        /omit-if-no-ref/
        pcie30x2m0_pins: pcie30x2m0-pins {
            rockchip,pins =
                /* pcie30x2_clkreqnm0 */
                <0 RK_PA6 2 &pcfg_pull_none>,
                /* pcie30x2_perstnm0 */
                <0 RK_PC6 3 &pcfg_pull_none>,
                /* pcie30x2_wakenm0 */
                <0 RK_PC5 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pcie30x2m1_pins: pcie30x2m1-pins {
            rockchip,pins =
                /* pcie30x2_clkreqnm1 */
                <2 RK_PD4 4 &pcfg_pull_none>,
                /* pcie30x2_perstnm1 */
                <2 RK_PD6 4 &pcfg_pull_none>,
                /* pcie30x2_wakenm1 */
                <2 RK_PD5 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pcie30x2m2_pins: pcie30x2m2-pins {
            rockchip,pins =
                /* pcie30x2_clkreqnm2 */
                <4 RK_PC2 4 &pcfg_pull_none>,
                /* pcie30x2_perstnm2 */
                <4 RK_PC4 4 &pcfg_pull_none>,
                /* pcie30x2_wakenm2 */
                <4 RK_PC3 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pcie30x2_buttonrstn: pcie30x2-buttonrstn {
            rockchip,pins =
                /* pcie30x2_buttonrstn */
                <0 RK_PB0 3 &pcfg_pull_none>;
        };
    };

    pdm {
        /omit-if-no-ref/
        pdmm0_clk: pdmm0-clk {
            rockchip,pins =
                /* pdm_clk0m0 */
                <1 RK_PA6 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pdmm0_clk1: pdmm0-clk1 {
            rockchip,pins =
                /* pdmm0_clk1 */
                <1 RK_PA4 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pdmm0_sdi0: pdmm0-sdi0 {
            rockchip,pins =
                /* pdmm0_sdi0 */
                <1 RK_PB3 2 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pdmm0_sdi1: pdmm0-sdi1 {
            rockchip,pins =
                /* pdmm0_sdi1 */
                <1 RK_PB2 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pdmm0_sdi2: pdmm0-sdi2 {
            rockchip,pins =
                /* pdmm0_sdi2 */
                <1 RK_PB1 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pdmm0_sdi3: pdmm0-sdi3 {
            rockchip,pins =
                /* pdmm0_sdi3 */
                <1 RK_PB0 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pdmm1_clk: pdmm1-clk {
            rockchip,pins =
                /* pdm_clk0m1 */
                <3 RK_PD6 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pdmm1_clk1: pdmm1-clk1 {
            rockchip,pins =
                /* pdmm1_clk1 */
                <4 RK_PA0 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pdmm1_sdi0: pdmm1-sdi0 {
            rockchip,pins =
                /* pdmm1_sdi0 */
                <3 RK_PD7 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pdmm1_sdi1: pdmm1-sdi1 {
            rockchip,pins =
                /* pdmm1_sdi1 */
                <4 RK_PA1 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pdmm1_sdi2: pdmm1-sdi2 {
            rockchip,pins =
                /* pdmm1_sdi2 */
                <4 RK_PA2 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pdmm1_sdi3: pdmm1-sdi3 {
            rockchip,pins =
                /* pdmm1_sdi3 */
                <4 RK_PA3 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pdmm2_clk1: pdmm2-clk1 {
            rockchip,pins =
                /* pdmm2_clk1 */
                <3 RK_PC4 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pdmm2_sdi0: pdmm2-sdi0 {
            rockchip,pins =
                /* pdmm2_sdi0 */
                <3 RK_PB3 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pdmm2_sdi1: pdmm2-sdi1 {
            rockchip,pins =
                /* pdmm2_sdi1 */
                <3 RK_PB4 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pdmm2_sdi2: pdmm2-sdi2 {
            rockchip,pins =
                /* pdmm2_sdi2 */
                <3 RK_PB7 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pdmm2_sdi3: pdmm2-sdi3 {
            rockchip,pins =
                /* pdmm2_sdi3 */
                <3 RK_PC0 5 &pcfg_pull_none>;
        };
    };

    pmic {
        /omit-if-no-ref/
        pmic_pins: pmic-pins {
            rockchip,pins =
                /* pmic_sleep */
                <0 RK_PA2 1 &pcfg_pull_none>;
        };
    };

    pmu {
        /omit-if-no-ref/
        pmu_pins: pmu-pins {
            rockchip,pins =
                /* pmu_debug0 */
                <0 RK_PA5 4 &pcfg_pull_none>,
                /* pmu_debug1 */
                <0 RK_PA6 3 &pcfg_pull_none>,
                /* pmu_debug2 */
                <0 RK_PC4 4 &pcfg_pull_none>,
                /* pmu_debug3 */
                <0 RK_PC5 4 &pcfg_pull_none>,
                /* pmu_debug4 */
                <0 RK_PC6 4 &pcfg_pull_none>,
                /* pmu_debug5 */
                <0 RK_PC7 4 &pcfg_pull_none>;
        };
    };

    pwm0 {
        /omit-if-no-ref/
        pwm0m0_pins: pwm0m0-pins {
            rockchip,pins =
                /* pwm0_m0 */
                <0 RK_PB7 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pwm0m1_pins: pwm0m1-pins {
            rockchip,pins =
                /* pwm0_m1 */
                <0 RK_PC7 2 &pcfg_pull_none>;
        };
    };

    pwm1 {
        /omit-if-no-ref/
        pwm1m0_pins: pwm1m0-pins {
            rockchip,pins =
                /* pwm1_m0 */
                <0 RK_PC0 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pwm1m1_pins: pwm1m1-pins {
            rockchip,pins =
                /* pwm1_m1 */
                <0 RK_PB5 4 &pcfg_pull_none>;
        };
    };

    pwm2 {
        /omit-if-no-ref/
        pwm2m0_pins: pwm2m0-pins {
            rockchip,pins =
                /* pwm2_m0 */
                <0 RK_PC1 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pwm2m1_pins: pwm2m1-pins {
            rockchip,pins =
                /* pwm2_m1 */
                <0 RK_PB6 4 &pcfg_pull_none>;
        };
    };

    pwm3 {
        /omit-if-no-ref/
        pwm3_pins: pwm3-pins {
            rockchip,pins =
                /* pwm3_ir */
                <0 RK_PC2 1 &pcfg_pull_none>;
        };
    };

    pwm4 {
        /omit-if-no-ref/
        pwm4_pins: pwm4-pins {
            rockchip,pins =
                /* pwm4 */
                <0 RK_PC3 1 &pcfg_pull_none>;
        };
    };

    pwm5 {
        /omit-if-no-ref/
        pwm5_pins: pwm5-pins {
            rockchip,pins =
                /* pwm5 */
                <0 RK_PC4 1 &pcfg_pull_none>;
        };
    };

    pwm6 {
        /omit-if-no-ref/
        pwm6_pins: pwm6-pins {
            rockchip,pins =
                /* pwm6 */
                <0 RK_PC5 1 &pcfg_pull_none>;
        };
    };

    pwm7 {
        /omit-if-no-ref/
        pwm7_pins: pwm7-pins {
            rockchip,pins =
                /* pwm7_ir */
                <0 RK_PC6 1 &pcfg_pull_none>;
        };
    };

    pwm8 {
        /omit-if-no-ref/
        pwm8m0_pins: pwm8m0-pins {
            rockchip,pins =
                /* pwm8_m0 */
                <3 RK_PB1 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pwm8m1_pins: pwm8m1-pins {
            rockchip,pins =
                /* pwm8_m1 */
                <1 RK_PD5 4 &pcfg_pull_none>;
        };
    };

    pwm9 {
        /omit-if-no-ref/
        pwm9m0_pins: pwm9m0-pins {
            rockchip,pins =
                /* pwm9_m0 */
                <3 RK_PB2 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pwm9m1_pins: pwm9m1-pins {
            rockchip,pins =
                /* pwm9_m1 */
                <1 RK_PD6 4 &pcfg_pull_none>;
        };
    };

    pwm10 {
        /omit-if-no-ref/
        pwm10m0_pins: pwm10m0-pins {
            rockchip,pins =
                /* pwm10_m0 */
                <3 RK_PB5 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pwm10m1_pins: pwm10m1-pins {
            rockchip,pins =
                /* pwm10_m1 */
                <2 RK_PA1 2 &pcfg_pull_none>;
        };
    };

    pwm11 {
        /omit-if-no-ref/
        pwm11m0_pins: pwm11m0-pins {
            rockchip,pins =
                /* pwm11_irm0 */
                <3 RK_PB6 5 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pwm11m1_pins: pwm11m1-pins {
            rockchip,pins =
                /* pwm11_irm1 */
                <4 RK_PC0 3 &pcfg_pull_none>;
        };
    };

    pwm12 {
        /omit-if-no-ref/
        pwm12m0_pins: pwm12m0-pins {
            rockchip,pins =
                /* pwm12_m0 */
                <3 RK_PB7 2 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pwm12m1_pins: pwm12m1-pins {
            rockchip,pins =
                /* pwm12_m1 */
                <4 RK_PC5 1 &pcfg_pull_none>;
        };
    };

    pwm13 {
        /omit-if-no-ref/
        pwm13m0_pins: pwm13m0-pins {
            rockchip,pins =
                /* pwm13_m0 */
                <3 RK_PC0 2 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pwm13m1_pins: pwm13m1-pins {
            rockchip,pins =
                /* pwm13_m1 */
                <4 RK_PC6 1 &pcfg_pull_none>;
        };
    };

    pwm14 {
        /omit-if-no-ref/
        pwm14m0_pins: pwm14m0-pins {
            rockchip,pins =
                /* pwm14_m0 */
                <3 RK_PC4 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pwm14m1_pins: pwm14m1-pins {
            rockchip,pins =
                /* pwm14_m1 */
                <4 RK_PC2 1 &pcfg_pull_none>;
        };
    };

    pwm15 {
        /omit-if-no-ref/
        pwm15m0_pins: pwm15m0-pins {
            rockchip,pins =
                /* pwm15_irm0 */
                <3 RK_PC5 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        pwm15m1_pins: pwm15m1-pins {
            rockchip,pins =
                /* pwm15_irm1 */
                <4 RK_PC3 1 &pcfg_pull_none>;
        };
    };

    refclk {
        /omit-if-no-ref/
        refclk_pins: refclk-pins {
            rockchip,pins =
                /* refclk_ou */
                <0 RK_PA0 1 &pcfg_pull_none>;
        };
    };

    sata {
        /omit-if-no-ref/
        sata_pins: sata-pins {
            rockchip,pins =
                /* sata_cpdet */
                <0 RK_PA4 2 &pcfg_pull_none>,
                /* sata_cppod */
                <0 RK_PA6 1 &pcfg_pull_none>,
                /* sata_mpswitch */
                <0 RK_PA5 2 &pcfg_pull_none>;
        };
    };

    sata0 {
        /omit-if-no-ref/
        sata0_pins: sata0-pins {
            rockchip,pins =
                /* sata0_actled */
                <4 RK_PC6 3 &pcfg_pull_none>;
        };
    };

    sata1 {
        /omit-if-no-ref/
        sata1_pins: sata1-pins {
            rockchip,pins =
                /* sata1_actled */
                <4 RK_PC5 3 &pcfg_pull_none>;
        };
    };

    sata2 {
        /omit-if-no-ref/
        sata2_pins: sata2-pins {
            rockchip,pins =
                /* sata2_actled */
                <4 RK_PC4 3 &pcfg_pull_none>;
        };
    };

    scr {
        /omit-if-no-ref/
        scr_pins: scr-pins {
            rockchip,pins =
                /* scr_clk */
                <1 RK_PA2 3 &pcfg_pull_none>,
                /* scr_det */
                <1 RK_PA7 3 &pcfg_pull_up>,
                /* scr_io */
                <1 RK_PA3 3 &pcfg_pull_up>,
                /* scr_rst */
                <1 RK_PA5 3 &pcfg_pull_none>;
        };
    };

    sdmmc0 {
        /omit-if-no-ref/
        sdmmc0_bus4: sdmmc0-bus4 {
            rockchip,pins =
                /* sdmmc0_d0 */
                <1 RK_PD5 1 &pcfg_pull_up_drv_level_2>,
                /* sdmmc0_d1 */
                <1 RK_PD6 1 &pcfg_pull_up_drv_level_2>,
                /* sdmmc0_d2 */
                <1 RK_PD7 1 &pcfg_pull_up_drv_level_2>,
                /* sdmmc0_d3 */
                <2 RK_PA0 1 &pcfg_pull_up_drv_level_2>;
        };

        /omit-if-no-ref/
        sdmmc0_clk: sdmmc0-clk {
            rockchip,pins =
                /* sdmmc0_clk */
                <2 RK_PA2 1 &pcfg_pull_up_drv_level_2>;
        };

        /omit-if-no-ref/
        sdmmc0_cmd: sdmmc0-cmd {
            rockchip,pins =
                /* sdmmc0_cmd */
                <2 RK_PA1 1 &pcfg_pull_up_drv_level_2>;
        };

        /omit-if-no-ref/
        sdmmc0_det: sdmmc0-det {
            rockchip,pins =
                /* sdmmc0_det */
                <0 RK_PA4 1 &pcfg_pull_up>;
        };

        /omit-if-no-ref/
        sdmmc0_pwren: sdmmc0-pwren {
            rockchip,pins =
                /* sdmmc0_pwren */
                <0 RK_PA5 1 &pcfg_pull_none>;
        };
    };

    sdmmc1 {
        /omit-if-no-ref/
        sdmmc1_bus4: sdmmc1-bus4 {
            rockchip,pins =
                /* sdmmc1_d0 */
                <2 RK_PA3 1 &pcfg_pull_up_drv_level_2>,
                /* sdmmc1_d1 */
                <2 RK_PA4 1 &pcfg_pull_up_drv_level_2>,
                /* sdmmc1_d2 */
                <2 RK_PA5 1 &pcfg_pull_up_drv_level_2>,
                /* sdmmc1_d3 */
                <2 RK_PA6 1 &pcfg_pull_up_drv_level_2>;
        };

        /omit-if-no-ref/
        sdmmc1_clk: sdmmc1-clk {
            rockchip,pins =
                /* sdmmc1_clk */
                <2 RK_PB0 1 &pcfg_pull_up_drv_level_2>;
        };

        /omit-if-no-ref/
        sdmmc1_cmd: sdmmc1-cmd {
            rockchip,pins =
                /* sdmmc1_cmd */
                <2 RK_PA7 1 &pcfg_pull_up_drv_level_2>;
        };

        /omit-if-no-ref/
        sdmmc1_det: sdmmc1-det {
            rockchip,pins =
                /* sdmmc1_det */
                <2 RK_PB2 1 &pcfg_pull_up>;
        };

        /omit-if-no-ref/
        sdmmc1_pwren: sdmmc1-pwren {
            rockchip,pins =
                /* sdmmc1_pwren */
                <2 RK_PB1 1 &pcfg_pull_none>;
        };
    };

    sdmmc2 {
        /omit-if-no-ref/
        sdmmc2m0_bus4: sdmmc2m0-bus4 {
            rockchip,pins =
                /* sdmmc2_d0m0 */
                <3 RK_PC6 3 &pcfg_pull_up_drv_level_2>,
                /* sdmmc2_d1m0 */
                <3 RK_PC7 3 &pcfg_pull_up_drv_level_2>,
                /* sdmmc2_d2m0 */
                <3 RK_PD0 3 &pcfg_pull_up_drv_level_2>,
                /* sdmmc2_d3m0 */
                <3 RK_PD1 3 &pcfg_pull_up_drv_level_2>;
        };

        /omit-if-no-ref/
        sdmmc2m0_clk: sdmmc2m0-clk {
            rockchip,pins =
                /* sdmmc2_clkm0 */
                <3 RK_PD3 3 &pcfg_pull_up_drv_level_2>;
        };

        /omit-if-no-ref/
        sdmmc2m0_cmd: sdmmc2m0-cmd {
            rockchip,pins =
                /* sdmmc2_cmdm0 */
                <3 RK_PD2 3 &pcfg_pull_up_drv_level_2>;
        };

        /omit-if-no-ref/
        sdmmc2m0_det: sdmmc2m0-det {
            rockchip,pins =
                /* sdmmc2_detm0 */
                <3 RK_PD4 3 &pcfg_pull_up>;
        };

        /omit-if-no-ref/
        sdmmc2m0_pwren: sdmmc2m0-pwren {
            rockchip,pins =
                /* sdmmc2m0_pwren */
                <3 RK_PD5 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        sdmmc2m1_bus4: sdmmc2m1-bus4 {
            rockchip,pins =
                /* sdmmc2_d0m1 */
                <3 RK_PA1 5 &pcfg_pull_up_drv_level_2>,
                /* sdmmc2_d1m1 */
                <3 RK_PA2 5 &pcfg_pull_up_drv_level_2>,
                /* sdmmc2_d2m1 */
                <3 RK_PA3 5 &pcfg_pull_up_drv_level_2>,
                /* sdmmc2_d3m1 */
                <3 RK_PA4 5 &pcfg_pull_up_drv_level_2>;
        };

        /omit-if-no-ref/
        sdmmc2m1_clk: sdmmc2m1-clk {
            rockchip,pins =
                /* sdmmc2_clkm1 */
                <3 RK_PA6 5 &pcfg_pull_up_drv_level_2>;
        };

        /omit-if-no-ref/
        sdmmc2m1_cmd: sdmmc2m1-cmd {
            rockchip,pins =
                /* sdmmc2_cmdm1 */
                <3 RK_PA5 5 &pcfg_pull_up_drv_level_2>;
        };

        /omit-if-no-ref/
        sdmmc2m1_det: sdmmc2m1-det {
            rockchip,pins =
                /* sdmmc2_detm1 */
                <3 RK_PA7 4 &pcfg_pull_up>;
        };

        /omit-if-no-ref/
        sdmmc2m1_pwren: sdmmc2m1-pwren {
            rockchip,pins =
                /* sdmmc2m1_pwren */
                <3 RK_PB0 4 &pcfg_pull_none>;
        };
    };

    spdif {
        /omit-if-no-ref/
        spdifm0_tx: spdifm0-tx {
            rockchip,pins =
                /* spdifm0_tx */
                <1 RK_PA4 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        spdifm1_tx: spdifm1-tx {
            rockchip,pins =
                /* spdifm1_tx */
                <3 RK_PC5 2 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        spdifm2_tx: spdifm2-tx {
            rockchip,pins =
                /* spdifm2_tx */
                <4 RK_PC4 2 &pcfg_pull_none>;
        };
    };

    spi0 {
        /omit-if-no-ref/
        spi0m0_pins: spi0m0-pins {
            rockchip,pins =
                /* spi0_clkm0 */
                <0 RK_PB5 2 &pcfg_pull_none>,
                /* spi0_misom0 */
                <0 RK_PC5 2 &pcfg_pull_none>,
                /* spi0_mosim0 */
                <0 RK_PB6 2 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        spi0m0_cs0: spi0m0-cs0 {
            rockchip,pins =
                /* spi0_cs0m0 */
                <0 RK_PC6 2 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        spi0m0_cs1: spi0m0-cs1 {
            rockchip,pins =
                /* spi0_cs1m0 */
                <0 RK_PC4 2 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        spi0m1_pins: spi0m1-pins {
            rockchip,pins =
                /* spi0_clkm1 */
                <2 RK_PD3 3 &pcfg_pull_none>,
                /* spi0_misom1 */
                <2 RK_PD0 3 &pcfg_pull_none>,
                /* spi0_mosim1 */
                <2 RK_PD1 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        spi0m1_cs0: spi0m1-cs0 {
            rockchip,pins =
                /* spi0_cs0m1 */
                <2 RK_PD2 3 &pcfg_pull_none>;
        };
    };

    spi1 {
        /omit-if-no-ref/
        spi1m0_pins: spi1m0-pins {
            rockchip,pins =
                /* spi1_clkm0 */
                <2 RK_PB5 3 &pcfg_pull_none>,
                /* spi1_misom0 */
                <2 RK_PB6 3 &pcfg_pull_none>,
                /* spi1_mosim0 */
                <2 RK_PB7 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        spi1m0_cs0: spi1m0-cs0 {
            rockchip,pins =
                /* spi1_cs0m0 */
                <2 RK_PC0 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        spi1m0_cs1: spi1m0-cs1 {
            rockchip,pins =
                /* spi1_cs1m0 */
                <2 RK_PC6 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        spi1m1_pins: spi1m1-pins {
            rockchip,pins =
                /* spi1_clkm1 */
                <3 RK_PC3 3 &pcfg_pull_none>,
                /* spi1_misom1 */
                <3 RK_PC2 3 &pcfg_pull_none>,
                /* spi1_mosim1 */
                <3 RK_PC1 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        spi1m1_cs0: spi1m1-cs0 {
            rockchip,pins =
                /* spi1_cs0m1 */
                <3 RK_PA1 3 &pcfg_pull_none>;
        };
    };

    spi2 {
        /omit-if-no-ref/
        spi2m0_pins: spi2m0-pins {
            rockchip,pins =
                /* spi2_clkm0 */
                <2 RK_PC1 4 &pcfg_pull_none>,
                /* spi2_misom0 */
                <2 RK_PC2 4 &pcfg_pull_none>,
                /* spi2_mosim0 */
                <2 RK_PC3 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        spi2m0_cs0: spi2m0-cs0 {
            rockchip,pins =
                /* spi2_cs0m0 */
                <2 RK_PC4 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        spi2m0_cs1: spi2m0-cs1 {
            rockchip,pins =
                /* spi2_cs1m0 */
                <2 RK_PC5 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        spi2m1_pins: spi2m1-pins {
            rockchip,pins =
                /* spi2_clkm1 */
                <3 RK_PA0 3 &pcfg_pull_none>,
                /* spi2_misom1 */
                <2 RK_PD7 3 &pcfg_pull_none>,
                /* spi2_mosim1 */
                <2 RK_PD6 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        spi2m1_cs0: spi2m1-cs0 {
            rockchip,pins =
                /* spi2_cs0m1 */
                <2 RK_PD5 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        spi2m1_cs1: spi2m1-cs1 {
            rockchip,pins =
                /* spi2_cs1m1 */
                <2 RK_PD4 3 &pcfg_pull_none>;
        };
    };

    spi3 {
        /omit-if-no-ref/
        spi3m0_pins: spi3m0-pins {
            rockchip,pins =
                /* spi3_clkm0 */
                <4 RK_PB3 4 &pcfg_pull_none>,
                /* spi3_misom0 */
                <4 RK_PB0 4 &pcfg_pull_none>,
                /* spi3_mosim0 */
                <4 RK_PB2 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        spi3m0_cs0: spi3m0-cs0 {
            rockchip,pins =
                /* spi3_cs0m0 */
                <4 RK_PA6 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        spi3m0_cs1: spi3m0-cs1 {
            rockchip,pins =
                /* spi3_cs1m0 */
                <4 RK_PA7 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        spi3m1_pins: spi3m1-pins {
            rockchip,pins =
                /* spi3_clkm1 */
                <4 RK_PC2 2 &pcfg_pull_none>,
                /* spi3_misom1 */
                <4 RK_PC5 2 &pcfg_pull_none>,
                /* spi3_mosim1 */
                <4 RK_PC3 2 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        spi3m1_cs0: spi3m1-cs0 {
            rockchip,pins =
                /* spi3_cs0m1 */
                <4 RK_PC6 2 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        spi3m1_cs1: spi3m1-cs1 {
            rockchip,pins =
                /* spi3_cs1m1 */
                <4 RK_PD1 2 &pcfg_pull_none>;
        };
    };

    tsadc {
        /omit-if-no-ref/
        tsadcm0_shut: tsadcm0-shut {
            rockchip,pins =
                /* tsadcm0_shut */
                <0 RK_PA1 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        tsadcm1_shut: tsadcm1-shut {
            rockchip,pins =
                /* tsadcm1_shut */
                <0 RK_PA2 2 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        tsadc_shutorg: tsadc-shutorg {
            rockchip,pins =
                /* tsadc_shutorg */
                <0 RK_PA1 2 &pcfg_pull_none>;
        };
    };

    uart0 {
        /omit-if-no-ref/
        uart0_xfer: uart0-xfer {
            rockchip,pins =
                /* uart0_rx */
                <0 RK_PC0 3 &pcfg_pull_up>,
                /* uart0_tx */
                <0 RK_PC1 3 &pcfg_pull_up>;
        };

        /omit-if-no-ref/
        uart0_ctsn: uart0-ctsn {
            rockchip,pins =
                /* uart0_ctsn */
                <0 RK_PC7 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        uart0_rtsn: uart0-rtsn {
            rockchip,pins =
                /* uart0_rtsn */
                <0 RK_PC4 3 &pcfg_pull_none>;
        };
    };

    uart1 {
        /omit-if-no-ref/
        uart1m0_xfer: uart1m0-xfer {
            rockchip,pins =
                /* uart1_rxm0 */
                <2 RK_PB3 2 &pcfg_pull_up>,
                /* uart1_txm0 */
                <2 RK_PB4 2 &pcfg_pull_up>;
        };

        /omit-if-no-ref/
        uart1m0_ctsn: uart1m0-ctsn {
            rockchip,pins =
                /* uart1m0_ctsn */
                <2 RK_PB6 2 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        uart1m0_rtsn: uart1m0-rtsn {
            rockchip,pins =
                /* uart1m0_rtsn */
                <2 RK_PB5 2 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        uart1m1_xfer: uart1m1-xfer {
            rockchip,pins =
                /* uart1_rxm1 */
                <3 RK_PD7 4 &pcfg_pull_up>,
                /* uart1_txm1 */
                <3 RK_PD6 4 &pcfg_pull_up>;
        };

        /omit-if-no-ref/
        uart1m1_ctsn: uart1m1-ctsn {
            rockchip,pins =
                /* uart1m1_ctsn */
                <4 RK_PC1 4 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        uart1m1_rtsn: uart1m1-rtsn {
            rockchip,pins =
                /* uart1m1_rtsn */
                <4 RK_PB6 4 &pcfg_pull_none>;
        };
    };

    uart2 {
        /omit-if-no-ref/
        uart2m0_xfer: uart2m0-xfer {
            rockchip,pins =
                /* uart2_rxm0 */
                <0 RK_PD0 1 &pcfg_pull_up>,
                /* uart2_txm0 */
                <0 RK_PD1 1 &pcfg_pull_up>;
        };

        /omit-if-no-ref/
        uart2m1_xfer: uart2m1-xfer {
            rockchip,pins =
                /* uart2_rxm1 */
                <1 RK_PD6 2 &pcfg_pull_up>,
                /* uart2_txm1 */
                <1 RK_PD5 2 &pcfg_pull_up>;
        };
    };

    uart3 {
        /omit-if-no-ref/
        uart3m0_xfer: uart3m0-xfer {
            rockchip,pins =
                /* uart3_rxm0 */
                <1 RK_PA0 2 &pcfg_pull_up>,
                /* uart3_txm0 */
                <1 RK_PA1 2 &pcfg_pull_up>;
        };

        /omit-if-no-ref/
        uart3m0_ctsn: uart3m0-ctsn {
            rockchip,pins =
                /* uart3m0_ctsn */
                <1 RK_PA3 2 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        uart3m0_rtsn: uart3m0-rtsn {
            rockchip,pins =
                /* uart3m0_rtsn */
                <1 RK_PA2 2 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        uart3m1_xfer: uart3m1-xfer {
            rockchip,pins =
                /* uart3_rxm1 */
                <3 RK_PC0 4 &pcfg_pull_up>,
                /* uart3_txm1 */
                <3 RK_PB7 4 &pcfg_pull_up>;
        };
    };

    uart4 {
        /omit-if-no-ref/
        uart4m0_xfer: uart4m0-xfer {
            rockchip,pins =
                /* uart4_rxm0 */
                <1 RK_PA4 2 &pcfg_pull_up>,
                /* uart4_txm0 */
                <1 RK_PA6 2 &pcfg_pull_up>;
        };

        /omit-if-no-ref/
        uart4m0_ctsn: uart4m0-ctsn {
            rockchip,pins =
                /* uart4m0_ctsn */
                <1 RK_PA7 2 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        uart4m0_rtsn: uart4m0-rtsn {
            rockchip,pins =
                /* uart4m0_rtsn */
                <1 RK_PA5 2 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        uart4m1_xfer: uart4m1-xfer {
            rockchip,pins =
                /* uart4_rxm1 */
                <3 RK_PB1 4 &pcfg_pull_up>,
                /* uart4_txm1 */
                <3 RK_PB2 4 &pcfg_pull_up>;
        };
    };

    uart5 {
        /omit-if-no-ref/
        uart5m0_xfer: uart5m0-xfer {
            rockchip,pins =
                /* uart5_rxm0 */
                <2 RK_PA1 3 &pcfg_pull_up>,
                /* uart5_txm0 */
                <2 RK_PA2 3 &pcfg_pull_up>;
        };

        /omit-if-no-ref/
        uart5m0_ctsn: uart5m0-ctsn {
            rockchip,pins =
                /* uart5m0_ctsn */
                <1 RK_PD7 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        uart5m0_rtsn: uart5m0-rtsn {
            rockchip,pins =
                /* uart5m0_rtsn */
                <2 RK_PA0 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        uart5m1_xfer: uart5m1-xfer {
            rockchip,pins =
                /* uart5_rxm1 */
                <3 RK_PC3 4 &pcfg_pull_up>,
                /* uart5_txm1 */
                <3 RK_PC2 4 &pcfg_pull_up>;
        };
    };

    uart6 {
        /omit-if-no-ref/
        uart6m0_xfer: uart6m0-xfer {
            rockchip,pins =
                /* uart6_rxm0 */
                <2 RK_PA3 3 &pcfg_pull_up>,
                /* uart6_txm0 */
                <2 RK_PA4 3 &pcfg_pull_up>;
        };

        /omit-if-no-ref/
        uart6m0_ctsn: uart6m0-ctsn {
            rockchip,pins =
                /* uart6m0_ctsn */
                <2 RK_PC0 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        uart6m0_rtsn: uart6m0-rtsn {
            rockchip,pins =
                /* uart6m0_rtsn */
                <2 RK_PB7 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        uart6m1_xfer: uart6m1-xfer {
            rockchip,pins =
                /* uart6_rxm1 */
                <1 RK_PD6 3 &pcfg_pull_up>,
                /* uart6_txm1 */
                <1 RK_PD5 3 &pcfg_pull_up>;
        };
    };

    uart7 {
        /omit-if-no-ref/
        uart7m0_xfer: uart7m0-xfer {
            rockchip,pins =
                /* uart7_rxm0 */
                <2 RK_PA5 3 &pcfg_pull_up>,
                /* uart7_txm0 */
                <2 RK_PA6 3 &pcfg_pull_up>;
        };

        /omit-if-no-ref/
        uart7m0_ctsn: uart7m0-ctsn {
            rockchip,pins =
                /* uart7m0_ctsn */
                <2 RK_PC2 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        uart7m0_rtsn: uart7m0-rtsn {
            rockchip,pins =
                /* uart7m0_rtsn */
                <2 RK_PC1 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        uart7m1_xfer: uart7m1-xfer {
            rockchip,pins =
                /* uart7_rxm1 */
                <3 RK_PC5 4 &pcfg_pull_up>,
                /* uart7_txm1 */
                <3 RK_PC4 4 &pcfg_pull_up>;
        };

        /omit-if-no-ref/
        uart7m2_xfer: uart7m2-xfer {
            rockchip,pins =
                /* uart7_rxm2 */
                <4 RK_PA3 4 &pcfg_pull_up>,
                /* uart7_txm2 */
                <4 RK_PA2 4 &pcfg_pull_up>;
        };
    };

    uart8 {
        /omit-if-no-ref/
        uart8m0_xfer: uart8m0-xfer {
            rockchip,pins =
                /* uart8_rxm0 */
                <2 RK_PC6 2 &pcfg_pull_up>,
                /* uart8_txm0 */
                <2 RK_PC5 3 &pcfg_pull_up>;
        };

        /omit-if-no-ref/
        uart8m0_ctsn: uart8m0-ctsn {
            rockchip,pins =
                /* uart8m0_ctsn */
                <2 RK_PB2 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        uart8m0_rtsn: uart8m0-rtsn {
            rockchip,pins =
                /* uart8m0_rtsn */
                <2 RK_PB1 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        uart8m1_xfer: uart8m1-xfer {
            rockchip,pins =
                /* uart8_rxm1 */
                <3 RK_PA0 4 &pcfg_pull_up>,
                /* uart8_txm1 */
                <2 RK_PD7 4 &pcfg_pull_up>;
        };
    };

    uart9 {
        /omit-if-no-ref/
        uart9m0_xfer: uart9m0-xfer {
            rockchip,pins =
                /* uart9_rxm0 */
                <2 RK_PA7 3 &pcfg_pull_up>,
                /* uart9_txm0 */
                <2 RK_PB0 3 &pcfg_pull_up>;
        };

        /omit-if-no-ref/
        uart9m0_ctsn: uart9m0-ctsn {
            rockchip,pins =
                /* uart9m0_ctsn */
                <2 RK_PC4 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        uart9m0_rtsn: uart9m0-rtsn {
            rockchip,pins =
                /* uart9m0_rtsn */
                <2 RK_PC3 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        uart9m1_xfer: uart9m1-xfer {
            rockchip,pins =
                /* uart9_rxm1 */
                <4 RK_PC6 4 &pcfg_pull_up>,
                /* uart9_txm1 */
                <4 RK_PC5 4 &pcfg_pull_up>;
        };

        /omit-if-no-ref/
        uart9m2_xfer: uart9m2-xfer {
            rockchip,pins =
                /* uart9_rxm2 */
                <4 RK_PA5 4 &pcfg_pull_up>,
                /* uart9_txm2 */
                <4 RK_PA4 4 &pcfg_pull_up>;
        };
    };

    vop {
        /omit-if-no-ref/
        vopm0_pins: vopm0-pins {
            rockchip,pins =
                /* vop_pwmm0 */
                <0 RK_PC3 2 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        vopm1_pins: vopm1-pins {
            rockchip,pins =
                /* vop_pwmm1 */
                <3 RK_PC4 2 &pcfg_pull_none>;
        };
    };
};

/*
 * This part is edited handly.
 */
&pinctrl {
    spi0-hs {
        /omit-if-no-ref/
        spi0m0_pins_hs: spi0m0-pins {
            rockchip,pins =
                /* spi0_clkm0 */
                <0 RK_PB5 2 &pcfg_pull_up_drv_level_1>,
                /* spi0_misom0 */
                <0 RK_PC5 2 &pcfg_pull_up_drv_level_1>,
                /* spi0_mosim0 */
                <0 RK_PB6 2 &pcfg_pull_up_drv_level_1>;
        };

        /omit-if-no-ref/
        spi0m0_cs0_hs: spi0m0-cs0 {
            rockchip,pins =
                /* spi0_cs0m0 */
                <0 RK_PC6 2 &pcfg_pull_up_drv_level_1>;
        };

        /omit-if-no-ref/
        spi0m0_cs1_hs: spi0m0-cs1 {
            rockchip,pins =
                /* spi0_cs1m0 */
                <0 RK_PC4 2 &pcfg_pull_up_drv_level_1>;
        };

        /omit-if-no-ref/
        spi0m1_pins_hs: spi0m1-pins {
            rockchip,pins =
                /* spi0_clkm1 */
                <2 RK_PD3 3 &pcfg_pull_up_drv_level_1>,
                /* spi0_misom1 */
                <2 RK_PD0 3 &pcfg_pull_up_drv_level_1>,
                /* spi0_mosim1 */
                <2 RK_PD1 3 &pcfg_pull_up_drv_level_1>;
        };

        /omit-if-no-ref/
        spi0m1_cs0_hs: spi0m1-cs0 {
            rockchip,pins =
                /* spi0_cs0m1 */
                <2 RK_PD2 3 &pcfg_pull_up_drv_level_1>;
        };
    };

    spi1-hs {
        /omit-if-no-ref/
        spi1m0_pins_hs: spi1m0-pins {
            rockchip,pins =
                /* spi1_clkm0 */
                <2 RK_PB5 3 &pcfg_pull_up_drv_level_1>,
                /* spi1_misom0 */
                <2 RK_PB6 3 &pcfg_pull_up_drv_level_1>,
                /* spi1_mosim0 */
                <2 RK_PB7 4 &pcfg_pull_up_drv_level_1>;
        };

        /omit-if-no-ref/
        spi1m0_cs0_hs: spi1m0-cs0 {
            rockchip,pins =
                /* spi1_cs0m0 */
                <2 RK_PC0 4 &pcfg_pull_up_drv_level_1>;
        };

        /omit-if-no-ref/
        spi1m0_cs1_hs: spi1m0-cs1 {
            rockchip,pins =
                /* spi1_cs1m0 */
                <2 RK_PC6 3 &pcfg_pull_up_drv_level_1>;
        };

        /omit-if-no-ref/
        spi1m1_pins_hs: spi1m1-pins {
            rockchip,pins =
                /* spi1_clkm1 */
                <3 RK_PC3 3 &pcfg_pull_up_drv_level_1>,
                /* spi1_misom1 */
                <3 RK_PC2 3 &pcfg_pull_up_drv_level_1>,
                /* spi1_mosim1 */
                <3 RK_PC1 3 &pcfg_pull_up_drv_level_1>;
        };

        /omit-if-no-ref/
        spi1m1_cs0_hs: spi1m1-cs0 {
            rockchip,pins =
                /* spi1_cs0m1 */
                <3 RK_PA1 3 &pcfg_pull_up_drv_level_1>;
        };
    };

    spi2-hs {
        /omit-if-no-ref/
        spi2m0_pins_hs: spi2m0-pins {
            rockchip,pins =
                /* spi2_clkm0 */
                <2 RK_PC1 4 &pcfg_pull_up_drv_level_1>,
                /* spi2_misom0 */
                <2 RK_PC2 4 &pcfg_pull_up_drv_level_1>,
                /* spi2_mosim0 */
                <2 RK_PC3 4 &pcfg_pull_up_drv_level_1>;
        };

        /omit-if-no-ref/
        spi2m0_cs0_hs: spi2m0-cs0 {
            rockchip,pins =
                /* spi2_cs0m0 */
                <2 RK_PC4 4 &pcfg_pull_up_drv_level_1>;
        };

        /omit-if-no-ref/
        spi2m0_cs1_hs: spi2m0-cs1 {
            rockchip,pins =
                /* spi2_cs1m0 */
                <2 RK_PC5 4 &pcfg_pull_up_drv_level_1>;
        };

        /omit-if-no-ref/
        spi2m1_pins_hs: spi2m1-pins {
            rockchip,pins =
                /* spi2_clkm1 */
                <3 RK_PA0 3 &pcfg_pull_up_drv_level_1>,
                /* spi2_misom1 */
                <2 RK_PD7 3 &pcfg_pull_up_drv_level_1>,
                /* spi2_mosim1 */
                <2 RK_PD6 3 &pcfg_pull_up_drv_level_1>;
        };

        /omit-if-no-ref/
        spi2m1_cs0_hs: spi2m1-cs0 {
            rockchip,pins =
                /* spi2_cs0m1 */
                <2 RK_PD5 3 &pcfg_pull_up_drv_level_1>;
        };

        /omit-if-no-ref/
        spi2m1_cs1_hs: spi2m1-cs1 {
            rockchip,pins =
                /* spi2_cs1m1 */
                <2 RK_PD4 3 &pcfg_pull_up_drv_level_1>;
        };
    };

    spi3-hs {
        /omit-if-no-ref/
        spi3m0_pins_hs: spi3m0-pins {
            rockchip,pins =
                /* spi3_clkm0 */
                <4 RK_PB3 4 &pcfg_pull_up_drv_level_1>,
                /* spi3_misom0 */
                <4 RK_PB0 4 &pcfg_pull_up_drv_level_1>,
                /* spi3_mosim0 */
                <4 RK_PB2 4 &pcfg_pull_up_drv_level_1>;
        };

        /omit-if-no-ref/
        spi3m0_cs0_hs: spi3m0-cs0 {
            rockchip,pins =
                /* spi3_cs0m0 */
                <4 RK_PA6 4 &pcfg_pull_up_drv_level_1>;
        };

        /omit-if-no-ref/
        spi3m0_cs1_hs: spi3m0-cs1 {
            rockchip,pins =
                /* spi3_cs1m0 */
                <4 RK_PA7 4 &pcfg_pull_up_drv_level_1>;
        };

        /omit-if-no-ref/
        spi3m1_pins_hs: spi3m1-pins {
            rockchip,pins =
                /* spi3_clkm1 */
                <4 RK_PC2 2 &pcfg_pull_up_drv_level_1>,
                /* spi3_misom1 */
                <4 RK_PC5 2 &pcfg_pull_up_drv_level_1>,
                /* spi3_mosim1 */
                <4 RK_PC3 2 &pcfg_pull_up_drv_level_1>;
        };

        /omit-if-no-ref/
        spi3m1_cs0_hs: spi3m1-cs0 {
            rockchip,pins =
                /* spi3_cs0m1 */
                <4 RK_PC6 2 &pcfg_pull_up_drv_level_1>;
        };

        /omit-if-no-ref/
        spi3m1_cs1_hs: spi3m1-cs1 {
            rockchip,pins =
                /* spi3_cs1m1 */
                <4 RK_PD1 2 &pcfg_pull_up_drv_level_1>;
        };
    };

    gmac-txd-level3 {
        /omit-if-no-ref/
        gmac0_tx_bus2_level3: gmac0-tx-bus2-level3 {
            rockchip,pins =
                /* gmac0_txd0 */
                <2 RK_PB3 1 &pcfg_pull_none_drv_level_3>,
                /* gmac0_txd1 */
                <2 RK_PB4 1 &pcfg_pull_none_drv_level_3>,
                /* gmac0_txen */
                <2 RK_PB5 1 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        gmac0_rgmii_bus_level3: gmac0-rgmii-bus-level3 {
            rockchip,pins =
                /* gmac0_rxd2 */
                <2 RK_PA3 2 &pcfg_pull_none>,
                /* gmac0_rxd3 */
                <2 RK_PA4 2 &pcfg_pull_none>,
                /* gmac0_txd2 */
                <2 RK_PA6 2 &pcfg_pull_none_drv_level_3>,
                /* gmac0_txd3 */
                <2 RK_PA7 2 &pcfg_pull_none_drv_level_3>;
        };

        /omit-if-no-ref/
        gmac1m0_tx_bus2_level3: gmac1m0-tx-bus2-level3 {
            rockchip,pins =
                /* gmac1_txd0m0 */
                <3 RK_PB5 3 &pcfg_pull_none_drv_level_3>,
                /* gmac1_txd1m0 */
                <3 RK_PB6 3 &pcfg_pull_none_drv_level_3>,
                /* gmac1_txenm0 */
                <3 RK_PB7 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        gmac1m0_rgmii_bus_level3: gmac1m0-rgmii-bus-level3 {
            rockchip,pins =
                /* gmac1_rxd2m0 */
                <3 RK_PA4 3 &pcfg_pull_none>,
                /* gmac1_rxd3m0 */
                <3 RK_PA5 3 &pcfg_pull_none>,
                /* gmac1_txd2m0 */
                <3 RK_PA2 3 &pcfg_pull_none_drv_level_3>,
                /* gmac1_txd3m0 */
                <3 RK_PA3 3 &pcfg_pull_none_drv_level_3>;
        };

        /omit-if-no-ref/
        gmac1m1_tx_bus2_level3: gmac1m1-tx-bus2-level3 {
            rockchip,pins =
                /* gmac1_txd0m1 */
                <4 RK_PA4 3 &pcfg_pull_none_drv_level_3>,
                /* gmac1_txd1m1 */
                <4 RK_PA5 3 &pcfg_pull_none_drv_level_3>,
                /* gmac1_txenm1 */
                <4 RK_PA6 3 &pcfg_pull_none>;
        };

        /omit-if-no-ref/
        gmac1m1_rgmii_bus_level3: gmac1m1-rgmii-bus-level3 {
            rockchip,pins =
                /* gmac1_rxd2m1 */
                <4 RK_PA1 3 &pcfg_pull_none>,
                /* gmac1_rxd3m1 */
                <4 RK_PA2 3 &pcfg_pull_none>,
                /* gmac1_txd2m1 */
                <3 RK_PD6 3 &pcfg_pull_none_drv_level_3>,
                /* gmac1_txd3m1 */
                <3 RK_PD7 3 &pcfg_pull_none_drv_level_3>;
        };
    };

    gmac-txc-level2 {
        /omit-if-no-ref/
        gmac0_rgmii_clk_level2: gmac0-rgmii-clk-level2 {
            rockchip,pins =
                /* gmac0_rxclk */
                <2 RK_PA5 2 &pcfg_pull_none>,
                /* gmac0_txclk */
                <2 RK_PB0 2 &pcfg_pull_none_drv_level_2>;
        };

        /omit-if-no-ref/
        gmac1m0_rgmii_clk_level2: gmac1m0-rgmii-clk-level2 {
            rockchip,pins =
                /* gmac1_rxclkm0 */
                <3 RK_PA7 3 &pcfg_pull_none>,
                /* gmac1_txclkm0 */
                <3 RK_PA6 3 &pcfg_pull_none_drv_level_2>;
        };

        /omit-if-no-ref/
        gmac1m1_rgmii_clk_level2: gmac1m1-rgmii-clk-level2 {
            rockchip,pins =
                /* gmac1_rxclkm1 */
                <4 RK_PA3 3 &pcfg_pull_none>,
                /* gmac1_txclkm1 */
                <4 RK_PA0 3 &pcfg_pull_none_drv_level_2>;
        };
    };

    gpio-func {
        /omit-if-no-ref/
        tsadc_gpio_func: tsadc-gpio-func {
            rockchip,pins =
                <0 RK_PA1 RK_FUNC_GPIO &pcfg_pull_none>;
        };
    };
};
